**Command Line Operation**

New 4Port/8Port/16Port/Plug-in 16Port OLT

Contents

[1. Read Instructions 24](#_Toc96881543)

[Document Scope 24](#_Toc96881544)

[Revision History 24](#_Toc96881545)

[Conventions for Command Line 24](#_Toc96881546)

[Conventions for Keyboard Operation 25](#_Toc96881547)

[Conventions for symbols 25](#_Toc96881548)

[Conventions for Words 26](#_Toc96881549)

[Precautions 26](#_Toc96881550)

[2. Command Line Interface View Introduce 27](#_Toc96881551)

[2.1. Command Line View Overview 28](#_Toc96881552)

[2.1.1. Enter Enable View 29](#_Toc96881553)

[2.1.2. Enter Config View 29](#_Toc96881554)

[2.1.3. Enter Interface View 29](#_Toc96881555)

[2.1.4. Enter ACL View 31](#_Toc96881556)

[2.1.5. Enter Multicast-vlan View 32](#_Toc96881557)

[2.1.6. Exit Arbitrary View 32](#_Toc96881558)

[3. OLT Device Upgrade Management 34](#_Toc96881559)

[3.1. Upgrade OLT software 34](#_Toc96881560)

[3.2. Check OLT Software and Hardware Version 35](#_Toc96881561)

[3.3. Show the progress of current load/copy/backup in olt 35](#_Toc96881562)

[3.4. Delete Loaded Files 36](#_Toc96881563)

[3.5. Enable/disable web 37](#_Toc96881564)

[3.6. Uninstall the Installed Web 37](#_Toc96881565)

[4. OLT Device Management 38](#_Toc96881566)

[4.1. OLT Reboot 38](#_Toc96881567)

[4.2. Config OLT Reset Button 38](#_Toc96881568)

[4.3. Config OLT Outband Manager IP 39](#_Toc96881569)

[4.3.1. Config OLT Outband Manager IP Address 39](#_Toc96881570)

[4.3.2. Config OLT Outband Manager IP Description 39](#_Toc96881571)

[4.3.3. Delete OLT Outband Manager IP Configuration 40](#_Toc96881572)

[4.3.4. Config Switch OLT Outband Manager IP 40](#_Toc96881573)

[4.3.5. Show MGMT IP Address 41](#_Toc96881574)

[4.3.6. Exit to Config View 41](#_Toc96881575)

[4.3.7. Exit to View 42](#_Toc96881576)

[4.4. Config OLT Inband Vlanif IP 42](#_Toc96881577)

[4.4.1. Config OLT Inband Vlanif Address 42](#_Toc96881578)

[4.4.2. Config OLT Inband Manager IP Description 43](#_Toc96881579)

[4.4.3. Config OLT DHCP-Client Option 60 43](#_Toc96881580)

[4.4.4. Delete OLT Inband Manager IP Configuration 44](#_Toc96881581)

[4.4.5. Config Switch OLT Outband Manager IP 44](#_Toc96881582)

[4.4.6. Show Vlanif IP Address 45](#_Toc96881583)

[4.4.7. Exit to Config View 46](#_Toc96881584)

[4.4.8. Exit to View 46](#_Toc96881585)

[4.4.9. Clear Statistics Interface Vlanif 46](#_Toc96881586)

[4.5. Show OLT Detail Information 47](#_Toc96881587)

[4.6. Config OLT User Logout Time 47](#_Toc96881588)

[4.7. Show OLT User Logout Time 48](#_Toc96881589)

[4.8. Logout System 48](#_Toc96881590)

[4.9. Exit OLT Current View Mode 49](#_Toc96881591)

[4.10. Config OLT DNS server IP Address 49](#_Toc96881592)

[4.11. Delete OLT DNS Server IP Address 50](#_Toc96881593)

[4.12. Show OLT DNS Server IP Address 50](#_Toc96881594)

[4.13. Config OLT Hostname 50](#_Toc96881595)

[4.14. Enable/disable PON laser control 51](#_Toc96881596)

[4.15. Config a Remote System Host 51](#_Toc96881597)

[4.16. Config Terminal Output Printing 52](#_Toc96881598)

[5. OLT Status Monitor 53](#_Toc96881599)

[5.1. Show OLT Fan Working Status 53](#_Toc96881600)

[5.2. Show OLT Working Temperature 53](#_Toc96881601)

[5.3. Show OLT Memory Usage 54](#_Toc96881602)

[5.4. Config OLT System Time 54](#_Toc96881603)

[5.5. Show OLT System Time 55](#_Toc96881604)

[5.6. Show OLT Boot Time and Running Time 55](#_Toc96881605)

[5.7. Config OLT NTP Time and Server 55](#_Toc96881606)

[5.8. Delete NTP Time and Server 56](#_Toc96881607)

[5.9. Show NTP Server Session Information 56](#_Toc96881608)

[5.10. Config OLT Systme Timezone 57](#_Toc96881609)

[5.11. Show OLT System Current Timezone 57](#_Toc96881610)

[5.12. Config OLT System Temperature Threshold 58](#_Toc96881611)

[5.13. Show OLT System Temperature Threshold 58](#_Toc96881612)

[5.14. Show OLT Local MAC Address Information 59](#_Toc96881613)

[5.15. Show OLT CPU Usage 59](#_Toc96881614)

[5.16. Show OLT History Input Command 60](#_Toc96881615)

[5.17. Enable/disable loop detection for the OLT system 60](#_Toc96881616)

[5.18. Config the loop detection interval of the OLT system 61](#_Toc96881617)

[5.19. View the loop detection status of the OLT system 61](#_Toc96881618)

[5.20. Config the Maximum Recorded Value of Performance Statistics 63](#_Toc96881619)

[5.21. Show the Maximum Recorded Value of Performance Statistics 63](#_Toc96881620)

[6. OLT Configuration Manage 64](#_Toc96881621)

[6.1. Auto-backup OLT Configuration 64](#_Toc96881622)

[6.2. Autoback OLT Time Configuration 64](#_Toc96881623)

[6.3. Backup OLT Configuration 65](#_Toc96881624)

[6.4. Download OLT Configuration 65](#_Toc96881625)

[6.5. Show OLT Current Configuration 66](#_Toc96881626)

[6.6. Auto-save OLT Configuration 67](#_Toc96881627)

[6.7. Save OLT Configuration 68](#_Toc96881628)

[6.8. Erase OLT Configuration 68](#_Toc96881629)

[6.9. Show OLT Auto-back 69](#_Toc96881630)

[6.10. Show autosave configuration 69](#_Toc96881631)

[6.11. Show OLT Saved-config 70](#_Toc96881632)

[7. OLT Login User Manage 71](#_Toc96881633)

[7.1. Add OLT New Login Username and Password 71](#_Toc96881634)

[7.2. Delete OLT Login User 71](#_Toc96881635)

[7.3. Change OLT Login User Password 72](#_Toc96881636)

[7.4. Show OLT Exist Username 72](#_Toc96881637)

[7.5. Show OLT Login User Information 73](#_Toc96881638)

[7.6. Kill OLT Online User 73](#_Toc96881639)

[7.7. Config the specified address segment to log in to the OLT 74](#_Toc96881640)

[7.8. View IP access table configuration 75](#_Toc96881641)

[8. OLT SNMP Config 76](#_Toc96881642)

[8.1. SNMP Enable and Disable 76](#_Toc96881643)

[8.2. Show OLT Snmp Agent Status 76](#_Toc96881644)

[8.3. Config OLT SNMP Community 77](#_Toc96881645)

[8.4. Show OLT SNMP Read Community 77](#_Toc96881646)

[8.5. Config OLT SNMP Write Community 78](#_Toc96881647)

[8.6. Show SNMP Write Community 78](#_Toc96881648)

[8.7. Config OLT SNMP Community Group with Authentication 78](#_Toc96881649)

[8.8. Config OLT SNMP Community Group with Unauth 79](#_Toc96881650)

[8.9. Config OLT SNMP Community Group with Privacy 80](#_Toc96881651)

[8.10. Config OLT SNMP Agent Description 81](#_Toc96881652)

[8.11. Configure SNMP Agent Location Information 81](#_Toc96881653)

[8.12. Configure SNMP Agent Contact Infomation 82](#_Toc96881654)

[8.13. Configure Snmp Agent System Name 82](#_Toc96881655)

[8.14. Show SNMP Agent System Info 83](#_Toc96881656)

[8.15. Config SNMP Trap IP 83](#_Toc96881657)

[8.16. Show SNMP Trap IP Infor 84](#_Toc96881658)

[8.17. Config SNMP Access User&Auth Mode &Password 84](#_Toc96881659)

[8.18. Show SNMP Access User 85](#_Toc96881660)

[9. Config OLT PPPoE Agent 87](#_Toc96881661)

[9.1. PPPoE Agent Enable and Disable 87](#_Toc96881662)

[9.2. Config PPPoE Forward Policy 87](#_Toc96881663)

[9.3. Config PPPoE Fill Format 88](#_Toc96881664)

[9.4. Show the Configuration of the PPPoE Agent. 88](#_Toc96881665)

[10. OLT Uplink Port Configuration 90](#_Toc96881666)

[10.1. OLT Uplink Basic Function Configuration 90](#_Toc96881667)

[10.1.1. Disable Uplink Port 90](#_Toc96881668)

[10.1.2. Enable Uplink Port 90](#_Toc96881669)

[10.1.3. Config Uplink Port Name 91](#_Toc96881670)

[10.1.4. Delete Uplink Port Name 91](#_Toc96881671)

[10.1.5. Config Uplink Electric Port Auto-negotiation 92](#_Toc96881672)

[10.1.6. Config Uplink Electric Port Duplex Mode 93](#_Toc96881673)

[10.1.7. Config Uplink Electric Port Speed 93](#_Toc96881674)

[10.1.8. Config Uplink Port Max-frame 94](#_Toc96881675)

[10.1.9. Delete Uplink Port Maximum-frame 94](#_Toc96881676)

[10.1.10. Config Uplink Port Flow-control Function 95](#_Toc96881677)

[10.1.11. Config Uplink Port MAC Address Learning Function 95](#_Toc96881678)

[10.1.12. Show OLT Uplink Port Property and Statuses 96](#_Toc96881679)

[10.1.13. Show OLT Uplink Port Optical Power Information 97](#_Toc96881680)

[10.2. Uplink Port Mirror Manage 98](#_Toc96881681)

[10.2.1. Config Uplink Port Mirror Function 98](#_Toc96881682)

[10.2.2. Delete Uplink Port Mirror Function 99](#_Toc96881683)

[10.2.3. Show Uplink Port Mirror Configuration 99](#_Toc96881684)

[10.3. Uplink Port Performance Statistics Function 100](#_Toc96881685)

[10.3.1. Config Uplink Port Performance Statistics Threshold 100](#_Toc96881686)

[10.3.2. Show Uplink Port Performance Statistics Threshold 102](#_Toc96881687)

[10.3.3. Clear Uplink Port Performance Statistics Infor 102](#_Toc96881688)

[10.3.4. Config Uplink Port Performance Statistics Period 103](#_Toc96881689)

[10.3.5. Config Uplink Port Performance Statistics Period 24H 103](#_Toc96881690)

[10.3.6. Show Uplink Port Current 15min Performance Statistics 104](#_Toc96881691)

[10.3.7. Show Uplink Port Current 24Hs Performance Statistics 105](#_Toc96881692)

[10.3.8. Show Uplink Port History 15min Performance Statistics 106](#_Toc96881693)

[10.3.9. Show Uplink Port History 24H Performance Statistics 108](#_Toc96881694)

[10.4. Uplink Port Storm Control Function 108](#_Toc96881695)

[10.4.1. Config Uplink Port Broadcast Storm Control Function 108](#_Toc96881696)

[10.4.2. Config Uplink Port Unknown Multicast Storm Control Function 109](#_Toc96881697)

[10.4.3. Config Uplink Port Unknown Unicast Storm Control 110](#_Toc96881698)

[10.5. Uplink Port Rate Limit Function 110](#_Toc96881699)

[10.5.1. Config Uplink Port Upstream and Downstream Rate Limit 110](#_Toc96881700)

[10.5.2. Delete Uplink Port Upstream and Downstream Rate Limit 111](#_Toc96881701)

[10.5.3. Show Uplink Port Upstream and Downstream Rate Limit Configuration 111](#_Toc96881702)

[10.6. Uplink Port Isolate Function 112](#_Toc96881703)

[10.6.1. Config Uplink Port Isolate 112](#_Toc96881704)

[10.6.2. Show Uplink Port Isolation Configuration Infor 112](#_Toc96881705)

[10.7. Uplink Port RSTP Function 113](#_Toc96881706)

[10.7.1. Config Uplink Port RSTP Cost 113](#_Toc96881707)

[10.7.2. Config Uplink Port RSTP Edged-port 114](#_Toc96881708)

[10.7.3. Config Uplink Port RSTP Mcheck Property 114](#_Toc96881709)

[10.7.4. Config Uplink Port RSTP Point-to-Point Link Function 115](#_Toc96881710)

[10.7.5. Config Uplink Port RSTP Priority 116](#_Toc96881711)

[10.7.6. Delete Uplink Port Configuration of RTSP 116](#_Toc96881712)

[10.7.7. Show Uplink Port RSTP Configuration 117](#_Toc96881713)

[10.8. OLT Uplink Port VLAN Config 118](#_Toc96881714)

[10.8.1. Config Uplink Port VLAN Mode 118](#_Toc96881715)

[10.8.2. Config Uplink Port Native-vlan 118](#_Toc96881716)

[10.8.3. Config Uplink Port Native-vlan Priority 119](#_Toc96881717)

[10.8.4. Config Uplink Port Access Mode VLAN 119](#_Toc96881718)

[10.8.5. Config Uplink Port Hybrid Mode VLAN 120](#_Toc96881719)

[10.8.6. Delete Uplink Port Hybrid Mode VLAN 121](#_Toc96881720)

[10.8.7. Config Uplink Port Trunk Mode VLAN 121](#_Toc96881721)

[10.8.8. Delete Uplink Port Trunk Mode VLAN 122](#_Toc96881722)

[10.8.9. Config Uplink Port Translate Mode VLAN 122](#_Toc96881723)

[10.8.10. Delete Uplink Port Translate Mode VLAN 123](#_Toc96881724)

[10.8.11. Config Uplink Port Protocol VLAN 123](#_Toc96881725)

[10.8.12. Show OLT Uplink Port VLAN Configuration 124](#_Toc96881726)

[10.9. OLT Uplink Port Loopback Detection 125](#_Toc96881727)

[10.9.1. Config Uplink port Loopback Detection 125](#_Toc96881728)

[10.9.2. Config Uplink port Loopback Detection Control Function 125](#_Toc96881729)

[10.9.3. Config Uplink port Loopback Detection Per-vlan 126](#_Toc96881730)

[10.10. Config Uplink Port Protocol-vlan 127](#_Toc96881731)

[11. OLT PON Port Configuration 128](#_Toc96881732)

[11.1. OLT PON Port Property Config 128](#_Toc96881733)

[11.1.1. Disable PON Port 128](#_Toc96881734)

[11.1.2. Enable PON Port 128](#_Toc96881735)

[11.1.3. Config PON Port Name 129](#_Toc96881736)

[11.1.4. Delete PON Port Name 129](#_Toc96881737)

[11.1.5. Config PON Port MTU 130](#_Toc96881738)

[11.1.6. Delete PON Port Frame-max 130](#_Toc96881739)

[11.1.7. Config PON Port Encrypt Mode and Key-exchange-time 130](#_Toc96881740)

[11.1.8. Config PON Port Flow-control Function 131](#_Toc96881741)

[11.1.9. Config Pon Port MAC Address Learning Function 132](#_Toc96881742)

[11.1.10. Show OLT PON Port Property and Status 132](#_Toc96881743)

[11.1.11. Show OLT PON Port Optical Power Information 134](#_Toc96881744)

[11.2. Config OLT PON Port Detect ONU Long Laser Function 135](#_Toc96881745)

[11.2.1. Config Auto Detect ONU Long Laser Function 135](#_Toc96881746)

[11.2.2. Config Manual Detect ONU Long Laser Function 136](#_Toc96881747)

[11.2.3. Show Detect ONU Long Laser Configuration 136](#_Toc96881748)

[11.3. OLT PON Port RSTP Function 137](#_Toc96881749)

[11.3.1. Config OLT PON Port RSTP Cost 137](#_Toc96881750)

[11.3.2. Config OLT PON Port RSTP Edged-port 137](#_Toc96881751)

[11.3.3. Config OLT PON Port RSTP Mcheck Property 138](#_Toc96881752)

[11.3.4. Config OLT PON Port RSTP Point-to-Point Link Function 138](#_Toc96881753)

[11.3.5. Config OLT PON Port RSTP Priority 139](#_Toc96881754)

[11.3.6. Delete OLT PON Port Configuration of RTSP 140](#_Toc96881755)

[11.4. Config OLT PON Port Mirror Function 140](#_Toc96881756)

[11.4.1. Config Pon Port Mirror Function 140](#_Toc96881757)

[11.4.2. Delete PON　Port Mirror Function 141](#_Toc96881758)

[11.4.3. Show PON Port Mirror Configuration 142](#_Toc96881759)

[11.5. OLT PON Port Performance Statistics Function 142](#_Toc96881760)

[11.5.1. Config PON Port Performance Statistics Period 15min 142](#_Toc96881761)

[11.5.2. Config PON Port Performance Statistics Period 15H 143](#_Toc96881762)

[11.5.3. Config PON Port Performance Statistics Threshold 143](#_Toc96881763)

[11.5.4. Clear PON Port Performance Statistics Infor 145](#_Toc96881764)

[11.5.5. Show PON Port Current 15min Performance Statistics 145](#_Toc96881765)

[11.5.6. Show PON Port Current 24Hs Performance Statistics 146](#_Toc96881766)

[11.5.7. Show PON Port History 15min Performance Statistics 147](#_Toc96881767)

[11.5.8. Show PON Port History 24H Performance Statistics 150](#_Toc96881768)

[11.5.9. Show PON Port Performance Statistics Threshold Configuration from Switch side 150](#_Toc96881769)

[11.5.10. Show PON Port Performance from Pon side 150](#_Toc96881770)

[11.6. OLT PON Port Storm Control Function 152](#_Toc96881771)

[11.6.1. Config PON Port Broadcast Storm Control Function 152](#_Toc96881772)

[11.6.2. Config PON Port Unknown Multicast Storm Control Function 152](#_Toc96881773)

[11.6.3. Config PON Port Unknown Unicast Storm Control 153](#_Toc96881774)

[11.7. OLT PON Port Rate Limit Function 154](#_Toc96881775)

[11.7.1. Config PON Port Egress and Ingress Rate Limit 154](#_Toc96881776)

[11.7.2. Delete PON Port Egress and Ingress Rate Limit 154](#_Toc96881777)

[11.7.3. Show PON Port Egress and Ingress Rate Limit Configuration 155](#_Toc96881778)

[11.8. OLT PON Port Isolate Function 156](#_Toc96881779)

[11.8.1. Config PON Port Isolate 156](#_Toc96881780)

[11.8.2. Config PON Port Ont-isolate Function 156](#_Toc96881781)

[11.8.3. Show PON Port Isolation Configuration Info 157](#_Toc96881782)

[11.9. OLT PON Port VLAN Config 158](#_Toc96881783)

[11.9.1. Config PON Port VLAN Mode 158](#_Toc96881784)

[11.9.2. Config PON Port Native-vlan 158](#_Toc96881785)

[11.9.3. Config PON Port Native-vlan Priority 159](#_Toc96881786)

[11.9.4. Config PON Port Access Mode VLAN 159](#_Toc96881787)

[11.9.5. Config PON Port Hybrid Mode VLAN 160](#_Toc96881788)

[11.9.6. Delete PON Port Hybrid Mode VLAN 161](#_Toc96881789)

[11.9.7. Config PON Port Trunk Mode VLAN 161](#_Toc96881790)

[11.9.8. Delete PON Port Trunk Mode VLAN 162](#_Toc96881791)

[11.9.9. Config PON Port Translate Mode VLAN 162](#_Toc96881792)

[11.9.10. Delete PON Port Translate Mode VLAN 163](#_Toc96881793)

[11.9.11. Config PON Port QinQ VLAN 163](#_Toc96881794)

[11.9.12. Delete PON Port QinQ VLAN 164](#_Toc96881795)

[11.9.13. Config PON Port Aggregation VLAN 164](#_Toc96881796)

[11.9.14. Delete PON Port Aggregation VLAN 165](#_Toc96881797)

[11.9.15. Config PON Port Protocol VLAN 166](#_Toc96881798)

[11.9.16. Show OLT PON Port VLAN Configuration 166](#_Toc96881799)

[11.9.17. Show PON Port Translate VLAN Configuration 167](#_Toc96881800)

[11.9.18. Show PON Port Aggregation VLAN Configuration 168](#_Toc96881801)

[11.10. OLT PON Port Loopback Detection 169](#_Toc96881802)

[11.10.1. Config PON port Loopback Detection 169](#_Toc96881803)

[11.10.2. Config PON port Loopback Detection Control Function 169](#_Toc96881804)

[11.10.3. Config PON port Loopback Detection Per-vlan 170](#_Toc96881805)

[12. OLT MAC Address Table Manage 171](#_Toc96881806)

[12.1. Config OLT MAC-address Black-hole 171](#_Toc96881807)

[12.2. Delete MAC-Address Black-hole 171](#_Toc96881808)

[12.3. Config OLT Mac Address Entries limit 172](#_Toc96881809)

[12.4. Add Static MAC Address Bind Function 173](#_Toc96881810)

[12.5. Delete Static MAC Address bind 174](#_Toc96881811)

[12.6. Config OLT MAC Address Aging Time 175](#_Toc96881812)

[12.7. Clear OLT MAC Address Table 176](#_Toc96881813)

[12.8. Clear OLT Port MAC Address Table 176](#_Toc96881814)

[12.9. According OLT VLAN Clear MAC Address Table 177](#_Toc96881815)

[12.10. Show OLT MAC Address Table 178](#_Toc96881816)

[12.11. Show OLT MAC Address Black Hole 178](#_Toc96881817)

[12.12. Show OLT Dynamic MAC Address Table 179](#_Toc96881818)

[12.13. Show MAC Address Table From ONU 180](#_Toc96881819)

[12.14. Show MAC Address Table From PON Port 181](#_Toc96881820)

[12.15. Show MAC Address Table From GE Port 182](#_Toc96881821)

[12.16. Show MAC Address Table From XGE Port 182](#_Toc96881822)

[12.17. Show MAC Address Table From Aggregation Group 183](#_Toc96881823)

[12.18. Show OLT Static MAC Address Tables 183](#_Toc96881824)

[12.19. Show OLT MAC Address Aging Time Configuration 184](#_Toc96881825)

[12.20. Show MAC Address Table From Specified Vlan 184](#_Toc96881826)

[13. OLT Global VLAN Configurationss 186](#_Toc96881827)

[13.1. OLT VLAN Basic Configuration 186](#_Toc96881828)

[13.1.1. Create OLT VLAN or VLAN List 186](#_Toc96881829)

[13.1.2. Detele OLT VLAN or VLAN List 186](#_Toc96881830)

[13.1.3. Config OLT VLAN or VLAN List Name 187](#_Toc96881831)

[13.1.4. Delete VLAN or VLAN List Name 188](#_Toc96881832)

[13.1.5. Show OLT VLAN Configuration 188](#_Toc96881833)

[13.1.6. Show OLT VLAN Translate Configuraiton 189](#_Toc96881834)

[13.2. Vlanif Configuration 190](#_Toc96881835)

[13.2.1. Create or Delete Vlanif Interface 190](#_Toc96881836)

[13.2.2. Create or Delete Vlanif IP Address 191](#_Toc96881837)

[13.2.3. Config Vlanif Interface Description 191](#_Toc96881838)

[13.2.4. Show Vlanif Interface Detail Information 192](#_Toc96881839)

[13.3. VLAN Policy Configuration 193](#_Toc96881840)

[13.3.1. Add VLAN Policy Based On Mac address 193](#_Toc96881841)

[13.3.2. Show MAC-VLAN Entry 194](#_Toc96881842)

[13.3.3. Add VLAN Policy Based On IP Address 194](#_Toc96881843)

[13.3.4. Show IP-Subnet-VLAN Entry 195](#_Toc96881844)

[13.3.5. Add VLAN Policy Based On Protocol 195](#_Toc96881845)

[13.3.6. Show Protocol-vlan Entry 196](#_Toc96881846)

[14. OLT IGMP Configuration 198](#_Toc96881847)

[14.1. Config IGMP Fast-leave Function 198](#_Toc96881848)

[14.2. Config IGMP Mode 198](#_Toc96881849)

[14.3. Config IGMP Proxy Parameter 200](#_Toc96881850)

[14.4. Config IGMP Forwarding Policy 201](#_Toc96881851)

[14.5. Show IGMP Configuration 202](#_Toc96881852)

[14.6. Show IGMP Forwarding Table 203](#_Toc96881853)

[14.7. Config Multicast VLAN 204](#_Toc96881854)

[14.8. Config IGMP Match Group 204](#_Toc96881855)

[14.9. Show IGMP Match Group 205](#_Toc96881856)

[14.10. Add IGMP Program 205](#_Toc96881857)

[14.11. Add Batch IGMP Program 206](#_Toc96881858)

[14.12. Delete IGMP Program 207](#_Toc96881859)

[14.13. Config IGMP Router-port 207](#_Toc96881860)

[14.14. Show IGMP Router-port 208](#_Toc96881861)

[14.15. Configure Unknow-multicast Forwarding Policy 208](#_Toc96881862)

[14.16. Show Unknow-multicast Forwarding Policy 209](#_Toc96881863)

[14.17. Add IGMP User（Member） in Multicast-vlan 209](#_Toc96881864)

[14.18. Show Multicast-vlan Member Configuration 209](#_Toc96881865)

[14.19. Config IGMP User Bind Rights Profile 210](#_Toc96881866)

[14.20. Config IGMP Preview 211](#_Toc96881867)

[14.21. Config IGMP Preview Profile 211](#_Toc96881868)

[14.22. Modify The Program permissions in IGMP Profile 212](#_Toc96881869)

[14.23. Config IGMP User 213](#_Toc96881870)

[14.24. Show IGMP Configuration 214](#_Toc96881871)

[15. STP Configuration 216](#_Toc96881872)

[15.1. Global STP Config 216](#_Toc96881873)

[15.2. Show STP Configuraiton 216](#_Toc96881874)

[15.3. Config STP Priority 218](#_Toc96881875)

[15.4. Config STP Bridge Forward-delay Time 218](#_Toc96881876)

[15.5. Config STP Bridge Hello Message Send Period Time 219](#_Toc96881877)

[15.6. Config STP Bridge Max-age Time 219](#_Toc96881878)

[15.7. Config STP BPDU TX Hold Count 220](#_Toc96881879)

[15.8. Config OLT STP Cost 220](#_Toc96881880)

[15.9. Config OLT STP Edged-port 221](#_Toc96881881)

[15.10. Config OLT STP Mcheck Property 221](#_Toc96881882)

[15.11. Config OLT STP Point-to-Poing Function 222](#_Toc96881883)

[15.12. Config OLT STP Priority 223](#_Toc96881884)

[15.13. Show OLT Port STP Configuration 223](#_Toc96881885)

[15.14. Show OLT Link-aggregation Group STP Configuration 224](#_Toc96881886)

[17. ACL Configuration Manage 226](#_Toc96881887)

[17.1. ACL Basic Configuration 226](#_Toc96881888)

[17.1.1. Creat ACL 226](#_Toc96881889)

[17.1.2. Delete ACL 227](#_Toc96881890)

[17.1.3. Config ACL Name 228](#_Toc96881891)

[17.1.4. Show ACL Configuration 228](#_Toc96881892)

[17.2. ACL Apply Time-range Cofiguration 228](#_Toc96881893)

[17.2.1. Config ACL Apply Relative Time-range 229](#_Toc96881894)

[17.2.2. Config ACL Apply Absolute Time-range 229](#_Toc96881895)

[17.2.3. Delete ACL Apply Time-range 230](#_Toc96881896)

[17.2.4. Show ACL Apply Time-range Configuration 230](#_Toc96881897)

[17.3. Config OLT Basic ACL Function 231](#_Toc96881898)

[17.4. Config OLT Advanced ACL Function 232](#_Toc96881899)

[17.5. Config OLT Link ACL Function 235](#_Toc96881900)

[17.6. Config OLT PON ACL Function 236](#_Toc96881901)

[17.7. Config ONU ACL Function 238](#_Toc96881902)

[17.8. Show OLT ACL Configuration 239](#_Toc96881903)

[17.9. Modify OLT ACL Rule ID 240](#_Toc96881904)

[18. ARP Configuration 241](#_Toc96881905)

[18.1. Config ARP age time 241](#_Toc96881906)

[18.2. Config Learned Gratuitous ARP. 241](#_Toc96881907)

[18.3. Config Send Gratuitous ARP Messages 242](#_Toc96881908)

[18.4. Config ARP Proxy within the VLAN 242](#_Toc96881909)

[18.5. Config ARP Mac Address Change Check 243](#_Toc96881910)

[18.6. Config ARP Proxy Inner the VLAN 243](#_Toc96881911)

[18.7. Config ARP quick-update 244](#_Toc96881912)

[18.8. Config OLT Static ARP 244](#_Toc96881913)

[18.9. Unbind OLT static arp 245](#_Toc96881914)

[18.10. Delete ARP Link Statistics 246](#_Toc96881915)

[18.11. Delete Dynamic ARP Configuration 246](#_Toc96881916)

[18.11.1. Delete dynamic ARP on a VLANIF interface. 246](#_Toc96881917)

[18.11.2. Delete Dynamic ARP for Different IPs 246](#_Toc96881918)

[18.11.3. Delete Dynamic ARP for Port 247](#_Toc96881919)

[18.11.4. Delete all Dynamic ARPs 247](#_Toc96881920)

[19. OLT QOS Configuraiton 248](#_Toc96881921)

[19.1. Config OLT Global QOS mode 248](#_Toc96881922)

[19.2. Config Traffic Control Based On ACL Rule 248](#_Toc96881923)

[19.2.1. Config Packet Filter Based On ACL Rulesss 248](#_Toc96881924)

[19.2.2. Changes Traffic DSCP Based On ACL Rule 249](#_Toc96881925)

[19.2.3. Config Traffic Mirror Based On ACL Rule 250](#_Toc96881926)

[19.2.4. Config Traffic Limit Based On ACL Rule 251](#_Toc96881927)

[19.2.5. Add Traffic Outer VLAN Based On ACL Rule 252](#_Toc96881928)

[19.2.6. Translate Traffic VLAN Based On ACL Rule 252](#_Toc96881929)

[19.2.7. Modify Traffic VLAN Priority Based On ACL Rule 253](#_Toc96881930)

[19.2.8. Config Traffic Redirect Based On ACL Rule 254](#_Toc96881931)

[19.2.9. Modify Traffic TOS Value Based On ACL Rule 255](#_Toc96881932)

[19.2.10. Config ACL Action and Bind ACL to PON Port 256](#_Toc96881933)

[19.2.11. Config ACL Action and Bind ACL to ONU 258](#_Toc96881934)

[19.2.12. Config statistics on matching ACL Rules 259](#_Toc96881935)

[19.2.13. Show ACL Bind Configuration 260](#_Toc96881936)

[19.2.14. Show Port Packet-filter Policy Configuration 260](#_Toc96881937)

[19.2.15. Show Port QOS Configuration Information 261](#_Toc96881938)

[19.3. Config OLT QOS Queue 262](#_Toc96881939)

[19.3.1. Config OLT QOS Queue Mapping Mode 262](#_Toc96881940)

[19.3.2. Config QOS Queue Mapping Mode Based On 802.1p 262](#_Toc96881941)

[19.3.3. Config OLT QOS Queue Scheduled Mode 263](#_Toc96881942)

[19.3.4. Show OLT QOS Queue Schedule Mode 265](#_Toc96881943)

[19.4. OLT Port QOS Queue Configuration 266](#_Toc96881944)

[19.4.1. Config OLT Port QOS Queue Mapping Mode 266](#_Toc96881945)

[19.4.2. Config OLT Port QOS Queue Mapping Mode Based On 802.1p 267](#_Toc96881946)

[19.4.3. Config OLT Port QOS Queue Schedule Mode 268](#_Toc96881947)

[19.4.4. Show OLT Port QOS Queue Schedule Mode 270](#_Toc96881948)

[19.5. Config Mapping of DSCP to 802.1p Priority 272](#_Toc96881949)

[19.6. Config Mapping of Tos to 802.1P Priority 272](#_Toc96881950)

[20. OLT DHCP Function Configuration 274](#_Toc96881951)

[20.1. OLT DHCP-Snooping Function Configuration 274](#_Toc96881952)

[20.1.1. Enable or Disable DHCP-Snooping Function 274](#_Toc96881953)

[20.1.2. Show DHCP-Snooping Configuration 274](#_Toc96881954)

[20.1.3. Config DHCP-Snooping Monitor VLAN 276](#_Toc96881955)

[20.1.4. Config DHCP-Snooping Trust Port 277](#_Toc96881956)

[20.1.5. Enable or Disable OLT DHCP-Snooping Source MAC Address Detect 278](#_Toc96881957)

[20.1.6. Config DHCP-Snooping Request Message Rate Limit 278](#_Toc96881958)

[20.1.7. Enable or Disable DHCP-Snooping Opton82 Function 279](#_Toc96881959)

[20.1.8. Config DHCP-Snooping Option82 Forwarding Policy 279](#_Toc96881960)

[20.1.9. Config DHCP-Snooping option82 Format 280](#_Toc96881961)

[20.1.10. Config DHCP-Snooping Port Binding Policy 281](#_Toc96881962)

[20.1.11. Delete DHCP-Snooping Bind-table 281](#_Toc96881963)

[20.1.12. Config DHCP-Snooping Bind-table Write-delay Time 282](#_Toc96881964)

[20.1.13. Config DHCP-Snooping Bind-table Delete-time 283](#_Toc96881965)

[20.1.14. Config DHCP-Snooping Bind-table Write-to-flash 283](#_Toc96881966)

[20.1.15. Save DHCP-Snooping Bind-table to Server 283](#_Toc96881967)

[20.1.16. Show DHCP-Snooping Bind-table Entry 284](#_Toc96881968)

[20.1.17. Enable or Disable DHCP-Snooping arp-reply-fast 285](#_Toc96881969)

[20.1.18. Enable or Disable DHCP-Snooping arp-detect Function 285](#_Toc96881970)

[20.2. OLT DHCP-Relay Function Configuration 286](#_Toc96881971)

[20.2.1. Enable or Disable DHCP-Relay Function 286](#_Toc96881972)

[20.2.2. Config DHCP-Relay Vlanif Interface and Server 286](#_Toc96881973)

[20.2.3. Show DHCP-Relay Configuration 287](#_Toc96881974)

[20.3. OLT DHCP-Client Function Configuration 287](#_Toc96881975)

[20.3.1. Enable or Disable DHCP-Client Function 287](#_Toc96881976)

[20.3.2. Config DHCP-Client Manual Renew IP Address 288](#_Toc96881977)

[20.3.3. Config DHCP-Client Manual Release IP Address 288](#_Toc96881978)

[20.3.4. Config DHCP-Client Option60 289](#_Toc96881979)

[20.3.5. Show DHCP-Client Configuration 289](#_Toc96881980)

[20.3.6. Show DHCP-Client Option60 Configuration 290](#_Toc96881981)

[21. OLT Link Aggregation Function Configuration 291](#_Toc96881982)

[21.1. OLT Link-Aggregation Group Basic Function Config 291](#_Toc96881983)

[21.1.1. Add or Delete Link-Aggregation Group Member 291](#_Toc96881984)

[21.1.2. Enable or Disable Link-Aggregation Group Flow-control Function 291](#_Toc96881985)

[21.1.3. Config Link-Aggregation Group System Priority 292](#_Toc96881986)

[21.1.4. Set Link-Aggregation Group Port Priority 292](#_Toc96881987)

[21.1.5. Show Link-Aggregation Group System Priority 293](#_Toc96881988)

[21.1.6. Show Link-Aggregation Group Priority 293](#_Toc96881989)

[21.1.7. Config Link-Aggregation Group Frame-max 294](#_Toc96881990)

[21.1.8. Config Link-Aggregation Group Unicast Load Balance Mode 294](#_Toc96881991)

[21.1.9. Config Link-Aggregation Group Non-unicast Load BalanceMode 295](#_Toc96881992)

[21.1.10. Config Link-Aggregation Group Name 295](#_Toc96881993)

[21.1.11. Delete Link-Aggregation Group Name 296](#_Toc96881994)

[21.1.12. Delete Link-Aggregation Group Priority 296](#_Toc96881995)

[21.1.13. Delete Link-Aggregation Group Frame-max 297](#_Toc96881996)

[21.1.14. Clear Link-Aggregation Group Statistics 297](#_Toc96881997)

[21.1.15. Enable or Disable Link-Aggregation Group 298](#_Toc96881998)

[21.2. Link-Aggregation Group STP Configuration 298](#_Toc96881999)

[21.2.1. Config Link-Aggregation Group STP Cost 298](#_Toc96882000)

[21.2.2. Enable or Disable Link-Aggregation Group STP Edged-port 299](#_Toc96882001)

[21.2.3. Config Link-Aggregation Group STP Mcheck Property 299](#_Toc96882002)

[21.2.4. Config Link-Aggregation Group STP Point-to-Point Function 300](#_Toc96882003)

[21.2.5. Config Link-Aggregation Group STP Priority 301](#_Toc96882004)

[21.2.6. Delete Link-Aggregation Group STP Configure 301](#_Toc96882005)

[21.3. Link-Aggregation Group VLAN Configuration 302](#_Toc96882006)

[21.3.1. Config Link-Aggregation Group VLAN Mode 302](#_Toc96882007)

[21.3.2. Config Link-Aggregation Group Native-vlan(access) 303](#_Toc96882008)

[21.3.3. Config Link-Aggregation Group Native-vlan Priority 303](#_Toc96882009)

[21.3.4. Config Link-Aggregation Group Access Mode VLAN 304](#_Toc96882010)

[21.3.5. Config Link-Aggregation Group Hybrid Mode VLAN 304](#_Toc96882011)

[21.3.6. Delete Link-Aggregation Group Hybrid Mode VLAN 305](#_Toc96882012)

[21.3.7. Config Link-Aggregation Group Trunk Mode VLAN 306](#_Toc96882013)

[21.3.8. Delete Link-Aggregation Group Trunk Mode VLAN 306](#_Toc96882014)

[21.4. Show Link-Aggregation Group Information 307](#_Toc96882015)

[21.4.1. Show Link-Aggregation Group VLAN Information 307](#_Toc96882016)

[21.4.2. Show Link-Aggregation Group STP Information 307](#_Toc96882017)

[21.4.3. Show Link-Aggregation Group Port Status 308](#_Toc96882018)

[21.4.4. Show Link-Aggregation Group STP Information Statistics Information 309](#_Toc96882019)

[21.4.5. Show Link-Aggregation Group Config Information 310](#_Toc96882020)

[22. OLT Routing Function 311](#_Toc96882021)

[22.1. Add or Delete Static Route 311](#_Toc96882022)

[22.2. Config Route ID 311](#_Toc96882023)

[22.3. Show IP Route Information 312](#_Toc96882024)

[22.4. Show IP Routing-table Information 312](#_Toc96882025)

[22.5. Config OLT RIP function 313](#_Toc96882026)

[22.5.1. Enable/Disable RIP 313](#_Toc96882027)

[22.5.2. Config the default route for importing RIP. 313](#_Toc96882028)

[22.5.3. Config the default metric value of the RIP for importing routes. 314](#_Toc96882029)

[22.5.4. Configure the management distance of RIP 314](#_Toc96882030)

[22.5.5. Config a specified neighbor route for RIP 315](#_Toc96882031)

[22.5.6. Config the RIP function on the specified network segment interface 315](#_Toc96882032)

[22.5.7. Config the RIP function on the VLANIF interface 316](#_Toc96882033)

[22.5.8. Config RIP metrics 316](#_Toc96882034)

[22.5.9. Config the passive interface of RIP 317](#_Toc96882035)

[22.5.10. Config import routes in RIP 317](#_Toc96882036)

[22.5.11. Config RIP static routes 318](#_Toc96882037)

[22.5.12. Config the timer time of RIP 319](#_Toc96882038)

[22.5.13. Config the version of RIP 319](#_Toc96882039)

[22.5.14. Create/delete the key of the RIPv2 keychain 320](#_Toc96882040)

[22.5.15. Create/delete an authentication key for the RIPv2 keychain 320](#_Toc96882041)

[22.5.16. Create/delete the receive lifetime of the RIPv2 keychain 321](#_Toc96882042)

[22.5.17. Create/delete the transmit lifetime of the RIPv2 keychain 322](#_Toc96882043)

[22.6. Config the RIP function of the vlanif interface 323](#_Toc96882044)

[22.6.1. Config the authentication mode and parameters of RIP 323](#_Toc96882045)

[22.6.2. Enable RIP to Send/Receive Messages 323](#_Toc96882046)

[22.6.3. Config the split horizon function of RIP 324](#_Toc96882047)

[22.6.4. Delete RIP configuration 324](#_Toc96882048)

[23. OLT Profile Configuration 326](#_Toc96882049)

[23.1. OLT DBA Profile Configurations 326](#_Toc96882050)

[23.1.1. Create DBA Profile 326](#_Toc96882051)

[23.1.2. Config DBA Profile Bandwith 326](#_Toc96882052)

[23.1.3. Commit DBA Profile Config 328](#_Toc96882053)

[23.1.4. Show OLT DBA Profile Information 329](#_Toc96882054)

[23.2. ont-lineprofile Configuraton 330](#_Toc96882055)

[23.2.1. Create ont-lineprofile 330](#_Toc96882056)

[23.2.2. Bind DBA Profile in ont-lineprofile 330](#_Toc96882057)

[23.2.3. Config FEC Function in ont-lineprofile 331](#_Toc96882058)

[23.2.4. Config Data Encryption in ont-lineprofile 331](#_Toc96882059)

[23.2.5. Config ONU-Car in ont-lineprofile 331](#_Toc96882060)

[23.2.6. Config queue thresholds for DBA queue sets 332](#_Toc96882061)

[23.2.7. Commit ont-lineprofile Configuration 332](#_Toc96882062)

[23.2.8. Show OLT ont-lineprofile Information 333](#_Toc96882063)

[23.3. ont-srvprofile Configuration 334](#_Toc96882064)

[23.3.1. Create ont-srvprofile 334](#_Toc96882065)

[23.3.2. Config ONU Capability in ont-srvprofile 334](#_Toc96882066)

[23.3.3. Config ONU Port Native-vlan in ont-lineprofile 335](#_Toc96882067)

[23.3.4. Config ONU Port VLAN in ont-srvprofile 335](#_Toc96882068)

[23.3.5. Config ONU VLAN Mode in ont-lineprofile 336](#_Toc96882069)

[23.3.6. Config ONU Port Multicast VLAN in ont-lineprofile 336](#_Toc96882070)

[23.3.7. Config ONU Port Downstream Rate limit in ont-lineprofile 337](#_Toc96882071)

[23.3.8. Config ONU Port Upstream Rate limit in ont-lineprofile 337](#_Toc96882072)

[23.3.9. Config ONU Port MAC Count Limit in ont-lineprofile 338](#_Toc96882073)

[23.3.10. Config ONU Port IGMP Number in ont-lineprofile 338](#_Toc96882074)

[23.3.11. Config ONU Port IGMP VLAN Process Mode in ont-lineprofile 339](#_Toc96882075)

[23.3.12. Config ONU IGMP Fast-leave Function in ont-lineprofile 339](#_Toc96882076)

[23.3.13. Enable or Disable ONU Loop Detect Function in ont-lineprofile 340](#_Toc96882077)

[23.3.14. Show ont-srvprofile Current Configuration 340](#_Toc96882078)

[23.3.15. Commit ont-srvprofile Configuration 342](#_Toc96882079)

[23.4. ont-slaprofile Configuration 342](#_Toc96882080)

[23.4.1. Creat ont-slaprofile 342](#_Toc96882081)

[23.4.2. Config the Cycle Length of the SLA Template. 343](#_Toc96882082)

[23.4.3. Config the Number of Services for the SLA Profile 343](#_Toc96882083)

[23.4.4. Config the Service Parameters of the SLA Profile. 344](#_Toc96882084)

[23.4.5. Commit ont-slaprofile Configuration 345](#_Toc96882085)

[23.4.6. Show ont-slaprofile Current Configuration 345](#_Toc96882086)

[23.5. OLT traffic-profile Configuration 346](#_Toc96882087)

[23.5.1. Create traffic-profile 346](#_Toc96882088)

[23.5.2. Modify traffic-profile 347](#_Toc96882089)

[23.5.3. Show OLT traffic-profile Information 348](#_Toc96882090)

[23.6. Config Alarm Profile 348](#_Toc96882091)

[23.6.1. Creat Low Alarm Profile 348](#_Toc96882092)

[23.6.2. Creat High Alarm Profile 351](#_Toc96882093)

[23.6.3. Show Alarm Profile 353](#_Toc96882094)

[23.6.4. Delete Alarm Profile 354](#_Toc96882095)

[23.7. Optical-alarm-profile Configuration 355](#_Toc96882096)

[23.7.1. Creat Optical Low Alarm Template 355](#_Toc96882097)

[23.7.2. Creat Optical High Alarm Template 357](#_Toc96882098)

[23.7.3. Show Optical-alarm-profile 358](#_Toc96882099)

[23.8. OLT VLAN Pool Configuration 359](#_Toc96882100)

[23.8.1. Create VLAN Pool 359](#_Toc96882101)

[23.8.2. Modify VLAN Pool 359](#_Toc96882102)

[23.8.3. Delete VLAN Pool 360](#_Toc96882103)

[23.8.4. Show OLT VLAN Pool Information 360](#_Toc96882104)

[24. ONU Management 362](#_Toc96882105)

[24.1. ONU Authentication Management 362](#_Toc96882106)

[24.1.1. Enable or Disable ONU Autofind Function 362](#_Toc96882107)

[24.1.2. Show Autofind ONU 362](#_Toc96882108)

[24.1.3. Aging time configuration of offline ONT 363](#_Toc96882109)

[24.1.4. Config the ONT registration migration detection switch 364](#_Toc96882110)

[24.1.5. MAC Address Method Authenticated ONU And Bind Profile 364](#_Toc96882111)

[24.1.6. Loid Method Authenticated ONU and Bind Profile 365](#_Toc96882112)

[24.1.7. Loid+Password Method Authenticated ONU and Bind Profile 366](#_Toc96882113)

[24.1.8. Config ONU Authmode 367](#_Toc96882114)

[24.1.9. Change ONU Bind Profile 367](#_Toc96882115)

[24.1.10. Config Pre-binding ONU Profile 368](#_Toc96882116)

[24.1.11. Confirm Autofind ONU 369](#_Toc96882117)

[24.1.12. Cancel Autofind ONU 370](#_Toc96882118)

[24.1.13. Re-register ONU 371](#_Toc96882119)

[24.1.14. Modify ONU Authmode 371](#_Toc96882120)

[24.1.15. Config ONU Black-list 372](#_Toc96882121)

[24.1.16. Delete Black-list Auth ONU 373](#_Toc96882122)

[24.1.17. Delete Authentication ONU 374](#_Toc96882123)

[24.1.18. Show ONU BlackList Authenticated Config 374](#_Toc96882124)

[24.1.19. Show ONU Black List 375](#_Toc96882125)

[24.1.20. Show ONU Predetermine Information 376](#_Toc96882126)

[24.1.21. Show ONU registration statistics 376](#_Toc96882127)

[24.1.22. Delete the user template of the predetermine ONU 377](#_Toc96882128)

[24.1.23. Show ONU Registered Status and Information 378](#_Toc96882129)

[24.1.24. Check the aging time configuration of the ONU 379](#_Toc96882130)

[24.1.25. Check the ONU registration migration detection status 380](#_Toc96882131)

[24.2. Policy-auth ONU and Batch Delivery Configuration Manage 380](#_Toc96882132)

[24.2.1. Enable or Disable Global Policy-auth ONU 380](#_Toc96882133)

[24.2.2. Enable or Disable Policy-auth ONU Under PON Port 381](#_Toc96882134)

[24.2.3. Config Policy-auth ONU Mode 381](#_Toc96882135)

[24.2.4. Config Policy-auth ONU Mode and Batch Delivery Configuration Match Mode 382](#_Toc96882136)

[24.2.5. Show Policy-auth ONT Configuration Information 384](#_Toc96882137)

[24.3. ONU Basic Function Management 384](#_Toc96882138)

[24.3.1. Active ONU 384](#_Toc96882139)

[24.3.2. Deactive ONU 385](#_Toc96882140)

[24.3.3. Reboot ONU 385](#_Toc96882141)

[24.3.4. Restore the ONU to factory settings 386](#_Toc96882142)

[24.3.5. ONU Remote Manage IP Function Config 386](#_Toc96882143)

[24.3.6. ONU Upstream Rate Limit Function Config 387](#_Toc96882144)

[24.3.7. ONU Downstream Rate Limit Function Config 388](#_Toc96882145)

[24.3.8. ONU MAC Aging Time Config 389](#_Toc96882146)

[24.3.9. Add ONU Description Information 389](#_Toc96882147)

[24.3.10. ONU Encryption Function Config 390](#_Toc96882148)

[24.3.11. Enable or Disable ONU FEC Function 390](#_Toc96882149)

[24.3.12. ONU Service-sla Function Config 391](#_Toc96882150)

[24.3.13. ONU SNMP Function Config 391](#_Toc96882151)

[24.3.14. Enable or Disable ONU Tx Optical Power Supply 392](#_Toc96882152)

[24.3.15. Show ONU ipconfig(Remote Manage IP Address) 393](#_Toc96882153)

[24.3.16. Show ONU SNMP Configuration 394](#_Toc96882154)

[24.3.17. Show ONU Capability Information 395](#_Toc96882155)

[24.3.18. Show ONU Configured Capability 396](#_Toc96882156)

[24.3.19. Show ONU Opitcal Power Information 397](#_Toc96882157)

[24.3.20. Show ONU Firmware Version 398](#_Toc96882158)

[24.3.21. Show ONU SNMP Config parameters 399](#_Toc96882159)

[24.3.22. Show Basic Information about all ONUs on the pon port 400](#_Toc96882160)

[24.3.23. Show the ONU binding Rate Limit Template Information 401](#_Toc96882161)

[24.3.24. Show the ONU speed limit template information 402](#_Toc96882162)

[24.3.25. Show the Reason for the Offline of all ONUs under the PON Port 403](#_Toc96882163)

[24.3.26. Show the Reason of ONU Offline under the PON Port 404](#_Toc96882164)

[24.3.27. Delete ONU Encrypt Feature 405](#_Toc96882165)

[24.3.28. Delete ONU FEC Feature 405](#_Toc96882166)

[24.3.29. Delete ONU Remote Management IP config 406](#_Toc96882167)

[24.3.30. Delete SLA Template Bount to ONU 406](#_Toc96882168)

[24.3.31. Delete ONU Rate Limit Function Config 407](#_Toc96882169)

[24.3.32. Delete ONU SNMP Function Config 407](#_Toc96882170)

[24.4. ONU Port VLAN Configuration(Non-template Mode) 408](#_Toc96882171)

[24.4.1. ONU Port Native-vlan(access) Configs 408](#_Toc96882172)

[24.4.2. ONU Port Vlan Config 408](#_Toc96882173)

[24.4.3. ONU Port Translation Mode VLAN Config 409](#_Toc96882174)

[24.4.4. ONU Port VLAN Pool Function Config 410](#_Toc96882175)

[24.4.5. ONU Port Transparent Mode VLAN Config 410](#_Toc96882176)

[24.4.6. Show ONU Port VLAN Configuration 411](#_Toc96882177)

[24.4.7. Show Real-time Information about the ONU Ethernet Port 412](#_Toc96882178)

[24.4.8. Delete VLAN that has been Added to an ONU Port 413](#_Toc96882179)

[24.5. ONU Port Management 414](#_Toc96882180)

[24.5.1. Enable or Disable ONU Port 414](#_Toc96882181)

[24.5.2. ONU Port Isolate Function Config 414](#_Toc96882182)

[24.5.3. ONU PON Port Performance Statistics Config 415](#_Toc96882183)

[24.5.4. ONU ETH Port Performance Statistics Config 416](#_Toc96882184)

[24.5.5. ONU CATV Port Enable or Disable 416](#_Toc96882185)

[24.5.6. ONU Port Auto-negotiation Function Config 417](#_Toc96882186)

[24.5.7. ONU Port Downstream Rate Limit Config 418](#_Toc96882187)

[24.5.8. ONU Port Upstream Rate Limit Config 418](#_Toc96882188)

[24.5.9. Enable or Disable ONU Port Flow Control Function 419](#_Toc96882189)

[24.5.10. Clear ONU Port Learned MAC 420](#_Toc96882190)

[24.5.11. Clear Performance Statistics of the ONU Port 421](#_Toc96882191)

[24.5.12. ONU Port MAC Count Limit Function Config 421](#_Toc96882192)

[24.5.13. ONU Port Multicast Group Number Limit Config 422](#_Toc96882193)

[24.5.14. ONU Port Multicast VLAN Process Mode Config 422](#_Toc96882194)

[24.5.15. ONU Port Speed and Duplex Mode Config 423](#_Toc96882195)

[24.5.16. ONU Port Storm-ctrl Function Config 424](#_Toc96882196)

[24.5.17. Enable or Disable ONU Port Loop Detect Function 425](#_Toc96882197)

[24.5.18. Enable or Disable ONU Port Loop Detected 426](#_Toc96882198)

[24.5.19. ONU Port Upstream classification/mapping/priority-mark Rule Config 427](#_Toc96882199)

[24.5.20. Show ONU Port Performance State 427](#_Toc96882200)

[24.5.21. Show ONU Port Performance Statistics 428](#_Toc96882201)

[24.5.22. Show the service flow classification/mapping/priority marking information of the ONU port. 431](#_Toc96882202)

[24.5.23. Show the MAC address learned on the ONU port 431](#_Toc96882203)

[24.5.24. Show the Policy Information of the ONU Ethernet Port 432](#_Toc96882204)

[24.5.25. Show the Storm Control Config of the ONU Ethernet Port 433](#_Toc96882205)

[24.5.26. Show ONU Port Attribute(Configuration) 434](#_Toc96882206)

[24.5.27. Show ONU CATV Port Status 435](#_Toc96882207)

[24.5.28. Show ONU Port Learned MAC Address Information 436](#_Toc96882208)

[24.5.29. Show ONU PON Port Performance Statistics 437](#_Toc96882209)

[24.5.30. Delete the Configured Bandwidth Rate Limit of ONU Port 438](#_Toc96882210)

[24.5.31. Delete the Number of Learned MAC Addresses Restricted by the ONU Port 438](#_Toc96882211)

[24.5.32. Delete the Maximum Number of Multicast Groups Restricted by the ONU Port 439](#_Toc96882212)

[24.5.33. Delete the Processing Mode of the Multicast Stream VLAN on the ONU Port 439](#_Toc96882213)

[24.5.34. Delete the Rules of ONU Port for the Upstream Service Flow 440](#_Toc96882214)

[24.6. ONU WIFI Config 441](#_Toc96882215)

[24.6.1. Enable or Disable WIFI 441](#_Toc96882216)

[24.6.2. Config Maximum Number of Wireless SSID User accesses 441](#_Toc96882217)

[24.6.3. Config Wireless SSID 442](#_Toc96882218)

[24.6.4. Config WIFI Properties 443](#_Toc96882219)

[24.6.5. WIFI Factory Reset 444](#_Toc96882220)

[24.6.6. Show Wireless SSID Information 444](#_Toc96882221)

[24.6.7. Show WIFI Information 445](#_Toc96882222)

[24.6.8. Show WIFI Version 446](#_Toc96882223)

[24.7. ONU IGMP Function Configuration(Non-template Mode) 446](#_Toc96882224)

[24.7.1. ONU IGMP Mode Config 446](#_Toc96882225)

[24.7.2. ONU Fsast-leave Function Config 447](#_Toc96882226)

[24.7.3. Config the multicast VLAN of the ONU port 447](#_Toc96882227)

[24.7.4. Show ONU Multicast-group Record 448](#_Toc96882228)

[24.7.5. Show ONU IGMP Mode 449](#_Toc96882229)

[24.7.6. Show ONU Port IGMP VLAN Tagstrip Mode 449](#_Toc96882230)

[24.7.7. Show ONU Port Multicast VLAN 450](#_Toc96882231)

[24.7.8. Disable the Multicast Fast Leave Function of the ONU 451](#_Toc96882232)

[24.7.9. Delete the Multicast VLAN of the ONU Port 451](#_Toc96882233)

[24.8. ONU Upgrade Management 452](#_Toc96882234)

[24.8.1. Transfer ONU Firmware to OLT 452](#_Toc96882235)

[24.8.2. Batch Upgrade ONU 453](#_Toc96882236)

[24.8.3. Start or Stop Batch Upgrade ONU 454](#_Toc96882237)

[24.8.4. Show ONU Upgrade Configuration Information 454](#_Toc96882238)

[24.8.5. Show ONU Upgrade Progress 455](#_Toc96882239)

[24.8.6. Separately Upgrade ONU Under PON Port 456](#_Toc96882240)

[24.8.7. Active and Commit ONU New Firmware 456](#_Toc96882241)

[24.8.8. Delete the ONU that Needs to be Upgraded 457](#_Toc96882242)

[24.9. Home Gateway Upgrade 458](#_Toc96882243)

[24.10. ONU Alarm Management 458](#_Toc96882244)

[24.10.1. ONU Opitcal Bias Current Alarm Function Config 458](#_Toc96882245)

[24.10.2. ONU Optical Voltage Alarm Function Config 459](#_Toc96882246)

[24.10.3. ONU Opitcal Power Alarm Function Config 461](#_Toc96882247)

[24.10.4. ONU Opitcal Temperature Alarm Function Config 462](#_Toc96882248)

[24.10.5. ONU Port CRC Checkout Alarm Function Config 463](#_Toc96882249)

[24.10.6. ONU Port Dropping Message Alarm Function Config 464](#_Toc96882250)

[24.10.7. ONU Port Dropevents Alarm Function Config 465](#_Toc96882251)

[24.10.8. ONU Port Error Message Alarm Function Config 466](#_Toc96882252)

[24.10.9. ONU Port Message Fragment Alarm Function Config 467](#_Toc96882253)

[24.10.10. ONU Port Message Jabber(time out) Alarm Function Config 468](#_Toc96882254)

[24.10.11. ONU Port Oversize Message Alarm Function Config 470](#_Toc96882255)

[24.10.12. ONU Port Ultra Short Message Alarm Function Config 471](#_Toc96882256)

[24.10.13. ONU CATV Alarm Threshold Config 472](#_Toc96882257)

[24.10.14. ONU CATV Output Gain Control Config 473](#_Toc96882258)

[24.10.15. Enable or Disable ONU Dying-gasp Alarm Function 474](#_Toc96882259)

[24.10.16. Bind Alarm-config to ONU 474](#_Toc96882260)

[24.10.17. Bind Optical-alarm-config to ONU 475](#_Toc96882261)

[24.10.18. Show ONU Dying-gasp Alarm Config Status 475](#_Toc96882262)

[24.10.19. Show ONU Optical power Alarm Config Status 477](#_Toc96882263)

[24.10.20. Show ONU ETH Port Alarm Config Status 478](#_Toc96882264)

[24.10.21. Show ONU PON Port Alarm Config Status 480](#_Toc96882265)

[24.10.22. Show ONU CATV Output Gain Control Information 482](#_Toc96882266)

[24.10.23. Show the ONU CATV Alarm Threshold Information. 482](#_Toc96882267)

[24.10.24. Show the Optical Alarm Template Information of the ONU 483](#_Toc96882268)

[24.10.25. Show ONU Alarm Template Information 484](#_Toc96882269)

[24.10.26. Delete an Alarm Template bound to ONU 486](#_Toc96882270)

[24.10.27. Delete the optical alarm template bound to the ONU 487](#_Toc96882271)

[24.11. ONU WAN Management 488](#_Toc96882272)

[24.11.1. Config parameters for the ONU WAN service 488](#_Toc96882273)

[24.11.2. Clear ONU WAN Config 489](#_Toc96882274)

[24.11.3. Show ONU WAN Name information 489](#_Toc96882275)

[24.11.4. Show ONU WAN State Information 490](#_Toc96882276)

[24.12. ONU voice service management 491](#_Toc96882277)

[24.12.1. Config Parameters for the Fax/Modem Service 491](#_Toc96882278)

[24.12.2. Config Global Parameters of the ONU Voice Module 492](#_Toc96882279)

[24.12.3. Config Parameters of the H.248 Protocol of the ONU Voice Module 493](#_Toc96882280)

[24.12.4. Config Parameters for H.248 RTP TID of the ONU Voice Module 494](#_Toc96882281)

[24.12.5. Config Parameters for H.248 User TID of the ONU Voice Module 495](#_Toc96882282)

[24.12.6. Config Thread Operation of the ONU Voice Module 496](#_Toc96882283)

[24.12.7. Config Switch for VOIP Ports of ONU Voice Module 496](#_Toc96882284)

[24.12.8. Config Parameters for SIP Protocol of ONU Voice Module 497](#_Toc96882285)

[24.12.9. Config Parameters for User SIP Protocol of the ONU Voice Module 499](#_Toc96882286)

[24.12.10. Show Basic Information about the ONU Voice Module. 499](#_Toc96882287)

[24.12.11. Show the POTS Port Status of the ONU Voice Module User. 500](#_Toc96882288)

[24.12.12. Show the Parameters of the Fax/Modem Service. 501](#_Toc96882289)

[24.12.13. Show Global Parameters of the ONU Voice Module 502](#_Toc96882290)

[24.12.14. Show the Parameters of the H.248 Protocol of the ONU Voice Module 503](#_Toc96882291)

[24.12.15. Show the Parameters of the H.248 RTP TID of the ONU Voice Module 504](#_Toc96882292)

[24.12.16. Show the Parameters of the H.248-rtp-tid-info of the ONU Voice Module 505](#_Toc96882293)

[24.12.17. Show the H.248 User TID Parameters of the ONU Voice Module 506](#_Toc96882294)

[24.12.18. Show the Running Status of the IAD under the H.248 Protocol of the ONU Voice Module 506](#_Toc96882295)

[24.12.19. Show the Parameters of the SIP Protocol of the ONU Voice Module 507](#_Toc96882296)

[24.12.20. Show the User Parameters of the SIP Protocol of the ONU Voice Module 508](#_Toc96882297)

[24.13. Config the DBA Queue Set of the ONU 509](#_Toc96882298)

[24.13.1. Config Queue Thresholds for DBA Queue Sets 509](#_Toc96882299)

[24.13.2. Delete queue thresholds for DBA queue sets 510](#_Toc96882300)

[25. OLT Log Management and Query 511](#_Toc96882301)

[25.1. Add Syslog Record Server 511](#_Toc96882302)

[25.2. Delete Syslog Record Server 511](#_Toc96882303)

[25.3. Enable or Disable Syslog Record to Server 512](#_Toc96882304)

[25.4. Enable or Disable Alarmlog Record to Server 512](#_Toc96882305)

[25.5. Active Syslog Record server 513](#_Toc96882306)

[25.6. Deactive Syslog Record Server 513](#_Toc96882307)

[25.7. Show Syslog Record Server Config Status 514](#_Toc96882308)

[25.8. Backup OLT Log 514](#_Toc96882309)

[25.9. Erase OLT Log 515](#_Toc96882310)

[25.10. Show OLT Log 515](#_Toc96882311)

[26. OLT Alarm Management and Query 517](#_Toc96882312)

[26.1. Clear Specified Active Alarm Entry 517](#_Toc96882313)

[26.2. Clear Active Alarm by Specified Alarmlevel 517](#_Toc96882314)

[26.3. Clear Active Alarm by Specified Board 518](#_Toc96882315)

[26.4. Clear Active Alarm by Specified GE Port 518](#_Toc96882316)

[26.5. Clear Active Alarm by Specified PON Port 518](#_Toc96882317)

[26.6. Clear Active Alarm by Specified XGE Port 519](#_Toc96882318)

[26.7. Config Alarmlevel for Specified Alarm 519](#_Toc96882319)

[26.8. Enable and Config Alarm Jitter-interval Time 520](#_Toc96882320)

[26.9. Enable or Disable Alarm Jitter-proof Function 520](#_Toc96882321)

[26.10. Enable or Disable Specified Alarm Record Output 521](#_Toc96882322)

[26.11. Enable or Disable Specified Level Alarm Output 521](#_Toc96882323)

[26.12. Enable or Disable All Alarms Output 522](#_Toc96882324)

[26.13. Enable or Disable Detail Alarm Output 523](#_Toc96882325)

[26.14. Show Specified Active Alarm Record 523](#_Toc96882326)

[26.15. Show Active Alarm Logs by Specified Level 524](#_Toc96882327)

[26.16. Show Active Alarm Logs by Specified Board 525](#_Toc96882328)

[26.17. Show Active Alarm Logs by Specified GE Port 525](#_Toc96882329)

[26.18. Show Active Alarm Logs by Specified PON Port 526](#_Toc96882330)

[26.19. Show Active Alarm Logs by Specified XGE Port 527](#_Toc96882331)

[26.20. Show All Active Alarm Log 527](#_Toc96882332)

[26.21. Show Specified Alarm History Record 528](#_Toc96882333)

[26.22. Show Alarm History Record by Specified Level 529](#_Toc96882334)

[26.23. Show Alarm History Record by Specified Board 530](#_Toc96882335)

[26.24. Show Alarm History Record by Specified GE Port 531](#_Toc96882336)

[26.25. Show Alarm History Record by Specified PON Port 531](#_Toc96882337)

[26.26. Show Alarm History Record by Specified XGE Port 532](#_Toc96882338)

[26.27. Show All Alarm History Record 533](#_Toc96882339)

[26.28. Show Alarm Jitter-proof Interval Time 533](#_Toc96882340)

[26.29. Show Alarm Basic Information 534](#_Toc96882341)

[27. OLT Event Management and Query 536](#_Toc96882342)

[27.1. Config Event Level 536](#_Toc96882343)

[27.2. Enable or Disable All Events Output 536](#_Toc96882344)

[27.3. Enable or Disable Detail Event Output 537](#_Toc96882345)

[27.4. Enable or Disable Specified Event Output 537](#_Toc96882346)

[27.5. Enable or Disable Specified Level Event Output 538](#_Toc96882347)

[27.6. Show All Event History Record 538](#_Toc96882348)

[27.7. Show Specified Event History Record 539](#_Toc96882349)

[27.8. Show Specified Level Event History Record 539](#_Toc96882350)

[27.9. Show Event History Record by Specified Board 540](#_Toc96882351)

[27.10. Show Event History Record by Specified GE Port 541](#_Toc96882352)

[27.11. Show Event History Record by Specified PON Port 541](#_Toc96882353)

[27.12. Show Event History Record by Specified XGE Port 542](#_Toc96882354)

[27.13. Show Event Basic Information 542](#_Toc96882355)

[28. Device Diagnostic Management 544](#_Toc96882356)

[28.1. Ping Diagnostic Test 544](#_Toc96882357)

[28.2 Traceroute Diagnostic Test 544](#_Toc96882358)

[Appendix 1 546](#_Toc96882359)

[Concluding Remarks 546](#_Toc96882360)

# Read Instructions

## Document Scope

|  |  |  |  |
| --- | --- | --- | --- |
| Reading Object | Product | Products Software Version | |
| Our company Employees, FTTX Operation&Maintenance Engineer, Customer’s Technical Engineer | EPON OLT（New 4Port/8Port/16Port/Plug-in 16Port OLT） | V1.4.X | |
| Compiling Department | Product Management Center Technical Support Department | Document Version | V1.3 |

## Revision History

|  |  |  |  |
| --- | --- | --- | --- |
| Date | Version | Description | Author |
| 2017-12-7 | V1.1 | The OLT version is switched to the V1.2.X, cli command line have been changed.update command line operation fully. | Technical Support  Department |
| 2018-7-26 | V1.2 | 1. The OLT version is switched to the V1.3.X version, the command line changes, and the command line manual (including template configuration, routing configuration, etc.) is fully updated.  2. Adding a plug-in 16-port OLT configuration instructions | Technical Support  Department |
| 2019-9-18 | V1.3 | The OLT version is switched to the V1.4.X version, the command line changes, and the command line manual is fully updated (including OLT RIP configuration, ONU wan configuration, voip configuration, etc.) | Technical Support  Department |

## Conventions for Command Line

| Format | Specification |
| --- | --- |
| Boldface | Key words of command line will be in boldface(unchanged) |
| Italics | Parameters of command line will be in italics(replace with actual value) |
| [] | Parameters in[]is optional |
| (x|y|…) | One of parameters in()should be chosen |
| [x|y|…] | None or one of parameters in[]should be chosen |
| <x-y> | One number from x to y should be chosen |
| $ | The next line behind$is annotation |

## Conventions for Keyboard Operation

|  |  |
| --- | --- |
| Format | Specification |
| Characters within angle brackets | Represents botton’s name,like<Enter>,<Tab>,<Backspace>,<a>,<?> |
| <button1+button2> | Press button1 and button2 at the same time,like<Ctrl+Alt+A>means pressing button of“Ctrl”,“Alt”,“A”at the same time. |
| <button1,button2> | Press button1 first,release button1,then press button2,like<Alt,F>means pressing“Alt”button first,release“Alt”,then press“F”button” |

## Conventions for symbols

This manual adopts the following highly visible symbols to get users attention when operating,and the explanation of these symbols are as follows:

Watch-out:The matters needs attention in operating,improper operations probably will cause loss of data and damage of device

Warning:Annotation behind this symbol needs special attention,improper operations probably will cause harm to health



Tips:Provide more clear and understandable explanations and descriptions in operating

## Conventions for Words

OLT：Represents the system of new 4Port/8Port/16Port/Plug-in 16Port OLT,includes main switch processing module and uplink ports connected with uplink devices like switch.

PON：Represents PON protocol processing module and PON ports connected with ONU.

## Precautions

* The command line described in the document is case sensitive in OLT.
* If we meet a command that cannot be inputed or is prompted for error,we can input **“?”** to see the latter command format.
* Input incomplete commands can be completed by pressing the **“Tab”** key.
* new 4Port/8Port/16Port EPON OLT are Pizza-Box OLT，only have one card，so,if we want to enter PON mode,need input interface epon 0/0
* Plug-in 16Port OLT is Plug-in card OLT,has four PON card,so the comamnd for entering PON mode is OLT(config)# interface epon 0/**<SlotID>** ,SlotID is Slot Number,range is 1-4，for example,the command for entering slot 1 is OLT(config)# interface epon 0/1

# Command Line Interface View Introduce

**View and view switching**

**Specification:**This command line environment includes several views as follows:

* **view view：**refers to view view or user mode in the below user will enter after inputting password,in which mode only simple commands can be processed.

This view shows like: OLT>

* **enable view：**refers to enable view or privileged mode in the below user will enter after inputting enable in view mode,this mode has higher authorities.

This view shows like: OLT#

* **config view：**refers to config view or global configuration mode in the below user will enter after inputting config in enable view.

This view shows like: OLT(config)#

* **ge interface view：**refers to ge/gigabit interface view/mode user will enter after inputting interface ge 0/0 in config view.

This view shows like: OLT(config-interface-ge-0/0)#

* **Xge interface view：**refers to xge/10-gigabit interface view/mode user will enter after inputting interface xge 0/0 in config view.

This view shows like: OLT(config-interface-xge-0/0)#

* **EPON interface view：**refers to EPON interface view/mode user will enter after inputting interface EPON 0/0 in config view.

This view shows like: OLT(config-interface-epon-0/0)#

* **Vlanif three-layer interface view：**User will enter this view after inputting interface vlanif *vlanID* in config view.

This view shows like: OLT(config-interface-vlanif-100)#

* **Management interface MGMT view：**User will enter this view after inputting interface mgmt in config view.

This view shows like: OLT(config-interface-mgmt)#

* **multicast-vlan view：**User will enter this view after inputting multicast-vlan vlanid in config view.

This view shows like: OLT(config-multicast-vlan-100)#

* **link-aggregation view：**User will enter this view after inputtinginterface link-aggregationin config view.

This view shows like: OLT(config-interface-aggregation)#

## Command Line View Overview

**Login**

**Username:**root

**Password:**admin

**Serial Interface**

(Bit number: 9600/s

Data bits: 8 Odd-even check: no

Stop bit: 1

Data flow control: no)

**PuTTY**

(telnet)

**view view**

OLT>

enable

**enable view**

OLT#

config

**Global configuration mode**

OLT(config)#

**Ge interface view**

OLT(config-interface-ge-0/0)#

GE port

**EPON interface view**

OLT(config-interface-epon-0/0)#

EPON port

**Mgmtinterface view** OLT(config-interface-mgmt)#

Mgmt interface

**Xge interface view**

OLT(config-interface-xge-0/0)#

XGE port

**multicast-vlan view**

OLT(config-multicast-vlan-100)#

multicast-vlan *vlanid*

*vlanID:*1-4094

Link-aggregation view

**Link-aggregation view**

OLT(config-interface-aggregation)#

**Vlanif layer3 interface view** OLT(config-interface-vlanif-100)#

interface vlanif *vlanID*

*vlanID:*1-4094

**Acl view**

OLT(acl-basic-2000)#

Acl view

btv view

**Btv view**

OLT(config-btv)#

### Enter Enable View

|  |  |
| --- | --- |
| Command | OLT>enable |
| Description | Enter enable view from view mode |

【Example】

Example：Enter enable view from view mode

|  |
| --- |
| OLT>enable  OLT# |

### Enter Config View

|  |  |
| --- | --- |
| Command | OLT#config |
| **Description** | Enter config view from enable mode |

【Example】

Example：Enter enable view from view mode.

|  |
| --- |
| OLT#config  OLT(config)# |

### Enter Interface View

| Command | OLT(config)#interface epon <FrameID/SlotID>  OLT(config)#interface ge <FrameID/SlotID>  OLT(config)#interface link-aggregation  OLT(config)#interface mgmt  OLT(config)#interface vlanif <vlan id>  OLT(config)#interface xge<FrameID/SlotID> |
| --- | --- |
| **view** | Config view |
| **Description** | Enter epon/ge/link-aggregation/mgmt/vlanif/xge view from config mode |
| <vlan id> | VLAN ID value,the range is 1-4094 |
| <FrameID/SlotID> | Device frame id/slot id,default as 0/0，Plug-in 16Port OLT the Frame default is 0,slot need check insert board to input id,the range is 1-4 |

【Example】

Example 1：Enter vlanif view from config mode

|  |
| --- |
| OLT(config)#interface vlanif 100  OLT(config-interface-vlanif-100)# |

Example 2：Enter ge view from config mode

|  |
| --- |
| OLT(config)#interface ge 0/0  OLT(config-interface-ge-0/0)#exit |

Example 3：Enter epon view from config mode

|  |
| --- |
| OLT(config)#interface epon 0/0  OLT(config-interface-epon-0/0)# |

### Enter ACL View

| Command | OLT(config)#acl <acl id> |
| --- | --- |
| **view** | Config view |
| **Description** | Enter acl view from config mode |
| <acl id> | <2000-2999>basic acl/  <3000-4999>advanced acl/  <5000-5999>link acl  <8000-8199>PON side acl  <9000-9499> ONT side acl |

【Example】

Example 1：Enter basic acl view from config mode

|  |
| --- |
| OLT(config)#acl 2000  ACL ID Create OK!  OLT(acl-basic-2000)# |

Example 2：Enter advanced acl view from config mode

|  |
| --- |
| OLT(config)#acl 3000  ACL ID Create OK!  OLT(acl-adv-3000)# |

Example 3：Enter link acl view from config mode

|  |
| --- |
| OLT(config)# acl 5000  ACL ID Create OK!  OLT(acl-link-5000)# |

Example 4：Enter pon side acl view from config mode

|  |
| --- |
| OLT(config)#acl 8000  OLT(acl-pon-8000)# |

Example 5：Enter ONT side acl view from config mode

|  |
| --- |
| OLT(config)# acl 9000  ACL ID Create OK!  OLT(acl-onu-9000)# |

### Enter Multicast-vlan View

|  |  |
| --- | --- |
| Command | OLT(config)#multicast-vlan <multicast-vlan id> |
| **view** | Config view |
| **Description** | Enter multicast-vlan view from config mode |
| <multicast-vlan ID> | Multicast vlan ID,the range is 1-4094. |

【Example】

Example 1：Enter multicast-vlan view from config mode

|  |
| --- |
| OLT(config)#multicast-vlan 100  OLT(config-multicast-vlan-100)# |

### Exit Arbitrary View

|  |  |
| --- | --- |
| Command | OLT(config)#exit |
| **Desceiption** | Exit current view to previous view. |

【Example】

Example 1：Exit config view to enable view.

|  |
| --- |
| OLT(config)#exit  OLT# |

# OLT Device Upgrade Management

## Upgrade OLT software

|  |  |
| --- | --- |
| Command | OLT(config)# load packetfile ftp <server-ip> <user-name> <user-password> | tftp <server-ip> <file-name> |
| **view** | Enable view、config view |
| **Description** | This command is used for upgrade olt software version and kernel version,it should be use in root account. |
| <ftp-server-ip> | The ip address of ftp server |
| <user-name> | The user name which had set in ftp server |
| <user-password> | The user password which had set in ftp server |
| <file-name> | The name of the OLT software to be downloaded. |

【Example】

Example 1：Upgrade olt software,its file name is New16Port\_FW\_V1.0.2\_150914\_1603.img,the ip address of ftp server is 192.168.1.16,ftp user name is admin,ftp user password is admin.After the olt displays“upgrade OK”,reboot the olt.

|  |
| --- |
| OLT(config)#load packetfile ftp 192.168.1.16 admin admin New16Port\_FW\_V1.0.2\_150  914\_1603.img  Broadcast message from root:  Upgrade is in process.  File[New16Port\_FW\_V1.0.2\_150914\_1603.img]download..........OK  File[New16Port\_FW\_V1.0.2\_150914\_1603.img]upgrade..........OK |

Example 2：Upgrade the kernel of olt,its file name is New16Port\_Kernel\_150914\_1605.img,the ip address of ftp server is 192.168.1.16,ftp user name is admin,ftp user password is admin.After the olt displays“upgrade OK”,reboot the olt.

|  |
| --- |
| OLT(config)#load packetfile ftp 192.168.1.16 admin admin New16Port\_Kernel\_150914  \_1605.img  Broadcast message from root:  Upgrade is in process.  File[New16Port\_Kernel\_150914\_1605.img]download.............OK  File[New16Port\_Kernel\_150914\_1605.img]upgrade.............OK |

## Check OLT Software and Hardware Version

|  |  |
| --- | --- |
| Command | OLT(config)# show version |
| **view** | enable view or config view |
| **Description** | This command can check the OLT hardware、software and kernel version information. |

【Example】

Example1：Check OLT firmware version.

|  |
| --- |
| OLT(config)# show version  Hardware version : V1.0B1  Firmware version : V1R03B002 (Mon, 07 Jan 2019 11:43:21 +0800)  Kernel version : V1.0.0\_190107 (Mon, 07 Jan 2019 11:33:47 +0800)  Web version : V1.1.0\_181125 (Sun, 25 Nov 2018 11:26:18 +0800)  OLT(config)# |

## Show the progress of current load/copy/backup in olt

|  |  |
| --- | --- |
| Command | OLT(config)#show progress load |
| **view** | Enable view,config view |
| **Description** | This command is used when the device is performing load,copy,and backup operations,if you need to see the progress of the current operation and understand the status of the operation. |

【Example】

Example 1：Check the status of load progress

|  |
| --- |
| OLT(config)#show progress load  -----------------------------------------------------------------------------  Transmit Protocal:FTP  FTP Server:192.168.1.16  FTP User Name:admin  FTP Password:admin  Transmit FileName:config  Transmit Action:Put  Transmit Status:Success  Transmit Progress:100%  -----------------------------------------------------------------------------  Load Operation:Null  Load FileName:config  ----------------------------------------------------------------------------- |

## Delete Loaded Files

|  |  |
| --- | --- |
| Command | OLT(config)# file delete [file-name] |
| **View** | config view |
| **Description** | This command is used to delete a single file in the file system. You can use this command to delete a file that was previously loaded or unused by the load file command. The files to be deleted can be stored in the flash or cf card. Use this command with caution. Once the file is deleted, it will not be recoverable. |
| [file-name] | Name of the OLT software to be deleted |

【Example】

Example 1：Delete all files

|  |
| --- |
| OLT(config)# file delete  ERROR: Not any user files!  OLT(config)# |

## Enable/disable web

| Command | OLT(config)# web server enable|disable |
| --- | --- |
| **View** | config view |
| **Description** | This command is used to enable or disable the WEB function. The web can be opened only if the web is enabled. |

【Example】

Example 1：Enable web.

|  |
| --- |
| OLT(config)# web server enable  Enable web server successful!  OLT(config)# |

## Uninstall the Installed Web

|  |  |
| --- | --- |
| Command | OLT(config)# web server enable|disable |
| **View** | config view |
| **Description** | This command is used to uninstall the installed WEB function. |

【Example】

Example 1：Uninstall the installed WEB function.

|  |
| --- |
| OLT(config)# web uninstall  Uninstall web server successful!  OLT(config)# |

# OLT Device Management

## OLT Reboot

|  |  |
| --- | --- |
| Command | OLT(config)#reboot |
| **view** | Enable view or config view |
| **Description** | This command is used for reboot OLT,only the root user group has this permission. |

【Example】

Example1：reboot OLT

|  |
| --- |
| OLT#reboot  Please check whether data has saved,the unsaved data will lose if reboot syst  em.Are you sure to reboot system?(y/n)[n]:y |

## Config OLT Reset Button

|  |  |
| --- | --- |
| Command | OLT(config)# reset key action set reboot|factory |
| **View** | Config view |
| **Description** | This command is used to control the reset button through the CLI to restore the OLT to the factory default or reset. After the setting is completed, press the reset button, the OLT will resume the factory or restart. |

【Example】

Example 1：Set the OLT reset button to restore the factory.

|  |
| --- |
| OLT(config)# reset key action set factory  Reset key action set factory reset successful!  OLT(config)# |

## Config OLT Outband Manager IP

### Config OLT Outband Manager IP Address

|  |  |
| --- | --- |
| Command | OLT(config-interface-mgmt)#ip address <ip-address> {<ip-address-mask>|<length of mask>} |
| **View** | Mgmt view |
| **Description** | The IP address command is used for configure IP addresses and subnet masks of management interfaces.You can visit OLT by this IP address. |
| <ip-address> | IP address.The IP address is divided into five categories,and the user can choose the appropriate IP subnet according to the actual situation.The host address part is all 0 or all 1 has special function,which cannot be used as the general IP address. |
| <ip-address-mask> | Subnet mask.Format for X.X.X.X |
| <length of mask> | length of subnet mask,the range is 0-32 |

【Example】

Example 1：Config the ip address of mgmt interface as 192.168.5.63,the length of subnet mask is 24.

|  |
| --- |
| OLT(config-interface-mgmt)#ip address 192.168.5.63 24  OLT(config-interface-mgmt)# |

### Config OLT Outband Manager IP Description

|  |  |
| --- | --- |
| Command | OLT(config-interface-mgmt)# description description-information |
| **View** | Mgmt view |
| **Description** | This command is used for name the OLT out-of-band management IP for user management. |
| description-information | Named name, the name length ranges from 1-128. |

【Example】

Example 1：Config the ip address of mgmt interface name as test.

|  |
| --- |
| OLT(config-interface-mgmt)# description test  Set interface description successfully!  OLT(config-interface-mgmt)# |

### Delete OLT Outband Manager IP Configuration

|  |  |
| --- | --- |
| Command | OLT(config-interface-mgmt)# no (description |ip address ) |
| **View** | Mgmt view |
| **Description** | This command is used for delete name or address of the OLT out-of-band management IP. |

【Example】

Example 1：Delete the ip address of mgmt interface name.

|  |
| --- |
| OLT(config-interface-mgmt)# no description  Delete interface description successfully!  OLT(config-interface-mgmt)# |

### Config Switch OLT Outband Manager IP

|  |  |
| --- | --- |
| Command | OLT(config-interface-mgmt)# (no) shutdown |
| **View** | Mgmt view |
| **Description** | This command is used for enable/disable the OLT out-of-band management IP. |

【Example】

Example 1：Enable the ip address of mgmt interface.

|  |
| --- |
| OLT(config-interface-mgmt)# no shutdown  OLT(config-interface-mgmt)# |

### Show MGMT IP Address

|  |  |
| --- | --- |
| Command | OLT(config)#show interface mgmt |
| **view** | Config view |
| **Description** | This command is used for query the ip address,mac address,the Maximum Transmit Unit and etc info of mgmt interface. |

【Example】

Example 1：Show the ip address,mac address,the Maximum Transmit Unit and etc info of mgmt interface

|  |
| --- |
| OLT(config)#show interface mgmt  Description:Outband management interface  The Maximum Transmit Unit is 1500 bytes  Internet Address is 192.168.5.63,netmask 255.255.255.0  Hardware address is E0:56:43:A9:B4:19  Recive 96006 packets,10423985 bytes  Transmit 10753 packets,783785 bytes  OLT(config)# |

### Exit to Config View

|  |  |
| --- | --- |
| Command | OLT(config-interface-mgmt)# exit |
| **View** | Mgmt view |
| **Description** | This command is used for Exit from mgmt view to config view |

【Example】

Example 1：Exit from mgmt view to config view.

|  |
| --- |
| OLT(config-interface-mgmt)# exit  OLT(config)# |

### Exit to View

|  |  |
| --- | --- |
| Command | OLT(config-interface-mgmt)# end |
| **View** | Mgmt view |
| **Description** | This command is used for exit from mgmt view to view. |

【Example】

Example 1：Exit from mgmt view to view.

|  |
| --- |
| OLT(config-interface-mgmt)# end  OLT> |

## Config OLT Inband Vlanif IP

### Config OLT Inband Vlanif Address

|  |  |
| --- | --- |
| Command | OLT(config-interface-vlanif-100)#ip address <ip-address> {<ip-address-mask>|<length of mask>} |
| **view** | Vlanif view |
| **Description** | The IP address command is used for configure the IP address and subnet mask of the VLAN interface.This command is used when the IP packet in the VLAN is required to participate in the three-tier forwarding.After the IP address of the configuration interface and the subnet mask are successful,the IP packet in the VLAN is forwarded by this ip in three layers. |
| <ip-address> | IP address.The IP address is divided into five categories,and the user can choose the appropriate IP subnet according to the actual situation.The host address part is all 0 or all 1 has special function,which cannot be used as the general IP address. |
| <ip-address-mask> | Subnet mask.Format for X.X.X.X |
| <length of mask> | length of subnet mask the range is 0-32 |

【Example】

Example 1：Config the ip address of vlanif interface as 192.168.100.1,subnet mask is 255.255.255.0.

|  |
| --- |
| OLT(config-interface-vlanif-100)#ip address 192.168.100.1 255.255.255.0  OLT(config-interface-vlanif-100)# |

### Config OLT Inband Manager IP Description

|  |  |
| --- | --- |
| Command | OLT(config-interface-vlanif-100)# description description-information |
| **View** | Vlanif view |
| **Description** | This command is used for name the OLT inband management IP for user management. |
| description-information | Named name, the name length ranges from 1-128. |

【Example】

Example 1：Config the vlanif-100 interface name as test.

|  |
| --- |
| OLT(config-interface-vlanif-100)# description test  Set interface description successfully!  OLT(config-interface-vlanif-100)# |

### Config OLT DHCP-Client Option 60

|  |  |
| --- | --- |
| Command | OLT(config-interface-vlanif-100)# dhcp-client (enable|disable|option60 option60|release|renew) |
| **View** | Vlanif view |
| **Description** | This command is used for configure the option60 information carried by the DHCP-Client when sending request packets. When the upstream device is configured with the DHCP Layer 3 relay function, you can use this command to configure the option60 information of the interface to match the configuration of the upstream device. |
| Option60 | The option60 information carried in the DHCP packets sent by the interface when the IP address is obtained through DHCP. Length is 1-32 |

【Example】

Example 1：Enable dhcp-client.

|  |
| --- |
| OLT(config-interface-vlanif-100)# dhcp-client enable  OLT(config-interface-vlanif-100)# |

### Delete OLT Inband Manager IP Configuration

|  |  |
| --- | --- |
| Command | OLT(config-interface-vlanif-100)# no (description |ip address|dhcp-client option60 ) |
| **View** | vlanif view |
| **Description** | This command is used for delete name,address or dhcp-client of the OLT out-of-band management IP. |

【Example】

Example 1：Delete the ip address of vlanif interface name.

|  |
| --- |
| OLT(config-interface-vlanif-100)# no description  Delete interface description successfully!  OLT(config-interface-vlanif-100)# |

### Config Switch OLT Outband Manager IP

|  |  |
| --- | --- |
| Command | OLT(config-interface-vlanif-100)# (no) shutdown |
| **View** | vlanif view |
| **Description** | This command is used for enable/disable the OLT inband management IP. |

【Example】

Example 1：Enable the ip address of vlanif interface.

|  |
| --- |
| OLT(config-interface-vlanif-100)# shutdown  OLT(config-interface-vlanif-100)# |

### Show Vlanif IP Address

|  |  |
| --- | --- |
| Command | OLT(config)#show interface vlanif <vlan-interface-number> |
| **view** | Config view |
| **Description** | This command is used for query the ip address,mac address,the Maximum Transmit Unit and etc info of vlanif interface. |
| <vlan-interface-number> | The id of vlanif interface,its range is 1-4094 |

【Example】

Example 1：Show the ip address,mac address,the Maximum Transmit Unit and etc info of vlanif interface

|  |
| --- |
| OLT(config)#show interface vlanif 100  Description:Inband interface vlanif100  The Maximum Transmit Unit is 1500 bytes  Internet Address is 192.168.100.1,netmask 255.255.255.0  Hardware address is E0:56:43:A9:B4:1A  Recive 0 packets,0 bytes  Transmit 0 packets,0 bytes  OLT(config)# |

Example 2:Show the information of all the vlanif interface

|  |
| --- |
| OLT(config)#show interface vlanif  Description:Inband interface vlanif100  The Maximum Transmit Unit is 1500 bytes  Internet Address is 192.168.100.1,netmask 255.255.255.0  Hardware address is E0:56:43:A9:B4:1A  Recive 0 packets,0 bytes  Transmit 0 packets,0 bytes  Description:Inband interface vlanif200  The Maximum Transmit Unit is 1500 bytes  Internet Address is 192.168.6.66,netmask 255.255.255.0  Hardware address is E0:56:43:A9:B4:1A  Recive 0 packets,0 bytes  Transmit 0 packets,0 bytes  OLT(config)# |

### Exit to Config View

|  |  |
| --- | --- |
| Command | OLT(config-interface-vlanif-100)# exit |
| **View** | vlanif view |
| **Description** | This command is used for Exit from vlanif view to config view |

【Example】

Example 1：Exit from vlanif view to config view.

|  |
| --- |
| OLT(config-interface-vlanif-100)# exit  OLT(config)# |

### Exit to View

|  |  |
| --- | --- |
| Command | OLT(config-interface-vlanif-100)# end |
| **View** | vlanif view |
| **Description** | This command is used for exit from vlanif view to view. |

【Example】

Example 1：Exit from vlanif view to view.

|  |
| --- |
| OLT(config-interface-vlanif-100)# end  OLT> |

### Clear Statistics Interface Vlanif

| Command | OLT(config)# clear statistics interface vlanif vlan-interface-number |
| --- | --- |
| **View** | Config view |
| **Description** | This command is used for clear statistics interface vlanif. |

【Example】

Example 1：Clear statistics interface vlanif.

|  |
| --- |
| OLT(config)# clear statistics interface vlanif 100  OLT(config)# |

## Show OLT Detail Information

|  |  |
| --- | --- |
| Command | OLT(config)#show device |
| **view** | Enable view,config view |
| **Description** | This command is used for Show the device model/mac address/SN/vendor name and etc info of olt. |

【Example】

Example 1：Show the device info of olt.

|  |
| --- |
| OLT(config)#show device  -----------------------------------------------------------------------------  Device model:epon  Device MAC address:E0:56:43:A9:B4:19  Device serial-number:AF1701-16080003  Device vendor name:XPON  -----------------------------------------------------------------------------  OLT(config)# |

## Config OLT User Logout Time

| Command | OLT(config)#exec-timeout <time> |
| --- | --- |
| **view** | enable view,config view |
| **Description** | This command is used for configure the user login timeout,which will automatically log out when the user does not do anything with the device at the set time.The default is 300 seconds. |
| <time> | The time of timeout,its unit is second. |

【Example】

Example 1：Config the timeout time as 36000s.

|  |
| --- |
| OLT(config)#exec-timeout 36000  OLT(config)# |

## Show OLT User Logout Time

|  |  |
| --- | --- |
| Command | OLT(config)#show exec-timeout |
| **view** | Enable view,config view |
| **Description** | This command is used for show the user timeout time. |

【Example】

Example 1：show the user timeout time

|  |
| --- |
| OLT#show exec-timeout  Timeout:36000s  OLT# |

## Logout System

|  |  |
| --- | --- |
| Command | OLT(config)#logout |
| **view** | View view,enable view,config view |
| **Description** | This command is used for logout current system |

【Example】

Example 1：Logout the system.

|  |
| --- |
| OLT#logout  >>User name: |

## Exit OLT Current View Mode

|  |  |
| --- | --- |
| Command | OLT(config)#end |
| **view** | Enable view,config view |
| **Description** | This command is used for enter view mode from current view. |

【Example】

Example 1：Exit config view to view mode

|  |
| --- |
| OLT(config)#end  OLT> |

## Config OLT DNS server IP Address

|  |  |
| --- | --- |
| Command | OLT(config)#dns server <ip-addr> |
| **view** | Config view |
| **Description** | This command is used for configure the ip address of DNS server. |
| <ip-addr> | IP address,format for X.X.X.X |

【Example】

Example 1：Config the ip address of olt’s DNS server as 192.168.5.1

|  |
| --- |
| OLT(config)#dns server 192.168.5.1  OLT(config)# |

## Delete OLT DNS Server IP Address

|  |  |
| --- | --- |
| Command | OLT(config)#no dns server <ip-addr> |
| **view** | Config view |
| **Description** | This command is used for delete the ip address of DNS server.when there is no parameter after dns server,it is used for delete the primary and secondary dns server. |
| <ip-addr> | IP address,format for X.X.X.X |

【Example】

Example 1：Remove the DNS server's IP address 192.168.5.1 in olt

|  |
| --- |
| OLT(config)#no dns server 192.168.5.1  OLT(config)# |

## Show OLT DNS Server IP Address

|  |  |
| --- | --- |
| Command | OLT(config)#show dns server |
| **view** | Config view |
| **Description** | This command is used for show ip address of DNS server. |

【Example】

Example 1：Show the ip address of the DNS server.

|  |
| --- |
| OLT(config)#show dns server  IPv4 Dns Servers:  Domain-server IpAddress  1 192.168.5.1  OLT(config) |

## Config OLT Hostname

| Command | OLT(config)#sysname <name> |
| --- | --- |
| **view** | Config view |
| **Description** | This command is used for set the olt’s sysname which is show in command windows. |
| <name> | Olt’s name,support 1-16 strings. |

【Example】

Example 1：Config the olt’s sysname as test.

|  |
| --- |
| OLT(config)#sysname test  test(config)# |

## Enable/disable PON laser control

|  |  |
| --- | --- |
| Command | OLT(config)# pon laser-control on|off |
| **View** | Config view |
| **Description** | This command is used to enable/disable PON laser control of the OLT. |

【Example】

Example 1： Enable/disable PON laser control of the OLT.

|  |
| --- |
| OLT(config)# pon laser-control on  OLT(config)# |

## Config a Remote System Host

|  |  |
| --- | --- |
| Command | OLT(config)# telnet ip-address|host-name tcp-port |
| **View** | config view |
| **Description** | This command is used to config a remote system host. |

【Example】

Example 1：Config the IP of the remote host and enter its terminal.

|  |
| --- |
| OLT(config)# telnet 192.168.5.68  \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*  \*\* GPON OLT Integrated Operating System. \*\*  \*\* Device Model : df1234s \*\*  \*\* Hardware version : V3.0 \*\*  \*\* Firmware version : V1.0.6\_190909 \*\*  \*\* BuildDate : Mon, 09 Sep 2019 11:08:59 +0800 \*\*  \*\* Mac Address : E0:56:B2:00:00:01 \*\*  \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*  >>User name: |

## Config Terminal Output Printing

|  |  |
| --- | --- |
| Command | OLT(config)# vty output <global> show-all|show-more |
| **View** | config view |
| **Description** | This command is used when the terminal has more output prints, show-all is full print, and show-more is part of the print. |

【Example】

Example 1：Config the terminal to output full print.

|  |
| --- |
| OLT(config)# vty output show-all  OLT(config)# |

# OLT Status Monitor

## Show OLT Fan Working Status

|  |  |
| --- | --- |
| Command | OLT(config)#show fan |
| **view** | enable view,config view |
| **Description** | This command is used for show the working status of fan. |

【Example】

Example 1：Show the working status of fan

|  |
| --- |
| OLT#show fan  -----------------------------------------------------------------------------  FAN[1]status:Normal(7200RPM)  FAN[2]status:Normal(7020RPM)  FAN[3]status:Normal(7140RPM)  -----------------------------------------------------------------------------  OLT# |

## Show OLT Working Temperature

|  |  |
| --- | --- |
| Command | OLT(config)#show temperature |
| **view** | enable view,config view |
| **Description** | This command is used for show the real time working temperature of olt |

【Example】

Example 1：Show the real time working temperature of olt

|  |
| --- |
| OLT#show temperature  The temperature of the board:45.0(C)  OLT# |

## Show OLT Memory Usage

|  |  |
| --- | --- |
| Command | OLT(config)#show memory |
| **view** | enable view,config view |
| **Description** | This command is used for show the memory usage of OLT. |

【Example】

Example 1：Show the memory usage of OLT.

|  |
| --- |
| OLT#show memory  -----------------------------------------------------------------------------  Total memory:242MB  Free memory:124MB  Utilization:49%  -----------------------------------------------------------------------------  OLT# |

## Config OLT System Time

|  |  |
| --- | --- |
| Command | OLT(config)#time <time> |
| **view** | config view |
| **Description** | This command is used for Set the system time of olt |
| <time> | Time,format for YYYY/MM/DD-HH:MM:SS |

【Example】

Example 1：Set the system time of olt

|  |
| --- |
| OLT(config)#time 2019/01/08-13:44:00  OLT(config)# |

## Show OLT System Time

|  |  |
| --- | --- |
| Command | OLT(config)#show time |
| **view** | enable view,config view |
| **Description** | This command is used for show the system time of olt. |

【Example】

Example 1：show the system time of olt.

|  |
| --- |
| OLT(config)# show time  2019-01-08 13:44:06 +00:00  OLT(config)# |

## Show OLT Boot Time and Running Time

|  |  |
| --- | --- |
| Command | OLT(config)#show uptime |
| **view** | enable view,config view |
| **Description** | This command is used for show the up time and boot time of the olt |

【Example】

Example 1：Show the up time and boot time of the olt

|  |
| --- |
| OLT# show uptime  System up time : 0 day 20 hour 47 minute 8 second  System boot time : Mon Jan 7 16:57:59 2019  OLT# |

## Config OLT NTP Time and Server

| Command | OLT(config)#ntp-service unicast-service {<ip-addr>|<domain name>} |
| --- | --- |
| **view** | config view |
| **Description** | This command is used for set the ip address of the NTP server. |
| <ip-addr> | Ip address of NTP server,format for X.X.X.X |
| <domain name> | The domain name of NTP server |

【Example】

Example 1：Set the NTP server’s ip address as 202.120.2.101

|  |
| --- |
| OLT(config)#ntp-service unicast-service 202.120.2.101  OLT(config)# |

## Delete NTP Time and Server

|  |  |
| --- | --- |
| Command | OLT(config)#no ntp-service unicast-service {<ip-addr>|<domain name>} |
| **view** | Config view |
| **Description** | This command is used for Delete the NTP server |
| <ip-addr> | IP address of NTP server,format for X.X.X.X |
| <domain name> | The domain name of NTP server |

【Example】

Example 1：Delete the NTP server’s ip address 202.120.2.101

|  |
| --- |
| OLT(config)#no ntp-service unicast-service 202.120.2.101  OLT(config)# |

## Show NTP Server Session Information

|  |  |
| --- | --- |
| Command | OLT(config)#show ntp-service session |
| **View** | Config view |
| **Description** | This command is used for show the session info of the NTP server |

【Example】

Example 1：Show the session info of the NTP server

|  |
| --- |
| OLT(config)#show ntp-service session  clock source:202.120.2.101  clock stratum:0  clock status:configured  reference clock ID:0.0.0.0  reach:0  current poll:64 secs  now:0  offset:+0.000000ms  delay:0.000000  disper:0.000000  OLT(config)# |

## Config OLT Systme Timezone

|  |  |
| --- | --- |
| Command | OLT(config)#timezone {gmt+/gmt} -<timezone> |
| **View** | Config view |
| **Description** | This command is used for set the system timezone of the olt.GMT+represents the eastern time zone,which means local time is faster than Greenwich mean time,and GMT-means the west time zone,which means local time is slower than Greenwich mean time. |
| <timezone> | The time of timezone,format for hh:mm.The max value of eastern timezone is 18:00,and the max value of west timezone is 18:00. |

【Example】

Example 1：Set the system timezone of the olt as gmt+08:00

|  |
| --- |
| OLT(config)#timezone gmt+08:00  OLT(config)# |

## Show OLT System Current Timezone

| Command | OLT(config)#show timezone |
| --- | --- |
| **View** | Config view |
| **Description** | This command is used for show the system current timezone of the olt |

【Example】

Example 1：Show the system current timezone of the olt

|  |
| --- |
| OLT(config)#show timezone  The current time zone:GMT+08:00  OLT(config)# |

## Config OLT System Temperature Threshold

|  |  |
| --- | --- |
| Command | OLT(config)# temperature threshold high-temperature value |
| **View** | config view |
| **Description** | This command is used to configure the temperature threshold of the OLT system. If the real-time temperature is higher than the configured system temperature threshold, the alarm will be reported. The default is 80℃. |
| *time* | Loop detection interval, ranging from 5 to 300, in seconds. |

【Example】

Example 1：Set the maximum OLT system temperature threshold to 40℃.

|  |
| --- |
| OLT(config)# temperature threshold high-temperature 40  OLT(config)# |

## Show OLT System Temperature Threshold

|  |  |
| --- | --- |
| Command | OLT(config)# show temperature threshold |
| **View** | config view |
| **Description** | This command is used to view the temperature threshold of the OLT system. |

【Example】

Example 1：View the OLT system temperature threshold.

|  |
| --- |
| OLT(config)# show temperature threshold  The temperature high-threshold of the system : 80(C)  OLT(config)# |

## Show OLT Local MAC Address Information

|  |  |
| --- | --- |
| Command | OLT(config)#show location<mac-addr> |
| **view** | config view |
| **Description** | This command is used for show the local mac address info of the olt |
| <mac-addr> | Mac address,format for xx:xx:xx:xx:xx:xx |

【Example】

Example 1：Show the local mac E0:56:43:A9:B4:1A info of the olt.

|  |
| --- |
| OLT(config)#show location E0:56:43:A9:B4:1A  -----------------------------------------------------------------------------  Total:2  -----------------------------------------------------------------------------  MAC VLAN Port MAC-Type  -----------------------------------------------------------------------------  E0:56:43:A9:B4:1A 100 cpu static  E0:56:43:A9:B4:1A 200 cpu static  -----------------------------------------------------------------------------  OLT(config)# |

## Show OLT CPU Usage

|  |  |
| --- | --- |
| Command | OLT(config)#show cpu |
| **View** | Config view |
| **Description** | This command is used for show the cpu status of the olt. |

【Example】

Example 1：Show the cpu status of the olt

|  |
| --- |
| OLT(config)#show cpu  -----------------------------------------------------------------------------  Utilization:54%  Load Average(1min):8.11  Load Average(5min):8.38  Load Average(15min):8.39  -----------------------------------------------------------------------------  OLT(config)# |

## Show OLT History Input Command

|  |  |
| --- | --- |
| Command | OLT(config)#show history |
| **View** | enable view,config view |
| **Description** | This command is used for show the command input history information of the olt |

【Example】

Example 1：Show the command input history information of the olt

|  |
| --- |
| OLT(config)#show history  enable  config  exec-timeout 36000  exit  show dns server  show cpu  OLT(config)# |

## Enable/disable loop detection for the OLT system

| Command | OLT(config)# loopback-detection enable|disable |
| --- | --- |
| **View** | config view |
| **Description** | This command is used to enable/disable loop detection of the system. |

【Example】

Example 1：Enable loop detection of the system.

|  |
| --- |
| OLT(config)# loopback-detection enable  OLT(config)# |

## Config the loop detection interval of the OLT system

|  |  |
| --- | --- |
| Command | OLT(config)# loopback-detection interval-time time |
| **View** | config view |
| **Description** | This command is used to configure the loop detection interval of the OLT system. |
| time | Loop detection interval, ranging from 5 to 300, in seconds. |

【Example】

Example 1：Set the loop detection interval of the OLT system to 30 seconds.

|  |
| --- |
| OLT(config)# loopback-detection interval-time 30  OLT(config)# |

## View the loop detection status of the OLT system

|  |  |
| --- | --- |
| Command | OLT(config)# show loopback-detection |
| **View** | config view |
| **Description** | This command is used to view the loop detection status of the OLT system. |

【Example】

Example 1：View the loop detection status of the OLT system.

|  |
| --- |
| OLT(config)# show loopback-detection  -----------------------------------------------------------------------------  System loopback-detection is running  Detection interval time is 30 seconds    Port Enable Per-vlan Control Loopback-status  ge0/0/1 dis dis dis undetected  ge0/0/2 dis dis dis undetected  ge0/0/3 dis dis dis undetected  ge0/0/4 dis dis dis undetected  ge0/0/5 dis dis dis undetected  ge0/0/6 dis dis dis undetected  ge0/0/7 dis dis dis undetected  ge0/0/8 dis dis dis undetected  xge0/0/1 dis dis dis undetected  xge0/0/2 dis dis dis undetected  pon0/0/1 dis dis dis undetected  pon0/0/2 dis dis dis undetected  pon0/0/3 dis dis dis undetected  pon0/0/4 dis dis dis undetected  pon0/0/5 dis dis dis undetected  pon0/0/6 dis dis dis undetected  pon0/0/7 dis dis dis undetected  pon0/0/8 dis dis dis undetected  pon0/0/9 dis dis dis undetected  pon0/0/10 dis dis dis undetected  pon0/0/11 dis dis dis undetected  pon0/0/12 dis dis dis undetected  pon0/0/13 dis dis dis undetected  pon0/0/14 dis dis dis undetected  pon0/0/15 dis dis dis undetected  pon0/0/16 dis dis dis undetected  -----------------------------------------------------------------------------  OLT(config)# |

## Config the Maximum Recorded Value of Performance Statistics

| Command | OLT(config)# statistics max-record <15min record-number of 15min> | <24hour record-number of 24hour > |
| --- | --- |
| **View** | config view |
| **Description** | This command is used to configure the maximum recorded value of OLT performance statistics. |
| record-number of 15min | Config the maximum recorded value of the performance statistics function with a time interval of 15 minutes, ranging from 1-96. |
| record-number of 24hour | Config the maximum recorded value of the performance statistics function with a 24-hour interval, ranging from 1-7. |

【Example】

Example 1：The maximum statistical value of the performance statistics function with a configuration interval of 24 hours is 6.

|  |
| --- |
| OLT(config)# statistics max-record 24hour 6  OLT(config)# |

## Show the Maximum Recorded Value of Performance Statistics

|  |  |
| --- | --- |
| Command | OLT(config)# show statistics max-record |
| **View** | config view |
| **Description** | This command is used to view the maximum recorded value of OLT performance statistics. |

【Example】

Example 1：View the maximum recorded value of performance statistics.

|  |
| --- |
| OLT(config)# show statistics max-record  Port statistics max record: 96(15min), 6(24hour)  OLT(config)# |

# OLT Configuration Manage

## Auto-backup OLT Configuration

|  |  |
| --- | --- |
| Command | OLT(config)#auto-backup server (alarm| configuration| log) (ftp server-ip-address user-name password |tftp server-ip-address) |
| **View** | config view |
| **Description** | Auto-backup of OLT configuration files.When the time for automatic backup is reached, OLT prints the autobackup configuration successfully prompting the backup successfully. |
| server-ip-address | ftp/tftp Server ip address |
| user-name | ftp/tftp user name |
| password | ftp/tftp password |

【Example】

Example1：Auto-backup OLT configuration，ftp server IP address is 192.168.5.183，ftp user name is amdin and password is admin.

|  |
| --- |
| OLT(config)# auto-backup server configuration ftp 192.168.5.183 admin admin  OLT(config)# |

## Autoback OLT Time Configuration

|  |  |
| --- | --- |
| Command | OLT(config)#auto-backup period (alarm| configuration| log) (disable|enable|interver backup-period time backup-time ) |
| **View** | config view |
| **Description** | Config time about the Auto-backup of OLT configuration files. |
| backup-period | Backup cycle, value range is 1-10, unit is days |
| backup-time | Backup time.Format is HH:MM |

【Example】

Example1：Auto-backup OLT configuration intervlan is one day ,time is 10:00.

|  |
| --- |
| OLT(config)# auto-backup period alarm interval 1 time 10:00  OLT(config)# |

## Backup OLT Configuration

|  |  |
| --- | --- |
| Command | OLT(config)#backup configuration ftp <server-ip-address> <user-name> <user-password> <filename> |
| **view** | enable view,config view |
| **Description** | Backup the config file of the olt |
| <server-ip-address> | IP address of the ftp server |
| <user-name> | ftp user name |
| <user-password> | ftp user password |
| <filename> | The name of the backup configuration file,set it by yourself,does not require a file format. |

【Example】

Example 1：Backup the device config file,the ftp user name is admin,password is admin,set the backup file’s name as config.

|  |
| --- |
| OLT(config)#backup configuration ftp 192.168.1.16 admin admin config  Start backup configuration files  The backup is successful  OLT(config)# |

## Download OLT Configuration

| Command | OLT(config)# load configuration format <txt|gz> <ftp server-ip-address user-name user-password |tftp server-ip-address > filename |
| --- | --- |
| **View** | Enable view,config view |
| **Description** | Download the configuration of the olt |
| server-ip-address | IP address of the ftp/tftp server |
| user-name | ftp user name |
| user-password | ftp user password |
| filename | The name of the configuration file to be downloaded,set it by yourself,does not require a file format. |

【Example】

Example 1：Download the configuration file,the ftp user name is admin,password is admin,set the file’s name as config.

|  |
| --- |
| OLT(config)# load configuration format txt tftp 192.168.5.184 test  The new configuration file will overwrite the old one  Are you sure to load new configuration file? (y/n):y  Start loading configuration  The loading is successful!  OLT(config)# |

## Show OLT Current Configuration

|  |  |
| --- | --- |
| Command | OLT(config)#show current-config |
| **View** | Enable view,config view |
| **Description** | This command is used for show the real time configuration file.This command is used when the user completes a set of configurations and verifies that the configuration is correct and needs to query the currently effective configuration command. |

【Example】

Example 1：Show current configuration

|  |
| --- |
| OLT(config)#show current-config  Current configuration:  !  spanning-tree enable  spanning-tree timer max-age 6  spanning-tree timer forward-delay 30  spanning-tree timer hello 1  spanning-tree priority 4096  !  interface ge  spanning-tree edged-port 1 enable  spanning-tree priority 1 16  spanning-tree cost 1 1600  spanning-tree mcheck 1 enable  exit |

## Auto-save OLT Configuration

|  |  |
| --- | --- |
| Command | OLT(config)#autosave {( interval (on|off|configuration interval ) | (time configuration time | on |off )} |
| **View** | Config view |
| **Description** | This command is used for automatically save the configuration file for the current device.The time to configure autosave must be configured with the autosave interval turned off.When the autosave is successful, OLT automatically prints the autosave configuration done! |

【Example】

Example 1：The time of autosave OLT configuration is 06:20.

|  |
| --- |
| OLT(config)# autosave time configuration 06:20  OLT(config)# |

## Save OLT Configuration

|  |  |
| --- | --- |
| Command | OLT(config)#save |
| **View** | enable view,config view |
| **Description** | This command is used for save the olt current configuration |

【Example】

Example 1：Save the olt current configuration

|  |
| --- |
| OLT(config)#save  The percentage of saved data is:0%  The percentage of saved data is:4%  The percentage of saved data is:9%  The percentage of saved data is:13%  The percentage of saved data is:18%  The percentage of saved data is:22%  The percentage of saved data is:27%  The percentage of saved data is:31%  The percentage of saved data is:36%  The percentage of saved data is:40%  The percentage of saved data is:45%  The percentage of saved data is:68%  The percentage of saved data is:81%  The percentage of saved data is:95%  The percentage of saved data is:100%  OLT(config)# |

## Erase OLT Configuration

|  |  |
| --- | --- |
| Command | OLT(config)#erase saved-config |
| **View** | Enable view,config view |
| **Description** | This command is used for erase the configuration,and after executing the command,reboot the OLT,and OLT will restore factory Settings. |

【Example】

Example 1：Erase the saved-config

|  |
| --- |
| OLT#erase saved-config  This command will clear the active board data that has been saved  Please rememb  er to backup the system configuration data  Are you sure to continue?(y/n)[n]:y  Successfully restored factory configuration! |

## Show OLT Auto-back

|  |  |
| --- | --- |
| Command | OLT(config)#show auto-backup (period|server) (alarm|log|configuration) config |
| **View** | Config view |
| **Description** | This command is used for show olt auto-backup time or server configuration. |

【Example】

Example1：Show auto-backup server configuration.

|  |
| --- |
| OLT(config)# show auto-backup server configuration  Trans mode : FTP  IP address : 192.168.5.183  User name : admin  OLT(config)# |

## Show autosave configuration

|  |  |
| --- | --- |
| Command | OLT(config)#show autosave configuration |
| **View** | Config view |
| **Description** | This command is used for show olt autosave configuration. |

【Example】

Example1：Show olt autosave configuration.

|  |
| --- |
| OLT(config)# show autosave configuration  System autosave interval switch: off  Autosave interval: 10 minutes  System autosave time switch: on  Autosave time: 06:20  OLT(config)# |

## Show OLT Saved-config

|  |  |
| --- | --- |
| Command | OLT(config)#show saved-config |
| **View** | enable view,config view |
| **Description** | This command is used for show saved-config |

【Example】

Example 1：show saved-config

|  |
| --- |
| OLT(config)#show saved-config  #Saving user:root  #Saving time:2017-03-20 19:00:02+0800  spanning-tree enable  spanning-tree timer max-age 6  spanning-tree timer forward-delay 30  spanning-tree timer hello 1  spanning-tree priority 4096  interface ge  spanning-tree edged-port 1 enable  spanning-tree priority 1 16  spanning-tree cost 1 1600  spanning-tree mcheck 1 enable  exit |

# OLT Login User Manage

## Add OLT New Login Username and Password

|  |  |
| --- | --- |
| Command | OLT(config)#user add <user-name> <user-password> {admin/guest/root} |
| **View** | Config view |
| **Description** | This command is used for add new users,new user passwords,and the new user groups are root,admin,and guest respectively.  Root:the user has all the permissions for the device.  Admin:users have configuration,view permissions,no restart,upgrade permissions.  Guest:the user has the view configuration,backup permission. |
| <user-name> | New user name |
| <user-password> | New user password |
| admin/guest/  root | The permissions of the new user,there are root/admin/guest respectively. |

【Example】

Example 1：Create an admin user,its name is test,password is test.

|  |
| --- |
| OLT(config)#user add test test admin  OLT(config)# |

## Delete OLT Login User

|  |  |
| --- | --- |
| Command | OLT(config)#user delete <name> |
| **View** | Config view |
| **Descripton** | This command is used for delete the user.caution:the root user cannot be delete. |
| <name> | The user name to be delete |

【Example】

Example 1：Delete the user test.

|  |
| --- |
| OLT(config)#user delete test  OLT(config)# |

## Change OLT Login User Password

|  |  |
| --- | --- |
| Command | OLT(config)#user password <user-name> <user-password> |
| **View** | Config view |
| **Description** | This command is used for change the password of the existing user. |
| <user-name> | The user name of the password to be changed. |
| <user-password> | New password |

【Example】

Example 1：Change the user password to 123456

|  |
| --- |
| OLT(config)#user password test 123456  OLT(config)# |

## Show OLT Exist Username

|  |  |
| --- | --- |
| Command | OLT(config)#show user |
| **View** | Config view |
| **Description** | This command is used for show all of the users which had been created in olt |

【Example】

Example 1：Show all of the users which had been created in olt

|  |
| --- |
| OLT(config)#show user  -----------------------------------------------------------------------------  User Group  ----------------------------------------------------------------------------  root root  yao guest  test admin  -----------------------------------------------------------------------------  OLT(config)# |

## Show OLT Login User Information

|  |  |
| --- | --- |
| Command | OLT(config)#show client |
| **View** | Config view |
| **Description** | This command is used for show the information of online user |

【Example】

Example 1：show the information of online user

|  |
| --- |
| OLT(config)#show client  ID Access-Type User-Name IP-Address Login-Time  ----------------------------------------------------------------------------  >32 Telnet root 192.168.5.67 03:52:47  46 Telnet root 192.168.5.20 00:07:45  OLT(config)# |

## Kill OLT Online User

|  |  |
| --- | --- |
| Command | OLT(config)#client kick-off <client-id> |
| **View** | Config view |
| **Description** | This command is used for kick the other online user off |
| <client-id> | Login user ID,the range can be 1-4294967295.This ID can be viewed through the show client command. |

【Example】

Example 1：Kick the cilent 44 off.

|  |
| --- |
| OLT#client kick-off 44  The user has been kicked off successfully  OLT# |

## Config the specified address segment to log in to the OLT

|  |  |
| --- | --- |
| Command | OLT(config)# (no) ip access-list deny|permit <ip-address wildcard-bits |any |host ip-address> |
| **View** | Config view |
| **Description** | This command is used to configure this parameter when a setting is required to allow access to the device at the specified address. You can control the users who log in to the device using telnet or ssh by setting the address range of the device to access the device based on the security policy. Delete using no. |
| ip-address | IP address to be configured, in the format x.x.x.x |
| *wildcard-bits* | Inverse mask configuration, 0 is the match, 1 is ignored |

【Example】

Example 1：Config an access device that allows the host address to be 192.168.5.184.

|  |
| --- |
| OLT(config)# ip access-list permit host 192.168.5.184  OLT(config)# |

Example 2：Delete the configuration of the ip access table.

|  |
| --- |
| OLT(config)# no ip access-list  Delete Access List Successful!  OLT(config)# |

## View IP access table configuration

|  |  |
| --- | --- |
| Command | OLT(config)# no ip access-list deny|permit <ip-address wildcard-bits |any |host ip-address> |
| **View** | Config view |
| **Description** | This command is used to view the configuration of the specified address segment of the login OLT. |
| ip-address | IP address to be configured, in the format x.x.x.x |
| *wildcard-bits* | Inverse mask configuration, 0 is the match, 1 is ignored |

【Example】

Example 1：View IP access table configuration。

|  |
| --- |
| OLT(config)# show ip access-list  ip access list  permit 192.168.5.184  OLT(config)# |

# OLT SNMP Config

## SNMP Enable and Disable

|  |  |
| --- | --- |
| Command | OLT(config)#snmp-agent {enable|disable} |
| **View** | config view |
| **Description** | The EMS can manager the olt,only if the snmp agent function is enabled.EMS can not manager the olt while this function is disabled. |
| enable|disable | disable：Disable the SNMP agent feature  enable e：Enable the SNMP agent feature |

【Example】

Example 1：Disable the SNMP agent feature

|  |
| --- |
| OLT(config)#snmp-agent disable  OLT(config)# |

Example 2:Enable the SNMP agent feature

|  |
| --- |
| OLT(config)#snmp-agent enable  OLT(config)# |

## Show OLT Snmp Agent Status

|  |  |
| --- | --- |
| Command | OLT(config)#show snmp-agent status |
| **View** | Config view |
| **Description** | This command is used for show the feature status of snmp agent |

【Example】

Example 1：Show the feature status of snmp agent

|  |
| --- |
| OLT(config)#show snmp-agent status  Snmp agent status:Enable  OLT(config)# |

## Config OLT SNMP Community

|  |  |
| --- | --- |
| Command | OLT(config)#snmp-agent community read<community-name> |
| **View** | Config view |
| **Description** | This command is used for config the read community name of SNMP |
| <community-name> | The name of read community and supports 1-32 characters.Generally set to public. |

【Example】

Example 1：Set the snmp agent read community’s name as public

|  |
| --- |
| OLT(config)#snmp-agent community read public |

## Show OLT SNMP Read Community

|  |  |
| --- | --- |
| Command | OLT(config)#show snmp-agent community read |
| **View** | Config view |
| **Description** | This command is used for show the snmp agent read community. |

【Example】

Example 1：Show the snmp agent read community.

|  |
| --- |
| OLT(config)#show snmp-agent community read  -----------------------------------------------------------------------------  Community-Name VACM-Name View-Name  ----------------------------------------------------------------------------  public default all  -----------------------------------------------------------------------------  OLT(config)# |

## Config OLT SNMP Write Community

|  |  |
| --- | --- |
| Command | OLT(config)#snmp-agent community write<community-name> |
| **View** | Config view |
| **Description** | This command is used for config the write community name of SNMP |
| <community-name> | The name of write community and supports 1-32 characters.Generally set to private. |

【Example】

Example 1：Set the snmp agent write community’s name as private

|  |
| --- |
| OLT(config)#snmp-agent community write private  OLT(config)# |

## Show SNMP Write Community

|  |  |
| --- | --- |
| Command | OLT(config)#show snmp-agent community read |
| **View** | Config view |
| **Description** | This command is used for show SNMP agent write community |

【Example】

Example 1：Show SNMP agent write community

|  |
| --- |
| OLT(config)#show snmp-agent community write  -----------------------------------------------------------------------------  Community-Name VACM-Name View-Name  ----------------------------------------------------------------------------  private default all  -----------------------------------------------------------------------------  OLT(config)# |

## Config OLT SNMP Community Group with Authentication

|  |  |
| --- | --- |
| Command | OLT(config)#snmp-agent group v3<group-name>authentication {[notify-view<none|all>][read-view<none|all>][write-view<none|all>]} |
| **View** | Config view |
| **Description** | This command is used for set secure based snmp agent group carrying with authentication |
| <group-name> | Group name,it supports 1-32 characters |
| notify-view | Specifies the notification view corresponding to the group name. |
| read-view | Set the read-only view corresponding to the group name |
| write-view | Set the read/write view corresponding to group name |
| none | Mismatch view |
| all | Match all the view |

【Example】

Example 1：Set secure based snmp agent group carrying with authentication,group name is test,corresponding to all the notification view.

|  |
| --- |
| OLT(config)#snmp-agent group v3 test authentication notify-view all  OLT(config)# |

## Config OLT SNMP Community Group with Unauth

| Command | OLT(config)#snmp-agent group v3<group-name>noauth {[notify-view <none|all>][ read-view <none|all>][ write-view <none|all>]} |
| --- | --- |
| **View** | Config view |
| **Description** | This command is used for Set secure mode based SNMP agent group without authentication |
| <group-name> | Group name,it supports 1-32 characters |
| notify-view | Specifies the notification view corresponding to the group name. |
| read-view | Set the read-only view corresponding to the group name |
| write-view | Set the read/write view corresponding to group name |
| none | Mismatch view |
| all | Match all the view |

【Example】

Example1:Set secure mode based SNMP agent group without authentication,group name is test,corresponding to all the read-view.

|  |
| --- |
| OLT(config)#snmp-agent group v3 test noauth read-view all  OLT(config)# |

## Config OLT SNMP Community Group with Privacy

| Command | OLT(config)#snmp-agent group v3<group-name>privacy {[notify-view <none|all>][ read-view <none|all>][ write-view <none|all>]} |
| --- | --- |
| **View** | Config view |
| **Description** | This command is used for configure a group of secure mode based SNMP agent which carrises with hidden property. |
| <group-name> | Group name,it supports 1-32 characters |
| notify-view | Specifies the notification view corresponding to the group name. |
| read-view | Set the read-only view corresponding to the group name |
| write-view | Set the read/write view corresponding to group name |
| none | Mismatch view |
| all | Match all the view |

【Example】

Example 1：Set secure mode based SNMP agent group carrying with hidden property,group name is test,corresponding to all the write-view.

|  |
| --- |
| OLT(config)#snmp-agent group v3 test privacy write-view all  OLT(config)# |

## Config OLT SNMP Agent Description

|  |  |
| --- | --- |
| Command | OLT(config)#snmp-agent sys-info description<description> |
| **View** | Config view |
| **Description** | This command is used for configure SNMP agent system description info |
| <description> | Description info,it supports 1-100 characters,the default value is description. |

【Example】

Example 1：Configure the SNMP agent system description info as test

|  |
| --- |
| OLT(config)#snmp-agent sys-info description test  OLT(config)# |

## Configure SNMP Agent Location Information

|  |  |
| --- | --- |
| Command | OLT(config)#snmp-agent sys-info location<location> |
| **View** | config view |
| **Description** | This command is used for configure SNMP agent system location info |
| <location> | Description info,it supports 1-100 characters.The default value is location |

【Example】

Example 1：Configure SNMP agent system location info as test1

|  |
| --- |
| OLT(config)#snmp-agent sys-info location test1  OLT(config)# |

## Configure SNMP Agent Contact Infomation

|  |  |
| --- | --- |
| Command | OLT(config)#snmp-agent sys-info contact <contact> |
| **View** | Config view |
| **Description** | This command is used for configure snmp agent contact info |
| <contact> | Description info,it supports 1-100 characters.The default value is contact |

【Example】

Example 1：Configure SNMP agent contact info as test2

|  |
| --- |
| OLT(config)#snmp-agent sys-info contact test2  OLT(config)# |

## Configure Snmp Agent System Name

|  |  |
| --- | --- |
| Command | OLT(config)#snmp-agent sys-info name <name> |
| **View** | Config view |
| **Description** | This command is used for config snmp agent system name |
| <name> | Description info,it supports 1-100 characters.The default value is name |

【Example】

Example 1：Configure the snmp agent system name as test3

|  |
| --- |
| OLT(config)#snmp-agent sys-info name test3  OLT(config)# |

## Show SNMP Agent System Info

|  |  |
| --- | --- |
| Command | OLT(config)#show snmp-agent sys-info |
| **View** | Config view |
| **Description** | This command is used for show snmp agent system info |

【Example】

Example 1：Show snmp agent system info

|  |
| --- |
| OLT(config)#show snmp-agent sys-info  The name of this managed node:  test3  The description of this managed node:  test  The contact person for this managed node:  test2  The physical location of this node:  test1  OLT(config)# |

## Config SNMP Trap IP

| Command | OLT(config)#snmp-agent trap <host-name> <ip-addr> <port> <community-name> |
| --- | --- |
| **View** | Config view |
| **Description** | This command is used for configure the alarm receive ip of snmp agent |
| <host-name> | Description info,it supports 1-32 characters |
| <ip-addr> | Alarm receive ip |
| <port> | Receive the alarm port number,the range is 1-65535. |
| <community-name> | Community name,it supports 1-32 characters. |

【Example】

Example 1：Configure the snmp agent alarm receive ip as 192.168.5.185,host is test,port number is 563,community name is public.

|  |
| --- |
| OLT(config)#snmp-agent trap test 192.168.5.185 563 public  OLT(config)# |

## Show SNMP Trap IP Infor

|  |  |
| --- | --- |
| Command | OLT(config)#show snmp-agent trap |
| **View** | Config view |
| **Description** | This command is used for show SNMP agent alarm receive ip info |

【Example】

Example 1：Show SNMP agent alarm receive ip info

|  |
| --- |
| OLT(config)#show snmp-agent trap  -----------------------------------------------------------------------------  Index Host-Name IP-Address Port Community-Name  ----------------------------------------------------------------------------  1 test 192.168.5.185 563 public  -----------------------------------------------------------------------------  OLT(config)# |

## Config SNMP Access User&Auth Mode &Password

| Command | OLT(config)#snmp-agent usm-user v3 <user-name> <group-id> authentication-mode md5 <md5-password> privacy-mode des56 <des56-password> |
| --- | --- |
| **View** | Config view |
| **Description** | This command is used for mapping the snmp agent access entity user to secure group,and configure authentication mode and password meanwhile.The authentication mode is optional parameter.Caution:it is need to create a group of secure mode based snmp agent. |
| <user-name> | Entity access user name |
| <group-id> | Group id which is based on user secure mode. |
| <md5-password> | User authentication password,its length is 8-64 characters. |
| <des56-password> | 56 bits DES encrypted password,its length is 8-64 characters. |

【Example】

Example 1：Set SNMP agent entity access user as test1,mapping it to group test which is based on secure mode,authentication mode is md5,the password is 12345678,the privacy mode is des56 and its password is 11111111

|  |
| --- |
| OLT(config)#snmp-agent usm-user v3 test1 test authentication-mode md5 12345678 privacy-mode des56 111111111  OLT(config)# |

## Show SNMP Access User

|  |  |
| --- | --- |
| Command | OLT(config)#show snmp-agent usm-user <user> |
| **View** | config view |
| **Description** | This command is used for show SNMP agent entity access user |
| <user> | Name of entity access user,it supports 1-64 characters.it’s optional,without this parameter it will show all the entity access user info,if it is added it will show the specified entity access user info. |

【Example】

Example 1：Show all the entity access user info

|  |
| --- |
| OLT(config)#show snmp-agent usm-user  User name:test  Group name:test  Authentication mode:md5  Authentication key:12345678  Privacy mode:des56  Privacy key:12345678  User name:test1  Group name:test  Authentication mode:md5  Authentication key:12345678  Privacy mode:des56  Privacy key:111111111  Total number:2  OLT(config)# |

Example 2：Show SNMP agent entity access user“test”info.

|  |
| --- |
| OLT(config)#show snmp-agent usm-user test  User name:test  Group name:test  Authentication mode:md5  Authentication key:12345678  Privacy mode:des56  Privacy key:12345678 |

# Config OLT PPPoE Agent

## PPPoE Agent Enable and Disable

|  |  |
| --- | --- |
| Command | OLT(config)# pppoe agent enable/disable |
| **View** | Config view |
| **Description** | Enable/Disable pppoe agent. |
| enable/disable | disable：disable pppoe agent.  enable：enable pppoe agent. |

【Example】

Example 1：Disable pppoe agent.

|  |
| --- |
| OLT(config)# pppoe agent disable  OLT(config)# |

## Config PPPoE Forward Policy

|  |  |
| --- | --- |
| Command | OLT(config)# pppoe agent policy (keep|drop|replace) |
| **View** | Config view |
| **Description** | This command is used to configure the forwarding policy of request packets. |
| keep | Forward pppoe message as it is |
| drop | Discard pppoe packets directly |
| replace | Replace the original pppoe message and then forward it |

【Example】

Example 1：Configure the forwarding policy of pppoe to forward according to the original forwarding policy.

|  |
| --- |
| OLT(config)# pppoe agent policy keep  OLT(config)# |

## Config PPPoE Fill Format

|  |  |
| --- | --- |
| Command | OLT(config)# pppoe agent format <type1|type2|type3|type4|type5> |
| **View** | Config view |
| **Description** | This command is used to configure the fill mode of the pppoe option. |
| <type1|type2|type3|type4|type5|type6|type7|type8> | type1：represents UNI+ONU MAC  type2：represents UNI+OLT MAC  type3：represents ONU+ONU MAC  type4：represents ONU+OLT MAC  type5：represents PON+OLT MAC |

【Example】

Example 1：Configure the fill mode of the pppoe option to UNI+ONU MAC

|  |
| --- |
| OLT(config)# pppoe agent format type1  OLT(config)# |

## Show the Configuration of the PPPoE Agent.

|  |  |
| --- | --- |
| Command | OLT(config)# show pppoe agent config |
| **View** | Config view |
| **Description** | This command is used to view the configuration of the pppoe agent. |

【Example】

Example 1：Show the configuration of the PPPoE agent.

|  |
| --- |
| OLT(config)# show pppoe agent config  pppoe agent enable  pppoeplus policy: keep  pppoeplus option82 format: type1  OLT(config)# |

# OLT Uplink Port Configuration

## OLT Uplink Basic Function Configuration

### Disable Uplink Port

|  |  |
| --- | --- |
| Command | OLT(config-interface-ge-0/0)#shutdown <port-list> |
| **View** | XGE view or GE view |
| **Description** | This command is used for disable the specified ge port. |
| <port-list> | The port list to be configured,format for 1,3-5,8. |

【Example】

Example 1：Disable the uplink port ge1-ge3 of olt.

|  |
| --- |
| OLT(config-interface-ge-0/0)#shutdown 1-3  OLT(config-interface-ge-0/0)# |

Example 2:Disable the uplink port ge5 and ge7 of olt.

|  |
| --- |
| OLT(config-interface-ge-0/0)#shutdown 5,7  OLT(config-interface-ge-0/0)# |

### Enable Uplink Port

|  |  |
| --- | --- |
| Command | OLT(config-interface-ge-0/0)#no shutdown <port-list> |
| **View** | XGE view or GE view |
| **Description** | This command is used for enable the specified ge port. |
| <port-list> | The port list to be configured,format for 1,3-5,8. |

【Example】

Example 1：Enable the uplink port ge1-ge3 of olt.

|  |
| --- |
| OLT(config-interface-ge-0/0)#no shutdown 1-3  OLT(config-interface-ge-0/0)# |

Example 2:Enable the uplink port ge5 and ge7 of olt.

|  |
| --- |
| OLT(config-interface-ge-0/0)#no shutdown 5,7  OLT(config-interface-ge-0/0)# |

### Config Uplink Port Name

|  |  |
| --- | --- |
| Command | OLT(config-interface-ge-0/0)#port-name <port-id> <name> |
| **View** | XGE view or GE view |
| **Description** | This command is used for name the ge port,it is convenient for user to manager. |
| <port-id> | The port id to be set,range for 1-8. |
| <name> | The port name to be set |

【Example】

Example 1：Set the port name of ge1 as test.

|  |
| --- |
| OLT(config-interface-ge-0/0)#port-name 1 test  OLT(config-interface-ge-0/0)# |

### Delete Uplink Port Name

|  |  |
| --- | --- |
| Command | OLT(config-interface-ge-0/0)#no port-name <port-id> |
| **View** | XGE view or GE view |
| **Description** | This command is used for restore the name of ge port to the default value. |
| <port-id> | The port id to be set,range for 1-8. |

【Example】

Example 1：Restore the name of ge1 to default value.

|  |
| --- |
| OLT(config-interface-ge-0/0)#no port-name 1  OLT(config-interface-ge-0/0)# |

### Config Uplink Electric Port Auto-negotiation

|  |  |
| --- | --- |
| Command | OLT(config-interface-ge-0/0)#auto-neg <port-list> {enable|disable} |
| **View** | GE view |
| **Description** | This command is used for enable|disable the auto-negotiation mode of Ethernet port.In the case of enabled,the Ethernet port will automatically negotiate port rate and duplex mode with the docking port,and the system will display as auto-negotiation,with the port rate up to 1000M in this mode.In the case of disabled,the rate and working mode of the port is the default value of the system or the set value(that is,mandatory). |
| <port-list> | The port list to be set,format for 5,6-7,8.Port 1-4 is uplink optical port,it does not support auto-negotiation. |
| enable|disable | Enable:Enable the function of port auto-negotiation  Disable:Disable the function of port auto-negotiation |

【Example】

Example 1：Enable the function of ge5 auto-negotiation

|  |
| --- |
| OLT(config-interface-ge-0/0)#auto-neg 5 enable  OLT(config-interface-ge-0/0)# |

Example 2:Disable the function of ge5 auto-negotiation

|  |
| --- |
| OLT(config-interface-ge-0/0)#auto-neg 5 disable  OLT(config-interface-ge-0/0)# |

### Config Uplink Electric Port Duplex Mode

|  |  |
| --- | --- |
| Command | OLT(config-interface-ge-0/0)#duplex <port-list> {full/half} |
| **View** | GE view |
| **Description** | This command is used for set the duplex mode of the Ethernet port.it will work in manual setting mode like full or half duplex.the default is full duplex. |
| <port-list> | The port list to be set,format for 5,6-7,8.Port 1-4 is uplink optical port,it does not support duplex mode setting.the default duplex mode of optical port and electrical port both are full duplex. |
| full/half | full:Full duplex  half:Half duplex |

【Example】

Example 1：Set the duplex mode of uplink port ge5 as half duplex.

|  |
| --- |
| OLT(config-interface-ge-0/0)#duplex 5 half  OLT(config-interface-ge-0/0)# |

### Config Uplink Electric Port Speed

|  |  |
| --- | --- |
| Command | OLT(config-interface-ge-0/0)#speed <port-list> {10/100} |
| **View** | GE view |
| **Description** | This command is used for set the Ethernet port rate that will make the port work in manual setting rate. |
| <port-list> | The port list to be set,format for 5,6-7,8.Port 1-4 is uplink optical port,it does not support the rate setting.the default rate of optical port and electric port both are 1000M. |
| 10/100 | 10:10Mbs  100:100Mbs  Caution:1000Mbs only support auto-negotiation. |

【Example】

Example 1：Set the rate of ge5 as 100Mbs.

|  |
| --- |
| OLT(config-interface-ge-0/0)#speed 5 100  OLT(config-interface-ge-0/0)# |

### Config Uplink Port Max-frame

|  |  |
| --- | --- |
| Command | OLT(config-interface-ge-0/0)# frame-max <port-list> <Maximum-frame-size> |
| **View** | XGE view or GE view |
| **Description** | The frame-max command is used for set the maximum frame length for port transfers.The system default maximum frame length is 1526. |
| <port-list> | The port list to be set,format for 5,6-7,8. |
| <Maximum-frame-size> | The range of mtu：328~16360.Particularly,the frame upper limit of pon port supports 2048. |

【Example】

Example 1：Set the mtu of ge1 as 2000.

|  |
| --- |
| OLT(config-interface-ge-0/0)# frame-max 1 2000  OLT(config-interface-ge-0/0)# |

### Delete Uplink Port Maximum-frame

|  |  |
| --- | --- |
| Command | OLT(config-interface-ge-0/0)#no frame-max <port-list> |
| **View** | XGE view or GE view |
| **Description** | This command is used for reset the default value of the maximum frame value to 1526. |
| <port-list> | The port list to be set,format for 5,6-7,8. |

【Example】

Example 1：Reset the mtu value of GE1 port to default 1526.

|  |
| --- |
| OLT(config-interface-ge-0/0)#no frame-max 1  OLT(config-interface-ge-0/0)# |

### Config Uplink Port Flow-control Function

|  |  |
| --- | --- |
| Command | OLT(config-interface-ge-0/0)#flow-control <port-list>{enable|disable} |
| **View** | XGE view or GE view |
| **Description** | This command is used for enable or disable the flow-control function of the Ethernet port. |
| <port-list> | The port list to be set,format for 5,6-7,8. |
| {enable|disable} | enable:Enable the flow-control  disable:Disable the flow-control |

【Example】

Example 1：Enable the flow-control function of port GE5.

|  |
| --- |
| OLT(config-interface-ge-0/0)#flow-control 5 enable  OLT(config-interface-ge-0/0)# |

### Config Uplink Port MAC Address Learning Function

|  |  |
| --- | --- |
| Command | OLT(config-interface-ge-0/0)#mac-address learning port <port-list> {enable|disable} |
| **View** | XGE view or GE view |
| **Description** | This command is used for enable or disable the learning mac function of GE port. |
| <port-list> | The port list to be set,the range for 1-16,format for 5,6-7,8. |
| {enable|disable} | Enable:Enable GE port’s learning mac function.  Disable:Disable GE port’s learning mac function. |

【Example】

Example 1：Enable GE1 port’s learning mac function.

|  |
| --- |
| OLT(config-interface-ge-0/0)#mac-address learning port 1 enable  OLT(config-interface-ge-0/0)# |

### Show OLT Uplink Port Property and Statuses

|  |  |
| --- | --- |
| Command | OLT(config-interface-ge-0/0)#show port state {<port-id>|all} |
| **View** | XGE view or GE view |
| **Description** | This command is used for show the status info of GE port. |
| {<port-id>|all} | Port-ID:Port id to be show,range for 1-8  All:Show the info of all the port |

【Example】

Example 1：Show property and status of all the GE port.

|  |
| --- |
| OLT(config-interface-ge-0/0)# show port state all  -----------------------------------------------------------------------------  Port Optic Pvid Auto Speed Dup Flow Learn Enable Link Frame  Status Nego /Mbps lex Ctrl Max  -----------------------------------------------------------------------------  ge0/0/1 absence 1 enable 1000 full on enable enable off 1526  ge0/0/2 absence 1 enable 1000 full on enable enable off 1526  ge0/0/3 absence 1 enable 1000 full on enable enable off 1526  ge0/0/4 absence 1 enable 1000 full on enable enable off 1526  ge0/0/5 - 1 enable 1000 full off enable enable off 1526  ge0/0/6 - 1 enable 1000 full off enable enable off 1526  ge0/0/7 - 1 enable 100 full off enable enable off 1526  ge0/0/8 - 1 enable 1000 full off enable enable off 1526  ----------------------------------------------------------------------------- |

Example 2:Show property and status of GE1.

|  |
| --- |
| OLT(config-interface-ge-0/0)# show port state 1  -----------------------------------------------------------------------------  Port name : ge0/0/1  Current port state : enable  Current link state : DOWN  The maximum frame size : 1526  Link speed : autonegotiation(1000 Mbps)  Link duplex : autonegotiation(FULL)  Flow-control : on  Maximum number of learned l2 entries : unlimited  Broadcasts stormcontrol : 150(pps)  Unknow multicasts stormcontrol : disable  Unknow unicasts stormcontrol : 150(pps)  -----------------------------------------------------------------------------  Native-vlan: 1 Link-type: Access Priority: 0  Untagged VLAN ID :  1  -----------------------------------------------------------------------------  Statistics 15 minute status : disable  Statistics 24 hour status : disable  Statistics from last clean(maybe the statistics would overflow):  Input(total):0 bytes  Input:unicast 0, broadcasts 0, multicasts 0, errors 0  Output(total):0 bytes  Output:unicast 0, broadcasts 0, multicasts 0, errors 0  ----------------------------------------------------------------------------- |

### Show OLT Uplink Port Optical Power Information

| Command | OLT(config-interface-ge-0/0)#show ddm-info <port-id> |
| --- | --- |
| **View** | GE view |
| **Description** | This command is used for show optical power info of optical GE port |
| <port-id> | Port id to be set,range for 1-4 |

【Example】

Example 1：Show the optical power info of optical port GE1.

|  |
| --- |
| OLT(config-interface-ge-0/0)#show ddm-info 1  -----------------------------------------------------------------------------  Temperature(C):37.6  Supply Voltage(V):3.32  TX Bias current(mA):32  TX power(dBm):-4.03  RX power(dBm):-15.49  -----------------------------------------------------------------------------  OLT(config-interface-ge-0/0)# |

## Uplink Port Mirror Manage

### Config Uplink Port Mirror Function

| Command | OLT(config-interface-ge-0/0)#mirror src-port <src-port-id> dst-port {ge/xge } <F/S/P> { all/egress/ingress} |
| --- | --- |
| **View** | XGE view or GE view |
| **Description** | This command is used for set the mirror function of the Ethernet port.When it is needed to copy the flow of a port to output in another port,or used to flow monitoring and network fault diagnosis,use this command.when the mirror function of the Ethernet port is set successfully,the message of specified direction in mirror source port will be completely copied to the destination mirror port. |
| <src-port-id> | The port list to be set,the range for 1-8 |
| ge/xge | ge:Giga GE port  xge:10gigabit XGE port |
| <F/S/P> | Destination mirror port id,range for 0/0/1-0/0/8. |
| all/egress/ingress | all:Mirror source port Tx and Rx two-way message.Tx and Rx message of mirror source is completely copied and output to destination mirror port.  egress:Mirror source port Tx message.Completely copy and output the Tx message of mirror source port to the mirror destination port.  ingress:Mirror source port Rx message.Completely copy and output the Rx message of mirror source port to mirror destination port. |

【Example】

Example 1：Mirror both the ingress and egress message of the port GE3 to the port GE5.

|  |
| --- |
| OLT(config-interface-ge-0/0)#mirror src-port 3 dst-port ge 0/0/5 all  OLT(config-interface-ge-0/0)# |

### Delete Uplink Port Mirror Function

|  |  |
| --- | --- |
| Command | OLT(config-interface-ge-0/0)#no mirror src-port<src-port-id> |
| **View** | XGE view or GE view |
| **Description** | This command is used for delete the mirror function configuration of the Ethernet port |
| <src-port-id> | Mirror source port id |

【Example】

Example 1：Delete port GE3 mirror function configuration.

|  |
| --- |
| OLT(config-interface-ge-0/0)#no mirror src-port 3  OLT(config-interface-ge-0/0)# |

### Show Uplink Port Mirror Configuration

|  |  |
| --- | --- |
| Command | OLT(config-interface-ge-0/0)#show mirror |
| **View** | XGE view or GE view |
| **Description** | This command is used for show the Ethernet port mirror function configuration info. |

【Example】

Example 1：Show the GE port mirror function configuration info.

|  |
| --- |
| OLT(config-interface-ge-0/0)#show mirror  -----------------------------------------------------------------------------  Destnation port:ge0/0/5  Source port Ingress Egress  ge0/0/3 Yes Yes  -----------------------------------------------------------------------------  OLT(config-interface-ge-0/0)# |

## Uplink Port Performance Statistics Function

### Config Uplink Port Performance Statistics Threshold

| Command | OLT(config-interface-ge-0/0)#statistics port <port-list> threshold <type> <upper-threshold> <lower-threshold> |
| --- | --- |
| **View** | XGE view or GE view |
| **Description** | This command is used for set the performance statistics threshold of GE port |
| <port-list> | The port list to be set,format for 5,6-7,8. |
| <type-ID> | Range for 1-64,among which:  1:rx-octets:Byte of receive message  2:rx-frames:Frame of receive massage  3:rx-bcasts:Received broadcast message  4:rx-mcasts:Received multicast message  5:rx-64octets:The received message with 64 Bytes  6:rx-65to127octets:The received message with 65-127 Bytes  7:rx-128to255octets:The received message with 128-255 Bytes  8:rx-256to511octets:The received message with 256-511 Bytes  9:rx-512to1023octets:The received message with 512-1023 Bytes  10:rx-1024to1518octets:The received message with 1024-1518 Bytes  13:rx-oversizes:Oversize received packet  20:rx-discards:The discard received message  23:tx-octets:The Byte of transmit message  24:tx-frames:Transmitted frame  25:tx-bcasts:Transmitted broadcast packet  26:tx-mcasts:Transmitted multicast packet  27:tx-64octets:Transmitted packet with 64 bytes  28:tx-65to127octets:Transmitted packet with 65-127 bytes  29:tx-128to255octets:Transmitted packet with 128-255 bytes  30:tx-256to511octets:Transmitted packet with 256-511 bytes  31:tx-512to1023octets:Transmitted packet with 512-1023 bytes  32:tx-1024to1518octets:Transmitted packet with 1024-1518 bytes  35:tx-oversizes:The oversize transmitted message  42:tx-discards:The discard transmitted message |
| <upper- threshold> | The upper limit of threshold,range for 0-4294967295 |
| <lower-threshold> | The lower limit of threshold,range for 0-4294967295 |

【Example】

Example 1：Set the received frame quantities of GE1 port statistics,upper limit for 50000,lower limit for 500.

|  |
| --- |
| OLT(config-interface-ge-0/0)#statistics port 1 threshold 35 50000 500  OLT(config-interface-ge-0/0)# |

### Show Uplink Port Performance Statistics Threshold

**Configuration**

|  |  |
| --- | --- |
| Command | OLT(config-interface-ge-0/0)#show statistics port <port-id> threshold |
| **View** | XGE view or GE view |
| **Description** | This command is used for show the configuration of GE port performance statistics threshold |
| <port-id> | Port id to be show,range for 1-8 |

【Example】

Example 1：Show the configuration of GE1 performance statistics threshold

|  |
| --- |
| OLT(config-interface-ge-0/0)#show statistics port 1 threshold  TX oversize frames:upper:50000 lower:500  OLT(config-interface-ge-0/0)# |

### Clear Uplink Port Performance Statistics Infor

| Command | OLT(config-interface-ge-0/0)# reset statistics port <port-ID> |
| --- | --- |
| **View** | XGE view or GE view |
| **Description** | This command is used for clear the performance statistics info of GE port |
| <port-id> | Port id to be show,range for 1-8 |

【Example】

Example 1：Clear the performance statistics info of GE1 port

|  |
| --- |
| OLT(config-interface-ge-0/0)#reset statistics port 1  OLT(config-interface-ge-0/0)# |

### Config Uplink Port Performance Statistics Period

**15minutes**

|  |  |
| --- | --- |
| Command | OLT(config-interface-ge-0/0)#statistics port <port-list> 15min {enable|disable} |
| **View** | XGE view or GE view |
| **Description** | This command is used for enable or disable 15 minutes time interval function of GE port performance statistics |
| <port-list> | Port list to be set,format for 1,6-7,8 |
| enable|disable | enable:Enable 15 minutes time interval performance statistics  disable:Disable 15 minutes time interval performance statistics |

【Example】

Example 1：Enable port GE1 15 minutes time interval performance statistics

|  |
| --- |
| OLT(config-interface-ge-0/0)#statistics port 1 15min enable  OLT(config-interface-ge-0/0)# |

### Config Uplink Port Performance Statistics Period 24H

| Command | OLT(config-interface-ge-0/0)#statistics port<port-list> 24hour {enable|disable} |
| --- | --- |
| **View** | XGE view or GE view |
| **Description** | This command is used for enable or disable 24 hours time interval function of GE port performance statistics |
| <port-list> | Port list to be set,format for 1,6-7,8 |
| {enable|disable} | enable:Enable 24 hours time interval performance statistics  disable:Disable 24 hours time interval performance statistics |

【Example】

Example 1：Enable port GE1 24 hours time interval performance statistics

|  |
| --- |
| OLT(config-interface-ge-0/0)#statistics port 1 24hour enable  OLT(config-interface-ge-0/0)# |

### Show Uplink Port Current 15min Performance Statistics

|  |  |
| --- | --- |
| Command | OLT(config-interface-ge-0/0)#show statistics port <port-id> current-15min |
| **View** | XGE view or GE view |
| **Description** | This command is used for show the GE port performance statistics for current 15 minutes |
| <port-id> | Port id to be show,range for 1-8 |

【Example】

Example 1：Show the port GE1 performance statistics for current 15 minutes

|  |
| --- |
| OLT(config-interface-ge-0/0)# show statistics port 1 current-15min  -----------------------------------------------------------------------------  Start time of this interval : 2019-01-08 16:29:00+00:00  Total elapsed seconds in this interval : 2  -----------------------------------------------------------------------------  RX TX  octets : 4751 : 64  frames : 54 : 1  unicast frames : 0 : 0  broadcast frames : 35 : 0  multicast frames : 19 : 1  discard frames : 49 : 0  error frames : 0 : 0  oversize frames : 0 : 0  frames 64 octets : 14 : 1  frames 65 to 127 octets : 35 : 0  frames 128 to 255 octets : 5 : 0  frames 256 to 511 octets : 0 : 0  frames 512 to 1023 octets : 0 : 0  frames 1024 to 1518 octets : 0 : 0  -----------------------------------------------------------------------------  OLT(config-interface-ge-0/0)# |

### Show Uplink Port Current 24Hs Performance Statistics

|  |  |
| --- | --- |
| Command | OLT(config-interface-ge-0/0)#show statistics port <port-id> current-24hour |
| **View** | XGE view or GE view |
| **Description** | This command is used for show the GE port performance statistics for current 24 hour |
| <port-id> | Port id to be show,range for 1-8 |

【Example】

Example 1：Show the port GE1 performance statistics for current 24 hours.

|  |
| --- |
| OLT(config-interface-ge-0/0)# show statistics port 1 current-24hour  -----------------------------------------------------------------------------  Start time of this interval : 2019-01-08 16:32:27+00:00  Total elapsed seconds in this interval : 5  -----------------------------------------------------------------------------  RX TX  octets : 0 : 0  frames : 0 : 0  unicast frames : 0 : 0  broadcast frames : 0 : 0  multicast frames : 0 : 0  discard frames : 0 : 0  error frames : 0 : 0  oversize frames : 0 : 0  frames 64 octets : 0 : 0  frames 65 to 127 octets : 0 : 0  frames 128 to 255 octets : 0 : 0  frames 256 to 511 octets : 0 : 0  frames 512 to 1023 octets : 0 : 0  frames 1024 to 1518 octets : 0 : 0  -----------------------------------------------------------------------------  OLT(config-interface-ge-0/0)# |

### Show Uplink Port History 15min Performance Statistics

|  |  |
| --- | --- |
| Command | OLT(config-interface-ge-0/0)#show statistics port <port-id> historic-15min <interval-number> |
| **View** | XGE view or GE view |
| **Description** | This command is used for show the GE port the past 15min performance statistics info |
| <port-id> | Port id to be show,range for 1-8 |
| <interval-number> | Interval number,range for 1-96.That means time=15min\*interval number. |

【Example】

Example 1：Show the port GE7 the past 15min performance statistics info

|  |
| --- |
| OLT(config-interface-ge-0/0)# show statistics port 7 historic-15min 1  -----------------------------------------------------------------------------  Start time of this interval : 2019-01-08 16:29:00+00:00  Interval number of historical 15 minutes : 1  The data for this interval is valid  Total monitored seconds in the historic interval : 900  -----------------------------------------------------------------------------  RX TX  octets : 2830116 : 1472  frames : 26332 : 23  unicast frames : 4 : 0  broadcast frames : 18668 : 0  multicast frames : 7660 : 23  discard frames : 24325 : 0  error frames : 0 : 0  oversize frames : 0 : 0  frames 64 octets : 2830 : 23  frames 65 to 127 octets : 18068 : 0  frames 128 to 255 octets : 4521 : 0  frames 256 to 511 octets : 555 : 0  frames 512 to 1023 octets : 357 : 0  frames 1024 to 1518 octets : 1 : 0  -----------------------------------------------------------------------------  OLT(config-interface-ge-0/0)# |

### Show Uplink Port History 24H Performance Statistics

| Command | OLT(config-interface-ge-0/0)#show statistics port <port-id> historic-24hour <interval-number> |
| --- | --- |
| **View** | XGE view or GE view |
| **Description** | This command is used for show the GE port the past 24 hours performance statistics info |
| <port-id> | Port id to be show,range for 1-8 |
| <interval-number> | Interval number,range for 1-7.That means time=24h\*interval number |

【Example】

Example 1：Show the port GE1 the past 24 hours performance statistics info

|  |
| --- |
| OLT(config-interface-ge-0/0)#show statistics port 5 historic-24hour 1  The data for this interval is invalid!  OLT(config-interface-ge-0/0)# |

## Uplink Port Storm Control Function

### Config Uplink Port Broadcast Storm Control Function

|  |  |
| --- | --- |
| Command | OLT(config-interface-ge-0/0)#traffic-suppress <port-id> broadcast {enable|disable} pps <value> |
| **View** | XGE view or GE view |
| **Description** | This command is used for enable or disable the broadcast storm suppression function and set the pulse value per second of the GE port.Preventing such information from occupying excessive network resources,resulting in network congestion. |
| <port-id> | Port id to be set,range for 1-8 |
| {enable|disable} | enable:Enable GE port broadcast storm suppression function  disable:Disable GE port broadcast storm suppression function |
| <value> | The number of pulses per second,range for 1-1488100,unit for pps |

【Example】

Example 1：Enable GE1 broadcast storm suppression function and set the number of pulses per second as 14000pps.

|  |
| --- |
| OLT(config-interface-ge-0/0)#traffic-suppress 1 broadcast enable pps 14000  OLT(config-interface-ge-0/0)# |

### Config Uplink Port Unknown Multicast Storm Control Function

|  |  |
| --- | --- |
| Command | OLT(config-interface-ge-0/0)#traffic-suppress <port-id> unknown-multicast {enable|disable} pps <value> |
| **View** | XGE view or GE view |
| **Description** | This command is used for enable or disable the unknown multicast storm suppression function and pulse value per second of the GE port.Preventing such information from occupying excessive network resources,resulting in network congestion. |
| <port-id> | Port id to be set,range for 1-8 |
| {enable|disable} | enable:Enable GE port broadcast storm suppression function  disable:Disable GE port broadcast storm suppression function |
| <value> | The number of pulses per second,range for 1-1488100,unit for pps |

【Example】

Example 1：Enable GE1 unknown multicast storm suppression function and set the number of pulses per second as 14000pps.

|  |
| --- |
| OLT(config-interface-ge-0/0)#traffic-suppress 1 unknown-multicast enable pps 14000  OLT(config-interface-ge-0/0)# |

### Config Uplink Port Unknown Unicast Storm Control

| Command | OLT(config-interface-ge-0/0)#traffic-suppress <port-id> unknown-unicast {enable|disable} pps <value> |
| --- | --- |
| **view** | XGE view or GE view |
| **Description** | This command is used for enable or disable the unknown unicast storm suppression function and pulse value per second of the GE port.Preventing such information from occupying excessive network resources,resulting in network congestion. |
| <port-id> | Port id to be set,range for 1-8 |
| {enable|disable} | enable:Enable GE port broadcast storm suppression function  disable:Disable GE port broadcast storm suppression function |
| <value> | The number of pulses per second,range for 1-1488100,unit for pps |

【Example】

Example 1：Enable GE1 unknown unicast storm suppression function and set the number of pulses per second as 14000pps.

|  |
| --- |
| OLT(config-interface-ge-0/0)#traffic-suppress 1 unknown-unicast enable pps 14000  OLT(config-interface-ge-0/0)# |

## Uplink Port Rate Limit Function

### Config Uplink Port Upstream and Downstream Rate Limit

|  |  |
| --- | --- |
| Command | OLT(config-interface-ge-0/0)#port-rate <port-list> {egress/ingress} <rate> |
| **view** | XGE view or GE view |
| **Description** | This command is used for configure a rate limit for the port,with a rate limit on the downlink or uplink direction of the port. |
| <port-list> | Port list to be set,format for 1,6-7,8 |
| egress/ingress | Egress:downlink  Ingress:uplink |
| <rate> | Rate,range for 64-10240000,unit is Kbps.The default value without rate limit. |

【Example】

Example 1：The GE1 port downstream rate limits as 102400

|  |
| --- |
| OLT(config-interface-ge-0/0)#port-rate 1 egress 102400  OLT(config-interface-ge-0/0)# |

### Delete Uplink Port Upstream and Downstream Rate Limit

|  |  |
| --- | --- |
| Command | OLT(config-interface-ge-0/0)#no port-rate <port-list> {egress/ingress} |
| **View** | XGE view or GE view |
| **Description** | This command is used for delete the upstream and downstream rate limit of GE port |
| <port-list> | Port list to be set,format for 1,6-7,8 |
| egress/ingress | Egress:downlink  Ingress:uplink |
| <rate> | Rate,range for 64-10240000,unit is Kbps. |

【Example】

Example 1：Delete the downstream rate limit of port GE1.

|  |
| --- |
| OLT(config-interface-ge-0/0)#no port-rate 1 egress  OLT(config-interface-ge-0/0)# |

### Show Uplink Port Upstream and Downstream Rate Limit Configuration

|  |  |
| --- | --- |
| Command | OLT(config-interface-ge-0/0)#show port-rate <port-list> |
| **View** | XGE view or GE view |
| **Description** | This command is used for show the upstream and downstream rate limitation info of GE port |
| <port-list> | Port list to be set,format for 1,6-7,8 |

【Example】

Example 1：Show the upstream and downstream rate limitation info of port GE1.

|  |
| --- |
| OLT(config-interface-ge-0/0)#show port-rate 1  Traffic shaping:  -----------------------------------------------------------------------------  port egress ingress  ge0/0/1 123000 0  OLT(config-interface-ge-0/0)# |

## Uplink Port Isolate Function

### Config Uplink Port Isolate

|  |  |
| --- | --- |
| Command | OLT(config-interface-ge-0/0)#isolate <port-list>{ enable|disable} |
| **View** | XGE view or GE view |
| **Description** | This command is used for enable or disable the function of GE port isolation.When port isolation is enabled,the port can not communicate with other ports.By default,it is disabled. |
| <port-list> | Port list to be set,format for 1,6-7,8 |
| {enable|disable} | Enable:enable the port isolation  Disable:disable the port isolation |

【Example】

Example 1：Enable the port isolation of GE1.

|  |
| --- |
| OLT(config-interface-ge-0/0)#isolate 1 enable  OLT(config-interface-ge-0/0)# |

### Show Uplink Port Isolation Configuration Infor

|  |  |
| --- | --- |
| Command | OLT(config-interface-ge-0/0)#show port isolate |
| **View** | XGE view or GE view |
| **Description** | This command is used for show the GE port isolation configuration info |

【Example】

Example 1：Show the GE port isolation configuration info

|  |
| --- |
| OLT(config-interface-ge-0/0)#show port isolate  Isolate among pon port:  pon0/0/1 pon0/0/2 pon0/0/3 pon0/0/4 pon0/0/5  pon0/0/6 pon0/0/7 pon0/0/8 pon0/0/9 pon0/0/10  pon0/0/11 pon0/0/12 pon0/0/13 pon0/0/14 pon0/0/15  pon0/0/16  Isolate among uplink port:  ge0/0/1  OLT(config-interface-ge-0/0)# |

## Uplink Port RSTP Function

### Config Uplink Port RSTP Cost

|  |  |
| --- | --- |
| Command | OLT(config-interface-ge-0/0)#spanning-tree cost <port-id> <cost> |
| **View** | XGE view or GE view |
| **Description** | This command is used for set RSTP cost of the GE port.When there are several link and are not root port between two device,the optimal path is decided by port cost. |
| <port-id> | Port id to be set,range for 1-8 |
| <cost> | Cost value,range for 1-200000000. |

【Example】

Example 1：Set the GE1 port RSTP cost as 2000.

|  |
| --- |
| OLT(config-interface-ge-0/0)#spanning-tree cost 1 2000  OLT(config-interface-ge-0/0)# |

### Config Uplink Port RSTP Edged-port

| Command | OLT(config-interface-ge-0/0)#spanning-tree edged-port <port-id> {enable|disable} |
| --- | --- |
| **View** | XGE view or GE view |
| **Description** | This command is used for set the RSTP edged-port of the GE port.If user specifies a port as edged-port,then when the port migrates forwarding status from congestion status,this port can migrate rapidly doing without waiting for delay time.the user can only set the port which is connected with the terminal as the edged-port.All ports are default to not edged-port. |
| <port-id> | Port id to be set,range for 1-8 |
| {enable|disable} | enable:Set the port as edged-port  disable:Set the port as not edged-port |

【Example】

Example 1：Set the port GE1 as edged-port.

|  |
| --- |
| OLT(config-interface-ge-0/0)#spanning-tree edged-port 1 enable  OLT(config-interface-ge-0/0)# |

### Config Uplink Port RSTP Mcheck Property

【Example】

|  |  |
| --- | --- |
| Command | OLT(config-interface-ge-0/0)#spanning-tree mcheck <port-id> |
| **View** | XGE view or GE view |
| **Description** | This command is used for set the RSTP mcheck property of GE port.Port mcheck property is used for detected whether the port which is running under STP compatible mode can migrate to RSTP mode.By setting mcheck,you can check whether there is a bridge running STP protocol within the network segment which is connected with current Ethernet port,If yes,RSTP protocol will migrate the protocol running mode of this port to STP mode. |
| <port-id> | Port id to be set,range for 1-8 |

Example 1：Set the mcheck of GE1.

|  |
| --- |
| OLT(config-interface-ge-0/0)#spanning-tree mcheck 1  OLT(config-interface-ge-0/0)# |

### Config Uplink Port RSTP Point-to-Point Link Function

|  |  |
| --- | --- |
| Command | OLT(config-interface-ge-0/0)#spanning-tree point-to-point <port-id> {auto/true/false} |
| **View** | XGE view or GE view |
| **Description** | This command is used for set point-to-point link of GE port spanning tree.If bridge works in RSTP mode,two ports which is connected by p2p link can migrate to forwarding status by sending synchronization message,it reduces the needless transfer delay time,if set this parameter as auto-mode,RSTP protocol can detect whether current Ethernet port has connected with point-to-point link automatically.The user can set by manually whether current Ethernet port connects with the p2p link.The recommendation is auto-mode. |
| <port-id> | Port id to be set,range for 1-8 |
| auto/true/false | auto:Set the point-to-point link as auto-mode  true:Connect GE port to point-to-point link  false:Disconnect GE port to point-to-point link |

【Example】

Example 1：Set the point-to-point link function of GE1 as true.

|  |
| --- |
| OLT(config-interface-ge-0/0)#spanning-tree point-to-point 1 true  OLT(config-interface-ge-0/0)# |

### Config Uplink Port RSTP Priority

| Command | OLT(config-interface-ge-0/0)#spanning-tree priority <port-id> <port-priority> |
| --- | --- |
| **View** | XGE view or GE view |
| **Description** | This command is used for set the RSTP priority of GE port.By setting the priority of the Ethernet port,You can specify that a particular Ethernet port is contained within the spanning tree.Generally,the smaller of the setting value is,the higher of the port priority,this Ethernet port is likely to include in spanning tree.If all the Ethernet port of the bridge adapt to the same index number,the priority of the Ethernet port depends on the index number of the Ethernet port. |
| <port-id> | Port id to be set,range for 1-8 |
| <port-priority> | Port priority,range for 0-240,step length for 16.the default is 128 |

【Example】

Example 1：Set the spanning tree priority of the GE1 as 160.

|  |
| --- |
| OLT(config-interface-ge-0/0)#spanning-tree priority 1 160  OLT(config-interface-ge-0/0)# |

### Delete Uplink Port Configuration of RTSP

|  |  |
| --- | --- |
| Command | OLT(config-interface-ge-0/0)# no spanning-tree (cost|priority) port-id |
| **View** | XGE view or GE view |
| **Description** | This command is used for delete uplink port configuration of RSTP cost and priority. The default of cost value is 20000, and the default of priority is 128 |
| port-id | Port id to be set,range for 1-8 |

【Example】

Example 1：Delete the priority of rstp in unlink port 1 .

|  |
| --- |
| OLT(config-interface-ge-0/0)# no spanning-tree priority 1  OLT(config-interface-ge-0/0)# |

### Show Uplink Port RSTP Configuration

| Command | OLT(config-interface-ge-0/0)#show port spanning-tree <port-id> |
| --- | --- |
| **View** | XGE view or GE view |
| **Description** | This command is used for show the RSTP configuration info of the GE port. |
| <port-id> | Port id to be show,range for 1-8 |

【Example】

Example 1：Show the RSTP configuration info of the port GE1.

|  |
| --- |
| OLT(config-interface-ge-0/0)#show port spanning-tree 1  -----------------------ge0/0/1 RSTP STATUS:--------------------------------  Port STP Mode:RSTP  Port Priority:128  Port Path Cost:20000  Port Edge Admin:NON-Edge  Port Edge Status:NEdge  Port Link Type Admin:Auto  Port Link Type Status:P2P  Port Role:Unknown  Port State:Down  -----------------------------------------------------------------------------  OLT(config-interface-ge-0/0)# |

## OLT Uplink Port VLAN Config

### Config Uplink Port VLAN Mode

| Command | OLT(config-interface-ge-0/0)#vlan mode <port-id> {access/hybrid/trunk} |
| --- | --- |
| **View** | XGE view or GE view |
| **Description** | This command is used for set the vlan mode of GE port,the default is access mode.In each vlan mode,the message processing way of the port is shown in**Appendix 1**. |
| <port-list> | Port list to be set,range for 1-16,format for 1,6-7,8. |
| access/hybrid/trunk | Access:This kind of port only belongs to one vlan,generally it is used for connect to computer. Trunk:This kind of ports can allow multi vlan pass,can receive and transfer the message of different vlan.Usually,it is used for connect to the port between switches. Hybrid:This kind of port allows multiple vlan pass,can receive and transfer the message of different vlan.It can be used to connect the port between switch or connect to the PC. |

【Example】

Example 1：Set the vlan mode of GE1 as access.

|  |
| --- |
| OLT(config-interface-ge-0/0)#vlan mode 1 access  OLT(config-interface-ge-0/0)# |

### Config Uplink Port Native-vlan

|  |  |
| --- | --- |
| Command | OLT(config-interface-ge-0/0)#vlan native-vlan <port-list> <vlan-id> |
| **View** | XGE view or GE view |
| **Description** | This command is used for set native vlan of the GE port.In each vlan mode,the message processing way of the port is shown in**Appendix 1**. |
| <port-list> | Port list to be set,range for 1-8,format for 1,2-3,4 |
| <vlan-id> | VLAN ID,range for 1-4094. |

【Example】

Example 1：Set the native vlan of the GE1 as 10.

|  |
| --- |
| OLT(config-interface-ge-0/0)#vlan native-vlan 1 10  OLT(config-interface-ge-0/0)# |

### Config Uplink Port Native-vlan Priority

|  |  |
| --- | --- |
| Command | OLT(config-interface-ge-0/0)#vlan native-vlan-priority <port-list> <priority> |
| **View** | XGE view or GE view |
| **Description** | This command is used for set the native vlan priority of the GE port,the default both are 0. |
| <port-list> | Port list to be set,range for 1-8,format for 1,2-3,4 |
| <priority> | Priority,range for 0-7 |

【Example】

Example 1：Set the native vlan priority of the GE1 port as 1.

|  |
| --- |
| OLT(config-interface-ge-0/0)#vlan native-vlan-priority 1 1  OLT(config-interface-ge-0/0)# |

### Config Uplink Port Access Mode VLAN

|  |  |
| --- | --- |
| Command | OLT(config-interface-ge-0/0)#vlan access <port-id> <vlan-id> |
| **View** | XGE view or GE view |
| **Description** | This command is used for set Access vlan of the GE port,the default access vlan both are 1.In each vlan mode,the message processing way of the port is shown inAppendix 1. |
| <port-id> | Port id to be set,range for 1-8 |
| <vlan-id> | Access VLAN ID,range for 1-4094 |

【Example】

Example1:Set the access vlan of the GE port as 100.

|  |
| --- |
| OLT(config-interface-ge-0/0)#vlan access 1 100  OLT(config-interface-ge-0/0)# |

### Config Uplink Port Hybrid Mode VLAN

|  |  |
| --- | --- |
| Command | OLT(config-interface-ge-0/0)#vlan hybrid <port-id> {tagged|untagged} <vlan-list> |
| **View** | XGE view or GE view |
| **Description** | This command is used for set hybrid vlan of the GE port,In each vlan mode,the message processing way of the port is shown in **Appendix 1**. |
| <port-id> | Port id to be set,range for 1-8 |
| {tagged|untagged} | tagged:Add corresponding vlan tag for the output message  untagged:Peel off corresponding vlan tag for output message |
| <vlan-list> | VLAN ID,range for 1-4094.Format can be 1,11-27,100 |

【Example】

Example 1：Add hybrid vlan of GE1 as 10-15 untagged.

|  |
| --- |
| OLT(config-interface-ge-0/0)#vlan hybrid 1 untagged 10-15  ge0/0/1:hybrid vlan added,failed:0,success:6  OLT(config-interface-ge-0/0)# |

Example 2:Add hybrid vlan of GE 1 as 101 tagged.

|  |
| --- |
| OLT(config-interface-ge-0/0)#vlan hybrid 1 tagged 101  ge0/0/1:hybrid vlan added,failed:0,success:1  OLT(config-interface-ge-0/0)# |

### Delete Uplink Port Hybrid Mode VLAN

|  |  |
| --- | --- |
| Command | OLT(config-interface-ge-0/0)#no vlan hybrid <port-id> {tagged|untagged} <vlan-list> |
| **View** | XGE view or GE view |
| **Description** | This command is used for delete the hybrid vlan of GE port.In each vlan mode,the message processing way of the port is shown inAppendix 1. |
| <port-id> | Port id to be set,range for 1-8 |
| {tagged|untagged} | tagged:Add corresponding vlan tag for the output message  untagged:Peel off corresponding vlan tag for output message |
| <vlan-list> | VLAN ID,range for 1-4094.Format can be 1,11-27,100 |

【Example】

Example 1：Delete GE1 hybrid vlan 10-15 tagged.

|  |
| --- |
| OLT(config-interface-ge)#no vlan hybrid 1 tagged 10-15  OLT(config-interface-ge)# |

### Config Uplink Port Trunk Mode VLAN

|  |  |
| --- | --- |
| Command | OLT(config-interface-ge-0/0)#vlan trunk <port-id> <vlan-list> |
| **View** | XGE view or GE view |
| **Description** | This command is used for set the trunk vlan of GE port.In each vlan mode,the message processing way of the port is shown inAppendix 1. |
| <port-id> | Port id to be set,range for 1-8 |
| <vlan-list> | VLAN list,range for 1-4094.Format can be 1,11-27,100 |

【Example】

Example 1：Set GE1 trunk vlan as 10-15.

|  |
| --- |
| OLT(config-interface-ge-0/0)#vlan trunk 1 10-15  ge0/0/1:trunk vlan allowed,failed:0,success:6  OLT(config-interface-ge-0/0)# |

### Delete Uplink Port Trunk Mode VLAN

|  |  |
| --- | --- |
| Command | OLT(config-interface-ge-0/0)#no vlan trunk <port-id> <vlan-list> |
| **View** | XGE view or GE view |
| **Description** | This command is used for delete the trunk vlan of GE port.In each vlan mode,the message processing way of the port is shown inAppendix 1. |
| <port-id> | Port id to be delete,range for 1-8 |
| <vlan-list> | VLAN list,range for 1-4094.Format can be 1,11-27,100 |

【Example】

Example 1：Delete GE1 trunk vlan 10-15.

|  |
| --- |
| OLT(config-interface-ge-0/0)#no vlan trunk 1 10-15  OLT(config-interface-ge-0/0)# |

### Config Uplink Port Translate Mode VLAN

| Command | OLT(config-interface-ge-0/0)#vlan translate <port-list> <old-vlan> <new-vlan> <new-priority> |
| --- | --- |
| **View** | XGE view or GE view |
| **Description** | This command is used for set the translate vlan of GE port.In the direction of upstream,it will transfer the old vlan into new vlan and update to new priority. |
| <port-list> | Port list to be set,range for 1-8 |
| <old-vlan> | Old vlan id,range for 1-4094 |
| <new-vlan> | New VLAN ID,range for 1-4094 |
| <new-priority> | New vlan priority,range for 0-7 |

【Example】  
Example 1：Translate the GE1’s old vlan 10 into new vlan 11 and the new priority translates into 3.

|  |
| --- |
| OLT(config-interface-ge-0/0)#vlan translate 1 10 11 3  OLT(config-interface-ge-0/0)# |

### Delete Uplink Port Translate Mode VLAN

|  |  |
| --- | --- |
| Command | OLT(config-interface-ge-0/0)#no vlan translate <port-list> <vlan-id> |
| **View** | XGE view or GE view |
| **Description** | This command is used for delete the translate vlan of GE port. |
| <port-list> | Port id to be delete,range for 1-8 |
| <vlan-id> | VLAN id,range for 1-4094. |

【Example】

Example 1：Delete the GE1 translate vlan 10.

|  |
| --- |
| OLT(config-interface-ge-0/0)#no vlan translate 1 10  OLT(config-interface-ge-0/0)# |

### Config Uplink Port Protocol VLAN

| Command | OLT(config-interface-ge-0/0)#protocol-vlan <protocol-index> {add/delete} port <port-list> <vlan-ID> |
| --- | --- |
| **View** | XGE view or GE view |
| **Description** | This command is used for bind a protocol vlan index for the port and port vlan,firstly it’s need to create a protocol vlan. |
| <protocol-index> | Protocol vlan index,range for 1-16 |
| add/delete | add:Add vlan  delete:Delete vlan |
| <port-list> | Port list to be set,format for 1,6-7,8 |
| <vlan-ID> | VLAN ID,range for 1-4094 |

【Example】

Example 1：Bind GE1 to protocol vlan index 1 and add into vlan 100.

|  |
| --- |
| OLT(config-interface-ge-0/0)#protocol-vlan 1 add port 1 100  OLT(config-interface-ge-0/0)# |

### Show OLT Uplink Port VLAN Configuration

|  |  |
| --- | --- |
| Command | OLT(config-interface-ge-0/0)#show port vlan <port-id> |
| **View** | XGE view or GE view |
| **Description** | This command is used for show the vlan info of GE port. |
| <port-id> | Port id to be show,range for 1-8 |

【Example】

Example 1：Show vlan info of port GE1.

|  |
| --- |
| OLT(config-interface-ge-0/0)#show port vlan 1  -----------------------------------------------------------------------------  Port:ge0/0/1 Mode:Access Native-Vlan:1 Priority:0  -----------------------------------------------------------------------------  Tagged-Vlan:  -  -----------------------------------------------------------------------------  Untagged-Vlan:  1  -----------------------------------------------------------------------------  OLT(config-interface-ge-0/0)# |

## OLT Uplink Port Loopback Detection

### Config Uplink port Loopback Detection

|  |  |
| --- | --- |
| Command | OLT(config-interface-ge-0/0)# loopback-detection port-list (enable|disable) |
| **View** | XGE view or GE view |
| **Description** | This command is used for enable or disable loop monitoring of the uplink port. On the access port, if the system finds that the port is monitored by loopback, the port performs the corresponding operation according to the loopback detection action, and reports the trap information to the terminal and deletes the MAC address forwarding entry corresponding to the port. On a trunk or a hybrid port, if the system finds that the port is monitored by loopback, the device only reports traps to the terminal. |
| port-list | The list of ports to be configured, in the format 1,6-7,8. The range of GE interfaces is 1-8; the range of XGE interfaces is 1-4. |

【Example】

Example 1：Enable uplink port 1 loopback-detection.

|  |
| --- |
| OLT(config-interface-ge-0/0)# loopback-detection 1 enable  OLT(config-interface-ge-0/0)# |

### Config Uplink port Loopback Detection Control Function

|  |  |
| --- | --- |
| Command | OLT(config-interface-ge-0/0)# loopback-detection port-list control (enable|disable) |
| **View** | XGE view or GE view |
| **Description** | This command is used for enable or disable the loop control monitoring of the uplink port. For a trunk or a hybrid port, when the loopback detection function of the port is enabled at the same time as the loopback detection function, the system performs corresponding operations on the port according to the loopback detection action, and reports the trap information to the terminal and deletes the port. MAC address forwarding entry. If it is a trunk port, it is found that the loop only reports errors. You need to set the port to be controlled. The access port is not required. |
| port-list | The list of ports to be configured, in the format 1,6-7,8. The range of GE interfaces is 1-8; the range of XGE interfaces is 1-4. |

【Example】

Example 1：Enable uplink port 1 loopback-detection control.

|  |
| --- |
| OLT(config-interface-ge-0/0)# loopback-detection 1 control enable  OLT(config-interface-ge-0/0)# |

### Config Uplink port Loopback Detection Per-vlan

|  |  |
| --- | --- |
| Command | OLT(config-interface-ge-0/0)# loopback-detection port-list per-vlan (enable|disable) |
| **View** | XGE view or GE view |
| **Description** | This command is used for enable monitoring for all vlans. For trunk ports, loop monitoring and loop controlled monitoring can only monitor the default vlan of the trunk port. Not valid for access port. |
| port-list | The list of ports to be configured, in the format 1,6-7,8. The range of GE interfaces is 1-8; the range of XGE interfaces is 1-4. |

【Example】

Example 1：Enable uplink port 1 loopback-detection per-vlan.

|  |
| --- |
| OLT(config-interface-ge-0/0)# loopback-detection 1 per-vlan enable  OLT(config-interface-ge-0/0)# |

## Config Uplink Port Protocol-vlan

|  |  |
| --- | --- |
| Command | OLT(config-interface-ge-0/0)# protocol-vlan protocol-index (add|delete) port port-list vlan-id |
| **View** | XGE view or GE view |
| **Description** | This command is used for create a protocol index and bind and unbind the uplink port to the established index number and add it to vlan100. To use this command, you must first establish a protocol vlan. |
| protocol-index | The established protocol index number that needs to be bound. The value ranges from 1 to 16. |
| port-list | The list of ports to be configured, in the format 1,6-7,8. The range of GE interfaces is 1-8; the range of XGE interfaces is 1-4. |
| ***vlan-id*** | The vlan to be bound. The range is 1-4094. |

【Example】

Example 1：Create an index 1, the mode is Ethernet, and the GE1 port binding protocol is indexed 1 and added to vlan100.

|  |
| --- |
| OLT(config)# protocol-vlan 1 mode ethernetii etype 0x8100  OLT(config)# interface ge 0/0  OLT(config-interface-ge-0/0)# protocol-vlan 1 add port 1 100  OLT(config-interface-ge-0/0)# |

# OLT PON Port Configuration

## OLT PON Port Property Config

### Disable PON Port

|  |  |
| --- | --- |
| Command | OLT(config-interface-epon-0/0)#shutdown <port-list> |
| **View** | EPON interface view |
| **Description** | This command is used for disable the specified pon port. |
| <port-list> | Port list to be set,range for 1-16,format for 1,3-5,8 |

【Example】

Example 1：Disable pon port 1-3.

|  |
| --- |
| OLT(config-interface-epon-0/0)#shutdown 1-3  OLT(config-interface-epon-0/0)# |

Example 2:Disable pon port 5 and 7.

|  |
| --- |
| OLT(config-interface-epon-0/0)#shutdown 5,7  OLT(config-interface-epon-0/0)# |

### Enable PON Port

|  |  |
| --- | --- |
| Command | OLT(config-interface-epon-0/0)#no shutdown <port-list> |
| **View** | EPON interface view |
| **Description** | This command is used for enable the specified pon port |
| <port-list> | Port list to be set,range for 1-16,format for 1,3-5,8 |

【Example】

Example 1：Enable pon port 1-3.

|  |
| --- |
| OLT(config-interface-epon-0/0)#no shutdown 1-3  OLT(config-interface-epon-0/0)# |

Example 2:Enable pon port 5 and 7.

|  |
| --- |
| OLT(config-interface-epon-0/0)#no shutdown 5,7  OLT(config-interface-epon-0/0)# |

### Config PON Port Name

|  |  |
| --- | --- |
| Command | OLT(config-interface-epon-0/0)#port-name <port-id> <name> |
| **View** | EPON interface view |
| **Description** | This command is used for set the name of pon port which is convenient for user to management |
| <port-id> | Port id to be set,range for 1-16 |
| <name> | Port name to be set |

【Example】

Example 1：Set the name of pon port as test.

|  |
| --- |
| OLT(config-interface-epon-0/0)#port-name 1 test  OLT(config-interface-epon-0/0)# |

### Delete PON Port Name

|  |  |
| --- | --- |
| Command | OLT(config-interface-epon-0/0)#no port-name <port-id> |
| **View** | EPON interface view |
| **Description** | This command is used for reset the name of pon port to default value. |
| <port-id> | Port id to be set,range for 1-16 |

【Example】

Example 1：Reset the name of pon1 to default value.

|  |
| --- |
| OLT(config-interface-epon-0/0)#no port-name 1  OLT(config-interface-epon-0/0)# |

### Config PON Port MTU

|  |  |
| --- | --- |
| Command | OLT(config-interface-epon-0/0)# frame-max port-list maximum-frame-size |
| **view** | EPON interface view |
| **Description** | This command is used for set the frame-max.The maximum transmission unit represents the size of the maximum transmission packet which transfers in the port for each unit time.The default value is 1526. |
| port-list | Port list to be set,range for 1-16,format for 1,3-5,8 |
| maximum-frame-size | The range of frame-max is 328~2048.specifically,the frame-max value of pon port is 2048. |

【Example】

Example 1：Set frame-max value of pon 1 as 1600.

|  |
| --- |
| OLT(config-interface-epon-0/0)# frame-max 1 1600  OLT(config-interface-epon-0/0)# |

### Delete PON Port Frame-max

|  |  |
| --- | --- |
| Command | OLT(config-interface-epon-0/0)# no frame-max port-list |
| **View** | EPON interface view |
| **Description** | This command is used for restore the pon port's mtu value as default 1526. |
| port-list | Port list to be set,range for 1-16,format for 16-7,8 |

【Example】

Example 1：Restore the frame-max value of pon1 as default 1526.

|  |
| --- |
| OLT(config-interface-epon-0/0)#no frame-max 1  OLT(config-interface-epon-0/0)# |

### Config PON Port Encrypt Mode and Key-exchange-time

|  |  |
| --- | --- |
| Command | OLT(config-interface-epon-0/0)#port encrypt <port-list> mode {aes-128/disable/triple-churning} key-exchange-time <time> |
| **View** | EPON interface view |
| **Description** | This command is used for set the encrypt mode and key-exchange-time.The default is not encrypted. |
| <port-list> | Port list to be set,range for 1-16,format for 1,6-7,8 |
| aes-128/disable/triple-churning | aes-128:An encrypted mode disable:Disable port encrypting function triple-churning:An encrypted mode |
| <time> | Key exchange time,range for 1-708,unit is second.It is optional. |

【Example】

Example 1：Set pon 1 encryption mode as aes-128

|  |
| --- |
| OLT(config-interface-epon-0/0)#port encrypt 1 mode aes-128  OLT(config-interface-epon-0/0)# |

### Config PON Port Flow-control Function

|  |  |
| --- | --- |
| Command | OLT(config-interface-epon-0/0)#flow-control <port-list> {enable|disable} |
| **View** | EPON interface view |
| **Description** | This command is used for set the flow-control function of pon port. |
| <port-list> | Port list to be set,range for 1-16,format for 1,6-7,8 |
| {enable|disable} | enable:Enable flow-control function of pon port  disable:Disable flow-control function of pon port |

【Example】

Example 1：Enable pon1 flow-control function.

|  |
| --- |
| OLT(config-interface-epon-0/0)#flow-control 1 enable  OLT(config-interface-epon-0/0)# |

### Config Pon Port MAC Address Learning Function

|  |  |
| --- | --- |
| Command | OLT(config-interface-epon-0/0)#mac-address learning port <port-list> {enable|disable} |
| **View** | EPON interface view |
| **Description** | This command is used for set pon port mac address learning function |
| <port-list> | Port list to be set,range for 1-16,format for 1,6-7,8 |
| {enable|disable} | Enable:Enable pon port mac address learning function  Disable:Disable pon port mac address learning function |

【Example】

Example 1：Enable pon1 mac address learning function

|  |
| --- |
| OLT(config-interface-epon-0/0)#mac-address learning port 1 enable  OLT(config-interface-epon-0/0)# |

### Show OLT PON Port Property and Status

|  |  |
| --- | --- |
| Command | OLT(config-interface-epon-0/0)#show port state {<port-id>/all} |
| **View** | EPON interface view |
| **Desscription** | This command is used for show the property info of pon port |
| <port-id>/all | Port-ID:Port id to be show,range for 1-16  All:Show the property info of all the pon port |

【Example】

Example 1：Show the property info of all the pon port

|  |
| --- |
| OLT(config-interface-epon-0/0)#show port state all  -----------------------------------------------------------------------------  F/S P Pvid Flow MAC Enable ONU MTU Link Auto Bandwidth Auth  Ctrl Learn State Isolate Find(Kbps)Mode  ----------------------------------------------------------------------------  0/0 1 1 on en en en 1500 off en 1000000 auto  0/0 2 1 on en en en 1500 off en 1000000 auto  0/0 3 1 on en en en 1500 off en 1000000 loid  0/0 4 1 on en en en 1500 off en 1000000 auto  0/0 5 1 on en en en 1500 off en 1000000 auto  0/0 6 1 on en en en 1500 off en 1000000 auto  0/0 7 1 on en en en 1500 off en 1000000 auto  0/0 8 1 on en en en 1500 off en 1000000 auto  0/0 9 1 on en en en 1500 off en 1000000 auto  0/0 10 1 on en en en 1500 off en 1000000 auto  0/0 11 1 on en en en 1500 off en 1000000 mac  0/0 12 1 on en en en 1500 off en 1000000 auto  0/0 13 1 on en en en 1500 off en 1000000 auto  0/0 14 1 on en en en 1500 off en 1000000 auto  0/0 15 1 on en en en 1500 off en 1000000 auto  0/0 16 1 on en en en 1500 off en 1000000 auto  -----------------------------------------------------------------------------  OLT(config-interface-epon-0/0)# |

Example 2:Show the property info of pon1.

|  |
| --- |
| OLT(config-interface-epon-0/0)#show port state 1  -----------------------------------------------------------------------------  Frame/Slot:0/0  Port:1  Port Name:pon0/0/1  Enable state:Enable  Encrpyt state:Disable  Key exchange time:-  ONU isolate state:Enable  Optical Module status:Normal  Link state:Down  Auto find:Enable  Auth Mode:auto  Policy Auth:Disable  Available bandwidth:1000000(Kbps)  Native vlan:1  Maximum Transmit Unit:1500  Flow-control:On  Maximum learned l2 entries:unlimited  Broadcast storm control:disable  Unknow multicast storm control:disable  Unknown unicast storm control:disable  Port 15 minute statistics status:enable  Port 24 hour statistics status:enable  -----------------------------------------------------------------------------  OLT(config-interface-epon-0/0)# |

### Show OLT PON Port Optical Power Information

| Command | OLT(config-interface-epon-0/0)#show port ddm-info <port-id> |
| --- | --- |
| **View** | EPON interface view |
| **Description** | This command is used for show configuration info of pon port such as optical power,optical module temperature,voltage,serial number and etc. |
| <port-id> | Port id to be show,range for 1-16 |

【Example】

Example 1：Show optical power info of pon1.

|  |
| --- |
| OLT(config-interface-epon-0/0)#show port ddm-info 1  -----------------------------------------------------------------------------  Temperature(C):41.9  Supply Voltage(V):3.32  TX Bias current(mA):11  TX power(dBm):4.66  RX power(dBm):-  ----------------------------------------------------------------------------  Vendor:T&W  Product name:TW5441H-C3AL  Version:1.0  Serial number:85165803D  -----------------------------------------------------------------------------  OLT(config-interface-epon-0/0)# |

## Config OLT PON Port Detect ONU Long Laser Function

### Config Auto Detect ONU Long Laser Function

|  |  |
| --- | --- |
| Command | OLT(config-interface-epon-0/0)#anti-rogueont auto-detect <port-id> {on/off} |
| **View** | EPON interface view |
| **Description** | This command is used for enable or disable the function of pon port automatic detecting onu long laser.In the case of enabling,when the onu appears long laser,olt will deliver an alarm info. |
| <port-id> | Port id to be set,range for 1-16,format for 1,6-7,8 |
| on/off | on:Enable pon port automatic detecting onu long laser  off:Disable pon port automatic detecting onu long laser |

【Example】

Example 1：Enable pon1 automatic detecting onu long laser

|  |
| --- |
| OLT(config-interface-epon-0/0)#anti-rogueont auto-detect 1 on  OLT(config-interface-epon-0/0)# |

### Config Manual Detect ONU Long Laser Function

|  |  |
| --- | --- |
| Command | OLT(config-interface-epon-0/0)#anti-rogueont manual-detect <port-id> |
| **View** | EPON interface view |
| **Description** | This command is used for set the pon port to detect the onu long laser by manually.The pon port start to detect onu long laser after executing this command. |
| <port-id> | Port id to be set,range for 1-16,format for 1,6-7,8 |

【Example】

Example 1：Set pon1 manually detecting onu long laser.

|  |
| --- |
| OLT(config-interface-epon-0/0)#anti-rogueont manual-detect 1  OLT(config-interface-epon-0/0)# |

### Show Detect ONU Long Laser Configuration

|  |  |
| --- | --- |
| Command | OLT(config-interface-epon-0/0)#show anti-rogueont auto-detect <port-id> status |
| **View** | EPON interface view |
| **Description** | This command is used for show the configuration info that pon port automatically detects onu long laser. |
| <port-id> | Port id to be set,range for 1-16,format for 1,6-7,8 |

【Example】

Example 1：Show the configuration info that pon1 automatically detects the onu long laser.

|  |
| --- |
| OLT(config-interface-epon-0/0)#show anti-rogueont auto-detect 1 status  -----------------------------------------------------------------------------  Detetion switch:off  Detetion interval:15(min)  -----------------------------------------------------------------------------  OLT(config-interface-epon-0/0)# |

## OLT PON Port RSTP Function

### Config OLT PON Port RSTP Cost

|  |  |
| --- | --- |
| Command | OLT(config-interface-epon-0/0)#spanning-tree cost <port-id> <cost> |
| **View** | Epon view |
| **Description** | This command is used for set RSTP cost of the pon port.When there are several link and are not root port between two device,the optimal path is decided by port cost. |
| <port-id> | Port id to be set,range for 1-16 |
| <cost> | Cost value,range for 1-200000000. |

【Example】

Example 1：Set the PON 1 port RSTP cost as 2000.

|  |
| --- |
| OLT(config-interface-epon-0/0)#spanning-tree cost 1 2000  OLT(config-interface-epon-0/0)# |

### Config OLT PON Port RSTP Edged-port

|  |  |
| --- | --- |
| Command | OLT(config-interface-epon-0/0)#spanning-tree edged-port <port-id> {enable|disable} |
| **View** | Epon view |
| **Description** | This command is used for set the RSTP edged-port of the pon port.If user specifies a port as edged-port,then when the port migrates forwarding status from congestion status,this port can migrate rapidly doing without waiting for delay time.the user can only set the port which is connected with the terminal as the edged-port.All ports are default to not edged-port. |
| <port-id> | Port id to be set,range for 1-16 |
| {enable|disable} | enable:Set the port as edged-port  disable:Set the port as not edged-port |

【Example】

Example 1：Set the port PON 1 as edged-port.

|  |
| --- |
| OLT(config-interface-epon-0/0)#spanning-tree edged-port 1 enable  OLT(config-interface-epon-0/0)# |

### Config OLT PON Port RSTP Mcheck Property

|  |  |
| --- | --- |
| Command | OLT(config-interface-epon-0/0)#spanning-tree mcheck <port-id> |
| **View** | Epon view |
| **Description** | This command is used for set the RSTP mcheck property of PON port.Port mcheck property is used for detected whether the port which is running under STP compatible mode can migrate to RSTP mode.By setting mcheck,you can check whether there is a bridge running STP protocol within the network segment which is connected with current Ethernet port,If yes,RSTP protocol will migrate the protocol running mode of this port to STP mode. |
| <port-id> | Port id to be set,range for 1-16 |

【Example】

Example 1：Set the mcheck of PON 1.

|  |
| --- |
| OLT(config-interface-epon-0/0)#spanning-tree mcheck 1  OLT(config-interface-epon-0/0)# |

### Config OLT PON Port RSTP Point-to-Point Link Function

|  |  |
| --- | --- |
| Command | OLT(config-interface-epon-0/0)#spanning-tree point-to-point <port-id> {auto/true/false} |
| **View** | Epon view |
| **Description** | This command is used for set point-to-point link of PON port spanning tree.If bridge works in RSTP mode,two ports which is connected by p2p link can migrate to forwarding status by sending synchronization message,it reduces the needless transfer delay time,if set this parameter as auto-mode,RSTP protocol can detect whether current Ethernet port has connected with point-to-point link automatically.The user can set by manually whether current Ethernet port connects with the p2p link.The recommendation is auto-mode. |
| <port-id> | Port id to be set,range for 1-16 |
| auto/true/false | auto:Set the point-to-point link as auto-mode  true:Connect GE port to point-to-point link  false:Disconnect GE port to point-to-point link |

【Example】

Example 1：Set the point-to-point link function of PON 1 as true.

|  |
| --- |
| OLT(config-interface-epon-0/0)#spanning-tree point-to-point 1 true  OLT(config-interface-epon-0/0)# |

### Config OLT PON Port RSTP Priority

|  |  |
| --- | --- |
| Command | OLT(config-interface-epon-0/0)#spanning-tree priority <port-id> <port-priority> |
| **View** | Epon view |
| **Description** | This command is used for set the RSTP priority of PON port.By setting the priority of the Ethernet port,You can specify that a particular Ethernet port is contained within the spanning tree.Generally,the smaller of the setting value is,the higher of the port priority,this Ethernet port is likely to include in spanning tree.If all the Ethernet port of the bridge adapt to the same index number,the priority of the Ethernet port depends on the index number of the Ethernet port. |
| <port-id> | Port id to be set,range for 1-16 |
| <port-priority> | Port priority,range for 0-240,step length for 16.the default is 128 |

【Example】

Example 1：Set the spanning tree priority of the PON 1 as 160.

|  |
| --- |
| OLT(config-interface-epon-0/0)#spanning-tree priority 1 160  OLT(config-interface-epon-0/0)# |

### Delete OLT PON Port Configuration of RTSP

|  |  |
| --- | --- |
| Command | OLT(config-interface-epon-0/0)# no spanning-tree (cost|priority) port-id |
| **View** | Epon view |
| **Description** | This command is used for delete OLT PON port configuration of RSTP cost and priority. The default of cost value is 20000, and the default of priority is 128 |
| port-id | Port id to be set,range for 1-16 |

【Example】

Example 1：Delete the priority of rstp in pon port 1 .

|  |
| --- |
| OLT(config-interface-epon-0/0)# no spanning-tree priority 1  OLT(config-interface-epon-0/0)# |

## Config OLT PON Port Mirror Function

### Config Pon Port Mirror Function

| Command | OLT(config-interface-epon-0/0)#mirror src-port <src-port-id> dst-port {ge/xge} <F/S/P> { all/egress/ingress} |
| --- | --- |
| **View** | EPON interface view |
| **Description** | This command is used for set the mirror function of the pon port.When it is needed to copy and output the flow of some pon port to other GE port or used to flow detection,network fault diagnosis and data analysis,use this command.When the pon port mirror is set successfully,the specified message of source mirror port will be completely copied to destination mirror port. |
| <src-port-id> | Source mirror port to be set,range for 1-16 |
| ge/xge | ge:Giga GE port  xge:10Giga GE port |
| <F/S/P> | Destination mirror port id,range for 0/0/1-0/0/8. |
| all/egress/ingress | all:Tx and Rx double direction message of source mirror port.Completely copy and output the rx and tx message of source mirror port to the destination mirror port.  egress:The tx message of source mirror port.Completely copy and output the tx message of source mirror port to destination mirror port.  ingress:The rx message of source mirror port.Completely copy and output the rx message of source mirror port to destination mirror port. |

【Example】

Example 1：Mirror the egress and ingress message of pon1 to GE5.

|  |
| --- |
| OLT(config-interface-epon-0/0)#mirror src-port 1 dst-port ge 0/0/5 all  OLT(config-interface-epon-0/0)# |

### Delete PON　Port Mirror Function

|  |  |
| --- | --- |
| Description | OLT(config-interface-epon-0/0)#no mirror src-port <src-port-id> |
| **View** | EPON interface view |
| **Description** | This command is used for cancel the pon port mirror setting. |
| <src-port-id> | Source mirror port id,range for 1-16 |

【Example】

Example 1：Cancel pon1 mirror setting.

|  |
| --- |
| OLT(config-interface-epon-0/0)#no mirror src-port 1  OLT(config-interface-epon-0/0)# |

### Show PON Port Mirror Configuration

|  |  |
| --- | --- |
| Command | OLT(config-interface-epon-0/0)#show mirror |
| **View** | EPON interface view |
| **Description** | This command is used for show the pon port mirror setting info. |

【Example】

Example 1：Show mirror setting info.

|  |
| --- |
| OLT(config-interface-epon-0/0)#show mirror  -----------------------------------------------------------------------------  Destnation port:ge0/0/5  Source port Ingress Egress  ge0/0/2 Yes Yes  pon0/0/1 Yes Yes  -----------------------------------------------------------------------------  OLT(config-interface-epon-0/0)# |

## OLT PON Port Performance Statistics Function

### Config PON Port Performance Statistics Period 15min

|  |  |
| --- | --- |
| Command | OLT(config-interface-epon-0/0)#statistics port <port-list>15min {enable|disable} |
| **View** | EPON interface view |
| **Description** | This command is used for set time interval of pon port performance statistic as 15min. |
| <port-list> | Port list to be set,range for 1-16,format for 1,6-7,8 |
| {enable|disable} | enable:Enable 15min performance statistics  disable:Disable 15min performance statistics |

【Example】

Example 1：Enable pon1 15min performance statistics function.

|  |
| --- |
| OLT(config-interface-epon-0/0)#statistics port 1 15min enable  OLT(config-interface-epon-0/0)# |

### Config PON Port Performance Statistics Period 15H

|  |  |
| --- | --- |
| Command | OLT(config-interface-epon-0/0)#statistics port <port-list> 24hour {enable|disable} |
| **View** | EPON interface view |
| **Description** | This command is used for enable or disable the 24h time interval performance statistics of pon port. |
| <port-list> | Port list to be set,range for 1-16,format for 1,6-7,8 |
| {enable|disable} | enable:Enable 24h performance statistics  disable:Disable 24h performance statistics |

【Example】

Example 1：Enable pon1 24h time interval performance statistics function.

|  |
| --- |
| OLT(config-interface-epon-0/0)#statistics port 1 24hour enable  OLT(config-interface-epon-0/0)# |

### Config PON Port Performance Statistics Threshold

|  |  |
| --- | --- |
| Command | OLT(config-interface-epon-0/0)#statistics port <port-list> threshold <type> <upper-threshold> |
| **View** | EPON interface view |
| **Description** | This command is used for set the threshold of pon port performance statistics. |
| <port-list> | Port list to be set,range for 1-16,format for 1,6-7,8 |
| <type-ID> | Range can be 1-64,among which:  1:rx-octets:Byte of received message  2:rx-frames:Frame of received message  3:rx-bcasts:The received broadcast message  4:rx-mcasts:The received multicast message  5:rx-64octets:The received frame packet length for 64 bytes  6:rx-65to127octets:The received frame packet length for 65-127 bytes  7:rx-128to255octets:The received frame packet length for 128-255 bytes  8:rx-256to511octets:The received frame packet length for 256-511 bytes  9:rx-512to1023octets:The received frame packet length for 512-1023 bytes  10:rx-1024to1518octets:The received frame packet length for 1024-1518 bytes  13:rx-oversizes:The oversize received packet  20:rx-discards:The discarded message at receiving  23:tx-octets:The byte of transmitted message  24:tx-frames:The frame of transmitted message  25:tx-bcasts:The transmitted broadcast packet  26:tx-mcasts:The transmitted multicast packet  27:tx-64octets:The transmitted frame packet length for 64 bytes  28:tx-65to127octets:The transmitted frame packet length for 65-127 bytes  29:tx-128to255octets:The transmitted frame packet length for 128-255 bytes  30:tx-256to511octets:The transmitted frame packet length for 256-511 bytes  31:tx-512to1023octets:The transmitted frame packet length for 512-1023 bytes  32:tx-1024to1518octets:The transmitted frame packet length for 1024-1518 bytes  35:tx-oversizes:The oversize transmitted packet  42:tx-discards:The discarded packet at transmitting |
| <upper-threshold> | Upper limit threshold,range for 0-4294967295 |
| <lower-threshold> | Lower limit of threshold,range for 0-4294967295 |

【Example】

Example 1：Set the pon port statistics received frame quantity upper limit and lower limit as 50000 and 500.

|  |
| --- |
| OLT(config-interface-epon-0/0)#statistics port 1 threshold 35 50000 500  OLT(config-interface-epon-0/0)# |

### Clear PON Port Performance Statistics Infor

|  |  |
| --- | --- |
| Command | OLT(config-interface-epon-0/0)#reset statistics port|pon-port <port-id> |
| **View** | EPON interface view |
| **Description** | This command is used for clear the pon port performance statistics info.The port obtains data from the switching side, and the pon-port obtains data from the PON chip. |
| <port-id> | Port id to be set,range for 1,6-7.8 |

【Example】

Example 1：Clear pon1 performance statistics info.

|  |
| --- |
| OLT(config-interface-epon-0/0)#reset statistics port 1  OLT(config-interface-epon-0/0)# |

### Show PON Port Current 15min Performance Statistics

|  |  |
| --- | --- |
| Command | OLT(config-interface-epon-0/0)#show statistics port <port-id> current-15min |
| **View** | EPON interface view |
| **Description** | This command is used for show current 15min statistics info of pon port. |
| <port-id> | Port id to be show,range for 1-16. |

【Example】

Example 1：Show current 15min statistics info of pon1.

|  |
| --- |
| OLT(config-interface-epon-0/0)# show statistics port 1 current-15min  -----------------------------------------------------------------------------  Start time of this interval : 2019-01-11 18:04:20+00:00  Total elapsed seconds in this interval : 33  -----------------------------------------------------------------------------  RX TX  octets : 0 : 241  frames : 0 : 2  unicast frames : 0 : 0  broadcast frames : 0 : 1  multicast frames : 0 : 1  discard frames : 0 : 0  error frames : 0 : 0  oversize frames : 0 : 0  frames 64 octets : 0 : 0  frames 65 to 127 octets : 0 : 1  frames 128 to 255 octets : 0 : 1  frames 256 to 511 octets : 0 : 0  frames 512 to 1023 octets : 0 : 0  frames 1024 to 1518 octets : 0 : 0  -----------------------------------------------------------------------------  OLT(config-interface-epon-0/0)# |

### Show PON Port Current 24Hs Performance Statistics

|  |  |
| --- | --- |
| Command | OLT(config-interface-epon-0/0)#show statistics port <port-id> current-24hour |
| View | EPON interface view |
| Description | This command is used for show current 24h statistics info of pon port |
| <port-id> | Port id to be set,range for 1-16 |

【Example】

Example 1：Show current 24h statistics info of pon 1.

|  |
| --- |
| OLT(config-interface-epon-0/0)# show statistics port 1 current-24hour  -----------------------------------------------------------------------------  Start time of this interval : 2019-01-11 18:07:04+00:00  Total elapsed seconds in this interval : 9  -----------------------------------------------------------------------------  RX TX  octets : 68 : 0  frames : 1 : 0  unicast frames : 0 : 0  broadcast frames : 1 : 0  multicast frames : 0 : 0  discard frames : 1 : 0  error frames : 0 : 0  oversize frames : 0 : 0  frames 64 octets : 0 : 0  frames 65 to 127 octets : 1 : 0  frames 128 to 255 octets : 0 : 0  frames 256 to 511 octets : 0 : 0  frames 512 to 1023 octets : 0 : 0  frames 1024 to 1518 octets : 0 : 0  -----------------------------------------------------------------------------  OLT(config-interface-epon-0/0)# |

### Show PON Port History 15min Performance Statistics

|  |  |
| --- | --- |
| Command | OLT(config-interface-epon-0/0)#show statistics port <port-id> historic-15min <interval-number> |
| View | EPON interface view |
| Description | This command is used for show performance statistics of pon port over the past 15min |
| <port-id> | Port id to be set,range for 1-16 |
| <interval-number> | Interval number,range for 1-96.Each interval for 15min,so the time=15min\*interval number. |

【Example】

Example 1：Show the past 15min statistics info of pon1.

|  |
| --- |
| OLT(config-interface-epon-0/0)#show statistics port 1 historic-15min 1  -----------------------------------------------------------------------------  Start time of this interval:2000-01-01 08:59:05+08:00  Interval number of historical 15 minutes:1  The data for this interval is valid  Total monitored seconds in the historic interval:900  -----------------------------------------------------------------------------  RX octets:0  RX frames:0  RX unicast frames:0  RX broadcast frames:0  RX multicast frames:0  RX discard frames:0  RX error frames:0  RX oversize frames:0  RX frames 64 octets:0  RX frames 65 to 127 octets:0  RX frames 128 to 255 octets:0  RX frames 256 to 511 octets:0  RX frames 512 to 1023 octets:0  RX frames 1024 to 1518 octets:0  TX octets:0  TX frames:0  TX unicast frames:0  TX broadcast frames:0  TX multicast frames:0  TX discard frames:0  TX error frames:0  TX oversize frames:0  TX frames 64 octets:0  TX frames 65 to 127 octets:0  TX frames 128 to 255 octets:0  TX frames 256 to 511 octets:0  TX frames 512 to 1023 octets:0  TX frames 1024 to 1518 octets:0  -----------------------------------------------------------------------------  OLT(config-interface-epon-0/0)# |

### Show PON Port History 24H Performance Statistics

|  |  |
| --- | --- |
| Command | OLT(config-interface-epon-0/0)#show statistics port <port-id> historic-24hour <interval-number> |
| **View** | EPON interface view |
| **Description** | This command is used for show the performance statistics of PON over the past 24 hours. |
| <port-id> | Port id to be show,range for 1-16. |
| <interval-number> | Interval number,range for 1-7.Each interval for 24h,so the time=24h\*interval number. |

【Example】

Example 1：Show the performance statistics of pon1 over the past 24h.

|  |
| --- |
| OLT(config-interface-epon-0/0)#show statistics port 1 historic-24hour 1  The data for this interval is invalid!  OLT(config-interface-epon-0/0)# |

### Show PON Port Performance Statistics Threshold Configuration from Switch side

|  |  |
| --- | --- |
| Command | OLT(config-interface-epon-0/0)#show statistics port <port-id> threshold |
| **View** | EPON interface view |
| **Description** | This command is used for show the threshold configuration of pon port performance statistics from switch side |
| <port-id> | Port id to be set,range for 1-16. |

【Example】

Example 1：Show threshold configuration of pon1 performance statistics.

|  |
| --- |
| OLT(config-interface-epon-0/0)#show statistics port 1 threshold  TX oversize frames:upper:50000 lower:500  OLT(config-interface-epon-0/0)# |

### Show PON Port Performance from Pon side

|  |  |
| --- | --- |
| Command | OLT(config-interface-epon-0/0)# show statistics pon-port port-ID |
| **View** | EPON interface view |
| **Description** | This command is used for show the pon port performance statistics from pon side |
| port-ID | Port id to be set,range for 1-16. |

【Example】

Example 1：Show PON port 9 performance

|  |
| --- |
| OLT(config-interface-epon-0/0)# show statistics pon-port 9  -----------------------------------------------------------------------------  RX TX  -----------------------------------------------------------------------------  bad\_sld : 0 : -  crc8\_err : 0 : -  bcast\_regreq : 0 : -  bcast\_crc32 : 0 : -  bcast\_reg : - : 0  bcast\_gate : - : 3523  good\_octets : 47979 : 2837430  ucast\_frames : 6 : 18  crc\_err\_frames : 0 : -  err\_frames : - : 0  mcast\_frames : 0 : 15583  bcast\_frames : 699 : 20855  oam\_frames : 1778 : 1778  pause\_frames : 0 : 0  ukn\_op\_frames : 0 : -  runt\_frames : 0 : -  giant\_frames : 0 : 0  64\_frames : 0 : 0  65\_127\_frames : 705 : 35625  128\_255\_frames : 0 : 519  256\_511\_frames : 0 : 303  512\_1023\_frames : 0 : 9  1024\_max\_frames : 0 : 0  -----------------------------------------------------------------------------  OLT(config-interface-epon-0/0)# |

## OLT PON Port Storm Control Function

### Config PON Port Broadcast Storm Control Function

|  |  |
| --- | --- |
| Command | OLT(config-interface-epon-0/0)#traffic-suppress <port-id> broadcast {enable|disable} pps <value> |
| **View** | EPON interface view |
| **Description** | This command is used for enable or disable broadcast storm suppression function and set the pulse number per second of pon port.Preventing such message from occupying excessive network source to result in network congestion. |
| <port-id> | Port id to be set,range for 1-16 |
| {enable|disable} | Enable:Enable broadcast storm suppression function of pon port  disable:Disable broadcast storm suppression function of pon port |
| <value> | Pulse number per second,range for 1-1488100,unit is pps |

【Example】

Example 1：Enable broadcast storm suppression function of pon1 and set the pulse number as 14000 pps.

|  |
| --- |
| OLT(config-interface-epon-0/0)#traffic-suppress 1 broadcast enable pps 14000  OLT(config-interface-epon-0/0)# |

### Config PON Port Unknown Multicast Storm Control Function

|  |  |
| --- | --- |
| Command | OLT(config-interface-epon-0/0)#traffic-suppress <port-id> unknown-multicast {enable|disable} pps<value> |
| **View** | PON view |
| **Description** | This command is used for enable or disable unknown multicast storm suppression function of pon port and set pulse number per second.preventing such message from occupying excessive network source to result in network congestion. |
| <port-id> | Port id to be set,range for 1-16. |
| {enable|disable} | Enable:Enable unknown multicast storm suppression function of pon port  disable:Disable unknown multicast storm suppression function of pon port |
| <value> | Pulse number per second,range for 1-1488100,unit is pps |

【Example】

Example 1：Enable unknown multicast storm suppression function of pon1 and set the pulse number as 14000 pps.

|  |
| --- |
| OLT(config-interface-epon-0/0)#traffic-suppress 1 unknown-multicast enable pps 14000  OLT(config-interface-epon-0/0)# |

### Config PON Port Unknown Unicast Storm Control

|  |  |
| --- | --- |
| Command | OLT(config-interface-epon-0/0)#traffic-suppress <port-id> unknown-unicast {enable|disable} pps <value> |
| **View** | EPON interface view |
| **Description** | This command is used for enable or disable unknown unicast storm suppression function of pon port and set pulse number per second.preventing such message from occupying excessive network source to result in network congestion. |
| <port-id> | Port id to be set,range for 1-16. |
| {enable|disable} | Enable:Enable unknown unicast storm suppression function of pon port  disable:Disable unknown unicast storm suppression function of pon port |
| <value> | Pulse number per second,range for 1-1488100,unit is pps |

【Example】

Example1:Enable unknown unicast storm suppression function of pon1 and set the pulse number as 14000 pps.

|  |
| --- |
| OLT(config-interface-epon-0/0)#traffic-suppress 1 unknown-unicast enable pps 14000  OLT(config-interface-epon-0/0)# |

## OLT PON Port Rate Limit Function

### Config PON Port Egress and Ingress Rate Limit

|  |  |
| --- | --- |
| Command | OLT(config-interface-epon-0/0)#port-rate <port-list> {egress/ingress} <rate> |
| **View** | EPON interface view |
| **Description** | This command is used for set a rate limitation value for egress or ingress message of pon port. |
| <port-list> | Port list to be set,range for 1-16,format for 1,6-7,8 |
| egress/ingress | Egress:Downstream direction  Ingress:Upstream direction |
| <rate> | Rate,range for 64-10240000,unit is Kbps.Pon port is without limitation by default |

【Example】

Example 1：Limit downstream rate of pon1 as 102400Kbps.

|  |
| --- |
| OLT(config-interface-epon-0/0)#port-rate 1 egress 102400  OLT(config-interface-epon-0/0)# |

### Delete PON Port Egress and Ingress Rate Limit

| Command | OLT(config-interface-epon-0/0)#no port-rate <port-list> {egress/ingress} |
| --- | --- |
| **View** | EPON interface view |
| **Description** | This command is used for cancel rate limitation of pon port. |
| <port-list> | Port list to be set,range for 1-16,format for 1,6-7,8 |
| {egress/ingress} | Egress:downstream  Ingress:upstream |
| <rate> | Rate,range for 64-10240000,unit is Kbps.Pon port is without limitation by default |

【Example】

Example 1：Cancel downstream rate limitation of pon1.

|  |
| --- |
| OLT(config-interface-epon-0/0)#no port-rate 1 egress  OLT(config-interface-epon-0/0)# |

### Show PON Port Egress and Ingress Rate Limit Configuration

|  |  |
| --- | --- |
| Command | OLT(config-interface-epon-0/0)#show port-rate <port-list> |
| **View** | EPON interface view |
| **Description** | This command is used for show upstream and downstream rate limited configuration info of pon port |
| <port-list> | Port list to be set,range for 1-16,format for 1,6-7,8 |

【Example】

Example 1：Show upstream and downstream rate limited configuration of pon1.

|  |
| --- |
| OLT(config-interface-epon-0/0)#show port-rate 1  Traffic shaping:  -----------------------------------------------------------------------------  port egress ingress  pon0/0/1 0 0  OLT(config-interface-epon-0/0)# |

## OLT PON Port Isolate Function

### Config PON Port Isolate

|  |  |
| --- | --- |
| Command | OLT(config-interface-epon-0/0)#isolate <port-list> {enable|disable} |
| **View** | EPON interface view |
| **Description** | This command is used for enable or disable the isolating function between port to port.The port can not communicate with other port when the isolating function is enabled.The default is enabled. |
| <port-list> | Port list to be set,range for 1-16,format for 1,6-7,8 |
| {enable|disable} | Enable:Enable port to port isolating function  Disable:Disable port to port isolating function |

【Example】

Example 1：Enable isolating function of pon1.

|  |
| --- |
| OLT(config-interface-epon-0/0)#isolate 1 enable  OLT(config-interface-epon-0/0)# |

### Config PON Port Ont-isolate Function

|  |  |
| --- | --- |
| Command | OLT(config-interface-epon-0/0)#ont-isolate <port-list> {enable|disable} |
| **View** | EPON interface view |
| **Description** | This command is used for enable or disable ont-isolate function of pon port.The ont that located in the same pon port can not communicate with each other when ont-isolate function is enabled.By default it is enabled. |
| <port-list> | Port list to be set,range for 1-16,format for 1,6-7,8 |
| {enable|disable} | Enable:Enable ont-isolate function  Disable:Disable ont-isolate function |

【Example】

Example 1：Disable ont-isolate function of pon1.

|  |
| --- |
| OLT(config-interface-epon-0/0)#ont-isolate 1 disable  OLT(config-interface-epon-0/0)# |

### Show PON Port Isolation Configuration Info

|  |  |
| --- | --- |
| Command | OLT(config-interface-epon-0/0)#show port isolate |
| **View** | EPON interface view |
| **Description** | This command is used for show isolating configuration info of pon port. |

【Example】

Example1:Show isolating configuration info of pon port

|  |
| --- |
| OLT(config-interface-epon-0/0)#show port isolate  Isolate among pon port:  pon0/0/1 pon0/0/2 pon0/0/3 pon0/0/4 pon0/0/5  pon0/0/6 pon0/0/7 pon0/0/8 pon0/0/9 pon0/0/10  pon0/0/11 pon0/0/12 pon0/0/13 pon0/0/14 pon0/0/15  pon0/0/16  Isolate among uplink port:  ge0/0/1  OLT(config-interface-epon-0/0)# |

## OLT PON Port VLAN Config

### Config PON Port VLAN Mode

|  |  |
| --- | --- |
| Command | OLT(config-interface-epon-0/0)#vlan mode <port-list> {access/hybrid/trunk} |
| **View** | EPON interface view |
| **Description** | This command is used for set vlan mode of pon port.The default is access mode.The processing way to message of the port is shown onAppendix 1 |
| <port-list> | Port list to be set,range for 1-16,format for 1,6-7,8 |
| access/hybrid/trunk | Access:This kind of port only belongs to one vlan,generally it is used for connect to the computer Trunk:This kind of port allows to several vlan passing,it can receive and transmit different vlan message,generally,it is used for connect to the port between Switch. Hybrid:This kind of port allows to several vlan passing,it can receive and transmit different vlan message,generally,it is used for connect to the port between Switch or connect to computer. |

【Example】

Example 1：Set the vlan mode of pon1 as access.

|  |
| --- |
| OLT(config-interface-epon-0/0)#vlan mode 1 access  OLT(config-interface-epon-0/0)# |

### Config PON Port Native-vlan

|  |  |
| --- | --- |
| Command | OLT(config-interface-epon-0/0)#vlan native-vlan <port-list> <vlan-ID> |
| **View** | EPON interface view |
| **Description** | This command is used for set native vlan of pon port,the default native vlan is 1.The processing way to message of the port is shown onAppendix 1 |
| <port-list> | Port list to be set,range for 1-16,format for 1,6-7,8 |
| <vlan-ID> | VLAN ID,range for 1-4094 |

【Example】

Example 1：Set the native vlan of pon1 as 10.

|  |
| --- |
| OLT(config-interface-epon-0/0)#vlan native-vlan 1 10  OLT(config-interface-epon-0/0)# |

### Config PON Port Native-vlan Priority

|  |  |
| --- | --- |
| Command | OLT(config-interface-epon-0/0)#vlan native-vlan-priority <port-list> <priority> |
| **View** | EPON interface view |
| **Description** | This command is used for set the native vlan priority of pon port,the default is 0. |
| <port-list> | Port list to be set,range for 1-16,format for 1,6-7,8 |
| <priority> | Priority,range for 0-7 |

【Example】

Example 1：Set native vlan of pon1 as 1.

|  |
| --- |
| OLT(config-interface-epon-0/0)#vlan native-vlan-priority 1 1  OLT(config-interface-epon-0/0)# |

### Config PON Port Access Mode VLAN

|  |  |
| --- | --- |
| Command | OLT(config-interface-epon-0/0)#vlan access <port-list> <vlan-id> |
| **View** | EPON interface view |
| **Description** | This command is used for set access vlan of pon port,the default access vlan is 1.The processing way to message of the port is shown onAppendix 1 |
| <port-list> | Port list to be set,range for 1-16,format for 1,6-7,8 |
| <vlan-id> | Access VLAN ID,range for 1-4094 |

【Example】

Example 1：Set the access vlan of pon1 as 100.

|  |
| --- |
| OLT(config-interface-epon-0/0)#vlan access 1 100  OLT(config-interface-epon-0/0)# |

### Config PON Port Hybrid Mode VLAN

|  |  |
| --- | --- |
| Command | OLT(config-interface-epon-0/0)#vlan hybrid <port-list> <{tagged|untagged}> <vlan-list> |
| **View** | PON view |
| **Description** | This command is used for set hybrid vlan of pon port.The processing way to message of the port is shown onAppendix 1 |
| <port-list> | Port list to be set,range for 1-16,format for 1,6-7,8 |
| {tagged|untagged} | tagged:Add vlan tag for tx message  untagged:Peel off the vlan tag for the tx message |
| <vlan-list> | VLAN ID,range for 1-4094.format for 1,11-27,100 |

【Example】

Example 1：Set vlan mode of pon1 as hybrid and add untagged vlan 10-15 to it.

|  |
| --- |
| OLT(config-interface-epon-0/0)#vlan hybrid 1 untagged 10-15  pon0/0/1:hybrid vlan added,failed:0,success:6  OLT(config-interface-ge-0/0)# |

Example 2:Set vlan mode of pon1 as hybrid and add vlan 101 tagged to it.

|  |
| --- |
| OLT(config-interface-epon-0/0)#vlan hybrid 1 tagged 101  pon0/0/1:hybrid vlan added,failed:0,success:1  OLT(config-interface-epon-0/0)# |

### Delete PON Port Hybrid Mode VLAN

|  |  |
| --- | --- |
| Command | OLT(config-interface-epon-0/0)#no vlan hybrid <port-id> <{tagged|untagged}> <vlan-list> |
| **View** | PON view |
| **Description** | This command is used for delete the hybrid vlan of pon port.The processing way to message of the port is shown onAppendix 1 |
| <port-id> | Port ID to be delete,range for 1-16 |
| {tagged|untagged} | tagged:Add vlan tag for tx message  untagged:Peel off the vlan tag for the tx message |
| <vlan-list> | VLAN ID,range for 1-4094.format for 1,11-27,100 |

【Example】

Example 1：Delete hybrid vlan 10-15 tagged of pon1.

|  |
| --- |
| OLT(config-interface-epon-0/0)#no vlan hybrid 1 tagged 10-15  OLT(config-interface-epon-0/0)# |

### Config PON Port Trunk Mode VLAN

|  |  |
| --- | --- |
| Command | OLT(config-interface-epon-0/0)#vlan trunk <port-list> <vlan-list> |
| **View** | EPON interface view |
| **Description** | This command is used for set the trunk vlan of pon port.The processing way to message of the port is shown onAppendix 1 |
| <port-list> | Port list to be set,range for 1-16,format for 1,6-7,8 |
| <vlan-list> | VLAN ID,range for 1-4094.Format can be 1,11-27,100 |

【Example】

Example1:Add trunk vlan 10-15 to pon1.

|  |
| --- |
| OLT(config-interface-epon-0/0)#vlan trunk 1 10-15  pon0/0/1:trunk vlan allowed,failed:0,success:6  OLT(config-interface-epon-0/0)# |

### Delete PON Port Trunk Mode VLAN

|  |  |
| --- | --- |
| Command | OLT(config-interface-epon-0/0)#no vlan trunk <port-id> <vlan-list> |
| **View** | PON view |
| **Description** | This command is used for delete the trunk vlan of pon port.The processing way to message of the port is shown onAppendix 1 |
| <port-id> | Port ID to be delete,range for 1-16 |
| <vlan-list> | VLAN ID,range for 1-4094.Format can be 1,11-27,100 |

【Example】

Example 1：Delete trunk vlan 10-15 of pon1.

|  |
| --- |
| OLT(config-interface-epon-0/0)#no vlan trunk 1 10-15  OLT(config-interface-epon-0/0)# |

### Config PON Port Translate Mode VLAN

|  |  |
| --- | --- |
| Command | OLT(config-interface-epon-0/0)#vlan translate <port-list> <old-vlan> <new-vlan> <new-priority> |
| **View** | EPON interface view |
| **Description** | This command is used for set translate vlan of pon port.In the upstream direction,it can translate old vlan into new vlan and update new priority |
| <port-list> | Port list to be set,range for 1-16,format is 1,6-7,8 |
| <old-vlan> | Old VLAN ID,range for 1-4094 |
| <new-vlan> | New VLAN ID,range for 1-4094 |
| <new-priority> | New VLAN priority,range for 0-7 |

【Example】

Example 1：Translate vlan 10 of pon1 into vlan 11 and update the priority as 3.

|  |
| --- |
| OLT(config-interface-epon-0/0)#vlan translate 1 10 11 3  OLT(config-interface-epon-0/0)# |

### Delete PON Port Translate Mode VLAN

|  |  |
| --- | --- |
| Command | OLT(config-interface-ge-0/0)#no vlan translate <port-list> <vlan-list> |
| **View** | PON view |
| **Description** | This command is used for delete the translate VLAN of pon port.In the upstream direction,it can translate old vlan into new vlan and update new priority |
| <port-list> | Port list to be delete,range for 1-16 |
| <vlan-list> | VLAN list to be delete,range for 1-4094 |

【Example】

Example 1：Delete translate vlan 10 of pon1.

|  |
| --- |
| OLT(config-interface-epon)#no vlan translate 1 10  OLT(config-interface-epon)# |

### Config PON Port QinQ VLAN

| Command | OLT(config-interface-epon-0/0)#vlan qinq <port-list> cvlan-range <start-cvlan> <end-cvlan> <qinq-svlan> <svlan-priority> |
| --- | --- |
| **View** | EPON interface view |
| **Description** | This command is used for set qinq vlan of pon port.In upstream direction,it can add a SVLAN for the stream between start-CVLAN and end-CVLAN.It need to create a SVLAN in global mode(config view) |
| <port-list> | Port list to be set,range for 1-16,format is 1,6-7,8 |
| <start-cvlan> | The inner start vlan,range for 1-4094 |
| <end-cvlan> | The inner end vlan,range for 1-4094 |
| <qinq-svlan> | The outer vlan,range for 1-4094 |
| <svlan-priority> | SVLAN priority,range for 0-7 |

【Example】

Example 1：The qinq setting of pon1:add a svlan 20 for the stream which is between vlan 10-15 and set its priority as 0.

|  |
| --- |
| OLT(config-interface-epon-0/0)#vlan qinq 1 cvlan-range 10 15 20 0  OLT(config-interface-epon-0/0)# |

### Delete PON Port QinQ VLAN

|  |  |
| --- | --- |
| Command | OLT(config-interface-epon-0/0)#no vlan qinq <port-list> cvlan-range <start-cvlan> <end-cvlan> |
| **View** | EPON interface view |
| **Description** | This command is used for delete qinq vlan of pon port.In upstream direction,it can add a SVLAN for the stream between start-CVLAN and end-CVLAN.It need to create a SVLAN in global mode(config view) |
| <port-list> | Port list to be set,range for 1-16,format is 1,6-7,8 |
| <start-cvlan> | The inner start vlan,range for 1-4094 |
| <end-cvlan> | The inner end vlan,range for 1-4094 |

【Example】

Example 1：Delete the qinq setting of pon1.

|  |
| --- |
| OLT(config-interface-epon-0/0)#no vlan qinq 1 cvlan-range 10 15  OLT(config-interface-epon-0/0)# |

### Config PON Port Aggregation VLAN

|  |  |
| --- | --- |
| Command | OLT(config-interface-epon-0/0)#vlan aggregation pon-port <port-list> cvlan-range <start-cvlan> <end-cvlan> <aggregation-svlan> <svlan-priority> |
| **View** | EPON interface view |
| **Description** | This command is used for set aggregation vlan of pon port.In upstream direction,it can translate the vlan which range is from start-cvlan to end-cvlan into svlan. |
| <port-list> | Port list to be set,range for 1-16,format is 1,6-7,8 |
| <start-cvlan> | The inner start vlan,range for 1-4094 |
| <end-cvlan> | The inner end vlan,range for 1-4094 |
| <aggregation-svlan> | SVLAN ID,the vlan after translating,range for 1-4094 |
| <svlan-priority> | Priority of SVLAN,range for 0-7 |

【Example】

Example 1：Translate the cvlan 10-15 of pon1 upstream direction into svlan 20.

|  |
| --- |
| OLT(config-interface-epon-0/0)#vlan aggregation pon-port 1 cvlan-range 10 15 20 0  OLT(config-interface-epon-0/0)# |

### Delete PON Port Aggregation VLAN

| Command | OLT(config-interface-epon-0/0)# no vlan aggregation all|<pon-port port-list all|cvlan-range start-cvlan end-cvlan aggregation-svlan>|< ont port-list ont-id all|cvlan-range start-cvlan end-cvlan aggregation-svlan> |
| --- | --- |
| **View** | EPON interface view |
| **Description** | This command is used for delete aggregation vlan of pon port. |
| port-list | Port list to be set,range for 1-16,format is 1,6-7,8 |
| start-cvlan | The inner start vlan,range for 1-4094 |
| end-cvlan | The inner end vlan,range for 1-4094 |
| aggregation-svlan | SVLAN ID,the vlan after translating,range for 1-4094 |

【Example】

Example 1：Delete all pon ports aggregation vlan config.

|  |
| --- |
| OLT(config-interface-epon-0/0)# no vlan aggregation all  OLT(config-interface-epon-0/0)# |

### Config PON Port Protocol VLAN

|  |  |
| --- | --- |
| Command | OLT(config-interface-epon-0/0)#protocol-vlan <protocol-index> {add|delete} port <port-list> <vlan-ID> |
| **View** | EPON interface view |
| **Description** | This command is used for bind a protocol vlan index for port and port vlan.Firstly,it needs to create a protocol-vlan in config view |
| <protocol-index> | Protocol vlan index,range for 1-16 |
| {add|delete} | add:Add vlan  delete:Delete vlan |
| <port-list> | Port list to be set,range for 1-16,format is 1,6-7,8 |
| <vlan-ID> | VLAN ID,range for 1-4094 |

【Example】

Example 1：Bind pon1 to protocol vlan index 1 and add it into vlan 100.

|  |
| --- |
| OLT(config-interface-epon-0/0)#protocol-vlan 1 add port 1 100  OLT(config-interface-epon-0/0)# |

### Show OLT PON Port VLAN Configuration

|  |  |
| --- | --- |
| Command | OLT(config-interface-ge-0/0)#show port vlan <port-id> |
| **View** | EPON interface view |
| **Description** | This command is used for show vlan info od pon port |
| <port-id> | Port-ID:Port id to be show,range for 1-16 |

【Example】

Example 1：Show vlan info of pon1.

|  |
| --- |
| OLT(config-interface-epon-0/0)#show port vlan 1  -----------------------------------------------------------------------------  Port:pon0/0/1 Mode:Access Native-Vlan:1 Priority:0  -----------------------------------------------------------------------------  Tagged-Vlan:  -  -----------------------------------------------------------------------------  Untagged-Vlan:  1  -----------------------------------------------------------------------------  OLT(config-interface-epon-0/0)# |

### Show PON Port Translate VLAN Configuration

|  |  |
| --- | --- |
| Command | OLT(config-interface-epon-0/0)#show vlan translate all |
| **View** | EPON interface view |
| **Description** | This command is used for show vlan translating info of all pon port |

【Example】

Example 1：Show VLAN translating info of all the pon port

|  |
| --- |
| OLT(config-interface-epon-0/0)#show vlan translate all  -----------------------------------------------------------------------------  index port oldvlan newvlan priority mode  -----------------------------------------------------------------------------  1 pon0/0/1 21 30--Translate  2 pon0/0/1 10-12 20 0 QinQ  -----------------------------------------------------------------------------  OLT(config-interface-epon-0/0)# |

### Show PON Port Aggregation VLAN Configuration

|  |  |
| --- | --- |
| Command | OLT(config-interface-epon-0/0)#show vlan aggregation pon-port {<port-id>/all} |
| **View** | EPON interface view |
| **Description** | This command is used for show aggregation vlan info of pon port |
| <port-id>/all | Port-ID:Port ID to be show,range for 1-16  All:Show aggregation vlan info of all the pon port |

【Example】

Example 1：Show aggregation vlan info of all the pon port

|  |
| --- |
| OLT(config-interface-epon-0/0)#show vlan aggregation pon-port all  -----------------------------------------------------------------------------  index port ontId cvlan svlan priority  -----------------------------------------------------------------------------  1 0/0/1--10-13 20 2  -----------------------------------------------------------------------------  OLT(config-interface-epon-0/0)# |

## OLT PON Port Loopback Detection

### Config PON port Loopback Detection

|  |  |
| --- | --- |
| Command | OLT(config-interface-epon-0/0)# loopback-detection port-list (enable|disable) |
| **View** | EPON view |
| **Description** | This command is used for enable or disable loop monitoring of the PON port. On the access port, if the system finds that the port is monitored by loopback, the port performs the corresponding operation according to the loopback detection action, and reports the trap information to the terminal and deletes the MAC address forwarding entry corresponding to the port. On a trunk or a hybrid port, if the system finds that the port is monitored by loopback, the device only reports traps to the terminal. |
| port-list | The list of ports to be configured, in the format 1,6-7,8. The range of EPON interfaces is 1-16. |

【Example】

Example 1：Enable pon port 1 loopback-detection.

|  |
| --- |
| OLT(config-interface-epon-0/0)# loopback-detection 1 enable  OLT(config-interface-epon-0/0)# |

### Config PON port Loopback Detection Control Function

|  |  |
| --- | --- |
| Command | OLT(config-interface-epon-0/0)# loopback-detection port-list control (enable|disable) |
| **View** | EPON view |
| **Description** | This command is used for enable or disable the loop control monitoring of the pon port. For a trunk or a hybrid port, when the loopback detection function of the port is enabled at the same time as the loopback detection function, the system performs corresponding operations on the port according to the loopback detection action, and reports the trap information to the terminal and deletes the port. MAC address forwarding entry. If it is a trunk port, it is found that the loop only reports errors. You need to set the port to be controlled. The access port is not required. |
| port-list | The list of ports to be configured, in the format 1,6-7,8. The range of EPON interfaces is 1-16. |

【Example】

Example 1：Enable PON port 1 loopback-detection control.

|  |
| --- |
| OLT(config-interface-epon-0/0)# loopback-detection 1 control enable  OLT(config-interface-epon-0/0)# |

### Config PON port Loopback Detection Per-vlan

|  |  |
| --- | --- |
| Command | OLT(config-interface-epon-0/0)# loopback-detection port-list per-vlan (enable|disable) |
| **View** | EPON view |
| **Description** | This command is used for enable monitoring for all vlans. For trunk ports, loop monitoring and loop controlled monitoring can only monitor the default vlan of the trunk port. Not valid for access port. |
| port-list | The list of ports to be configured, in the format 1,6-7,8. The range of EPON interfaces is 1-16. |

【Example】

Example 1：Enable PON port 1 loopback-detection per-vlan.

|  |
| --- |
| OLT(config-interface-epon-0/0)# loopback-detection 1 per-vlan enable  OLT(config-interface-epon-0/0)# |

# OLT MAC Address Table Manage

## Config OLT MAC-address Black-hole

|  |  |
| --- | --- |
| Command | OLT(config)#mac-address black-hole vlan <vlan-id> <mac-address> |
| **View** | Config view |
| **Description** | This command is used for specify a black hole mac address table.If source mac address or destination mac address of some message is equal to the mac address in black hole mac address table,the Switch will discard this message. |
| <vlan-id> | VLAN id,range for 1-4094 |
| <mac-address> | Mac address,format for XX:XX:XX:XX:XX:XX |

【Example】

Example 1：Add mac 00:00:00:12:34:56 to black hole mac address table of vlan 100

|  |
| --- |
| OLT(config)#mac-address black-hole vlan 100 00:00:00:12:34:56  OLT(config)# |

## Delete MAC-Address Black-hole

|  |  |
| --- | --- |
| Command | OLT(config)#no mac-address black-hole vlan <vlan-id> <mac-address> |
| **View** | Config view |
| **Description** | This command is used for delete black-hole mac address |
| <vlan-id> | VLAN ID,range for 1-4094。 |
| <mac-address> | Mac address,format for XX:XX:XX:XX:XX:XX |

【Example】

Example 1：Delete vlan 100 black-hole mac address 00:00:00:12:34:56

|  |
| --- |
| OLT(config)#no mac-address black-hole vlan 100 00:00:00:12:34:56  OLT(config)# |

## Config OLT Mac Address Entries limit

|  |  |
| --- | --- |
| Command | OLT(config)#mac-address limit port {epon/ge/xge } F/S <port-list> <number> |
| **View** | Config view |
| **Description** | This command is used for set the maximum mac address learning entry,when the quantity of mac address is out of this value,OLT will discard the other mac address except the learned mac. |
| epon/ge/xge | epon:PON port  ge:ge uplink port  xge:xge 10giga uplink port |
| F/S | FrameID/SlotID,<0-0>/<0-0>,the value of 1U olt is 0/0 |
| <port-list> | Port list to be set,range for 1-16,format is 1,6-7,8 |
| <number> | The number of mac address,range for 0-8092,zero means without limitation.The default is 0. |

【Example】

Example 1：Set the maximum learning mac address entry of GE5 as 500

|  |
| --- |
| OLT(config)#mac-address limit port ge 0/0 5 500  OLT(config)# |

## Add Static MAC Address Bind Function

|  |  |
| --- | --- |
| Command | OLT(config)#mac-address static port {epon/ge/ xge} F/S/P {lag <manual-group-ID>/<lacp-group-ID>)} vlan <vlan-ID> <mac-address> |
| **View** | Config view |
| **Description** | This command is used for set the static mac address.With this function,the devices needn’t mac address learning process,it can transfer the message according to static mac. |
| epon/ge/xge/lag | epon:Pon port,range for 0/0/1-16  ge:GE uplink port,range for 0/0/1-8  xge:10giga xge uplink port,range for 0/0/1-2  Lag:Port aggregation group,range for 1-8,9-16 |
| F/S/P | FrameID/SlotID/PortID,<0-0>/<0-0>/<1-16> |
| <manual-group-ID>|<lacp-group-ID> | manual-group-ID,range for 1-8  lacp-group-ID,range for 9-16 |
| <vlan-ID> | VLAN ID,range for 1-4094。 |
| <mac-address> | Mac address,format for XX:XX:XX:XX:XX:XX |

【Example】

Example 1：Bind mac address e0:67:b3:12:eb:f6 with GE5 and vlan 100.

|  |
| --- |
| OLT(config)#mac-address static port ge 0/0/5 vlan 100 e0:67:b3:12:eb:f6  OLT(config)# |

Example 2:Bind mac address e0:67:b3:12:eb:f6 with pon1 and vlan 100.

|  |
| --- |
| OLT(config)#mac-address static port epon 0/0/1 vlan 100 e0:67:b3:12:eb:f7  OLT(config)# |

Example 3:Bind mac address e0:67:b3:12:eb:f6 with XGE1 and vlan 100.

|  |
| --- |
| OLT(config)#mac-address static port xge 0/0/1 vlan 100 e0:67:b3:12:eb:f8  OLT(config)# |

Example 4:Bind mac address e0:67:b3:12:eb:f6 with lag1 and vlan 100.

|  |
| --- |
| OLT(config)#mac-address static port lag 1 vlan 100 e0:67:b3:12:eb:f9  OLT(config)# |

## Delete Static MAC Address bind

|  |  |
| --- | --- |
| Command | OLT(config)#no mac-address static port {epon/ge/ xge} F/S/P {lag <manual-group-ID>|<lacp-group-ID>)} vlan <vlan-ID> <mac-address> |
| **View** | Config view |
| **Description** | This command used to delete static mac address of olt |
| epon/ge/xge/lag | epon:Pon port,range for 0/0/1-16  ge:GE uplink port,range for 0/0/1-8  xge:10giga xge uplink port,range for 0/0/1-2  Lag:Port aggregation group,range for 1-8,9-16 |
| F/S/P | FrameID/SlotID/PortID，<0-0>/<0-0>/<1-16>， |
| <manual-group-ID>/<lacp-group-ID> | FrameID/SlotID/PortID,<0-0>/<0-0>/<1-16> |
| <vlan-ID> | manual-group-ID,range for 1-8  lacp-group-ID,range for 9-16 |
| <mac-address> | VLAN ID,range for 1-4094。 |

【Example】

Example 1：No bind the mac address e0:67:b3:12:eb:f6 with the GE5 and vlan 100.

|  |
| --- |
| OLT(config)#no mac-address static port ge 0/0/5 vlan 100 e0:67:b3:12:eb:f6  OLT(config)# |

Example 2:No bind the mac address e0:67:b3:12:eb:f6 with the pon1 and vlan 100.

|  |
| --- |
| OLT(config)#no mac-address static port epon 0/0/1 vlan 100 e0:67:b3:12:eb:f7  OLT(config)# |

Example 3:No bind the mac address e0:67:b3:12:eb:f6 with the XGE1 and vlan 100.

|  |
| --- |
| OLT(config)#no mac-address static port xge 0/0/1 vlan 100 e0:67:b3:12:eb:f8  OLT(config)# |

Example 4:No bind the mac address e0:67:b3:12:eb:f6 with the lag1 and vlan 100.

|  |
| --- |
| OLT(config)#no mac-address static port lag 1 vlan 100 e0:67:b3:12:eb:f9  OLT(config)# |

## Config OLT MAC Address Aging Time

|  |  |
| --- | --- |
| Command | OLT(config)#mac-address timer {<aging-time>/no-aging} |
| **View** | Config view |
| **Description** | This command is used for set the dynamic table body aging time of the system mac address table.it takes effect immediately after successful setting,system will check the dynamic address by timing,if the system has not transmit or receive any message with specified source mac address during the aging time,this mac address will be deleted from mac address table.Dynamic mac address aging timer can release the source of mac address table to learn new mac address. |
| {<aging-time>/no-aging} | <aging-time>:mac address aging time,range for 10-1000000,unit is second  no-aging:Set mac address without aging time.when it is no need to open mac address aging function,use this parameter |

【Example】

Example 1：Set mac address aging time as 1000 second.

|  |
| --- |
| OLT(config)#mac-address timer 1000  OLT(config)# |

## Clear OLT MAC Address Table

|  |  |
| --- | --- |
| Command | OLT(config)#mac-address flush {all/dynamic/black-hole/static} |
| **View** | Config view |
| **Description** | This command is used for clear the mac address table of olt |
| {all/dynamic/black-hole/static} | All:All the mac address in the table  Dynamic:Dynamic mac address  black-hole:Black hole mac address  Static:Static mac address |

【Example】

Example 1：Clear all the mac address in the mac address table.

|  |
| --- |
| OLT(config)#mac-address flush all  OLT(config)# |

## Clear OLT Port MAC Address Table

| Command | OLT(config)#mac-address flush port {epon/ge/ xge} F/S/P / {lag <manual-group-ID>/<lacp-group-ID>/all/dynamic/ static } |
| --- | --- |
| **View** | Config view |
| **Description** | This command is used for clear the MAC address learned by the port of OLT |
| {epon/ge/xge/lag} | epon:Pon port,range for 0/0/1-16  ge:GE uplink port,range for 0/0/1-8  xge:10giga xge uplink port,range for 0/0/1-2  Lag:Port aggregation group,range for 1-8,9-16 |
| F/S/P | FrameID/SlotID/PortID，<0-0>/<0-0>/<1-16>， |
| <manual-group-ID>/<lacp-group-ID> | FrameID/SlotID/PortID,<0-0>/<0-0>/<1-16> |
| all/dynamic/static | All:All the mac address in the table  Dynamic:Dynamic mac address  Static:Static mac address |

【Example】

Example 1：Clear the MAC address learned by GE1.

|  |
| --- |
| OLT(config)#mac-address flush port ge 0/0/1 all  OLT(config)# |

## According OLT VLAN Clear MAC Address Table

|  |  |
| --- | --- |
| Command | OLT(config)#mac-address flush vlan<vlan-ID> {all/black-hole/dynamic/static} |
| **View** | Config view |
| **Description** | This command is used for clear the mac address learned by the vlan of olt |
| <vlan-ID> | Vlan id |
| all/black-hole/dynamic/static | All:All the mac address in the table  Dynamic:Dynamic mac address  black-hole:Black hole mac address  Static:Static mac address |

【Example】

Example 1：Clear all the mac address learned by vlan 100.

|  |
| --- |
| OLT(config)#mac-address flush vlan 100 all  OLT(config)# |

## Show OLT MAC Address Table

|  |  |
| --- | --- |
| Command | OLT(config)#show mac-address all |
| **View** | Config view |
| **Description** | This command is used for show all the mac address learn by olt |

【Example】

Example 1：Show all the mac address learned by olt.

|  |
| --- |
| OLT(config)#show mac-address all  -----------------------------------------------------------------------------  Total:3  -----------------------------------------------------------------------------  MAC VLAN Port MAC-Type  -----------------------------------------------------------------------------  E0:56:43:A9:B4:1A 100 cpu static  E0:56:43:A9:B4:1A 200 cpu static  E0:56:43:A9:B4:1A 1000 cpu static  -----------------------------------------------------------------------------  OLT(config)# |

## Show OLT MAC Address Black Hole

|  |  |
| --- | --- |
| Command | OLT(config)#show mac-address black-hole |
| **View** | Config view |
| **Description** | This command is used for show all the black hole mac address of olt |

【Example】

Example1:Show all the black hole mac address of olt.

|  |
| --- |
| OLT(config)#show mac-address black-hole  <cr>-Please press ENTER to execute command  OLT(config)#show mac-address black-hole  -----------------------------------------------------------------------------  Total:1  -----------------------------------------------------------------------------  MAC VLAN Port MAC-Type  -----------------------------------------------------------------------------  00:12:13:23:45:32 100 cpu blackhole  -----------------------------------------------------------------------------  OLT(config)# |

## Show OLT Dynamic MAC Address Table

|  |  |
| --- | --- |
| Command | OLT(config)#show mac-address dynamic |
| **View** | Config view |
| **Description** | This command is used for show all the dynamic mac address learned by olt |

【Example】

Example 1：Show all the dynamic mac address learned by olt.

|  |
| --- |
| OLT(config)#show mac-address dynamic  -----------------------------------------------------------------------------  Total:3  -----------------------------------------------------------------------------  MAC VLAN Port MAC-Type  -----------------------------------------------------------------------------  02:02:5C:6E:0F:17 1 ge0/0/5 dynamic  F4:06:69:B3:74:8C 1 ge0/0/5 dynamic  00:0A:C2:22:B0:9D 1 ge0/0/5 dynamic  -----------------------------------------------------------------------------  OLT(config)# |

## Show MAC Address Table From ONU

|  |  |
| --- | --- |
| Command | OLT(config)#show mac-address ont F/S/P <onu-id> |
| **View** | Config view |
| **Description** | This command is used for show the mac address learned by onu |
| F/S/P | FrameID/SlotID/PortID,range for<0-0>/<0-0>/<1-16> |
| <onu-id> | ONU id,range for 1-64 |

【Example】

Example 1：Show mac address learned by pon1 ont 4.

|  |
| --- |
| OLT(config)#show mac-address ont 0/0/1 4  -----------------------------------------------------------------------------  Total:1  -----------------------------------------------------------------------------  MAC VLAN Port ONU-Id MAC-Type  -----------------------------------------------------------------------------  E0:67:B3:0D:0E:01 1 pon0/0/1 4 dynamic  -----------------------------------------------------------------------------  OLT(config)# |

## Show MAC Address Table From PON Port

|  |  |
| --- | --- |
| Command | OLT(config)#show mac-address port epon F/S/P with-ont-location |
| **View** | Config view |
| **Description** | This command is used for show the mac address learned by pon port and show the onu id that the mac address had through |
| F/S/P | FrameID/SlotID/PortID,range for<0-0>/<0-0>/<1-16> |
| with-ont-location | This parameter is optional,if it is added,it will show the onu id that the mac address had through |

【Example】

Example 1：Show the mac address learned by pon1 and show the onu id that the mac address had through

|  |
| --- |
| OLT(config)#show mac-address port epon 0/0/1 with-ont-location  -----------------------------------------------------------------------------  Total:1  -----------------------------------------------------------------------------  MAC VLAN Port ONU-Id MAC-Type  -----------------------------------------------------------------------------  E0:67:B3:0D:0E:01 1 pon0/0/1 4 dynamic  -----------------------------------------------------------------------------  OLT(config)#show mac-address port epon 0/0/1  -----------------------------------------------------------------------------  Total:1  -----------------------------------------------------------------------------  MAC VLAN Port MAC-Type  -----------------------------------------------------------------------------  E0:67:B3:0D:0E:01 1 pon0/0/1 dynamic  -----------------------------------------------------------------------------  OLT(config)# |

## Show MAC Address Table From GE Port

|  |  |
| --- | --- |
| Command | OLT(config)#show mac-address port ge <F/S/P> |
| **View** | Config view |
| **Description** | This command is used for show the mac address learned by GE port. |
| <F/S/P> | FrameID/SlotID/PortID,range for<0-0>/<0-0>/<1-8> |

【Example】

Example 1：Show the mac address learned by GE5

|  |
| --- |
| OLT(config)#show mac-address port ge 0/0/5  -----------------------------------------------------------------------------  Total:9  -----------------------------------------------------------------------------  MAC VLAN Port MAC-Type  -----------------------------------------------------------------------------  3C:95:09:4F:30:D1 1 ge0/0/5 dynamic  84:5B:12:66:C0:E2 1 ge0/0/5 dynamic  02:02:5C:6E:0F:17 1 ge0/0/5 dynamic  E0:67:B3:46:50:DD 1 ge0/0/5 dynamic  00:E0:FC:09:BC:F9 1 ge0/0/5 dynamic  B8:81:98:78:36:10 1 ge0/0/5 dynamic  00:DB:DF:9C:FA:0E 1 ge0/0/5 dynamic  00:0A:C2:22:B0:9D 1 ge0/0/5 dynamic  6C:3B:6B:32:83:1C 1 ge0/0/5 dynamic  -----------------------------------------------------------------------------  OLT(config)# |

## Show MAC Address Table From XGE Port

| Command | OLT(config)#show mac-address port xge <F/S/P> |
| --- | --- |
| **View** | Config view |
| **Description** | This command is used for show the mac address learned by XGE port. |
| <F/S/P> | FrameID/SlotID/PortID，<0-0>/<0-0>/<1-2> |

【Example】

Example 1：Show mac address learned by XGE1.

|  |
| --- |
| OLT(config)#show mac-address port xge 0/0/1  There is not any MAC address record!  OLT(config)# |

## Show MAC Address Table From Aggregation Group

|  |  |
| --- | --- |
| Command | OLT(config)#show mac-address port lag {<manual group id>|<Lacp group id>} |
| **View** | Config view |
| **Description** | This command is used for show mac address learned by port aggregation group. |
| {<Manual group id>|<Lacp group id>} | manual-group-ID,range for 1-8  lacp-group-ID,range for 9-16 |

【Example】

Example 1：Show mac address learned by port link aggregation group 1.

|  |
| --- |
| OLT(config)#show mac-address port lag 1  There is not any MAC address record!  OLT(config)# |

## Show OLT Static MAC Address Tables

|  |  |
| --- | --- |
| Command | OLT(config)#show mac-address static |
| **View** | Config view |
| **Description** | This command is used for show all the static mac address of olt. |

【Example】

Example 1：Show all the static mac address of olt.

|  |
| --- |
| OLT(config)#show mac-address static  -----------------------------------------------------------------------------  Total:3  -----------------------------------------------------------------------------  MAC VLAN Port MAC-Type  -----------------------------------------------------------------------------  E0:56:43:A9:B4:1A 100 cpu static  E0:56:43:A9:B4:1A 200 cpu static  E0:56:43:A9:B4:1A 1000 cpu static  -----------------------------------------------------------------------------  OLT(config)# |

## Show OLT MAC Address Aging Time Configuration

|  |  |
| --- | --- |
| Command | OLT(config)#show mac-address timer |
| **View** | Config view |
| **Description** | This command is used for show the mac address aging time of OLT. |

【Example】

Example 1：Show mac address aging time of olt.

|  |
| --- |
| OLT(config)#show mac-address timer  MAC aging time:300s  OLT(config)# |

## Show MAC Address Table From Specified Vlan

| Command | OLT(config)#show mac-address vlan <vlan-id> |
| --- | --- |
| **View** | Config view |
| **Description** | This command is used for show the mac address of specified vlan. |
| <vlan-id> | VLAN ID to be show,range for 1-4094 |

【Example】

Example 1：Show mac address of vlan 100.

|  |
| --- |
| OLT(config)#show mac-address vlan 100  -----------------------------------------------------------------------------  Total:2  -----------------------------------------------------------------------------  MAC VLAN Port MAC-Type  -----------------------------------------------------------------------------  E0:56:43:A9:B4:1A 100 cpu static  00:12:13:23:45:32 100 cpu blackhole  -----------------------------------------------------------------------------  OLT(config)# |

# OLT Global VLAN Configurationss

## OLT VLAN Basic Configuration

### Create OLT VLAN or VLAN List

|  |  |
| --- | --- |
| Command | OLT(config)#vlan vlan-list |
| **View** | Config view |
| **Description** | This command is used for create a vlan or a vlan list. |
| <vlan-list> | ID of vlan,range for 1-4094 |

【Example】

Example 1：Create vlan 100.

|  |
| --- |
| OLT(config)#vlan 100  Create vlan successfully:100  OLT(config)# |

Example 2:Create a vlan list 110-120.

|  |
| --- |
| OLT(config)#vlan 110-120  Create vlan successfully:110-120  OLT(config)# |

### Detele OLT VLAN or VLAN List

|  |  |
| --- | --- |
| Command | OLT(config)#no vlan <vlan-list> |
| **View** | Config view |
| **Description** | This command is used for delete one or batch of vlan |
| <vlan-list> | VLAN id to be delete,range for 1-4094 |

【Example】

Example 1：Delete vlan 100.

|  |
| --- |
| OLT(config)#no vlan 100  Delete vlan successfully:100  OLT(config)# |

Example 2:Delete vlan list 110-120.

|  |
| --- |
| OLT(config)#no vlan 110-120  Delete vlan successfully:110-120  OLT(config)# |

### Config OLT VLAN or VLAN List Name

|  |  |
| --- | --- |
| Command | OLT(config)#vlan-name <vlan-list> < vlan-name> |
| **View** | Config view |
| **Description** | This command is used for set the vlan name. |
| <vlan-name> | Vlan name,length for 1-17 letters |

【Example】

Example 1：Set the name of vlan 100 as test.

|  |
| --- |
| OLT(config)#vlan-name 100 test  OLT(config)# |

Example 2:Set the name of vlan list 100-120 as test.

|  |
| --- |
| OLT(config)#vlan-name 100-120 test  OLT(config)# |

### Delete VLAN or VLAN List Name

|  |  |
| --- | --- |
| Command | OLT(config)#no vlan-name <vlan-list> <vlan-name> |
| **View** | Config view |
| **Description** | This command is used for delete the name of vlan. |
| <vlan-list> | VLAN id to be set,range for 1-4094 |

【Example】

Example 1：Delete the name of vlan 100.

|  |
| --- |
| OLT(config)#no vlan-name 100  OLT(config)# |

Example 2:Delete the name of vlan list 100-120.

|  |
| --- |
| OLT(config)#no vlan-name 100-120  OLT(config)# |

### Show OLT VLAN Configuration

|  |  |
| --- | --- |
| Coammand | OLT(config)#show vlan {all/<vlan-list>} |
| **View** | Config view |
| **Description** | This command is used for show vlan info. |
| <vlan-list> | VLAN id to be show,range for 1-4094 |

【Example】

Example 1：Show the info of vlan 100.

|  |
| --- |
| OLT(config)#show vlan 100  -----------------------------------------------------------------------------  Vlan-ID:100 Vlan-Name:test  Untagged-Ports:-  Tagged-Ports:-  -----------------------------------------------------------------------------  OLT(config)# |

Example 2:Show info of all the vlan.

|  |
| --- |
| OLT(config)#show vlan all  -----------------------------------------------------------------------------  Vlan-ID:1 Vlan-Name:vlan1  Untagged-Ports:  ge0/0/1 ge0/0/2 ge0/0/3 ge0/0/4 ge0/0/5  ge0/0/6 ge0/0/7 ge0/0/8 xge0/0/1 xge0/0/2  pon0/0/1 pon0/0/2 pon0/0/3 pon0/0/4 pon0/0/5  pon0/0/6 pon0/0/7 pon0/0/8 pon0/0/9 pon0/0/10  pon0/0/11 pon0/0/12 pon0/0/13 pon0/0/14 pon0/0/15  pon0/0/16 lag1 lag2 lag3 lag4  lag5 lag6 lag7 lag8 lag1  lag2 lag3 lag4 lag5 lag6  lag7 lag8  Tagged-Ports:-  -----------------------------------------------------------------------------  Vlan-ID:2 Vlan-Name:vlan2  Untagged-Ports:-  Tagged-Ports:- |

### Show OLT VLAN Translate Configuraiton

| Command | OLT(config)#show vlan translate all |
| --- | --- |
| **View** | Config view |
| **Description** | This command is used for show vlan translating list. |

【Example】

Example 1：Show translating list of vlan 100.

|  |
| --- |
| OLT(config)#show vlan translate all  -----------------------------------------------------------------------------  index port oldvlan newvlan priority mode  -----------------------------------------------------------------------------  1 pon0/0/5 800 800--Translate  2 pon0/0/14 2000-2124 38 0 QinQ  3 pon0/0/1 1000 37 0 QinQ  4 pon0/0/14 1000 37 0 QinQ  -----------------------------------------------------------------------------  OLT(config)# |

## Vlanif Configuration

### Create or Delete Vlanif Interface

|  |  |
| --- | --- |
| Command | OLT(config)#{no} interface vlanif <vlan-list> |
| **View** | Config view |
| **Description** | This command is used for create or delete a vlanif interface |
| <vlan-list> | VLAN id to be set,range for 1-4094 |

【Example】

Example 1：Create a interface vlanif 100 and enter the configure view,the precondition is that the vlan 100 had been created.

|  |
| --- |
| OLT(config)#interface vlanif 100  OLT(config-interface-vlanif-100)# |

Example 2:Delete the vlanif 100.

|  |
| --- |
| OLT(config)#no interface vlanif 100  OLT(config)# |

### Create or Delete Vlanif IP Address

|  |  |
| --- | --- |
| Command | OLT(config-interface-vlanif-100)#{no} ip address <Ip address> {<IP address mask|length-mask>} |
| **View** | Vlanif interface |
| **Description** | This command is used for create or delete the ip address of vlanif interface |
| <Ip address> | IP address of vlanif,format for X.X.X.X |
| <IP address mask> | IP address mask of vlanif interface,format for X.X.X.X |
| <length-mask> | Length of net mask,range for 0-32 |

【Example】

Example 1：Set the ip address and net mask of vlanif interface as 192.168.1.100 and

255.255.255.0

|  |
| --- |
| OLT(config-interface-vlanif-100)#ip address 192.168.1.100 255.255.255.0  OLT(config-interface-vlanif-100)# |

Example 2:Delete the ip address of vlanif.

|  |
| --- |
| OLT(config-interface-vlanif-100)#no ip address  OLT(config-interface-vlanif-100)# |

### Config Vlanif Interface Description

|  |  |
| --- | --- |
| Command | OLT(config-interface-vlanif-100)#description <description information> |
| **View** | VLANIF view |
| **Description** | This command is used for set the description of vlanif interface |
| <description information> | The description of vlanif,length for 1-128 |

【Example】

Example 1：Set the description of vlanif 100 as test.

|  |
| --- |
| OLT(config)#interface vlanif 100  OLT(config-interface-vlanif-100)#description test  Set interface description successfully!  OLT(config-interface-vlanif-100)# |

### Show Vlanif Interface Detail Information

|  |  |
| --- | --- |
| Command | OLT(config)#show interface vlanif <vlan-id> |
| **View** | Config view |
| **Description** | This command is used for show the detail info of one or whole vlanif interface |
| <vlan-id> | VLAN ID to be show |

【Example】

Example 1：Show the info of vlanif 100

|  |
| --- |
| OLT(config)#show interface vlanif 100  Description:Inband interface vlanif100  The Maximum Transmit Unit is 1500 bytes  Internet Address is 192.168.1.100,netmask 255.255.255.0  Hardware address is E0:56:43:A9:B4:1A  Recive 0 packets,0 bytes  Transmit 0 packets,0 bytes  OLT(config)# |

Example 2:Show the info of whole vlanif interface.

|  |
| --- |
| OLT(config)#show interface vlanif  Description:Inband interface vlanif100  The Maximum Transmit Unit is 1500 bytes  Internet Address is 192.168.1.100,netmask 255.255.255.0  Hardware address is E0:56:43:A9:B4:1A  Recive 0 packets,0 bytes  Transmit 0 packets,0 bytes  Description:Inband interface vlanif1000  The Maximum Transmit Unit is 1500 bytes  Internet Address is 192.168.2.100,netmask 255.255.255.0  Hardware address is E0:56:43:A9:B4:1A  Recive 0 packets,0 bytes  Transmit 0 packets,0 bytes  OLT(config)# |

## VLAN Policy Configuration

### Add VLAN Policy Based On Mac address

|  |  |
| --- | --- |
| Command | OLT(config)#mac-vlan <mac-address> <vlan-id> <priority> |
| **View** | Config view |
| **Description** | This command is used for add mac-vlan,when the ingress message of olt is untagged and the destination mac is equal to the setting mac too,this message will be added a corresponding vlan and priority label.  Delete mac-vlan:no mac-vlan<mac-address>/all |
| <mac-address> | Mac address,format for xx.xx.xx.xx.xx.xx。 |
| <vlan-id> | VLAN id,range for 1-4094. |
| <priority> | priority |

【Example】

Example 1：Add mac-vlan 100 and priority 0 to mac address 13:20:12:08:97:23

|  |
| --- |
| OLT(config)#mac-vlan 13:20:12:08:97:23 100 0  OLT(config)# |

### Show MAC-VLAN Entry

|  |  |
| --- | --- |
| Command | OLT(config)#show mac-vlan all |
| **View** | Config view |
| **Description** | This command is used for show mac-vlan entry |

【Example】

Example 1：Show mac-vlan entry

|  |
| --- |
| OLT(config)#show mac-vlan all  -----------------------------------------------------------------------------  index mac-address vlan priority  1 13:20:12:08:97:23 100 0  OLT(config)# |

### Add VLAN Policy Based On IP Address

| Command | OLT(config)#ip-subnet-vlan <ip-addr> {length-mask|mask} <vlan-id> <priority> |
| --- | --- |
| **View** | Config view |
| **Description** | This command is used for add ip-subnet-vlan,when the ingress message of olt is untagged and the destination ip address is equal to the setting ip address too,this message will be added a corresponding vlan and priority label.  Delete ip-subnet-vlan entry:no ip-subnet-vlan<ip address><length>/<mask> |
| <ip-addr> | IP address,format for x.x.x.x |
| <length-mask|mask> | length of net mask,range for 0-32  Mask:net mask,format for x.x.x.x |
| <vlan-id> | VLAN id,range for 1-4094 |
| <priority> | VLAN priority |

【Example】

Example 1：Create an ip-subnet-vlan,set ip address as 192.168.5.34,net mask length for 24,vlan for 100,priority for 0.

|  |
| --- |
| OLT(config)#ip-subnet-vlan 192.168.5.34 24 100 0  OLT(config)# |

### Show IP-Subnet-VLAN Entry

|  |  |
| --- | --- |
| Command | OLT(config)#show ip-subnet-vlan all |
| **View** | Config view |
| **Description** | This command is used for show the entry of ip-subnet-vlan |

【Example】

Example 1：Show all the entry of ip-subnet-vlan.

|  |
| --- |
| OLT(config)#show ip-subnet-vlan all  -----------------------------------------------------------------------------  ip-address netmask vlan priority  192.168.5.0 255.255.255.0 100 0  -----------------------------------------------------------------------------  OLT(config)# |

### Add VLAN Policy Based On Protocol

|  |  |
| --- | --- |
| Command | OLT(config)#protocol-vlan <protocol-index> {at|ipv4|ipv6|} {<ethernetii|snap}  OLT(config)#protocol-vlan <protocol-index> <ipx> {ethernetii|snap|llc|snap}  OLT(config)#protocol-vlan <protocol-index> mode {ethernetii|snap} etype <ethertype id> |
| **View** | Config view |
| **Description** | This command is used for create protocol-vlan.Protocol-vlan can be bound to GE port,pon port,xge port,it is used for protocol translation for switch data.  Delete the protocol vlan:no protocol-vlan<1-16>/all |
| <protocol-index> | protocol-vlan index,range for 1-16 |
| <parameter> | at:appletalk protocol  ipv4:IPv4 protocol  ipv6:IPv6 protocol  Ipx:IPx protocol  ethernetii:Type of Ethernet protocol  snap:Type of snap protocol  llc:Type of llc protocol  raw:Type of raw protocol  etype:ethertype |
| <ethertype id> | The number of ethertype,range for 0x0001-0xffff |

【Example】

Example 1：Create a protocol-vlan which index is 1,mode is ethernetii and bind it to GE1 and vlan 100.

|  |
| --- |
| OLT(config)#protocol-vlan 1 mode ethernetii etype 0x8100  OLT(config)#interface ge 0/0  OLT(config-interface-ge-0/0)#protocol-vlan 1 add port 1 100  OLT(config-interface-ge-0/0)# |

### Show Protocol-vlan Entry

|  |  |
| --- | --- |
| Command | OLT(config)#show protocol-vlan all |
| **View** | Config view |
| **Description** | This command is used for show all the protocol-vlan entry. |

【Example】

Example 1：Show all the protocol-vlan entry.

|  |
| --- |
| OLT(config)#show protocol-vlan all  -----------------------------------------------------------------------------  index frame ethtype port vlan id  1 ethii unknow(0x8100)ge0/0/1 100  -----------------------------------------------------------------------------  OLT(config)# |

# 

# OLT IGMP Configuration

## Config IGMP Fast-leave Function

|  |  |
| --- | --- |
| Command | OLT(config)#igmp fast-leave {on|off} |
| **View** | Config view |
| **Description** | igmp fast-leave off:  Close igmp-snooping igmp fast-leave function.After executing this command,after the ont receiving igmp leave message of user,it needs to send specific group query message to assure whether the user is online,if the group query message has timeout,but ont still has not receive the user report message,ont will infer the user has offline and renew the local multicast table entry.When the user needn’t cut the channel fastly,using this parameter.  igmp fast-leave on:  Open igmp-snooping igmp fast-leave function.After executing this command,after the ont receiving igmp leave message of user,ont renew the local multicast table immediately according to the igmp leave message with no need of sending specific group query message to assure whether the user has offline.When the user needs to cut the channel fastly,using this parameter. |
| {on|off} | Off:Close igmp-snooping igmp fast-leave function of olt  On:Open igmp-snooping igmp fast-leave function of olt |

【**Example**】

**Example 1：**Open igmp-snooping igmp fast-leave function of olt

|  |
| --- |
| OLT(config)#igmp fast-leave on  OLT(config)# |

## Config IGMP Mode

| Command | OLT(config)#igmp mode {ctc|snooping|proxy|disable} |
| --- | --- |
| **View** | Config view |
| **Description** | This command is used for set the mode of igmp |
| {ctc|snooping|proxy|disable} | igmp mode ctc:  Ctc is a controlled multicast mode.traditional multicast service is uncontrollable,user can join in a multicast group by sending igmp report message,then it can receive the multicast message of the multicast group.Its core idea is to set the limits of authority for the user's accessing to a multicast group.when the user request to join in a multicast group,olt must authenticate to this request,and reject to illegal or ultra vires request.Ctc mode of olt reaches its goal by intercepting the igmp report message which is sent by ont to control the creation of second layer multicast transmission table.After the olt receiving report message of multicast user,olt finds the user’s using authority template according to the user vlan.if the multicast group is not included in the using authority template,olt will intercept this report message and do not generate transmission table,thus the user can not receive the multicast data stream;.if the multicast group is included in the using authority template list,and if the list joins in template by view mode,the report message is permitted to pass.if the list joins in template by preview mode,the report message can pass too,but the olt will activate a timer,when it is timeout,the multicast group transmission table will be deleted,the igmp report message will be intercept,the preview function is realized by this way.  Otherwise,ont multicast mode must be set as ctc mode,the command is“ont multicast-mode”,in this mode,when the multicast user has passed the authentication,olt will issue the corresponding extension oam message to maintain the multicast table entry of ont to realize the controlling of multicast service.  igmp mode snooping  Set the igmp mode of multicast vlan as IGMP snooping.IGMP snooping obtains relevant info to maintain the multicast transmission table by monitoring the communication between the user and multicast router.system does not make any process to multicast message of this multicast vlan,just transparent it.  igmp mode proxy:  Set the igmp mode of multicast vlan as IGMP proxy.igmp proxy intercepts the igmp message between user and multicast router and proceeds coherent processing,then transmits it to the upper multicast router.From the view of user,the system is equivalent to multicast server;From the view of upper device,the system is equivalent to multicast user.IGMP proxy mode degrees the multicast protocol message traffic in the network.  igmp mode disable:Close the multicast function |

【Example】

Example 1：Set igmp mode as proxy.

|  |
| --- |
| OLT(config)#igmp mode proxy  OLT(config)# |

## Config IGMP Proxy Parameter

|  |  |
| --- | --- |
| Command | OLT(config)#igmp proxy {gen\_interval|gen\_response|robustness|source-ip|sp\_count|sp\_interval|sp\_response} |
| **View** | Config view |
| **Description** | This command is used for set parameter of IGMP Proxy |
| <gen\_interval|gen\_response|robustness|source-ip|sp\_count|sp\_interval|sp\_response> | gen\_interval-General query interval  This command is used for set general query interval.system send the gen\_interval aiming at all program to assure whether the user is watching a program.If the system has not receive the report message of user,it will be regarded as that there is no user watching this program,and this program data stream will be stopped.it can avoid the bandwidth waste from that the user does not watch program but still receiving the multicast stream.  gen\_response-General query max response time//This command is used for set general query max response time.  robustness-Robustness keyword  This command is used for set robustness keyword.According to network stability variation,the user hopes to adjust to robustness keyword,using this command.System uses this robustness keyword to assure the aging time of multicast user after setting.Robustness keyword is a coefficient which is used for enhance the robustness of the system,it directly effects to the length of multicast user aging time,in addiction,it effects to the frequency of gen\_interval message.If a subnet is likely to occur to packet loss,robustness keyword should be increase to ensure the stability of multicast user.  source-ip-Source ip of igmp proxy message  This command is used for set the source ip of gen\_interval or specific group query message which is sent to user by igmp router.If this ip does not be assigned,system will send the gen\_interval query message or specific group message with the default ip.  sp\_count-igmp specific query count  This command is used for set the query counts of igmp specific query.System aims at a specific program and sends N(N is set by this command)times specific igmp query message to assure whether the user is watching this program,if there is no user’s feedback report message,system will regard that no user is watching this program and the system will not send the program data to user,it can avoid that the user does not watching this program but still receiving the multicast stream,it prevents system from bandwidth waste.  sp\_interval-Specific query interval  This command is used for set specific query interval.system send the specific query message aiming at a specified program to assure whether the user is watching a program.If the system has not receive the report message of user,it will be regarded as that there is no user watching this program,and this program data stream will be stopped.it can avoid the bandwidth waste from that the user does not watch program but still receiving the multicast stream.  sp\_response-Specific query max response time |

【Example】

Example 1：Set igmp proxy specific query count as 1,gen\_interval as 250s,gen\_response as 10,robustness as 2

|  |
| --- |
| OLT(config)#igmp proxy sp\_count 1  OLT(config)#igmp proxy gen\_interval 250  OLT(config)#igmp proxy gen\_response 10  OLT(config)#igmp proxy robustness 2  OLT(config)# |

## Config IGMP Forwarding Policy

|  |  |
| --- | --- |
| Command | OLT(config)#igmp policy {discard|pass} |
| **View** | Config view |
| **Description** | This command is used for set transmission policy of igmp message |
| {discard|pass} | Discard:Discard the unknown igmp protocol message  Pass:the igmp protocol message is set as transparent |

【Example】

Example 1：Discard the unknown igmp protocol message

|  |
| --- |
| OLT(config)#igmp policy discard  OLT(config)# |

## Show IGMP Configuration

|  |  |
| --- | --- |
| Command | OLT(config)#show igmp config |
| **View** | Config view,btv view,multicast vlan view |
| **Description** | This command is used for show igmp config.including igmp state,fast leave state,General query max response time(s),query interval,source ip and etc. |

【Example】

Example 1：Show igmp config.

|  |
| --- |
| OLT(config)#show igmp config  -----------------------------------------------------------------------------  Global config:  Igmp mode:Proxy  Igmp policy:Discard  Fast leave:Off  -----------------------------------------------------------------------------  Proxy config:  Robustness count:2  General query max response time(s):10  General query interval(s):125  Specific query interval(ms):1000  Specific query count:2  Specific query max response time(ms):800  Source ip of the proxy:192.168.1.253  -----------------------------------------------------------------------------  OLT(config)# |

## Show IGMP Forwarding Table

|  |  |
| --- | --- |
| Command | OLT(config)#show igmp group {all|ip-address|vlan} |
| **View** | Config view,btv view,multicast vlan view |
| **Description** | This command is used for show igmp group. |
| {all|ip-address|vlan} | All:show all the igmp group.  vlan-id:show igmp group of specified vlan id  ip-address:show igmp group of specified channel ip address |

【Example】

Example 1：Show all the igmp group.

|  |
| --- |
| OLT(config)#show igmp group all  ERROR:There is not any group address record.  OLT(config)# |

## Config Multicast VLAN

|  |  |
| --- | --- |
| Command | OLT(config)#multicast-vlan <vlan-id> |
| **View** | Config view |
| **Description** | This command is used for create multicast vlan and enter multicast vlan mode,”no”command is used for delete it.Multicast vlan is a kind of vlan application,in this mode,user can set relevant parameters of multicast. |
| <vlan-id> | Multicast vlan id.only after the corresponding vlan is created the multicast vlan can be used. |

【Example】

Example 1：Create multicast vlan 100 and enter enter multicast vlan mode.

|  |
| --- |
| OLT(config)#multicast-vlan 100  OLT(multicast-vlan-100)# |

## Config IGMP Match Group

|  |  |
| --- | --- |
| Command | OLT(config)#igmp match group ip <start-ip> to-ip <end-ip> |
| **View** | multicast-vlan view |
| **Description** | This command is used for set dynamic program library,this range ip address makes up a channel group,it can set limits of authority for these channel in btv mode. |
| <start-ip> | Match start ip,it must be multicast ip address |
| <end-ip> | Match end ip,it must be multicast ip address |

【Example】

Example 1：Set a dynamic program library:224.1.1.1-224.2.2.2

|  |
| --- |
| OLT(config-multicast-vlan-100)#igmp match group ip 224.1.1.1 to-ip 224.2.2.2  OLT(config-multicast-vlan-100)# |

## Show IGMP Match Group

|  |  |
| --- | --- |
| Command | OLT(config)#show igmp match group {vlan-id|all} |
| **View** | multicast-vlan view,config view |
| **Description** | This command is used for show igmp match group |
| {vlan-id|all} | vlan-id:multicast vlan id  all:all of the multicast vlan |

【Example】

Example 1：Show igmp match group vlan 100

|  |
| --- |
| OLT(config)#show igmp match group vlan 100  Total Match Group:1  -----------------------------------------------------------------------------  MVlan Match Mode Program  100 disable 224.1.1.1-224.2.2.2  -----------------------------------------------------------------------------  OLT(config)# |

## Add IGMP Program

| Command | OLT(config-multicast-vlan-100)#igmp program add program-index <Program-index> ip <ip-addr> |
| --- | --- |
| **View** | multicast-vlan view |
| **Description** | This command is used for add static multicast program.it needs to pre-allocation multicast program library,The authorized user can view or preview the program in the specified multicast vlan. |
| <Program-index> | Multicast program index |
| <ip-addr> | multicasst ip address,format is X.X.X.X |

【Example】

Example 1：Set static multicast program,and binds it to program index 2.

|  |
| --- |
| OLT(config-multicast-vlan-100)#igmp program add program-index 2 ip 239.1.1.1  OLT(config-multicast-vlan-100)# |

## Add Batch IGMP Program

|  |  |
| --- | --- |
| Command | OLT(config-multicast-vlan-100)#igmp program add program-index <Program-index> batch ip <ip-addr> to-ip <ip-addr> |
| **View** | multicast-vlan view |
| **Description** | This command is used for add static multicast program.If igmp match mode is enabled,it needs to pre-allocation multicast program library,The authorized user can view or preview the program in the specified multicast vlan. |
| <Program-index> | Igmp program index |
| <ip-addr> | It refers to the beginning and ending igmp IP,forming an igmp range. |

【Example】

Example 1：It configures batch static igmp program from 224.1.1.1 to 224.1.1.1.3,and binding program-index 3.

|  |
| --- |
| OLT(config-multicast-vlan-100)#igmp program add program-index 3 batch ip 224.1.1.1 to-ip 224.1.1.3  OLT(config-multicast-vlan-100)# |

## Delete IGMP Program

|  |  |
| --- | --- |
| Command | OLT(config-multicast-vlan-100)#igmp program delete {all|program-index<Program-index>} |
| **View** | multicast-vlan view |
| **Description** | This command is used for delete igmp program.When it doesn’t want users to watch multicast program,using this command to delete igmp program from program database.Once deleting one program,users will not watch this program. |
| <Program-index> | igmp program index |
| <all> | all igmp programs |

【Example】

Example 1：Delete static igmp program-index 2

|  |
| --- |
| OLT(config-multicast-vlan-100)#igmp program delete program-index 2  OLT(config-multicast-vlan-100)# |

## Config IGMP Router-port

|  |  |
| --- | --- |
| Command | OLT(config-multicast-vlan-100)#igmp router-port ge|xge <port-id> |
| **View** | multicast-vlan view |
| **Description** | This command is used for configure igmp router-port.For ctc mode,users need to configure router-port to realize the below devices forwarding. |
| <port-id> | ge/xge port number |

【Example】

Example 1：configure ge5 port as router-port

|  |
| --- |
| OLT(config-multicast-vlan-100)#igmp router-port ge 0/0/5  OLT(config-multicast-vlan-100)# |

## Show IGMP Router-port

|  |  |
| --- | --- |
| Command | OLT(config-multicast-vlan-100)#show igmp router-port vlan <vlan-id> |
| **View** | multicast-vlan view |
| **Description** | This command is used for view IGMP router-port |
| <vlan-id> | Multicast-vlan id |

【Example】

Example 1：View multicast-vlan 100 router-port

|  |
| --- |
| OLT(config-multicast-vlan-100)#show igmp router-port vlan 100  VID:100  Router:ge0/0/5  OLT(config-multicast-vlan-100)# |

## Configure Unknow-multicast Forwarding Policy

|  |  |
| --- | --- |
| Command | OLT(config-multicast-vlan-100)#igmp multicast-unknown policy {discard|transparent} |
| **View** | multicast-vlan view |
| **Description** | This command is used for configure multicast-unknown service flow suppression policy.If service flow carriers special-purpose multicast-unknown,thus configuring transparent.No special-purpose multicast-unknown occupies bandwidth,thus setting discard. |
| {discard|transparent} | Discard:System discard received multicast-unknown service flow  Transparent:System transparent received multicast-unknown service flow. |

【Example】

Example 1：Configure multicast-unknown policy as discard.

|  |
| --- |
| OLT(config-multicast-vlan-100)#igmp multicast-unknown policy discard  OLT(config-multicast-vlan-100)# |

## Show Unknow-multicast Forwarding Policy

|  |  |
| --- | --- |
| Command | OLT(config-multicast-vlan-100)#show igmp multicast-unknown policy vlan <vlan-id> |
| **View** | multicast-vlan view |
| **Description** | This command is used for view multicast-unknown service flow suppress policy. |
| <vlan-id> | Multicast-vlan id |

【Example】

Example 1：View multicast-unknown service flow suppression policy

|  |
| --- |
| OLT(config-multicast-vlan-100)#show igmp multicast-unknown policy vlan 100  Unknown multicast policy is discard.  OLT(config-multicast-vlan-100)# |

## Add IGMP User（Member） in Multicast-vlan

|  |  |
| --- | --- |
| Command | OLT(config-multicast-vlan-100)#igmp member user-index <User-index> |
| **View** | Multicast-vlan view |
| **Description** | This command is used for add igmp user to multicast-vlan |
| <User-index> | configured igmp user |

【Example】

Example 1：Add igmp user 1 to multicast-vlan 100

|  |
| --- |
| OLT(config-multicast-vlan-100)#igmp member user-index 1  OLT(config-multicast-vlan-100)# |

## Show Multicast-vlan Member Configuration

| Command | OLT(config-multicast-vlan-100)#show igmp multicast-vlan-member {all|vlan-id} |
| --- | --- |
| **View** | Config view and multicast-vlan view |
| **Description** | This command is used for view multicast-vlan member |
| <all|vlan-id> | all:view all  vlan-id:view the specified vlan-id member |

【Example】

Example 1：View all multicast-vlan member

|  |
| --- |
| OLT(config-multicast-vlan-100)#show igmp multicast-vlan-member all  Total Mvlan Member:1  -----------------------------------------------------------------------------  User-Index Port ONUId Vlan Authority Mvlan Max-program  1 pon0/0/1 1 100 no-auth 100 8  -----------------------------------------------------------------------------  OLT(config-multicast-vlan-100)# |

## Config IGMP User Bind Rights Profile

|  |  |
| --- | --- |
| Command | OLT(config-btv)#igmp control {bind/delete} user-index <user-index> profile-index <profile-index> |
| **View** | btv view |
| **Description** | This command is used for bind igmp user and rights profile. |
| <User-index> | configured user group,range for 0-4095 |
| <profile-index> | Configured rights profile,range for 1-2000 |

【Example】

Example 1：bind igmp user 1 and rights profile 1

|  |
| --- |
| OLT(config-btv)#igmp control bind user-index 1 profile-index 1  OLT(config-btv)# |

## Config IGMP Preview

|  |  |
| --- | --- |
| Command | OLT(config-btv)#igmp preview (auto-reset-time time |disable | enable |reset) |
| **View** | Btv view |
| **Description** | This command is used for enable multicast preview.Use this command when you need to provide program preview functionality for multicast users.After the function is enabled, the user can preview the program with preview rights, and preview relevant parameters take effect.The igmp preview disable command is used for disable the multicast preview function.Use this command when you need to turn off program preview for all multicast users.After the function is turned off, users cannot preview all programs including those with preview rights, and relevant parameters of preview are invalid. |
| time | When the number of multicast preview is automatically reset, the system will reset the number of preview for all users once the time is reached.Time type is HH:MM:SS,default:4:00:00.Delete multicast preview times automatically reset time with the command: OLT(config-btv)# no igmp preview auto-reset-time |

【Example】

Example1：Enable IGMP preview

|  |
| --- |
| OLT(config-btv)# igmp preview enable  OLT(config-btv)# |

## Config IGMP Preview Profile

| Command | OLT(config-btv)#igmp preview-profile (add preview-index preview-index duration duration-time interval interval-value count count-value | delete (all| preview-index preview-index) ) |
| --- | --- |
| **View** | Btv view |
| **Description** | This command is used for add a preview template for a multicast program.Use this command when you need to adjust the preview function of the program, such as extending the preview time and increasing the number of preview times.After the preview template is successfully added, if the user previews the multicast program that references the preview template, the parameters in the template take effect. |
| preview-index | IGMP preview index,range for 0-31 |
| duration-time | Maximum preview times.If the user previews the program more than the maximum preview times, the program can not preview again. Range for 10-6000,unit is s. |
| interval-value | Minimum time interval between two previews.If the time interval between the user’s two preview of program doesn’t reach this time interval, the user can’t preview again temporarily. |
| count-value | Preview times，range for 1-255 |

【Example】

Example1：Config IGMP preview index is 1, duration is 10,interval is 50 and count is 5

|  |
| --- |
| OLT(config-btv)# igmp preview-profile add preview-index 1 duration 10 interval 50 count 5  OLT(config-btv)# |

## Modify The Program permissions in IGMP Profile

| Command | OLT(config-btv)#igmp profile ((add profile-index profile-index)| (delete profile-index profile-index)|(profile-index profile-index ((add program-index program-index forbidden|preview preview-index preview-index|watch) |(delete program-index program-index) |(modify program-index program-index forbidden|preview preview-index preview-index |watch )) |
| --- | --- |
| **View** | Btv view |
| **Description** | This command is used for modify the program permission in IGMP profile. After modified it, the users binded with this profile will accord the new profile to authentication. When modify it, have to creat igmp profile and igmp program index. |
| Profile-index | IGMP profile index. Range for 1-2000 |
| program-index | IGMP program index. When add the program to profile or modify program permissions according to program index, have to use this parameter. Range for 1-2000 |
| Preview-index | IGMP preview programs index.range for 0-31 |
| forbidden | Set the program permissions to forbidden. |
| preview | Set the program permissions to preview. |
| watch | Set the program permissions to watch. |

【Example】

Example1：In the IGMP profile 1,add the permissions of program index 1 is forbidden.

|  |
| --- |
| OLT(config-btv)# igmp profile add profile-index 1  OLT(config-btv)# igmp profile profile-index 1 add program-index 1 forbidden  OLT(config-btv)# |

## Config IGMP User

| Command | OLT(config-btv)#igmp user ((add user-index user-index pon F/S/P ont ont-id vlan eth-uni-port ((auth |no-auth) max-program max-program ) |
| --- | --- |
| **View** | Btv view |
| **Description** | This command is used for config igmp user. |
| user-index | IGMP program index.Range for 0-4095. |
| F/S/P | Used to represent OLT frame number/slot number/port number, range for 0/0/1-16 |
| ont-id | Bind ONU id ,range for 1-64 |
| Eth-uni-port | Bind ONU’s lan port ,range for 1-24 |
| max-program | Maximum number of user program allowed at the same time , range for 1-32 |

【Example】

Example1：Config IGMP user index is 1 ,bind pon port1 onu 1 uni1 ,and at the same time ,maximum number of user program allowed at the same time is 2.

|  |
| --- |
| OLT(config-btv)# igmp user add user-index 1 pon 0/0/1 ont 1 vlan 1 auth max-program 2  OLT(config-btv)# |

## Show IGMP Configuration

|  |  |
| --- | --- |
| Command | OLT(config-btv)#show igmp ((control (all|user-index user-index)) |(group (all|ip-address ip-address|vlan vlan-id))|(match group (all|vlan vlan-id))|(multicast-unknown policy vlan vlan-id)|(multicast-vlan-member (all|vlan vlan-id))|(preview (all|auto-reset-time|preview-index preview-index))|(profile all| profile-index profile-index))|(program all| program-index program -index))|(router-port vlan vlan-id)|(user (all|online (all|port pon F/S/P ont ont-id))) |
| **View** | Btv view |
| **Description** | This command is used for show igmp configuration,igmp group configuration,multicast-member,preview configuration and igmp user information. |
| user-index | IGMP user index,range for 0-4095 |
| F/S/P | Used to represent OLT frame number/slot number/port number,range for 0/0/1-16 |
| ont-id | Need to bind ONTID，range for 1-64 |
| preview-index | IGMP preview index,range for 0-31 |
| program-index | IGMP program index,range for 1-2000 |

【Example】

Example 1：Show IGMP program table

|  |
| --- |
| OLT(config-btv)# show igmp program program-index 1  ERROR : There is not any program record.  OLT(config-btv)# |

# STP Configuration

## Global STP Config

|  |  |
| --- | --- |
| Command | OLT(config)#spanning-tree {enable|disable} |
| **View** | Config view |
| **Description** | This command is used for on/off the global STP protocol.All the configuration about STP protocol will make effect only if the STP is enabled in global mode and port. |
| {enable|disable} | Enable:Enable global STP protocol  Disable:Disable global STP protocol |

【Example】

Example 1：Enable STP in global mode.

|  |
| --- |
| OLT(config)#spanning-tree enable  OLT(config)# |

## Show STP Configuraiton

|  |  |
| --- | --- |
| Command | OLT(config)#show spanning-tree info |
| **View** | Config view |
| **Description** | This command is used for show configuration info of STP |

【Example】

case1:Show configuration info of STP

|  |
| --- |
| OLT(config)#show spanning-tree info  -----------------------------------------------------------------------------  RSTP switch status:Enable  Bridge ID[PRI-MAC]:32768-e0:56:43:a9:b4:1a  Root Bridge ID[PRI-MAC]:32768-e0:56:43:a9:b4:1a  Bridge max age(s):20  Bridge hello time(s):2  Bridge forward delay(s):15  Transmit Hold Count:3  Root Path Cost:0  -----------------------------------------------------------------------------  Port Status:  -----------------------------------------------------------------------------  Port Priority Path Edge Link Role State  Cost Status Type  -----------------------------------------------------------------------------  ge0/0/1 128 20000 NEdge P2P Unknown Down  ge0/0/2 128 20000 NEdge P2P Unknown Down  ge0/0/3 128 20000 NEdge P2P Unknown Down  ge0/0/4 128 20000 NEdge P2P Unknown Down  ge0/0/5 128 20000 NEdge P2P Unknown Down  ge0/0/6 128 200000 NEdge P2P Designated Forwarding  ge0/0/7 128 20000 NEdge P2P Unknown Down  ge0/0/8 128 20000 NEdge P2P Unknown Down  xge0/0/1 128 2000 NEdge P2P Unknown Down  xge0/0/2 128 2000 NEdge P2P Unknown Down  lag1 128 20000 NEdge P2P Unknown Down  lag2 128 20000 NEdge P2P Unknown Down  lag3 128 20000 NEdge P2P Unknown Down  lag4 128 20000 NEdge P2P Unknown Down  lag5 128 20000 NEdge P2P Unknown Down  lag6 128 20000 NEdge P2P Unknown Down  lag7 128 20000 NEdge P2P Unknown Down  lag8 128 20000 NEdge P2P Unknown Down  lagL9 128 20000 NEdge P2P Unknown Down  lagL10 128 20000 NEdge P2P Unknown Down  lagL11 128 20000 NEdge P2P Unknown Down  lagL12 128 20000 NEdge P2P Unknown Down  lagL13 128 20000 NEdge P2P Unknown Down  lagL14 128 20000 NEdge P2P Unknown Down  lagL15 128 20000 NEdge P2P Unknown Down  lagL16 128 20000 NEdge P2P Unknown Down  -----------------------------------------------------------------------------  OLT(config)# |

## Config STP Priority

|  |  |
| --- | --- |
| Command | OLT(config)#spanning-tree priority <rstp bridge priority> |
| **View** | Config view |
| **Description** | This command is used for set priority of specified spanning tree for the device.Whether the device will be select as root bridge depends on the priority of device.When it needs to specify a device as root bridge,use this command to set the priority of device.whether the device will be selected as root bridge of spanning tree deciding by the priority value. |
| <rstp bridge priority> | Priority of device.Step size for 4096.The smaller the priority is,the higher class the device.  Range for 0-61440,Step size for 4096. |

【Example】

Example 1：Set the priority of spanning tree as 4096.

|  |
| --- |
| OLT(config)#spanning-tree priority 4096  OLT(config)# |

## Config STP Bridge Forward-delay Time

|  |  |
| --- | --- |
| Command | OLT(config)#spanning-tree timer forward-delay <timer> |
| **View** | Config view |
| **Description** | This command is used for set the device forward-delay time of spanning tree.To prevent the device from occurring to temporary loop,it needs to wait for sometime in device status migrating.After setting the forward delay time,status migrate according to this time interval.Range for 4-30s. |
| <timer> | Status migrate time interval.it relates to the switch network diameter.generally,the bigger the diameter is,the longer forward delay time should be set.Range for 4-30s.The default value is 15s. |

【Example】

Example 1：Set the forward delay time as 20s.

|  |
| --- |
| OLT(config)#spanning-tree timer forward-delay 20  OLT(config)# |

## Config STP Bridge Hello Message Send Period Time

|  |  |
| --- | --- |
| Command | OLT(config)#spanning-tree timer hello <time> |
| **View** | Config view |
| **Description** | This command is used for set transmission period of the spanning tree hello time.Network bridge sends the hello message within a certain time interval,it is used for affirm whether the link is normal.After setting,device will send the hello message to neighbor Switch according to corresponding time interval. |
| <time> | Hello time interval.The appropriate hello time interval can ensure that the switch can find the link fault in the network in time without taking up too much network resources.Range for 1-2s,the default is 2s. |

【Example】

Example 1：Set the hello time’s transmission period as 1s.

|  |
| --- |
| OLT(config)#spanning-tree timer hello 1  OLT(config)# |

## Config STP Bridge Max-age Time

|  |  |
| --- | --- |
| Command | OLT(config)#spanning-tree timer max-age <time> |
| **View** | Config view |
| **Description** | This command is used for set max age time.It is used for estimate whether the message is time out.After setting max age time,the device will discard the time out message.range for 6-40s,the default is 20s. |
| <time> | Max age time |

【Example】

Example 1：Set the max age time as 6s.

|  |
| --- |
| OLT(config)#spanning-tree timer max-age 6  OLT(config)# |

## Config STP BPDU TX Hold Count

|  |  |
| --- | --- |
| Command | OLT(config)#spanning-tree hold-count <hold-count> |
| **View** | Config view |
| **Description** | BPDU is the message frame exchanged between the switches that run STP.BPDU includes path and priority info of STP,STP determines the root bridge and root bridge path by BPDU. |
| <hold-count> | BPDU transmission rate,the maximum transmission number of BPDU in each hello time period,range for 1-10,unit is pps. |

【Example】

Example 1：Set the hold-count as 2 pps.

|  |
| --- |
| OLT(config)#spanning-tree hold-count 2  OLT(config)# |

## Config OLT STP Cost

|  |  |
| --- | --- |
| Command | OLT(config)#spanning-tree <link-aggregation group group-id |port port-ID> cost <cost> |
| **View** | Config view |
| **Description** | This command is used for set the cost of GE port spanning tree.when there are multi links between two devices but not the root port,device determines the optimal path by the cost. |
| <port-id> | Port id to be set |
| <cost> | Cost value,range for 1-200000000 |

【Example】

Example 1：Set the cost of GE1 spanning tree as 2000.

|  |
| --- |
| OLT(config)#spanning-tree port ge 0/0/1 cost 2000  OLT(config)# |

## Config OLT STP Edged-port

|  |  |
| --- | --- |
| Command | OLT(config)#spanning-tree <link-aggregation group group-id |port port-ID> edged-port {enable|disable} |
| **View** | Config view |
| **Description** | This command is used for set spanning tree edged-port of GE port.If user specifies a port as edged-port,then the port can rapidly migrate from blocking status to forwarding status without waiting for delay time.User can only set the port which is connected with terminal as edged-port.The default is not edged-port. |
| <port-id> | Port id to be set |
| {enable|disable} | enable:Set this port as edged-port  disable:Set this port as non-edged-port |

【Example】

Example 1：Set GE1 as edged-port.

|  |
| --- |
| OLT(config)#spanning-tree port ge 0/0/1 edged-port enable  OLT(config)# |

## Config OLT STP Mcheck Property

| Command | OLT(config)#spanning-tree <link-aggregation group group-id |port port-ID> mcheck |
| --- | --- |
| **View** | Config view |
| **Description** | This command is used for set mcheck property of GE port spanning tree.Mcheck property is used for detect whether the device which is running in STP compatible mode can transfer to RSTP mode.We can check whether there are any network bridge existing in the network segment connected with current ethernet port.If it is yes,RSTP protocol will transfer the port protocol running mode to STP mode. |
| <port-id> | Port id to be set,range for 1-8 |

【Example】

Example 1：Set the mheck property of GE1.

|  |
| --- |
| OLT(config)#spanning-tree port ge 0/0/1 mcheck  OLT(config)# |

## Config OLT STP Point-to-Poing Function

|  |  |
| --- | --- |
| Command | OLT(config)#spanning-tree <link-aggregation group group-id |port port-ID> point-to-point {auto/true/false} |
| **View** | Config view |
| **Description** | This command is used for set P2P function of GE port spanning tree.if the bridge is working in RSTP mode,a couple of port connected by P2P link can migrate to forwarding status by transferring synchronize message which decreases unnecessary transmission delay time.If set it as auto mode,RSTP protocol can detect automatically whether the current ethernet port has connection with P2P link.it can set as manual mode also,but what we suggestion is setting it as auto mode. |
| <port-id> | Port id to be set,range for 1-8 |
| {auto/true/false} | auto:Auto connect to P2P link  true:Connect the GE port with P2P link  false:Disconnect the GE port with P2P link |

【Example】

Example 1：Set the running mode of GE1 P2P link as true.

|  |
| --- |
| OLT(config)#spanning-tree port ge 0/0/1 point-to-point true  OLT(config)# |

## Config OLT STP Priority

|  |  |
| --- | --- |
| Command | OLT(config)#spanning-tree <link-aggregation group group-id |port port-ID> priority <port-priority> |
| **View** | Config view |
| **Description** | This command is used for set the priority of GE port.It can include specified ethernet port into spanning tree by setting ethernet port priority,generally,the smaller the value is,the higher the port priority is,and this port is more likely to include into spanning tree.If all the ethernet port of network bridge adopts to the same priority value,the priority of ethernet port is depended on port index number. |
| <port-id> | Port id to be set,range for 1-8 |
| <port-priority> | Port priority,range for 0-240,step size for 16.The default value is 128. |

【Example】

Example 1：Set the priority as 160 for GE1 spanning tree.

|  |
| --- |
| OLT(config)#spanning-tree port ge 0/0/1 priority 160  OLT(config)# |

## Show OLT Port STP Configuration

|  |  |
| --- | --- |
| Command | OLT(config)#show spanning-tree port {ge|xge} <port-id> |
| **view** | Config view |
| **Description** | This command is used for show spanning tree configuration info of GE port |
| <port-id> | Port id to be set. |

【Example】

Example 1：Show spanning tree configuration info of GE1.

|  |
| --- |
| OLT(config)#show spanning-tree port ge 0/0/1  -----------------------ge0/0/1 RSTP STATUS:--------------------------------  Port STP Mode:RSTP  Port Priority:160  Port Path Cost:2000  Port Edge Admin:Edge  Port Edge Status:Edge  Port Link Type Admin:P2P  Port Link Type Status:P2P  Port Role:Unknown  Port State:Down  -----------------------------------------------------------------------------  OLT(config)# |

## Show OLT Link-aggregation Group STP Configuration

|  |  |
| --- | --- |
| Command | OLT(config)#show spanning-tree link-aggregation group <group-id> |
| **View** | Config view |
| **Description** | This command is used for show configuration info of spanning tree link-aggregation group. |
| <group-id> | Group id to be set. |

【Example】

Example 1：show configuration info of spanning tree link-aggregation group1

|  |
| --- |
| OLT(config)#show spanning-tree link-aggregation group 1  -----------------------lag1 RSTP STATUS:--------------------------------  Port STP Mode:RSTP  Port Priority:128  Port Path Cost:20000  Port Edge Admin:NON-Edge  Port Edge Status:NEdge  Port Link Type Admin:Auto  Port Link Type Status:P2P  Port Role:Unknown  Port State:Down  -----------------------------------------------------------------------------  OLT(config)# |

# 

# ACL Configuration Manage

## ACL Basic Configuration

### Creat ACL

|  |  |
| --- | --- |
| Command | OLT(config)# acl acl-id |
| **View** | Config view |
| **Description** | This command is used for create a acl. |
| acl-id | <2000-2999> basic acl  <3000-4999> advanced acl  <5000-5999> link acl  <8000-8199> PON side acl  <9000-9499> ONT side acl |

【Example】

Example 1：Creat basic acl 2000：

|  |
| --- |
| OLT(config)# acl 2000  ACL ID Create OK!  OLT(acl-basic-2000)# |

Example 2：Creat advanced acl 3000：

|  |
| --- |
| OLT(config)# acl 3000  ACL ID Create OK!  OLT(acl-adv-3000)# |

Example 3：Creat link acl 5000：

|  |
| --- |
| OLT(config)# acl 5000  ACL ID Create OK!  OLT(acl-link-5000)# |

Example 4：Creat PON side acl 8000：

|  |
| --- |
| OLT(config)# acl 8000  OLT(acl-pon-8000)# |

Example 5：Creat ONT side acl 9000：

|  |
| --- |
| OLT(config)# acl 9000  ACL ID Create OK!  OLT(acl-onu-9000)# |

### Delete ACL

|  |  |
| --- | --- |
| Command | OLT(config)#no acl (acl-id | all ) |
| **View** | Config view |
| **Description** | This command is used for delete acl or all acl |
| (acl-id | all ) | ACL id to be delete,range for 2000-5999,8000-8199,9000-9499 |

【Example】

Example 1：Delete acl 3000.

|  |
| --- |
| OLT(config)# no acl 3000  Number of acl: 1, success: 1  OLT(config)# |

Example 2:Delete all acl.

|  |
| --- |
| OLT(config)# no acl all  Number of PON ACLs that can be delete: 200, success: 0  Number of ONT ACLs that can be delete: 500, success: 1  Number of acl: 2, success: 2  OLT(config)# |

### Config ACL Name

|  |  |
| --- | --- |
| Command | OLT(acl-adv-3000)# acl name ACL-name |
| **View** | basic acl view，advanced acl view，link acl view，PON side acl view,  ONT side acl view |
| **Description** | This command is used for set the acl name. |
| ACL-name | ACL name,length for 1-10 letters |

【Example】

Example 1：Set the name of ACL 3000 as test.

|  |
| --- |
| OLT(acl-adv-3000)# acl name test  OLT(acl-adv-3000)# |

### Show ACL Configuration

|  |  |
| --- | --- |
| Coammand | OLT(acl-adv-3000)# show current |
| **View** | basic acl view，advanced acl view，link acl view，PON side acl vie,  ONT side acl view |
| **Description** | This command is used for show ACL info. |

【Example】

Example 1：Show the info of acl 3000.

|  |
| --- |
| OLT(acl-adv-3000)# show current  Advanced ACL 3000, 1 rules hold  rule 1 permit icmp  OLT(acl-adv-3000)# |

## ACL Apply Time-range Cofiguration

ACL time range is distributed into **relative time** and **absolute time**:

**Relative time**:Periodicity time,for example,from 8:30 to 18:30 every Monday.

**Absolute time**:From a specific time to another specific time,for example,from 06/08/2006 12:00am to 08/08/2006 18:00.

### Config ACL Apply Relative Time-range

|  |  |
| --- | --- |
| Command | OLT(config)#time-range <time-name> <start-time> to <end-time> <days> |
| **View** | Config view |
| **Description** | This command is used for set the time range of relative time |
| <time-name> | Time range name,it is quoted when setting ACL rules. |
| <start-time> | The start time of relative time,format for HH:MM.It determines a time range with the end time,days define the date when the time range take effect,triple parameters determine a time range. |
| <end-time> | The end time of relative time,format for HH:MM.It determines a time range with the start time,days define the date when the time range take effect,triple parameters determine a time range. |

【Example】

**Example 1：**Set a relative time,names it as worktime,the effective time is from 8:00 to 18:30 every Monday.

|  |
| --- |
| OLT(config)#time-range worktime 08:00 to 18:30 mon  OLT(config)# |

### Config ACL Apply Absolute Time-range

|  |  |
| --- | --- |
| Command | OLT(config)#time-range <time-name> from <start-time> to <end-time> |
| **View** | Config view |
| **Description** | This command is used for set the time range of absolute time. |
| <time-name> | Name of time range,it is quoted when setting ACL rules. |
| <start-time> | The start time of absolute time,format for HH:MM YYYY/MM/DD |
| <end-time> | The end time of absolute time,format for HH:MM YYYY/MM/DD |

【Example】

Example 1：Set an absolute time,names it as test,the effective is from 5/1/2017 8:40 to 12/7/2017 18:00.

|  |
| --- |
| OLT(config)#time-range test from 8:40 2017/5/1 to 18:00 2017/12/7  OLT(config)# |

### Delete ACL Apply Time-range

|  |  |
| --- | --- |
| Command | OLT(config)##no time-range {time-name/all} |
| **View** | Config view |
| **Description** | This command is used for delete the time range that had been set |
| {time-name} | Name of time range,input the name of time range to be deleted,“all”means all the time range that had set. |

【Example】

Example 1：Delete the time range named test

|  |
| --- |
| OLT(config)#no time-range test  OLT(config)# |

### Show ACL Apply Time-range Configuration

|  |  |
| --- | --- |
| Command | OLT(config)##show time-range {time-name/all} |
| **View** | Config view |
| **Description** | This command is used for show the configured time range |
| {time-name} | Name of time range,input the name of time range to be deleted,“all”means all the time range that had set. |

【Example】

Example 1：Show the time range named test.

|  |
| --- |
| OLT(config)#show time-range test  Current time is 2017-12-07 11:40 Thurday  Time-range:test(Active)  From 2017-05-01 08:40 to 2017-12-07 18:00  OLT(config)# |

## Config OLT Basic ACL Function

|  |  |
| --- | --- |
| Command | OLT(acl-basic-2000)#rule <rule-id> {permit|deny} source {ip-address|any} <sour-wildcard> time-range <name> |
| **View** | basic acl view |
| **Description** | This command is used for create ACL rule in Acl-basic mode or Acl6-basic mode.when it needs to set rule according to source ip address of message,using this command.We can use packet filter command to filter the message by quoting the ACL rule after setting the acl rule,or uses cooperatively with qos strategy to provide QoS.  “no rule”is used for delete acl rule. |
| <rule-id> | Rule id of ACL,the bigger the id is,the higher the priority. |
| {permit|deny} | Deny:Deny the matched message flow passing  Permit:Permit the matched message flow passing |
| {ip-address|any} | ip-address:The source ip segment in ACL rule.  any:Match to all source ip address |
| <sour-wildcard> | wildcard mask:ip address and wildcard mask are used to match the host id,it tells to the device should be match to which bit of an ip address by labeling“0”and“1”.“1”means overlook this bit,“0”means this bit needing to be check. |
| <name> | Set the effective time range of ACL rule |

【Example】

Example 1：In worktime range,specify the GE1 receive the message of 10.10.10.2 only.

|  |
| --- |
| OLT(config)#time-range worktime 8:00 to 18:00 working-day  OLT(config)#acl 2000  OLT(acl-basic-2000)#rule 2 permit source 10.10.10.2 0.0.0.0 time-range working-day  OLT(acl-basic-2000)#rule 1 deny source any time-range working-day  OLT(acl-basic-2000)#exit  OLT(config)#packet-filter inbound 2000 port ge 0/0 1  OLT(config)# |

## Config OLT Advanced ACL Function

|  |  |
| --- | --- |
| Command | OLT(acl-adv-3000)#  When the protocol is TCP,the command based ipv4 for:  rule <rule-id> {permit| deny} tcp {[soure <ip-address> <sour-wildcard>] | any] | [destination <ip-address> <sour-wildcard> | any] | [src-port <port-list>] | [dest-port <port-list>] | [precedence <procedence-value> ] | [dscp <dscp-value>] |[time-range <time-range-name>]}  When the protocol is UDP,the command based ipv4 for:  rule <rule-id> {permit|deny} udp {[soure <ip-address> <sour-wildcard>] | any] | [destination <ip-address> <sour-wildcard> | any] | [src-port <port-list>] | [dest-port <port-list>] | [precedence <procedence-value> ] | [dscp <dscp-value>] |[time-range <time-range-name>]}  When the protocol is IP,the command based ipv4 for:  rule <rule-id> {permit|deny} ip {[soure <ip-address> <sour-wildcard>] | any] | [destination <ip-address> <sour-wildcard> | any] | [precedence <procedence-value> ] | [dscp <dscp-value>] |[time-range <time-range-name>]}  When the protocol is ipinip,the command based ipv4 for:  rule <rule-id> {permit|deny}) ipinip {[soure <ip-address> <sour-wildcard>] | any] | [destination <ip-address> <sour-wildcard> | any] | [precedence <procedence-value> ] | [dscp <dscp-value>] |[time-range <time-range-name>]}  When the protocol is icmp,the command based ipv4 for:  rule <rule-id> id {permit|deny} icmp {[soure <ip-address> <sour-wildcard>] | any] | [destination <ip-address> <sour-wildcard> | any] | [precedence <procedence-value> ] | [dscp <dscp-value>] |[time-range <time-range-name>]}  When the protocol is other protocol,the command based ipv4 for:  rule <rule-id> {permit|deny} <protocol-id> {[soure <ip-address> <sour-wildcard>] | any] | [destination <ip-address> <sour-wildcard> | any] | [precedence <procedence-value> ] | [dscp <dscp-value>] |[time-range <time-range-name>]}  Adjust the rule command format as:  rule <rule-id> {down/move/up}  Delete or modify the format of command based ipv4 for:  no rule <rule-id> {source|destination|precedence|dscp|src-port|dest-port|time-range|precedence|all} |
| **View** | adv acl view |
| **Description** | This command is used for create ACL rule in Acl-adv mode or Acl6-adv mode.when it needs to set rule according to source address/destination address/ip protocol type/of message or aiming at the protocol characteristic,using this command.We can use packet filter command to filter the message by quoting the ACL rule after setting the acl rule,or uses cooperatively with qos strategy to provide QoS.  “no rule”is used for delete acl rule. |
| <rule-id> | Rule id of ACL,the bigger the id is,the higher the priority. |
| {permit|deny} | Deny:Deny the matched message flow passing  Permit:Permit the matched message flow passing |
| {ip-address|any} | ip-address:The source ip segment in ACL rule.  any:Match to all source ip address |
| {sour-wildcard} | wildcard mask:ip address and wildcard mask are used to match the host id,it tells to the device should be match to which bit of an ip address by labeling“0”and“1”.“1”means overlook this bit,“0”means this bit needing to be check. |
| <time-range-name> | The effective time range of acl |
| <soure> | Source ip address of acl matched message |
| <destination> | Destination ip address of acl matched message |
| <precedence> | The priority of ip layer matched by acl |
| <dscp> | Differentiated services code point |
| <dest-port> | The destination port of TCP or UDP matched by ACL |
| <src-port> | The source port of TCP or UDP matched by ACL |
| <Ipinip> | ACL matches to ipinip(double ip layer)message.That is to say ip data encapsulation and tunnel,which encapsulates ip within ip,protocol number is 4,it is the same as its definition in RFC 2003.It describes how to obtain the ip datagram and load to another ip datagram.In mobile IP,the new header specifies how the encapsulated datagram is sent to the forwarding address of the mobile node. |

【Example】

**Example 1：**Create an advanced ACL and matches it to all icmp message.

|  |
| --- |
| OLT(acl-adv-3000)#rule 1 permit icmp  OLT(acl-adv-3000)# |

Example 2:Delete ACL rule 1.

|  |
| --- |
| OLT(acl-adv-3000)#no rule 1 all  OLT(acl-adv-3000)# |

## Config OLT Link ACL Function

| Command | OLT(acl-link-5000)#rule <rule-id> {permit|deny} {[cos <cos-value> ] | [destination <des-mac-address> <mac-addrmac-wildcard>] | [ source <src-mac-address> <mac-addrmac-wildcard>] | [ inner-cos <inner-cos-value>] | [ vlan <vlan-id>] | [inner-vlan <inner-vlan-id>] | [ type <Ethernet-type>] |[time-range <time-range-name>]} |
| --- | --- |
| **View** | Link acl view |
| **Description** | This command is used for create ACL rule in Acl-link mode.when it needs to set rule according to link layer info such as source mac address/source VLAN ID/second layer protocol type/destination mac address of message and etc,using this command.We can use packet filter command to filter the message by quoting the ACL rule after setting the acl rule,or uses cooperatively with qos strategy to provide QoS.  “no rule”is used for delete acl rule. |
| <rule-id> | Rule id of ACL,the bigger the id is,the higher the priority. |
| {permit|deny} | Deny:Deny the matched message flow passing  Permit:Permit the matched message flow passing |
| <destination> | The destination mac address of message matched by acl |
| <source> | The source mac address of message matched by acl |
| <mac-addr> | Mac address |
| <mac-wildcard> | wildcard mask of mac address:mac address and wildcard mask are used to match the host mac address,it tells to the device should be match to which bit of a mac address by labeling“0”and“1”.“1”means overlook this bit,“0”means this bit needing to be check. |
| <time-range-name> | The effective time range of acl |
| <inner-cos-value> | Match the inner vlan cos value of second layer message |
| <cos-value> | Match the outer vlan cos value of second layer message |
| <vlan-id> | Match the outer vlan id |
| <inner-vlan-id> | Match the inner vlan id |
| <Ethernet-type> | Match ethernet type field |

【Example】

Example 1：In work time range,specifying the GE1 receives the message from destination mac address 22-22-22-22-22 only.

|  |
| --- |
| OLT(config)#time-range worktime 8:00 to 18:00 working-day  OLT(config)#acl 5000  OLT(acl-link-5000)#rule 2 permit destination 22:22:22:22:22:22 0000-0000-0000  OLT(acl-link-5000)#rule 1deny destination 22:22:22:22:22:22 FFFF-FFFF-FFFF  OLT(acl-link-5000)#exit  OLT(config)#packet-filter inbound 5000 port ge 0/0 1  OLT(config)# |

## Config OLT PON ACL Function

|  |  |
| --- | --- |
| Command | OLT(acl-pon-8000)#{[8021p]|[dscp]|[end]|[eth-type]|[exit]|[ip]|[mac]|[no]|[port]|[protocol]|[show]|[tag-num]|[vlan-id]} |
| **View** | Pon acl view |
| **Description** | This command is used for create ACL rule in pon-acl mode.when it needs to set rule according to link layer info such as source mac address/source VLAN ID/second layer protocol type/destination mac address of message and etc,using this command.We can use packet filter command to filter the message by quoting the ACL rule after setting the acl rule,or uses cooperatively with qos strategy to provide QoS.  “no rule”is used for delete acl rule. |
| [8021p] | IEEE 8021p matching |
| [dscp] | DSCP matching |
| [end] | End current mode and change to view mode |
| [eth-type] | Ethernet type matching |
| [exit] | Exit current mode and down to previous mode |
| [ip] | IP address matching |
| [mac] | MAC address matching |
| [no] | Negate a command or set its defaults |
| [port] | IP protocol port matching |
| [protocol] | IP protocol matching |
| [show] | Show information |
| [tag-num] | VLAN tag number matching |
| [vlan-id] | VLAN ID matching |

【Example】

**Example 1：**Apply acl 8001 to pon 1 downstream data flow.its function is adding inner vlan 121 for downstream data flow in pon 1 which carries with dst-ip 192.168.1.1 and src-ip 192.168.2.2

|  |
| --- |
| OLT(config)#acl 8001  OLT(acl-pon-8001)#ip dst-ip 192.168.1.1 src-ip 192.168.2.2  Exit!  OLT(config)#Traffic-modify pon-port 0/0 1 downstream precedence 4 acl 8001 add-inner-vlan 121 |

## Config ONU ACL Function

|  |  |
| --- | --- |
| Command | OLT(acl-onu-9000)#rule {rule-id} match {[cos]|[dscp-v4]|[dscp-v6]|[dst-ip]|[dst-mac]|[dst-port]|[eth-type]|[ip-version]|[protocol]|[src-ip]|[src-mac]|[src-port]|[vlan-id]} |
| **View** | Onu acl |
| **Description** | This command is used for create ACL rule in pon-acl mode.when it needs to set rule according to link layer info such as source mac address/source VLAN ID/second layer protocol type/destination mac address of message and etc,using this command.We can use packet filter command to filter the message by quoting the ACL rule after setting the acl rule,or uses cooperatively with qos strategy to provide QoS.  “no rule”is used for delete acl rule. |
| <rule-id> | Rule id of ACL,the bigger the id is,the higher the priority. |
| cos | 802.1p priority |
| dscp-v4 | DSCPv4 |
| dscp-v6 | DSCPv6 |
| dst-ip | Destination IP address |
| dst-mac | Destination MAC address |
| dst-port | Destination IP protocol port |
| eth-type | Ethernet type |
| ip-version | IP version |
| protocol | IP protocol |
| src-ip | Source IP address |
| src-mac | Source MAC address |
| src-port | Source IP protocol port |
| vlan-id | VLAN ID |

【Example】

Example 1：Create acl 9000 and set rule 1,apply it to ont 1’s eth 1 in pon 1,its function is mapping the flow which carries with dst-ip 192.168.1.3 to queue 0 and marks its priority as 0.

|  |
| --- |
| OLT(config)#acl 9000  ACL ID Create OK!  OLT(acl-onu-9000)#rule 1 match dst-ip always-match 192.168.1.3  OLT(acl-onu-9000)#exit  OLT(config)#interface epon 0/0  OLT(config-interface-epon-0/0)#ont port classification 1 1 eth 1 acl 9000 rule 1 precedence 4 queue-mapped 0 priority-mark 0  OLT(config)# |

## Show OLT ACL Configuration

|  |  |
| --- | --- |
| Command | OLT(config)#show acl {acl-id|all/detail} |
| **View** | Config view |
| **Description** | This command is used for show the configuration of acl. |
| <acl-id> | ACL id to be show |
| **<all>** | Show all the acl |
| <detail> | Detail info |

【Example】

Example 1：Show the configuration fo all acl

|  |
| --- |
| OLT(config)#show acl all  Basic ACL 2000,0 rules hold  Advanced ACL 3000,0 rules hold  Link ACL 5000,0 rules hold  OLT(config)# |

## Modify OLT ACL Rule ID

|  |  |
| --- | --- |
| Command | OLT(configacl-basic-2000)#rule <ruld id> {up/down/move to} |
| **View** | basic acl view,adv acl view,Link acl view |
| **Description** | acl acl-id down:The rule id is reduced by one without changing the rule content  acl acl-id up:Add one for rule id without changing the rule content  acl acl-id move to:Modify the value of rule-id to a specify rule id without change the rule content.  (the rule which had been bound to the port can not adjust the value of rule id) |
| <ruld id> | Rule id |
| {up/down/move to} | down:The rule id is reduced by one without changing the rule content  up:Add one for rule id without changing the rule content  move to:Modify the value of rule-id to a specified rule id without change the rule content. |

【Example】

Example 1：Modify rule 1 as rule 3.

|  |
| --- |
| OLT(acl-basic-2000)#rule 1 move to 3  OLT(acl-basic-2000)# |

# ARP Configuration

## Config ARP age time

|  |  |
| --- | --- |
| Command | OLT(config)# arp age time set time-value |
| **View** | Config view |
| **Description** | This command is used for set arp dynamic age time. Once this command set successfully, for these arp which have been existed will restart the clock. Aging at new set time. |
| time-value | Aging time for dynamic arp table,range for 60-300,usit is s. |

【Example】

Example1：Config aging time for dynamic arp is 100.

|  |
| --- |
| OLT(config)# arp age time set 100  OLT(config)# |

## Config Learned Gratuitous ARP.

|  |  |
| --- | --- |
| Command | OLT(config)# arp gratuitous arp learning (enable|disable) |
| **View** | Config view |
| **Description** | This command is used for enable or disable learn gratuitous arp function. Gratuitous arp message is the device send destination ip is the same as source ip address. It’s mainly used for equipment report their own mac address actively, in order to other devices learn arp table. |
| (enable|disable) | enable:enable learn gratuitous arp  disable:disable learn gratuitous arp |

【Example】

Example1：enable learn gratuitous arp

|  |
| --- |
| OLT(config)# arp gratuitous arp learning enable  OLT(config)# |

## Config Send Gratuitous ARP Messages

|  |  |
| --- | --- |
| Command | OLT(config)# arp gratuitous arp send (enable|disable|time (time-value|default)) |
| **View** | Config view |
| **Description** | This command is used for enable or disable gratuitous arp messages to be sent within the vlanif interface periodically. When enable it, the system will send a gratuitous arp to the network side port every 5 minutes.When disable it,the system will not send arp gratuitous periodically. During exist a number of arp gratuitous messages in the network reasulted high cpu utilization rate of the device, there is a way to enable send arp gratuitous periodically to reduce cpu utilization rate. |
| (enable|disabletime (time-value|default)) | enable:enable gratuitous arp messages to be sent within the vlanif interface periodically  disable:disable gratuitous arp messages to be sent within the vlanif interface periodically  time:set the time of sending gratuitous arp messages, range for 1-60,unit is s |

【Example】

Example1：enable gratuitous arp messages to be sent within the vlanif interface periodically

|  |
| --- |
| OLT(config)# arp gratuitous arp send enable  OLT(config)# |

## Config ARP Proxy within the VLAN

|  |  |
| --- | --- |
| Command | OLT(config)# arp inner-sub-vlan-proxy (enable|disable) vlanif (vlan-id | all ) |
| **View** | Config view |
| **Description** | This command is used for enable or disable arp proxy within vlan. Arp proxy is device recieve arp request message, destination ip address and ip address inner port are in the same segment network, arp proxy within the vlan will take effect at the moment. |
| (enable|disable) | enable:enable arp proxy within vlan  disable:disable arp proxy within vlan |
| (vlan-id | all ) | vlan-id: vlan-if interface ,range for 1-4094  all：all layer3 virtual interface |

【Example】

Example1：enable arp proxy within vlan to all layer3 virtual interface

|  |
| --- |
| OLT(config)# arp inner-sub-vlan-proxy enable vlanif all  OLT(config)# |

## Config ARP Mac Address Change Check

|  |  |
| --- | --- |
| Command | OLT(config)# arp mac address change check (enable |disable) |
| **View** | Config view |
| **Description** | This command is used for enable or disable arp mac address change check. After MAC and ip address bind statically, will check mac address used ip address change or not. |
| (enable|disable) | enable:enable arp mac address change check  disable:disable arp mac address change check |

【Example】

Example1：enable arp mac address change check

|  |
| --- |
| OLT(config)# arp mac address change check enable  OLT(config)# |

## Config ARP Proxy Inner the VLAN

|  |  |
| --- | --- |
| Command | OLT(config)# arp proxy (enable |disable) vlanif (vlan-id | all ) |
| **View** | Config view |
| **Description** | This command is used for enable or disable arp procy inner the vlan. |
| (enable|disable) | enable:enable arp procy inner the vlan  disable:disable arp procy inner the vlan |
| (vlan-id | all ) | vlan-id: vlan-if interface ,range for 1-4094  all：all layer3 virtual interface |

【Example】

Example1：enable arp proxy with vlanif 1217

|  |
| --- |
| OLT(config)# arp proxy enable vlanif 1217  OLT(config)# |

## Config ARP quick-update

|  |  |
| --- | --- |
| Command | OLT(config)# arp quick-update (enable|disable) |
| **View** | Config view |
| **Description** | This command is used for enable or disable arp quick-update. The arpquick update is same ip in the same device, if change port or mac address, equipment will update arp corresponding port and mac in native arp without waiting for learning again after arp aging orginally. |
| (enable|disable) | enable:enable arp quick-update  disable:disable arp quick-update |

【Example】

Example1：enable arp quick-update

|  |
| --- |
| OLT(config)# arp quick-update enable  OLT(config)# |

## Config OLT Static ARP

| Command | OLT(config)# arp static IP-address mac-address vid vlan-id port (ge F/S/P |epon F/S/P|xge F/S/P|lag flame-id slot-id) |
| --- | --- |
| **View** | Config view |
| **Description** | This command is used for bind static arp. |
| IP-address | Config ip address.format is X.X.X.X |
| mac-address | Config mac address.format is XX:XX:XX:XX:XX:XX |
| vlan-id | Config VLAN ID ,range for 1-4094 |
| ge F/S/P |  epon F/S/P|  xge F/S/P|  lag flame-id slot-id | ge：GE port，config frame number/slot number/port number，range for <0-0>/<0-0>/<1-8>  epon:EPON port，config frame number/slot number/port number，range for<0-0>/<0-0>/<1-16>  xge：XGE port，config frame number/slot number/port number，range for <0-0>/<0-0>/<1-2>  lag：link aggregation group，config frame number range for<1-8>or slot number range for<9-16> |

【Example】

Example1：bind static arp

|  |
| --- |
| OLT(config)# arp static 192.168.5.188 00:00:00:11:22:33 vid 100 port epon 0/0/1  OLT(config)# |

## Unbind OLT static arp

|  |  |
| --- | --- |
| Command | OLT(config)# no arp static (ip-address | all) |
| **View** | Config view |
| **Description** | This command is used for unbind static arp |
| (ip-address | all) | ip-address: unbind ip address with static arp  all:unbind all ip addresses with static arp |

【Example】

Example1：Unbind static ip with ip address 192.168.5.188

|  |
| --- |
| OLT(config)# no arp static 192.168.5.188  OLT(config)# |

## Delete ARP Link Statistics

|  |  |
| --- | --- |
| Command | OLT(config)# reset arp connected route-statistics |
| **View** | config view |
| **Description** | This command is used to delete ARP link statistics. |

【Example】

Example 1：Delete ARP link statistics.

|  |
| --- |
| OLT(config)# reset arp connected route-statistics  OLT(config)# |

## Delete Dynamic ARP Configuration

### Delete dynamic ARP on a VLANIF interface.

|  |  |
| --- | --- |
| Command | OLT(config)# reset arp dynamic interface vlanif vlan-id |
| **View** | config view |
| **Description** | This command is used to delete dynamic ARP on a VLANIF interface. |

【Example】

Example 1：Delete dynamic ARP on a VLANIF interface 20.

|  |
| --- |
| OLT(config)# reset arp dynamic interface vlanif 20  OLT(config)# |

### Delete Dynamic ARP for Different IPs

|  |  |
| --- | --- |
| Command | OLT(config)# reset arp dynamic ip ip-address |
| **View** | config view |
| **Description** | This command is used to delete dynamic ARP for different IPs. |

【Example】

Example 1：Delete dynamic ARP with IP address 192.168.10.2

|  |
| --- |
| OLT(config)# reset arp dynamic ip 192.168.10.2  OLT(config)# |

### Delete Dynamic ARP for Port

|  |  |
| --- | --- |
| Command | OLT(config)# reset arp dynamic port ((lag group-ip)|(ge|epon|xge) F/S/P) |
| **View** | config view |
| **Description** | This command is used to delete the dynamic ARP of a port. |

【Example】

Example 1：Delete the dynamic ARP of the PON1 port.

|  |
| --- |
| OLT(config)# reset arp dynamic port epon 0/0/1  OLT(config)# |

### Delete all Dynamic ARPs

|  |  |
| --- | --- |
| Command | OLT(config)# reset arp dynamic all |
| **View** | config view |
| **Description** | This command is used to delete all dynamic ARPs. |

【Example】

Example 1：Delete all dynamic ARPs.

|  |
| --- |
| OLT(config)# reset arp dynamic all  OLT(config)# |

# OLT QOS Configuraiton

## Config OLT Global QOS mode

|  |  |
| --- | --- |
| Command | OLT(config)#qos global mode {device-based|port-based} |
| **View** | Config view |
| **Description** | This command is used for set global QOS mode |
| {device-based|port-based} | device-based:device-based QOS  port-based:port-based QOS |

【Example】

Example 1：Set device-based QOS.

|  |
| --- |
| OLT(config)#qos global mode device-based  OLT(config)# |

## Config Traffic Control Based On ACL Rule

### Config Packet Filter Based On ACL Rulesss

|  |  |
| --- | --- |
| Command | OLT(config)# packet-filter {inbound|outbound} <acl-id> rule-id <rule-id> port {ge| epon|xge} <port-id> |
| **View** | Config view |
| **Description** | This command is used for match the acl rule for the specified port.When it needs to filter the the flow in port by acl rule,using this command.  “no packet-filter......”is used for delete the acl rule in specified port. |
| {inbound|outbound} | inbound:The ingress flow  Outbound:The egress flow |
| <acl-id> | ACL id |
| <rule-id> | Rule id in acl |
| <port-id> | Port list |

【Example】

Example 1：In the work time range,specify GE1 can only receive the message from mac address 22-22-22-22-22-22.

|  |
| --- |
| OLT(config)#time-range worktime 8:00 to 18:00 working-day  OLT(config)#acl 2000  OLT(acl-basic-2000)#rule 2 permit source 10.10.10.2 0.0.0.0 time-range worktime  OLT(acl-basic-2000)#rule 1 deny source any time-range worktime  OLT(acl-basic-2000)#exit  OLT(config)#packet-filter inbound 2000 port ge 0/0 1  OLT(config)# |

### Changes Traffic DSCP Based On ACL Rule

|  |  |
| --- | --- |
| Command | OLT(config)#traffic-dscp {inbound|outbound} <acl-id> rule-id <rule-id> port {ge|pon|xge} <port-id> remark-dscp <remark-dscp-value> |
| **View** | Config view |
| **Description** | This command is used for match the acl for specified port to re-mark the value of DSCP.  “no traffic-dscp......”is used cancel the acl in specified port. |
| {inbound|outbound} | inbound:The ingress flow  Outbound:The egress flow |
| <acl-id> | ACL id |
| <rule-id> | Rule id in acl |
| <port-id> | Port list |
| <remark-dscp-value> | Remark DSCP value |

【Example】

Example 1：In work timme range,re-mark the DSCP value as 43 for the message from 10.10.10.2.

|  |
| --- |
| OLT(config)#time-range worktime 8:00 to 18:00 working-day  OLT(config)#acl 2000  OLT(acl-basic-2000)#rule 2 permit source 10.10.10.2 0.0.0.0 time-range worktime  OLT(acl-basic-2000)#exit  OLT(config)#traffic-dscp inbound 2000 port ge 0/0 1 remark-dscp 43  OLT(config)# |

### Config Traffic Mirror Based On ACL Rule

|  |  |
| --- | --- |
| Command | OLT(config)#traffic-mirror inbound <acl-id> rule-id <rule-id> port {ge| pon|xge} <port-id> to {ge|xge} <port-id> |
| **View** | Config view |
| **Description** | This command is used for mirror the acl matched flow for specified port.  “no traffic-mirror......”is used for cancel the acl matched flow mirror in specified port. |
| <acl-id> | ACL id |
| <rule-id> | Rule id in acl |
| <port-id> | Port id |

【Example】

Example 1：In work time range,mirror the message from GE1 10.10.10.2 to the port 2.

|  |
| --- |
| OLT(config)#time-range worktime 8:00 to 18:00 working-day  OLT(config)#acl 2000  OLT(acl-basic-2000)#rule 2 permit source 10.10.10.2 0.0.0.0 time-range worktime  OLT(acl-basic-2000)#exit  OLT(config)#traffic-mirror inbound 2000 port ge 0/0 1 to ge 0/0 2  OLT(config)# |

### Config Traffic Limit Based On ACL Rule

|  |  |
| --- | --- |
| Command | OLT(config)##traffic--limit {inbound|outbound} <acl-id> rule-id <rule-id> port {ge|pon|xge} <port-id> cir <rate-value> pir <rate-value> exceed {drop|remark-dscp} |
| **View** | Config view |
| **Description** | This command is used for set traffic-limit for specified port by match the acl.  “no traffic-limit......”is used for delete the acl matched traffic-limit in specified port. |
| {inbound|outbound} | inbound:The ingress flow  Outbound:The egress flow |
| <acl-id> | ACL id |
| <rule-id> | Rule id in acl |
| <port-list> | Port list |
| {drop|remark-dscp} | drop:discard  remark:Re-mark the DSCP value |

【Example】

Example 1：In work time range,set the traffic-limit for the ingress direction message from GE1 10.10.10.2.In which the cir is 1M,pir is 100M,and discard the transfinite flow.

|  |
| --- |
| OLT(config)#time-range worktime 8:00 to 18:00 working-day  OLT(config)#acl 2000  OLT(acl-basic-2000)#rule 2 permit source 10.10.10.2 0.0.0.0 time-range worktime  OLT(acl-basic-2000)#exit  OLT(config)#traffic-limit inbound *2000* port ge 0/0*1* cir 1024 pir 102400 exceed drop  OLT(config)# |

### Add Traffic Outer VLAN Based On ACL Rule

|  |  |
| --- | --- |
| Command | OLT(config)##traffic-outervlan inbound <acl-id> rule-id <rule-id> port {ge|pon|xge} <port-id> vlan <vlan-id> |
| **View** | Config view |
| **Description** | This command is used for add outer vlan for acl matched folw in specified port.  “no traffic-outervlan......”is used for cancel the command mention above. |
| <acl-id> | ACL id |
| <rule-id> | Rule id in acl |
| <port-id> | Port id |
| <vlan-id> | Outer vlan id |

【Example】

Example 1：In work time range,add outer vlan 10 for the message from GE1 10.10.10.2

|  |
| --- |
| OLT(config)#time-range worktime 8:00 to 18:00 working-day  OLT(config)#acl 2000  OLT(acl-basic-2000)#rule 2 permit source 10.10.10.2 0.0.0.0 time-range worktime  OLT(acl-basic-2000)#exit  OLT(config)#traffic-outervlan inbound 2000 port ge 0/0/1 vlan 10  OLT(config)# |

### Translate Traffic VLAN Based On ACL Rule

| Command | OLT(config)##traffic-translate inbound <acl-id> rule-id <rule-id> port {ge|pon|xge} <port-id> vlan <vlan-id> |
| --- | --- |
| **View** | Config view |
| **Description** | This command is used for translate the vlan id of acl matched port’s egress or ingress flow into new vlan id. |
| <acl-id> | ACL id |
| <rule-id> | Rule id in acl |
| <port-id> | Port id |
| <vlan-id> | New vlan id |

【Example】

Example 1：Translate the vlan id of the flow in GE5 which had been bound to acl2000 and rule2 into vlan 19.

|  |
| --- |
| OLT(config)#traffic-translate inbound 2000 rule-id 2 port ge 0/0/5 vlan 19  OLT(config)# |

### Modify Traffic VLAN Priority Based On ACL Rule

|  |  |
| --- | --- |
| Command | OLT(config)#traffic-priority inbound <acl-id> rule-id <rule-id> port{ge| pon|xge} <port-id> remark-priority <pri-value> |
| **View** | Config view |
| **Description** | This command is used for set the acl vlan priority for specified port.  “no traffic-priority......”is used for cancel the vlan priority on specified port. |
| <acl-id> | ACL id |
| <rule-id> | Rule id in acl |
| <port-id> | Port id |
| <pri-value> | Priority value |

【Example】

Example 1：In work time range,set the vlan priority as 2 for the message from GE1 10.10.10.2.

|  |
| --- |
| OLT(config)#time-range worktime 8:00 to 18:00 working-day  OLT(config)#acl 2000  OLT(acl-basic-2000)#rule 2 permit source 10.10.10.2 0.0.0.0 time-range worktime  OLT(acl-basic-2000)#exit  OLT(config)#traffic-priority inbound 2000 port ge 0/0 1 remark-priority 2  OLT(config)# |

### Config Traffic Redirect Based On ACL Rule

|  |  |
| --- | --- |
| Command | OLT(config)##traffic-redirect inbound <acl-id> rule-id <rule-id> port {ge| pon|xge} <port-id> to <ge | xge> <port-list> |
| **View** | Config view |
| **Description** | This command is used for set traffic-redirect for acl matched flow in specified port.  “no traffic-redirect”is used for cancel the traffic-redirect.  (Redirect the acl matched message in specified port or port list to other port and transfer.After setting,the old port will not transfer the redirect message,but it will be transferred by the new port.In addition,a correct vlan setting in the port is needed) |
| <acl-id> | ACL id |
| <rule-id> | Rule id in acl |
| <port-list> | Port list |

【Example】

Example 1：In work time range,redirect the message from GE1 10.10.10.2 to GE2.

|  |
| --- |
| OLT(config)#time-range worktime 8:00 to 18:00 working-day  OLT(config)#acl 2000  OLT(acl-basic-2000)#rule 2 permit source 10.10.10.2 0.0.0.0 time-range worktime  OLT(acl-basic-2000)#exit  OLT(config)#traffic-redirect inbound 2000 port ge 0/0 1 to ge 0/0 2  OLT(config)# |

### Modify Traffic TOS Value Based On ACL Rule

|  |  |
| --- | --- |
| Command | OLT(config)#traffic-tos {inbound|outbound} <acl-id> rule-id <rule-id> port {ge| pon|xge} <port-id> remark-tos <Tos value> |
| **View** | Config view |
| **Description** | This command is used for modify the tos value of the acl matched value. |
| <acl-id> | ACL id |
| <rule-id> | Rule id in acl |
| <port-id> | Port list |
| <Tos value> | Tos vlaue |

【Example】

Example 1：In work time range,modify the tos value of the message from GE1 10.10.10.2 as 3.

|  |
| --- |
| OLT(config)#time-range worktime 8:00 to 18:00 working-day  OLT(config)#acl 2000  OLT(acl-basic-2000)#rule 2 permit source 10.10.10.2 0.0.0.0 time-range worktime  OLT(acl-basic-2000)#exit  OLT(config)#traffic-tos inbound 2000 rule-id 2 port ge 0/0 1 remark-tos 3  OLT(config)# |

### Config ACL Action and Bind ACL to PON Port

|  |  |
| --- | --- |
| Command | OLT(config)#traffic-modify pon-port <port-id> {downstream|upstream} precedence <precedence-id> acl <acl-id> <action> |
| **View** | Config view |
| **Description** | This command is used for set the pon-acl matched flow(it uses with pon acl 8000-8199) |
| <acl-id> | ACL id |
| <rule-id> | Rule id in acl |
| <port-id> | Port id |
| <Precedence-id> | ACL priority,the command with higher priority will execute firstly. |
| <downstream|upstream> | downstream  upstream |
| <action> | 8021p:vlan priority  deny:Deny corresponding flow passing  add-inner-vlan:Add inner vlan for the highest priority acl matched flow in pon port.  add-top-vlan:Add outer vlan for the highest priority acl matched flow in pon port.  strip-inner-vlan:Peel the inner vlan for the highest priority acl matched flow in pon port.  strip-top-vlan:Peel the outer vlan for the highest priority acl matched flow in pon port.  swap-inner-vlan:Replace the inner vlan of the highest priority acl matched flow in pon port.  swap-top-vlan:Replace the outer vlan of the highest priority acl matched flow in pon port. |

【Example】

Example 1：Add outer vlan 1000 for the flow which vlan is 100-200 in pon1 upstream direction.

|  |
| --- |
| OLT(config)#acl 8000  OLT(acl-pon-8000)#vlan-id top-vid 100 to 200  OLT(acl-pon-8000)#exit  OLT(config)#traffic-modify pon-port 0/0 1 upstream precedence 4 acl 8000 add-top-vlan 1000  OLT(config)# |

### Config ACL Action and Bind ACL to ONU

|  |  |
| --- | --- |
| Command | OLT(config)#traffic-modify ont <port-id> <onu-id> <downstream|upstream> precedence <precedence-id> acl <acl-id> <action> |
| **View** | Config view |
| **Description** | The traffic-modify command is used for modify the data of the PON port and the ONU (this command is used together with the pon acl (8000-8199) part) |
| <acl-id> | ACL id |
| <rule-id> | Rule id in acl |
| <port-list> | Port list |
| <onu-id> | ONU id |
| <Precedence-id> | ACL priority,the command with higher priority will execute firstly. |
| <downstream|upstream> | downstream  upstream |
| <action> | 8021p:vlan priority  deny:Deny corresponding flow passing  add-inner-vlan:Add inner vlan for the highest priority acl matched flow in pon port.  add-top-vlan:Add outer vlan for the highest priority acl matched flow in pon port.  strip-inner-vlan:Peel the inner vlan for the highest priority acl matched flow in pon port.  strip-top-vlan:Peel the outer vlan for the highest priority acl matched flow in pon port.  swap-inner-vlan:Replace the inner vlan of the highest priority acl matched flow in pon port.  swap-top-vlan:Replace the outer vlan of the highest priority acl matched flow in pon port. |

【Example】

Example 1： Apply the outer vlan 1000 to the data of the uplink data stream vlan of the ONU1 under the PON from 100 to 200.

|  |
| --- |
| OLT(config)# acl 8000  OLT(acl-pon-8000)# vlan-id top-vid 100 to 200  OLT(acl-pon-8000)# exit  OLT(config)# traffic-modify ont 0/0 1 1 upstream precedence 4 acl 8000 add-top-vlan 1000  OLT(config)# |

### Config statistics on matching ACL Rules

|  |  |
| --- | --- |
| Command | OLT(config)# traffic-statistic <clear-counters> <inbound|outbound> <acl-id> rule-id <rule-id> port <ge | pon | xge> <port-list> |
| **View** | Config view |
| **Description** | This command is used to configure the flow of incoming data from the port matching the acl rule. Clear-counters are used to clear data statistics; |
| <acl-id> | ACL id |
| <rule-id> | ACL rule ID |
| <port-list> | Port list |

【Example】

Example 1：Config statistics on the port data matching the acl2000 rule and view it.

|  |
| --- |
| OLT(config)# traffic-statistic inbound 2000 port epon 0/0 1  OLT(config)#  OLT(config)# show qos info all port epon 0/0/1  traffic-mirror on epon 0/0/1:  Inbound:  Matches: acl 2000 rule 1 running  Packets: 0  Bytes: 0  OLT(config)# |

### Show ACL Bind Configuration

|  |  |
| --- | --- |
| Command | OLT(config)#show traffic-modify {all|pon-port|ont} |
| **View** | Config view |
| **Description** | This command is used for show configuration info of pon-acl traffic-modify |
| {all|ont-pon|ont} | all:show all the configuration info of pon-acl  pon-port:show pon-acl configuration info of pon port  ont:show pon-acl configuration info of onu |

【Example】

Example 1：Show all the configuration info of pon-acl

|  |
| --- |
| OLT(config)#show traffic-modify all  traffic-modify pon-port 0/0 1 upstream precedence 4 acl 8000 add-top-vlan 1000  traffic-modify ont 0/0 1 1 upstream precedence 4 acl 8000 swap-top-vlan 1000  OLT(config)# |

### Show Port Packet-filter Policy Configuration

| Command | OLT(config)#show packet-filter {all|port} |
| --- | --- |
| **View** | Config view |
| **Description** | This command is used for show packet-filter strategy in the port |
| {all|port} | all:Show all the packet filter configuration  port:Show packet filter strategy of specified port |

【Example】

Example 1：Show all the packet filter configuration

|  |
| --- |
| OLT(config)#show packet-filter all  -----------------------------------------------------------------------------  inbound acl 2000 rule 1 port ge 0/0 1 running  inbound acl 2000 rule 2 port ge 0/0 1 not running  inbound acl 2000 rule 3 port ge 0/0 1 not running  -----------------------------------------------------------------------------  OLT(config)# |

### Show Port QOS Configuration Information

|  |  |
| --- | --- |
| Command | OLT(config)#show qos-info {all|traffic-dscp|traffic-tos|traffic-limit|traffic-mirror|traffic-outervlan|traffic-priority|traffic-redirect|traffic-statistic|traffic-translate|} port {ge| pon|xge} <port-id> |
| **View** | Config view |
| **Description** | This command is used for show qos strategy of the port |
| <all> | All of the qos strategy |
| <port-list> | Port list |

【Example】

Example 1：Show all the QOS strategy of GE1.

|  |
| --- |
| OLT(config)#show qos-info all port ge 0/0/1  traffic-tos on ge 0/0/1:  Inbound:  Matches:acl 2000 rule 1 running  Remark-tos:3  OLT(config)# |

## Config OLT QOS Queue

### Config OLT QOS Queue Mapping Mode

|  |  |
| --- | --- |
| Command | OLT(config)#qos cosq-map mode {cos|diffserv|tos} |
| **View** | Config view |
| **Description** | This command is used for set the mapping mode of system queue |
| <cos|diffserv|tos> | Cos:The mapping mode is based on 802.1p  diffserv:The mapping mode is based on diffserv  Tos:The mapping mode is based on tos |

【Example】

Example 1：Set the QOS mapping mode as 802.1p.

|  |
| --- |
| OLT(config)#qos cosq-map mode cos  OLT(config)# |

### Config QOS Queue Mapping Mode Based On 802.1p

|  |  |
| --- | --- |
| Command | OLT(config)#qos cosq-map cos0 <Queue id> cos1 <Queue id> cos2 <Queue id> cos3 <Queue id> cos4 <Queue id> cos5 <Queue id> cos6 <Queue id> cos7 <Queue id> |
| **View** | Config view |
| **Description** | This command is used for set the mapping table of system queue and 802.1p |
| <Queue id> | Queue id,range for 0-7 |

【Example】

Example 1：Set the mapping table of system queue and 802.1p

|  |
| --- |
| OLT(config)#qos cosq-map cos0 1 cos1 2 cos2 3 cos3 4 cos4 5 cos5 6 cos6 7 cos7 0  OLT(config)#  OLT(config)#show qos queue-scheduler  Queue scheduler mode:SP  -----------------------------------------------------------------------------  Queue Scheduler Mode WRR Weight Bandwidth(kbps)  -----------------------------------------------------------------------------  0 SP--  1 SP--  2 SP--  3 SP--  4 SP--  5 SP--  6 SP--  7 SP--  -----------------------------------------------------------------------------  Queue map mode:Cos  -----------------------------------------------------------------------------  Priority Queue  -----------------------------------------------------------------------------  0 1  1 2  2 3  3 4  4 5  5 6  6 7  7 0  ----------------------------------------------------------------------------- |

### Config OLT QOS Queue Scheduled Mode

| Command | OLT(config)# qos queue-scheduler strict-priority  OLT(config)#qos queue-scheduler wrr <queue0-weight queue1-weight queue2-weight queue3-weight queue4-weight queue5-weight queue6-weigh tqueue7-weight>  OLT(config)#qos queue-scheduler bandwidth queue0 <bandwidth> queue1 <bandwidth> queue2 <bandwidth> cos3 <bandwidth> queue4 <bandwidth> queue5 <bandwidth> queue6<bandwidth> queue7 <bandwidth> |
| --- | --- |
| **View** | Config view |
| **Description** | This command is used for set system queue scheduled mode.The message which is sending from the same port is divided into several queue by Queue scheduling,and schedules them between queue and queue,it decides the sending sequence of queue.when the user needs to select different queue scheduling mode according to the importance of service,and ensure that the QoS guarantees are still available for important business when the network is blocked,using this command.After setting,the system will send the queue message according to new dispatching mode.  System support PQ,WRR,WRR+PQ dispatching mode.when a queue is null,it can switch to next queue immediately and dispatch,which can make full use of bandwidth source. |
| strict-priority | Strict-priority scheduling,When this mode is applied,the system schedules strictly according to the priority of the queue.Only high priority queue is null,the low priority queue can be scheduled.The disadvantage of the PQ scheduling mode shows as follows:  When the blocking is happening,if the high priority queue has some groups existing for a long time,corresponding apply will time out for the reason that the message with low priority can not be scheduled in time. |
| wrr | Weighted Round Robin.When this mode is applied,it needs to match a weight for each queue(weight means the obtained resource proportion),it takes turns to scheduling according to the weight in queue and assure each queue can obtain definite service.Each queue has the same priority but different weights,the bigger weight it is,the longer scheduling time obtained by this queue.In this way it can assure the lowest priority queue which can obtain definite service at least.avoiding that the message in low priority queue can not obtain service for a long time when adopting the PQ scheduling mode.  queue0-weight/queue1-weight/queue2-weight/queue3-weight/queue4-weight/queue5-weight/queue6-weight/queue7-weight:the weight of each queue.system supports 8 queues,the weight’s sum of 8 queues is 100. |
| WRR+PQ | WRR+PQ scheduling mode is a mixture of WRR and PQ scheduling modes.When the scheduling mode is WRR,and the weight value of queue has 0,the queue scheduling mode is PQ+WRR.In this mode,system will schedule the queue with 0 weight first according to PQ mode,and then schedules the queue with non-zero weight according to WRR mode,the priority of PQ queue is higher than WRR queue in the meantime.  System default scheduling mode is PQ mode. |

【Example】

Example 1：Set the scheduling mode of pon1 as WRR mode,let the messages with various kinds of priority can be scheduled.The weight of queue 0-7 is 15 15 20 10 10 10 10 10.

|  |
| --- |
| OLT(config)#qos queue-scheduler port-based epon 0/0 1 wrr 15 15 20 10 10 10 10 10  OLT(config)# |

### Show OLT QOS Queue Schedule Mode

|  |  |
| --- | --- |
| Command | OLT(config)#show qos queue-schedule |
| **View** | Config view |
| **Description** | This command is used for show system queue-schedule mode. |

【Example】

Example 1：Show system queue-schedule mode.

|  |
| --- |
| OLT(config)#show qos queue-scheduler  Queue scheduler mode:SP  -----------------------------------------------------------------------------  Queue Scheduler Mode WRR Weight Bandwidth(kbps)  -----------------------------------------------------------------------------  0 SP--  1 SP--  2 SP--  3 SP--  4 SP--  5 SP--  6 SP--  7 SP--  -----------------------------------------------------------------------------  Queue map mode:Cos  -----------------------------------------------------------------------------  Priority Queue  -----------------------------------------------------------------------------  0 1  1 2  2 3  3 4  4 5  5 6  6 7  7 0  OLT(config)# |

## OLT Port QOS Queue Configuration

### Config OLT Port QOS Queue Mapping Mode

|  |  |
| --- | --- |
| Command | OLT(config)# qos cosq-map port-based <epon|ge|xge> <port-id> mode <cos|diffserv|tos> |
| **View** | Config view |
| **Description** | This command is used for set mapping mode of port-based queue |
| {cos|diffserv|tos} | Cos:The mapping mode is based on 802.1p  diffserv:The mapping mode is based on diffserv  Tos:The mapping mode is based on tos |

【Example】

Example 1：Set the mapping mode of pon1 queue as 802.1q.

|  |
| --- |
| OLT(config)#qos global mode port-based  OLT(config)#qos cosq-map port-based cos epon 0/0 1  OLT(config)# |

### Config OLT Port QOS Queue Mapping Mode Based On 802.1p

| Command | OLT(config)# qos cosq-map port-based <epon|ge|xge> <port-id> to-pbits cos cos0 <Queue id> cos1 <Queue id> cos2 <Queue id> cos3 < Queue id> cos4 <Queue id> cos5 <Queue id> cos6 <Queue id> cos7 <Queue id>  OLT(config)# qos cosq-map port-based <epon|ge|xge> <port-id> to-pbits diffserv <dscp-list> <priority>  OLT(config)# qos cosq-map port-based <epon|ge|xge> <port-id> to-pbits tos <tos-list> <priority> |
| --- | --- |
| **View** | Config view |
| **Description** | This command is used for set the mapping table between port-based queue and 802.1p |
| <Queue id> | Queue id,range for 0-7 |
| <dscp-list> | Dscp id,range for 0-63，format as 1,3-5,8 |
| <tos-list> | tos id,range for 0-7，format as 1,3-5,7 |
| <priority> | Priority, range for 0-7 |

【Example】

Example 1：Set the mapping table between queue and 802.1q

|  |
| --- |
| OLT(config)# qos cosq-map port-based epon 0/0 1 to-pbits cos cos0 1 cos1 3  OLT(config)# qos cosq-map port-based epon 0/0 1 to-pbits diffserv 1 2  OLT(config)# qos cosq-map port-based epon 0/0 2 to-pbits tos 2 3  OLT(config)# |

### Config OLT Port QOS Queue Schedule Mode

|  |  |
| --- | --- |
| Command | OLT(config)#qos queue-scheduler port-based {epon|ge|xge} <port-id> strict-priority  OLT(config)#qos queue-scheduler port-based {epon|ge|xge} <port-id> wrr <queue0-weight queue1-weight queue2-weight queue3-weight queue4-weight queue5-weight queue6-weigh tqueue7-weight>  OLT(config)#qos queue-scheduler bandwidth queue0 <bandwidth> queue1 <bandwidth> queue2 <bandwidth> cos3 <bandwidth> queue4 <bandwidth> queue5 <bandwidth> queue6<bandwidth> queue7 <bandwidth> |
| **View** | Config view |
| **Description** | This command is used for set system queue scheduled mode.The message which is sending from the same port is divided into several queue by Queue scheduling,and schedules them between queue and queue,it decides the sending sequence of queue.when the user needs to select different queue scheduling mode according to the importance of service,and ensure that the QoS guarantees are still available for important business when the network is blocked,using this command.After setting,the system will send the queue message according to new dispatching mode.  System support PQ,WRR,WRR+PQ dispatching mode.when a queue is null,it can switch to next queue immediately and dispatch,which can make full use of bandwidth source. |
| strict-priority | Strict-priority scheduling,When this mode is applied,the system schedules strictly according to the priority of the queue.Only high priority queue is null,the low priority queue can be scheduled.The disadvantage of the PQ scheduling mode shows as follows:  When the blocking is happening,if the high priority queue has some groups existing for a long time,corresponding apply will time out for the reason that the message with low priority can not be scheduled in time. |
| wrr | Weighted Round Robin.When this mode is applied,it needs to match a weight for each queue(weight means the obtained resource proportion),it takes turns to scheduling according to the weight in queue and assure each queue can obtain definite service.Each queue has the same priority but different weights,the bigger weight it is,the longer scheduling time obtained by this queue.In this way it can assure the lowest priority queue which can obtain definite service at least.avoiding that the message in low priority queue can not obtain service for a long time when adopting the PQ scheduling mode.  queue0-weight/queue1-weight/queue2-weight/queue3-weight/queue4-weight/queue5-weight/queue6-weight/queue7-weight:the weight of each queue.system supports 8 queues,the weight’s sum of 8 queues is 100. |
| WRR+PQ | WRR+PQ scheduling mode is a mixture of WRR and PQ scheduling modes.When the scheduling mode is WRR,and the weight value of queue has 0,the queue scheduling mode is PQ+WRR.In this mode,system will schedule the queue with 0 weight first according to PQ mode,and then schedules the queue with non-zero weight according to WRR mode,the priority of PQ queue is higher than WRR queue in the meantime.  System default scheduling mode is PQ mode. |

【Example】

Example 1：Set the scheduling mode of pon1 as WRR mode,let the messages with various kinds of priority can be scheduled.The weight of queue 0-7 is 15 15 20 10 10 10 10 10.

|  |
| --- |
| OLT(config)#qos queue-scheduler wrr 15 15 20 10 10 10 10 10  OLT(config)# |

### Show OLT Port QOS Queue Schedule Mode

|  |  |
| --- | --- |
| Command | OLT(config)#show qos queue-schedule port-based {epon|ge|xge} <port-id> |
| **View** | Config view |
| **Description** | This command is used for show port-based queue-schedule mode |

【Example】

Example 1：Show pon1 queue-schedule mode

|  |
| --- |
| OLT(config)#show qos queue-scheduler port-based epon 0/0/1  Queue scheduler mode on epon 0/0/1:WRR  -----------------------------------------------------------------------------  Queue Scheduler Mode WRR Weight Bandwidth(kbps)  -----------------------------------------------------------------------------  0 WRR 15-  1 WRR 15-  2 WRR 20-  3 WRR 10-  4 WRR 10-  5 WRR 10-  6 WRR 10-  7 WRR 10-  -----------------------------------------------------------------------------  Queue map mode on epon 0/0/1:Cos  -----------------------------------------------------------------------------  Priority Queue  -----------------------------------------------------------------------------  0 1  1 2  2 3  3 4  4 5  5 6  6 7  7 0  -----------------------------------------------------------------------------  OLT(config)# |

## Config Mapping of DSCP to 802.1p Priority

| Command | OLT(config)#dscp-to-pbits dscp-list 802.1p-priority |
| --- | --- |
| **View** | Config view |
| **Description** | This command is used for configure mapping of DSCP to 802.1p priority.The access devices depend on 802.1p priority for scheduling .And ip network depends on DSCP priority for scheduling .In order to ensure Qos information will not discard during access devices sending user messages to ip network, so have to configure DSCP and 802.1p priority mapping. It must be configured based on the mapping relationship (diffserv) of the differentiated service model; |
| dscp-list | User ip messages’ DSCP threshold information list, range for 0-63,format:1,3-5 |
| 802.1p-priority | Mapping to egress messages’ 802.1p priority, range for 0-7 |

【Example】

Example 1：Configure DSCP list 1 mapping to 802.1p 1

|  |
| --- |
| OLT(config)# dscp-to-pbits 1 1  OLT(config)# |

## Config Mapping of Tos to 802.1P Priority

|  |  |
| --- | --- |
| Command | OLT(config)# tos-to-pbits tos-list 802.1p-priority |
| **View** | Config view |
| **Description** | This command is used to configure the mapping between tos and 802.1p priorities. This command must be configured in qos tos mode. |
| tos-list | Tos information list, range 0-7, format is 1,3-5 |
| 802.1p-priority | The 802.1p priority mapped to the egress packet, ranging from 0 to 7. |

【Example】

Example 1：Configure the tos list to map 2 priority to 802.1p 3.

|  |
| --- |
| OLT(config)# tos-to-pbits 2 3  OLT(config)# |

# OLT DHCP Function Configuration

## OLT DHCP-Snooping Function Configuration

### Enable or Disable DHCP-Snooping Function

|  |  |
| --- | --- |
| Command | OLT(config)#dhcp-Snooping {enable|disable} |
| **View** | Config view |
| **Description** | This command is used for enable or disable dhcp-snooping function,after enabling this function,the functions showing as follows will be opened at the same time:  Trust/un-trust port,MAC address detect,DHCP message rate limit in untrust port,port recovery,option82,dynamic ARP detect and ARP fast reply. |
| {enable|disable} | Enable:enable dhcp-snooping function  Disable:disable dhcp-snooping function |

【Example】

Example 1：Enable dhcp-snooping function

|  |
| --- |
| OLT(config)#dhcp-snooping enable  OLT(config)# |

### Show DHCP-Snooping Configuration

|  |  |
| --- | --- |
| Command | OLT(config)#show dhcp-snooping configuration |
| **View** | Config view |
| **Description** | This command is used for show configuration of DHCP-Snooping |

【Example】

Example 1：Show configuration of DHCP-Snooping

|  |
| --- |
| OLT(config)#show dhcp-snooping configuration  -----------------------------------------------------------------------------  DHCP Snooping Configurations  -----------------------------------------------------------------------------  Switch DHCP Snooping status:Enable  DHCP Snooping verification of hwaddr status:Disable  DHCP Snooping option82 status:Disable  DHCP Snooping option82 policy:Keep  DHCP Snooping option82 format:Type1  DHCP Snooping database wirte-delay time:7200(s)  Switch ARP dectection status:Disable  Switch ARP reply-fast status:Disable  DHCP Snooping is configured on following vlans:  -----------------------------------------------------------------------------  -  Port Trusted Rate-limit(pps)  -----------------------------------------------------------------------------  ge0/0/1 No 300  ge0/0/2 No 300  ge0/0/3 No 300  ge0/0/4 No 300  ge0/0/5 No 300  ge0/0/6 No 300  ge0/0/7 No 300  ge0/0/8 No 300  xge0/0/1 No 300  xge0/0/2 No 300  pon0/0/1 No 300  pon0/0/2 No 300  pon0/0/3 No 300  pon0/0/4 No 300  pon0/0/5 No 300  pon0/0/6 No 300  pon0/0/7 No 300  pon0/0/8 No 300  pon0/0/9 No 300  pon0/0/10 No 300  pon0/0/11 No 300  pon0/0/12 No 300  pon0/0/13 No 300  pon0/0/14 No 300  pon0/0/15 No 300  pon0/0/16 No 300  lag1 No 300  lag2 No 300  lag3 No 300  lag4 No 300  lag5 No 300  lag6 No 300  lag7 No 300  lag8 No 300  lagL9 No 300  lagL10 No 300  lagL11 No 300  lagL12 No 300  lagL13 No 300  lagL14 No 300  lagL15 No 300  lagL16 No 300  -----------------------------------------------------------------------------  OLT(config)# |

### Config DHCP-Snooping Monitor VLAN

| Command | OLT(config)#dhcp-snooping vlan <vlan-list> |
| --- | --- |
| **View** | Config view |
| **Description** | This command is used for add specified monitoring vlan.DHCP message which includes into monitoring vlan will be monitored,DHCP message which does not include into monitoring vlan will be transferred with original shape.  “no dhcp-snooping vlan <vlan-list>”is used for delete the specified monitoring vlan. |
| <vlan-list> | Vlan list |

【Example】

Example 1：Add monitoring vlan 100,200,300

|  |
| --- |
| OLT(config)#dhcp-snooping vlan 100,200,300  OLT(config)# |

### Config DHCP-Snooping Trust Port

|  |  |
| --- | --- |
| Command | OLT(config)#dhcp-snooping trust port {epon/ge/xge/lag} 0/0 <port id> |
| **View** | Config view |
| **Description** | This command is used for add dhcp-snooping trust port,trust port can receive all the DHCP message,untrust port can not receive DHCP reply message.  “no dhcp-snooping ust port {epon/ge/xge/lag} 0/0 <port id>”is used for delete the trust port. |
| {epon/ge/xge/lag} | Port type  Epon:Pon port  Ge:Giga uplink port  Xge:10 giga uplink port  Lag:link aggregation group |
| 0/0 | Frame id/slot id,the default is 0/0 |
| <pord-id> | Port list,format for 1,2-3,4 |

【Example】

Example 1：Add GE1 to dhcp-snooping trust port.

|  |
| --- |
| OLT(config)#dhcp-snooping trust port ge 0/0 1  OLT(config)# |

### Enable or Disable OLT DHCP-Snooping Source MAC Address Detect

|  |  |
| --- | --- |
| Command | OLT(config)#dhcp-snooping chaddr-check {enable|disable} |
| **View** | Config view |
| **Description** | This command is used for enable or disable dhcp-snooping chaddr-check,check whether the source mac address of dhcp request message received by untrust port is the same with CHADDR field,if yes,checking it,else discarding. |
| {enable|disable} | Enable:open dhcp-snooping chaddr-check  Disable:close dhcp-snooping chaddr-check |

【Example】

Example 1：Enable dhcp-snooping chaddr-check function

|  |
| --- |
| OLT(config)#dhcp-snooping chaddr-check enable  OLT(config)# |

### Config DHCP-Snooping Request Message Rate Limit

| Command | OLT(config)#dhcp-snooping limit-rate <Rate> port {epon/ge/xge/lag} 0/0 <port-id> |
| --- | --- |
| **View** | Config view |
| **Description** | This command is used for set rate limitation of dhcp request message received by untrust port,the message will be discard when it out of range.Rate limitation can be set in trust port but it will not take effect unless set this port as untrust port. |
| <Rate> | Rate of dhcp request message,range for 1-2048,unit is pps |
| {epon/ge/xge/lag} | Port type  Epon:Pon port  Ge:Giga uplink port  Xge:10 giga uplink port  Lag:link aggregation group |
| <port id> | Port list,format for 1,2-3,4 |

【Example】

Example 1：The rate limitation of DHCP request message received by GE6 is 20pps.

|  |
| --- |
| OLT(config)#dhcp-snooping limit-rate 20 port ge 0/0 6  OLT(config)# |

### Enable or Disable DHCP-Snooping Opton82 Function

|  |  |
| --- | --- |
| Command | OLT(config)#dhcp-snooping option82 {enable|disable} |
| **View** | Config view |
| **Description** | This command is used for enable|disable dhcp-snooping option82 function.This command inserts option82 information into dhcp request message received by untrust port and peels the option82 information from dhcp reply message received by trust port. |
| {enable|disable} | Enable:Enable dhcp-snooping option82 function  Disable:Disable dhcp-snooping option82 function |

【Example】

Example 1：Enable dhcp-snooping option82 function

|  |
| --- |
| OLT(config)#dhcp-snooping option82 enable  OLT(config)# |

### Config DHCP-Snooping Option82 Forwarding Policy

| Command | OLT(config)#dhcp-snooping option82 policy {keep|drop|replace} |
| --- | --- |
| **View** | Config view |
| **Description** | This command is used for set the option82 forwarding policy of dhcp request message. |
| keep | Transmit option82 dhcp message according to the original shape |
| drop | Discard the option82 dhcp message |
| replace | Replace old option82 in the dhcp message and then transmit |

【Example】

Example 1：Set the dhcp option82 transmission policy as keep.

|  |
| --- |
| OLT(config)#dhcp-snooping option82 policy keep  OLT(config)# |

### Config DHCP-Snooping option82 Format

|  |  |
| --- | --- |
| Command | OLT(config)#dhcp-snooping option82 format {type1|type2|type3|type4|type5|type6|type7|type8} |
| **View** | Config view |
| **Description** | This command is used for set the format of dhcp-snooping option82 |
| <type1|type2|type3|type4|type5|type6|type7|type8> | type1:UNI+ONU MAC  type2:UNI+OLT MAC  type3:ONU+ONU MAC  type4:ONU+OLT MAC  type5:PON+OLT MAC  type6：ONU MAC+OLT MAC  type7：UNI ID+OLT Hostname  type8：PON ID ONU ID+EltexLTPX |

【Example】

Example 1：set the format of dhcp-snooping option82 as type1.

|  |
| --- |
| OLT(config)#dhcp-snooping option82 format type1  OLT(config)# |

### Config DHCP-Snooping Port Binding Policy

|  |  |
| --- | --- |
| Command | OLT(config)#dhcp-snooping binding<mac address><ip address> <vlan id> <port id> |
| **View** | Config view |
| **Description** | This command is used for set the binding strategy of dhcp request message |
| <mac address> | MAC in static binding table,format for AA:BB:CC:DD:EE:FF |
| <ip address> | IP in static binding table,format for A.B.C.D |
| <vlan id> | vlan in static binding table,range for<1-4094> |
| <port id> | Port type  Epon:Pon port  Ge:Giga uplink port  Xge:10 giga uplink port  Lag:link aggregation group |

【Example】

Example 1：Add a static binding table entry,mac address is 00:0f:1f:c5:10:08,ip is 192.168.1.101,vlan is 100,port id is GE8.

|  |
| --- |
| OLT(config)#dhcp-snooping binding 00:0f:1f:c5:10:08 192.168.1.101 100 port ge 0/0/8  OLT(config)# |

### Delete DHCP-Snooping Bind-table

| Command | OLT(config)#dhcp-snooping bind-table clear {all|static|dynamic|ip-address|vlan} |
| --- | --- |
| **View** | Config view |
| **Description** | This command is used for clear dhcp-snooping bind-table. |
| **all** | Clear all the dhcp-snooping bind-table entry. |
| **static** | Clear the static dhcp-snooping bind-table entry. |
| dynamic | Clear the dynamic dhcp-snooping bind-table entry. |
| Ip-address | Delete the bind-table by specified ip |
| vlan | Delete the bind-table by specified vlan id |

【Example】

Example 1：Clear all the dhcp-snooping bind-table entry.

|  |
| --- |
| OLT(config)#dhcp-snooping bind-table clear all  OLT(config)# |

### Config DHCP-Snooping Bind-table Write-delay Time

|  |  |
| --- | --- |
| Command | OLT(config)#dhcp-snooping bind-table write-delay <Delay time> |
| **View** | Config view |
| **Description** | This command is used for set dhcp-snooping bind-table write-delay time.After dhcp-snooping binding-table having been updated and waiting for write-delay time,the flash will be written |
| **<Delay time>** | Write-delay time,range for 240-86400,unit is second. |

【Example】

Example 1：When the dhcp-snooping has been updated,the flash will be written after 4min.

|  |
| --- |
| OLT(config)#dhcp-snooping bind-table write-delay 240  OLT(config)# |

### Config DHCP-Snooping Bind-table Delete-time

|  |  |
| --- | --- |
| Command | OLT(config)#dhcp-snooping bind-table delete-time <time> |
| **View** | Config view |
| **Description** | This command is used for set dhcp-snooping bind-table dynamic entry delete-time.dynamic table will not be deleted immediately when the lease time is over,but it will be deleted after waiting for the delete-time. |
| <time> | Dynamic table delay delete-time,range for 1-86400,unit is second |

【Example】

Example 1：When the lease time is expiration dynamic table will be deleted after 240s latter.

|  |
| --- |
| OLT(config)#dhcp-snooping bind-table delete-time 240  OLT(config)# |

### Config DHCP-Snooping Bind-table Write-to-flash

|  |  |
| --- | --- |
| Command | OLT(config)#dhcp-snooping bind-table write-to-flash |
| **View** | Config view |
| **Description** | This command is used for write the dhcp-snooping bind-table to the flash by manually. |

【Example】

Example 1：Write the dhcp-snooping bind-table to the flash.

|  |
| --- |
| OLT(config)#dhcp-snooping bind-table write-to-flash  OLT(config)# |

### Save DHCP-Snooping Bind-table to Server

| Command | OLT(config)#dhcp-snooping bind-table save-to-tftp <IP address> |
| --- | --- |
| **View** | Config view |
| **Description** | This command is used for write the dhcp-snooping bind-table to the flash by manually and save it to the server |
| <IP address> | The ip address of the TFTP server |

【Example】

Example 1：Write the dhcp-snooping bind-table to the flash by manually and save it to the server 192.168.1.1

|  |
| --- |
| OLT(config)#dhcp-snooping bind-table save-to-tftp 192.168.1.1  OLT(config)# |

### Show DHCP-Snooping Bind-table Entry

|  |  |
| --- | --- |
| Command | OLT(config)#show dhcp-snooping bind-table {all|static|dynamic|ip-address|vlan} |
| **View** | Config view |
| **Description** | This command is used for show dhcp-snooping bind-table according to the type. |
| all | Show all the dhcp-snooping bind-table entry. |
| static | Show the static dhcp-snooping bind-table entry. |
| dynamic | Show the dynamic dhcp-snooping bind-table entry. |
| Ip-address | Show the bind-table by specified ip |
| vlan | Show the bind-table by specified vlan id |

【Example】

Example 1：Show all the dhcp-snooping bind-table entry.

|  |
| --- |
| OLT(config)#show dhcp-snooping bind-table all  -----------------------------------------------------------------------------  database entries count:1 database entries delete time:240(s)  -----------------------------------------------------------------------------  MacAddress IpAddress Vlan Port Lease(s)Type Status  -----------------------------------------------------------------------------  00:0F:1F:C5:10:08 192.168.1.101 100 ge0/0/8-Static Valid  -----------------------------------------------------------------------------  OLT(config)# |

### Enable or Disable DHCP-Snooping arp-reply-fast

|  |  |
| --- | --- |
| Command | OLT(config)#dhcp-snooping arp-reply-fast {enable|disable} |
| **View** | Config view |
| **Description** | This command is used for enable or disable arp-reply-fast function.After enabling this function,system accordings to dhcp-snooping bind-table to judge whether it will execute arp-reply-fast function.When this function is enabled,detecting the Arp message,if there is record in dhcp-snooping bind-table,arp request message will be replied fast rather than transmit to the upper network,thus reducing arp broadcast message. |
| {enable|disable} | Enable:enable dhcp-snooping arp-reply-fast function  Disable:disable dhcp-snooping arp-reply-fast function |

【Example】

Example 1：Enable dhcp-snooping arp-reply-fast function

|  |
| --- |
| OLT(config)#dhcp-snooping arp-reply-fast enable  OLT(config)# |

### Enable or Disable DHCP-Snooping arp-detect Function

| Command | OLT(config)#dhcp-snooping arp-detect {enable|disable} |
| --- | --- |
| **View** | Config view |
| **Description** | This command is used for enable or disable arp-detect function.After enabling this function,system judge whether the user of arp message is legal according to dhcp-snooping bind-table,thus preventing from the illegal arp attack. |
| {enable|disable} | Enable:Enable dhcp-snooping arp-detect function  Disable:Disable dhcp-snooping arp-detect function |

【Example】

Example 1：Disable dhcp-snooping arp-detect function

|  |
| --- |
| OLT(config)#dhcp-snooping arp-detect enable  OLT(config)# |

## OLT DHCP-Relay Function Configuration

### Enable or Disable DHCP-Relay Function

|  |  |
| --- | --- |
| Command | OLT(config)#dhcp-relay {enable|disbale} |
| **View** | Config view |
| **Description** | This command is used for enable or disable dhcp-relay function. |
| {enable|disable} | Enable:Enable dhcp-relay function  Disable:Disable dhcp-relay function |

【Example】

Example 1：Enable dhcp-relay function

|  |
| --- |
| OLT(config)#dhcp-relay enable  OLT(config)# |

### Config DHCP-Relay Vlanif Interface and Server

|  |  |
| --- | --- |
| Command | OLT(config)#dhcp-relay vlanif <vlan-id> server <IP address> |
| **View** | Config view |
| **Description** | This command is used for set the ip address of DHCP-Relay server |
| <IP address> | The ip address of dhcp-relay server in vlanif |

【Example】

Example 1：Set The ip address of dhcp-relay server in vlanif 100 as 192.168.100.1

|  |
| --- |
| OLT(config)#dhcp-relay vlanif 100 server 192.168.100.1  OLT(config)# |

### Show DHCP-Relay Configuration

|  |  |
| --- | --- |
| Command | OLT(config)#show dhcp-relay configuration |
| **View** | Config view |
| **Description** | This command is used for show configuration of dhcp-relay |

【Example】

Example 1：Show configuration of dhcp-relay.

|  |
| --- |
| OLT(config)#show dhcp-relay configuration  -----------------------------------------------------------------------------  Switch DHCP Relay status:Enable  -----------------------------------------------------------------------------  Vlanif Vlanif-Ip Vlanif-netmask Server-Ip  -----------------------------------------------------------------------------  100--192.168.100.1  -----------------------------------------------------------------------------  OLT(config)# |

## OLT DHCP-Client Function Configuration

### Enable or Disable DHCP-Client Function

|  |  |
| --- | --- |
| Command | OLT(config-interface-vlanif-100)#dhcp-client {enable|disable} |
| **View** | Vlanif view |
| **Description** | This command is used for enable or disable dhcp client function |
| {enable|disable} | Enable:Enable dhcp client function  Disable:Disable dhcp-rela function |

【Example】

Example 1：Enable dhcp client function in vlanif 100

|  |
| --- |
| OLT(config-interface-vlanif-100)#dhcp-client enable  OLT(config-interface-vlanif-100)# |

### Config DHCP-Client Manual Renew IP Address

|  |  |
| --- | --- |
| Command | OLT(config-interface-vlanif-100)#dhcp-client renew |
| **View** | Vlanif view |
| **Description** | This command is used for enable the switch of renew in vlanif interface.It can be used when the vlanif interface needs to obtain the ip address actively,this command will trigger the system sending request message and asks for the dhcp server renewing the lease or renewing the ip address. |

【Example】

Example1:Enable the switch of renew in vlanif 100.

|  |
| --- |
| OLT(config-interface-vlanif-100)#dhcp-client renew  OLT(config-interface-vlanif-100)# |

### Config DHCP-Client Manual Release IP Address

|  |  |
| --- | --- |
| Command | OLT(config-interface-vlanif-100)#dhcp-client release |
| View | Vlanif view |
| **Description** | This command is used for release the ip address of vlanif.Executing this command will trigger the system sending release message to inform the dhcp server to releasing the ip address of vlanif. |

【Example】

Example 1：Release the ip address of vlanif 100.

|  |
| --- |
| OLT(config-interface-vlanif-100)#dhcp-client release  OLT(config-interface-vlanif-100)# |

### Config DHCP-Client Option60

|  |  |
| --- | --- |
| Command | OLT(config-interface-vlanif-100)#dhcp-client option60<option60> |
| **View** | Vlanif view |
| **Description** | This command is used for set option60 info carrying by the dhcp-client request message.When the uplink device had set a strategy that proceeds dhcp third layer relay according to option60,we can use this command to set option60 in vlanif interface to match the uplink device.  “no dhcp-client option60”is used for delete the configuration of option60 and revert to default value. |
| <option60> | The info of option60 |

【Example】

Example1:Set option60 of dhcp client in vlanif 100 as“test”.

|  |
| --- |
| OLT(config-interface-vlanif-100)#dhcp-client option60 test  OLT(config-interface-vlanif-100)# |

### Show DHCP-Client Configuration

|  |  |
| --- | --- |
| Command | OLT(config)#show dhcp-client |
| **View** | Config view |
| **Description** | This command is used for show the configuration of dhcp-client |

【Example】

Example 1：Show the configuration of dhcp-client.

|  |
| --- |
| OLT(config)#show dhcp-client  ---------------------------------------------------------------------------  Index Name FSM IP/MASK Leased Until Time  ---------------------------------------------------------------------------  1 vlanif100 INIT-/--  ---------------------------------------------------------------------------  OLT(config)# |

### Show DHCP-Client Option60 Configuration

|  |  |
| --- | --- |
| Command | OLT(config)#show dhcp-client option60 |
| **View** | Config view |
| **Description** | This command is used for show dhcp-client option60 info of each vlanif interface. |

【Example】

Example 1：Show dhcp-client option60 info of each vlanif interface.

|  |
| --- |
| OLT(config)#show dhcp-client option60  ---------------------------------------------------------------------------  VLANIF OPTION60  ---------------------------------------------------------------------------  100 test  ---------------------------------------------------------------------------  OLT(config)# |

# OLT Link Aggregation Function Configuration

## OLT Link-Aggregation Group Basic Function Config

### Add or Delete Link-Aggregation Group Member

|  |  |
| --- | --- |
| Command | OLT(config-interface-aggregation)#member {add/delete} {ge|xge} 0/0 <port-list> link-aggregation group <group-id> |
| **View** | link-aggregation view |
| **Description** | Device supports 16 aggregation group,this command is used for add or delete member port in corresponding aggregation group. |
| <port-list> | Port id |
| <group-id> | **Group id,1-8 is static aggregation group,9-16 is dynamic aggregation group** |

【Example】

Example 1：Add ge1 and ge2 to link-aggregation group 1.

|  |
| --- |
| OLT(config-interface-aggregation)#member add ge 0/0 1,2 link-aggregation group 1  OLT(config-interface-aggregation)# |

Example 2:Delete ge1 and ge2 from link-aggregation group 1.

|  |
| --- |
| OLT(config-interface-aggregation)#member delete ge 0/0 1,2 link-aggregation group 1  OLT(config-interface-aggregation)# |

### Enable or Disable Link-Aggregation Group Flow-control Function

| Command | OLT(config-interface-aggregation)#flow-control <group-id> {enable|disable} |
| --- | --- |
| **View** | link-aggregation view |
| **Description** | This command is used for enable or disable aggregation group flow control function |
| <group-id> | **Group id,1-8 is static aggregation group,9-16 is dynamic aggregation group** |

【Example】

Example 1：Enable the flow control function of aggregation group1

|  |
| --- |
| OLT(config-interface-aggregation)#flow-control 1 enable  OLT(config-interface-aggregation)# |

### Config Link-Aggregation Group System Priority

|  |  |
| --- | --- |
| Command | OLT(config-interface-aggregation)#lacp set system priority <priority value> |
| **View** | link-aggregation view |
| **Description** | This command is used for set system priority |
| <priority value> | Priority value,range for<0-65535>/default |

【Example】

Example 1：Set system priority as 3000.

|  |
| --- |
| OLT(config-interface-aggregation)#lacp set system priority 3000  OLT(config-interface-aggregation)# |

### Set Link-Aggregation Group Port Priority

|  |  |
| --- | --- |
| Command | OLT(config-interface-aggregation)#link-aggregation port-priority <ge|xge> 0/0 <port-list> <priority value> |
| **View** | link-aggregation view |
| **Description** | This command is used for set port priority |
| <port-list> | Port list to be set |
| <priority value> | Priority value,range for<0-65535> |

【Example】

Example 1：Set link-aggregation port priority of ge1 as 3000

|  |
| --- |
| OLT(config-interface-aggregation)#link-aggregation port-priority ge 0/0 1 3000  OLT(config-interface-aggregation)# |

### Show Link-Aggregation Group System Priority

|  |  |
| --- | --- |
| Command | OLT(config-interface-aggregation)#show lacp system priority |
| **View** | link-aggregation view |
| **Description** | This command is used for show lacp system priority |

【Example】

Example 1：Show lacp system priority

|  |
| --- |
| OLT(config-interface-aggregation)#show lacp system priority  lacp system priority value:3000  OLT(config-interface-aggregation)# |

### Show Link-Aggregation Group Priority

|  |  |
| --- | --- |
| Command | OLT(config-interface-aggregation)#show link-aggregation port-priority <ge|xge> 0/0 <port-list> <lacp/manual> |
| **View** | link-aggregation view |
| **Description** | This command is used for show port priority of link-aggregation. |
| <port-list> | Port list to be set |

【Example】

Example 1：Show ge1 port priority of link aggregation

|  |
| --- |
| OLT(config-interface-aggregation)#show link-aggregation port-priority ge 0/0/1 lacp  lacp port priority:32768  OLT(config-interface-aggregation)# |

### Config Link-Aggregation Group Frame-max

|  |  |
| --- | --- |
| Command | OLT(config-interface-aggregation)# frame-max port-list maximum-frame-size |
| **View** | link-aggregation view |
| **Description** | This command is used for set mtu of link-aggregation |
| port-list | Group id,1-8 is static aggregation group,9-16 is dynamic aggregation group |
| maximum-frame-size | The value of frame-max,range for 328-16360 |

【Example】

Example 1：Set the frame-max of link-aggregation group1 as 2000

|  |
| --- |
| OLT(config-interface-aggregation)# frame-max 1 2000  OLT(config-interface-aggregation)# |

### Config Link-Aggregation Group Unicast Load Balance Mode

|  |  |
| --- | --- |
| Command | OLT(config-interface-aggregation)#link-aggregation group <group-id> unicast balance {dest-ip|dest-mac|source-dest-ip|source-dest-mac|source-ip|source-mac} |
| **View** | link-aggregation view |
| **Description** | This command is used for set unicast data balance mode of link aggregation |
| <group-id> | **Group id,1-8 is static aggregation group,9-16 is dynamic aggregation group** |
| <balance> | dest-ip:Load sharing unicast according to destination ip address  dest-mac:Load sharing unicast according to destination mac address  source-dest-ip:Load sharing unicast according to source and destination ip address  source-dest-mac:Load sharing unicast according to source and destination mac address  source-ip:Load sharing unicast according to source ip address  source-mac:Load sharing unicast according to source mac address(default) |

【Example】

Example 1：Set the unicast load balance mode of link-aggregation mode as dest-ip.

|  |
| --- |
| OLT(config-interface-aggregation)#link-aggregation group 1 unicast balance dest-ip  OLT(config-interface-aggregation)# |

### Config Link-Aggregation Group Non-unicast Load BalanceMode

|  |  |
| --- | --- |
| Command | OLT(config-interface-aggregation)#link-aggregation group non-unicast balance (|dest-mac|source-dest-mac|source-mac|source-port) |
| **View** | link-aggregation view |
| **Description** | This command is used for set unicast data balance mode of link aggregation |
| <group-id> | **Group id,1-8 is static aggregation group,9-16 is dynamic aggregation group** |
| <balance> | dest-mac:Load sharing non-unicast according to destination mac address  source-dest-mac:Load sharing non-unicast according to source and destination mac address  source-mac:Load sharing non-unicast according to source mac address(default)  Source-port:Load sharing non-unicast according to source port(default) |

【Example】

Example 1：Set the unicast load balance mode of link-aggregation mode as source-port.

|  |
| --- |
| OLT(config-interface-aggregation)#link-aggregation group non-unicast balance source-port  OLT(config-interface-aggregation)# |

### Config Link-Aggregation Group Name

| Command | OLT(config-interface-aggregation)#port-name <group-id> <port name> |
| --- | --- |
| **View** | link-aggregation view |
| **Description** | Set the name of link-aggregation group |
| <group-id> | Group id,1-8 is static aggregation group,9-16 is dynamic aggregation group |
| <port name> | Name of aggregation group,length for<1-17> |

【Example】

Example 1：Name link-aggregation group1 as test

|  |
| --- |
| OLT(config-interface-aggregation)#port-name 1 test  OLT(config-interface-aggregation)# |

### Delete Link-Aggregation Group Name

|  |  |
| --- | --- |
| Command | OLT(config-interface-aggregation)# no port-name <group-id> |
| **View** | link-aggregation view |
| **Description** | Delete the name of link-aggregation group |
| <group-id> | Group id,1-8 is static aggregation group,9-16 is dynamic aggregation group |

【Example】

Example 1：Delete name link-aggregation group1.

|  |
| --- |
| OLT(config-interface-aggregation)# no port-name 1  OLT(config-interface-aggregation)# |

### Delete Link-Aggregation Group Priority

| Command | OLT(config-interface-aggregation)# no link-aggregation port-priority <ge|xge> F/S/P (lacp|manual) |
| --- | --- |
| **View** | link-aggregation view |
| **Description** | Delete the priority of link-aggregation group |
| F/S/P | Frame-number/Slot-number/Port-number,range for 0/0/1-8 |

【Example】

Example 1：Delete priority link-aggregation group1.

|  |
| --- |
| OLT(config-interface-aggregation)# no link-aggregation port-priority ge 0/0/1 manual  OLT(config-interface-aggregation)# |

### Delete Link-Aggregation Group Frame-max

|  |  |
| --- | --- |
| Command | OLT(config-interface-aggregation)# no frame-max port-list |
| **View** | link-aggregation view |
| **Description** | This command is used for delete the maximum frame length of a configured port and restore it to the default value of 1526. |
| port-list | Group id,1-8 is static aggregation group,9-16 is dynamic aggregation group |

【Example】

Example 1：Delete frame-max link-aggregation group1.

|  |
| --- |
| OLT(config-interface-aggregation)# no frame-max 1  OLT(config-interface-aggregation)# |

### Clear Link-Aggregation Group Statistics

|  |  |
| --- | --- |
| Command | OLT(config-interface-aggregation)#reset statistics port <group-id> |
| **View** | link-aggregation view |
| **Description** | This command is used for clear the link-aggregation statistic data |
| <group-id> | Group id,1-8 is static aggregation group,9-16 is dynamic aggregation group |

【Example】

Example 1：Clear the statistic data of link-aggregation group 1.

|  |
| --- |
| OLT(config-interface-aggregation)#reset statistics port 1  OLT(config-interface-aggregation)# |

### Enable or Disable Link-Aggregation Group

|  |  |
| --- | --- |
| Command | OLT(config-interface-aggregation)#{no} shutdown <group-id> |
| **View** | link-aggregation view |
| **Description** | Open or shutdown link-aggregation group,open by default. |
| <group-id> | Group id,1-8 is static aggregation group,9-16 is dynamic aggregation group |

【Example】

Example 1：Shutdown link-aggregation group1.

|  |
| --- |
| OLT(config-interface-aggregation)#shutdown 1  OLT(config-interface-aggregation)# |

Example 2:Open link-aggregation group1.

|  |
| --- |
| OLT(config-interface-aggregation)#no shutdown 1  OLT(config-interface-aggregation)# |

## Link-Aggregation Group STP Configuration

### Config Link-Aggregation Group STP Cost

| Command | OLT(config-interface-aggregation))#spanning-tree cost <group-id> <cost> |
| --- | --- |
| **View** | link-aggregation view |
| **Description** | This command is used for set the spanning tree cost of link-aggregation group.The optimal path is determined by port cost when there are multi links between two device but nor root port in them. |
| <group-id> | Group id,1-8 is static aggregation group,9-16 is dynamic aggregation group |
| <cost> | Cost value,range for 1-200000000 |

【Example】

Example 1：Set the spanning tree cost of link-aggregation group1 as 2000.

|  |
| --- |
| OLT(config-interface-aggregation))#spanning-tree cost 1 2000  OLT(config-interface-aggregation))# |

### Enable or Disable Link-Aggregation Group STP Edged-port

|  |  |
| --- | --- |
| Command | OLT(config-interface-aggregation))#spanning-tree edged-port <group-id> {enable|disable} |
| **View** | link-aggregation view |
| **Description** | This command is used for set the edged-port of the link-aggregation group.If user specifies a port as edged-port,then when the port migrates forwarding status from congestion status,this port can migrate rapidly doing without waiting for delay time.the user can only set the port which is connected with the terminal as the edged-port.All ports are default to not edged-port. |
| <group-id> | Group id,1-8 is static aggregation group,9-16 is dynamic aggregation group |
| {enable|disable} | enable:Set this port as edged-port  disable:Set this port as not edged-port |

【Example】

Example 1：Set the edged-port of link aggregation group1.

|  |
| --- |
| OLT(config-interface-aggregation))#spanning-tree edged-port 1 enable  OLT(config-interface-aggregation))# |

### Config Link-Aggregation Group STP Mcheck Property

|  |  |
| --- | --- |
| Command | OLT(config-interface-aggregation))#spanning-tree mcheck <group-id> |
| **View** | link-aggregation view |
| **Description** | This command is used for set the RSTP mcheck property of link-aggregation group.Port mcheck property is used for detected whether the port which is running under STP compatible mode can migrate to RSTP mode.By setting mcheck,you can check whether there is a bridge running STP protocol within the network segment which is connected with current Ethernet port,If yes,RSTP protocol will migrate the protocol running mode of this port to STP mode. |
| <group-id> | Group id,1-8 is static aggregation group,9-16 is dynamic aggregation group |

【Example】

Example 1：Set mcheck property of link-aggregation group1.

|  |
| --- |
| OLT(config-interface-aggregation))#spanning-tree mcheck 1  OLT(config-interface-aggregation))# |

### Config Link-Aggregation Group STP Point-to-Point Function

|  |  |
| --- | --- |
| Command | OLT(config-interface-aggregation))#spanning-tree point-to-point <group-id> {auto/true/false} |
| **View** | link-aggregation view |
| **Description** | This command is used for set point-to-point link of link-aggregation group spanning tree.If bridge works in RSTP mode,two ports which is connected by p2p link can migrate to forwarding status by sending synchronization message,it reduces the needless transfer delay time,if set this parameter as auto-mode,RSTP protocol can detect whether current Ethernet port has connected with point-to-point link automatically.The user can set by manually whether current Ethernet port connects with the p2p link.The recommendation is auto-mode. |
| <group-id> | Group id,1-8 is static aggregation group,9-16 is dynamic aggregation group |
| auto/true/false | auto:Set the point-to-point link as auto-mode  true:Connect link-aggregation group to point-to-point link  false:Disconnect link-aggregation group to point-to-point link |

【Example】

Example 1：Set spanning tree point-to-point of link-aggregation as true.

|  |
| --- |
| OLT(config-interface-aggregation))#spanning-tree point-to-point 1 true  OLT(config-interface-aggregation))# |

### Config Link-Aggregation Group STP Priority

|  |  |
| --- | --- |
| Command | OLT(config-interface-aggregation))#spanning-tree priority <group-id> <port-priority> |
| **View** | link-aggregation view |
| **Description** | This command is used for set the RSTP priority of link-aggregation group.By setting the priority of the link-aggregation group,You can specify that a particular link-aggregation group is contained within the spanning tree.Generally,the smaller of the setting value is,the higher of the link-aggregation group priority,this link-aggregation group is likely to include in spanning tree.If all the link-aggregation group of the bridge adapt to the same index number,the priority of the link-aggregation group depends on the index number of the link-aggregation group. |
| <group-id> | Group id,1-8 is static aggregation group,9-16 is dynamic aggregation group |
| <port-priority> | Priority value,range for 0-240,step length for 16.The default value is 128. |

【Example】

Example 1：Set spanning tree priority of link-aggregation group 1 as 160.

|  |
| --- |
| OLT(config-interface-aggregation))#spanning-tree priority 1 160  OLT(config-interface-aggregation))# |

### Delete Link-Aggregation Group STP Configure

| Command | OLT(config-interface-aggregation))# no spanning-tree (priority|cost) group-id |
| --- | --- |
| **View** | link-aggregationView |
| **Description** | This command is used for delete configuration of STP in link-aggregation. |
| group-id | Group id,1-8 is static aggregation group,9-16 is dynamic aggregation group |

【Example】

Example1：delete configuration of STP in link-aggregation.

|  |
| --- |
| OLT(config-interface-aggregation))# no spanning-tree priority 1  OLT(config-interface-aggregation))# |

## Link-Aggregation Group VLAN Configuration

### Config Link-Aggregation Group VLAN Mode

|  |  |
| --- | --- |
| Command | OLT(config-interface-aggregation)#vlan mode <group-id> {access/hybrid/trunk} |
| **View** | link-aggregation view |
| **Description** | This command is used for set vlan mode of link-aggregation group.The default is access mode.In each vlan mode,the message processing way of the port is showed in Appendix1 |
| <group-id> | Group id,1-8 is static aggregation group,9-16 is dynamic aggregation group |
| access/hybrid/trunk | Access:This kind of port only belongs to one vlan,generally it is used for connect to computer. Trunk:This kind of ports can allow multi vlan pass,can receive and transfer the message of different vlan.Usually,it is used for connect to the port between switches. Hybrid:This kind of port allows multiple vlan pass,can receive and transfer the message of different vlan.It can be used to connect the port between switch or connect to the PC. |

【Example】

Example 1：Set the vlan mode of link-aggregation group 1 as access.

|  |
| --- |
| OLT(config-interface-aggregation)#vlan mode 1 access  OLT(config-interface-aggregation)# |

### Config Link-Aggregation Group Native-vlan(access)

|  |  |
| --- | --- |
| Command | OLT(config-interface-aggregation)#vlan native-vlan <group-id> <vlan-id> |
| **View** | link-aggregation view |
| **Description** | This command is used for set Native VLAN of link-aggregation group,the default is 1.In each vlan mode,the message processing way of the port is showed in Appendix1 |
| <group-id> | Group id,1-8 is static aggregation group,9-16 is dynamic aggregation group |
| <vlan-id> | VLAN ID,range for 1-4094. |

【Example】

Example 1：Set native vlan of link-aggregation group1 as 10.

|  |
| --- |
| OLT(config-interface-aggregation)#vlan native-vlan 1 10  OLT(config-interface-aggregation)# |

### Config Link-Aggregation Group Native-vlan Priority

|  |  |
| --- | --- |
| Command | OLT(config-interface-aggregation)#vlan native-vlan-priority <group-id> <priority> |
| **View** | link-aggregation view |
| **Description** | This command is used for set native vlan priority of link-aggregation group,the default is 0. |
| <group-id> | Group id,1-8 is static aggregation group,9-16 is dynamic aggregation group |
| <priority> | Range of priority for 0-7 |

【Example】

Example 1：Set native vlan priority of link-aggregation group1 as 1.

|  |
| --- |
| OLT(config-interface-aggregation)#vlan native-vlan-priority 1 1  OLT(config-interface-aggregation)# |

### Config Link-Aggregation Group Access Mode VLAN

|  |  |
| --- | --- |
| Command | OLT(config-interface-aggregation)#vlan access <group-id> <vlan-id> |
| **View** | link-aggregation view |
| **Description** | This command is used for set Access VLAN of link aggregation,the default is 1..In each vlan mode,the message processing way of the port is showed inAppendix1 |
| <group-id> | **Group id,1-8 is static aggregation group,9-16 is dynamic aggregation group** |
| <vlan-id> | Access VLAN ID,range for 1-4094 |

【Example】

Example 1：Set access vlan of link-aggregation group1 as 100.

|  |
| --- |
| OLT(config-interface-aggregation)#vlan access 1 100  OLT(config-interface-aggregation)# |

### Config Link-Aggregation Group Hybrid Mode VLAN

| Command | OLT(config-interface-aggregation)#vlan hybrid <group-id> {tagged|untagged} <vlan-list> |
| --- | --- |
| **View** | link-aggregation view |
| **Description** | This command is used for set hybrid VLAN of link aggregation,the default is 1..In each vlan mode,the message processing way of the port is showed inAppendix1 |
| <group-id> | **Group id,1-8 is static aggregation group,9-16 is dynamic aggregation group** |
| {tagged|untagged} | tagged:Add corresponding vlan tag for egress message  untagged:Peel off corresponding vlan tag for egress message |
| <vlan-list> | VLAN ID,range for 1-4094.format is 1,11-27,100 |

【Example】

Example 1：Add untagged hybrid vlan 10-15 for link-aggregation group1.

|  |
| --- |
| OLT(config-interface-aggregation)#vlan hybrid 1 untagged 10-15  lag1:hybrid vlan added,failed:0,success:6  OLT(config-interface-aggregation)# |

Example 2:Add tagged hybrid vlan 101 for link-aggregation group1.

|  |
| --- |
| OLT(config-interface-aggregation)#vlan hybrid 1 tagged 101  lag1:hybrid vlan added,failed:0,success:1  OLT(config-interface-aggregation)# |

### Delete Link-Aggregation Group Hybrid Mode VLAN

|  |  |
| --- | --- |
| Command | OLT(config-interface-aggregation)#no vlan hybrid <group-id> {tagged|untagged} <vlan-list> |
| **View** | link-aggregation view |
| **Description** | This command is used for delete hybrid VLAN of link aggregation,the default is 1..In each vlan mode,the message processing way of the port is showed inAppendix1 |
| <group-id> | **Group id,1-8 is static aggregation group,9-16 is dynamic aggregation group** |
| {tagged|untagged} | tagged:Add corresponding vlan tag for egress message  untagged:Peel off corresponding vlan tag for egress message |
| <vlan-list> | VLAN ID,range for 1-4094.format is 1,11-27,100 |

【Example】

Example 1：Delete tagged hybrid vlan 10-15 for link-aggregation group1.

|  |
| --- |
| OLT(config-interface-ge)#no vlan hybrid 1 tagged 10-15  OLT(config-interface-ge)# |

### Config Link-Aggregation Group Trunk Mode VLAN

|  |  |
| --- | --- |
| Command | OLT(config-interface-aggregation)#vlan trunk <group-id> <vlan-list> |
| **View** | link-aggregation view |
| **Description** | This command is used for delete trunk VLAN of link aggregation,the default is 1..In each vlan mode,the message processing way of the port is showed inAppendix1 |
| <group-id> | **Group id,1-8 is static aggregation group,9-16 is dynamic aggregation group** |
| <vlan-list> | VLAN ID,range for 1-4094.format is 1,11-27,100 |

【Example】

Example 1：Add trunk vlan 10-15 for link-aggregation group1.

|  |
| --- |
| OLT(config-interface-aggregation)#vlan trunk 1 10-15  lag1:trunk vlan allowed,failed:0,success:6  OLT(config-interface-aggregation)# |

### Delete Link-Aggregation Group Trunk Mode VLAN

|  |  |
| --- | --- |
| Command | OLT(config-interface-aggregation)#no vlan trunk <group-id> <vlan-list> |
| **View** | link-aggregation view |
| **Description** | This command is used for delete trunk VLAN of link aggregation,the default is 1..In each vlan mode,the message processing way of the port is showed inAppendix1 |
| <group-id> | **Group id,1-8 is static aggregation group,9-16 is dynamic aggregation group** |
| <vlan-list> | VLAN ID,range for 1-4094.format is 1,11-27,100 |

【Example】

Example 1：Delete trunk vlan 10 for link-aggregation group1.

|  |
| --- |
| OLT(config-interface-aggregation)#no vlan trunk 1 10  OLT(config-interface-aggregation)# |

## Show Link-Aggregation Group Information

### Show Link-Aggregation Group VLAN Information

|  |  |
| --- | --- |
| Command | OLT(config-interface-aggregation)#show port vlan <group-id> |
| **View** | link-aggregation view |
| **Description** | This command is used for show vlan info of link-aggregation group |
| <group-id> | **Group id,1-8 is static aggregation group,9-16 is dynamic aggregation group** |

【Example】

Example 1：Show vlan info of link-aggregation group1

|  |
| --- |
| OLT(config-interface-aggregation)#show port vlan 1  -----------------------------------------------------------------------------  Port:lag1 Mode:Access Native-Vlan:1 Priority:0  -----------------------------------------------------------------------------  Tagged-Vlan:  -  -----------------------------------------------------------------------------  Untagged-Vlan:  1  -----------------------------------------------------------------------------  OLT(config-interface-aggregation)# |

### Show Link-Aggregation Group STP Information

| Command | OLT(config-interface-aggregation)#show port spanning-tree <group-id> |
| --- | --- |
| **View** | link-aggregation view |
| **Description** | This command is used for show spanning tree info of link-aggregation group |
| <group-id> | **Group id,1-8 is static aggregation group,9-16 is dynamic aggregation group** |

【Example】

Example1:Show spanning tree info of link-aggregation group 1.

|  |
| --- |
| OLT(config-interface-aggregation)#show port spanning-tree 1  -----------------------lag1 RSTP STATUS:--------------------------------  Port STP Mode:RSTP  Port Priority:128  Port Path Cost:20000  Port Edge Admin:NON-Edge  Port Edge Status:NEdge  Port Link Type Admin:Auto  Port Link Type Status:P2P  Port Role:Unknown  Port State:Down  -----------------------------------------------------------------------------  OLT(config-interface-aggregation)# |

### Show Link-Aggregation Group Port Status

|  |  |
| --- | --- |
| Command | OLT(config-interface-aggregation)#show port state <group-id> |
| **View** | link-aggregation view |
| **Description** | This command is used for show port state of link-aggregation group |
| <group-id> | **Group id,1-8 is static aggregation group,9-16 is dynamic aggregation group** |

【Example】

Example 1：Show port state of link-aggregation group1.

|  |
| --- |
| OLT(config-interface-aggregation)#show port state 1  -----------------------------------------------------------------------------  Port name:test  Current port state:enable  Current link state:DOWN  The maximum transmit unit:1500  Link speed:autonegotiation(1000 Mbps)  Link duplex:autonegotiation(FULL)  Flow-control:supported  -----------------------------------------------------------------------------  Native-vlan:1 Link-type:Access Priority:0  Untagged VLAN ID:  1  -----------------------------------------------------------------------------  OLT(config-interface-aggregation)# |

### Show Link-Aggregation Group STP Information Statistics Information

|  |  |
| --- | --- |
| Command | OLT(config-interface-aggregation)#show statistics port <group-id> |
| **View** | link-aggregation view |
| **Description** | This command is used for show statistic info of link-aggregation group |
| <group-id> | **Group id,1-8 is static aggregation group,9-16 is dynamic aggregation group** |

【Example】

Example 1：Show statistic info of link-aggregation group1.

|  |
| --- |
| OLT(config-interface-aggregation)#show statistics port 1  member ge0/0/1 statistics:  -----------------------------------------------------------------------------  Direction Total Uncast Bcast Mcast Err  (bytes)(pkts)(pkts)(pkts)(pkts)  ----------------------------------------------------------------------------  RX 0 0 0 0 0  TX 0 0 0 0 0  -----------------------------------------------------------------------------  link-aggregation group 1 statistics:  -----------------------------------------------------------------------------  Direction Total Uncast Bcast Mcast Err  (bytes)(pkts)(pkts)(pkts)(pkts)  ----------------------------------------------------------------------------  RX 0 0 0 0 0  TX 0 0 0 0 0  -----------------------------------------------------------------------------  OLT(config-interface-aggregation)# |

### Show Link-Aggregation Group Config Information

|  |  |
| --- | --- |
| Command | OLT(config-interface-aggregation)#show link-aggregation group <group-id> |
| **View** | link-aggregation view |
| **Description** | This command is used for show link-aggregation group matching state |
| <group-id> | **Group id,1-8 is static aggregation group,9-16 is dynamic aggregation group** |

【Example】

Example 1：Show matching state of link aggregation group1.

|  |
| --- |
| OLT(config-interface-aggregation)#show link-aggregation group 1  Lag Lag Select Unselect Load Master  ID Type Ports Ports Balance Port  1 Manual-ge0/0/1,dest-ip-  OLT(config-interface-aggregation)# |

# OLT Routing Function

## Add or Delete Static Route

|  |  |
| --- | --- |
| Command | OLT(config)#{no} ip route-static <Ip-addr> <IP address mask> <Gateway address> |
| **View** | Config view |
| **Description** | This command is used for add or delete static route of olt,it can set a strip of static route only. |
| <no> | Delete the command |
| <ip-addr> | IP address.IP address is divided into 5 types,user can select a suitable ip subnet according to the use case,the ip address with 32bits 0 or 32bits 1 has special function,so it can not use as general ip address,format for X.X.X.X |
| <IP address mask> | Subnet mask,format for X.X.X.X |
| <Gateway address> | Gateway address,format for X.X.X.X |

【Example】

Example 1：Set a strip of static route of olt,gateway is 192.168.2.253.

|  |
| --- |
| OLT(config)#ip route-static 0.0.0.0 0.0.0.0 192.168.5.253  Successfully add static routing entries!  OLT(config)# |

Example 2:Delete a static route.

|  |
| --- |
| OLT(config)#no ip route-static 192.168.3.0 255.255.255.0 192.168.5.1  Successfully Del static routing entries!  OLT(config)# |

## Config Route ID

| Command | OLT(config)# (no) router-id ip-address |
| --- | --- |
| **View** | Config view |
| **Description** | This command is used to configure or delete the route ID of the RIP. |
| ip-address | IP address ,format is x.x.x.x |

【Example】

Example 1：Config route-id ip.

|  |
| --- |
| OLT(config)# router-id 192.168.20.12  OLT(config)# |

## Show IP Route Information

|  |  |
| --- | --- |
| Command | OLT(config)#show ip route |
| **View** | Config view |
| **Description** | This command is used for show ip route info |

【Example】

Example 1：Show ip route info

|  |
| --- |
| OLT(config)#show ip route  Flags:U-use,M-Mutipath,E-ECMP  Destination/Mask Proto Pre Cost NextHop Interface flag  192.168.1.0/24 Direct 1 0\*vlanIf2  0.0.0.0/0 Static 2 2 192.168.5.253 vlanIf0 U  192.168.3.0/24 Static 2 2 192.168.5.1 vlanIf0 U  OLT(config)# |

## Show IP Routing-table Information

| Command | OLT(config)#show ip routing-table all |
| --- | --- |
| **View** | Config view |
| **Description** | This command is used for show ip routing-table info |

【Example】

Example 1：Show ip routing-table info

|  |
| --- |
| OLT(config)#show ip routing-table all  Flags:U-use,M-Mutipath,E-ECMP  Destination/Mask Proto Pre Cost NextHop Interface flag  192.168.1.0/24 Direct 1 0\*vlanIf2 U  0.0.0.0/0 Static 2 2 192.168.5.253 vlanIf0 U  192.168.3.0/24 Static 2 2 192.168.5.1 vlanIf0 U  OLT(config)# |

## Config OLT RIP function

### Enable/Disable RIP

|  |  |
| --- | --- |
| Command | OLT(config)# (no) router rip |
| **View** | config view |
| **Description** | This command is used to enable the RIP function and enter the router mode or disable the RIP function. |

【Example】

Example 1：Enable the RIP function and enter the router mode.

|  |
| --- |
| OLT(config)# router rip  OLT(config-router)# |

### Config the default route for importing RIP.

| Command | OLT(config-router)# (no) default-information originate (metric metric-value ) |
| --- | --- |
| **View** | router view |
| **Description** | This command is used to enable or disable the import of default routes in RIP. |
| metric-value | The metric value to be configured, in the range of 0 to 16. |

【Example】

Example 1：Enable the import of the default route and set the metric value in RIP.

|  |
| --- |
| OLT(config-router)# default-information originate metric 2  OLT(config-router)# |

### Config the default metric value of the RIP for importing routes.

|  |  |
| --- | --- |
| Command | OLT(config-router)# (no) default-metric default-metric |
| **View** | router view |
| **Description** | This command is used to configure or delete the default metric value of the RIP of the imported route. |
| default-metric | The metric value to be configured, in the range of 1 to 16. |

【Example】

Example 1：Configure the default metric value of the RIP for importing routes.

|  |
| --- |
| OLT(config-router)# default-metric 1  OLT(config-router)# |

Example 2：Delete the default metric value of the imported RIP in batches.

|  |
| --- |
| OLT(config-router)# no default-metric  OLT(config-router)# |

### Configure the management distance of RIP

| Command | OLT(config-router)# (no) distance distance-value ip-source-prefix access-list-name |
| --- | --- |
| **View** | router view |
| **Description** | This command is used to configure or delete the management distance of RIP and change the priority of RIP. The default RIP is 120. |
| distance-value | The administrative distance value to be configured, ranging from 1 to 255. |
| ip-source-prefix | Source IP prefix in the format x.x.x.x/M |
| access-list-name | Access list name |

【Example】

Example 1：Config the management distance of RIP.

|  |
| --- |
| OLT(config-router)# distance 1 192.168.12.1/24 test  OLT(config-router)# |

### Config a specified neighbor route for RIP

|  |  |
| --- | --- |
| Command | OLT(config-router)# (no) neighbor ip-address |
| **View** | router view |
| **Description** | This command is used to configure or delete the specified neighbor route of RIP. |
| ip-address | Specifies the IP address of the neighbor in the format x.x.x.x |

【Example】

Example 1：Configure a specified neighbor route for RIP.

|  |
| --- |
| OLT(config-router)# neighbor 192.168.50.2  OLT(config-router)# |

### Config the RIP function on the specified network segment interface

| Command | OLT(config-router)# (no) network (ip-address|network-number)/ length-mask |
| --- | --- |
| **View** | router view |
| **Description** | This command is used to configure or delete the RIP function on the specified network segment interface. |
| (ip-address|network-number) | Specifies the IP address/network number of the network segment interface in the format x.x.x.x |
| length-mask | Specifies the subnet mask length of the interface on the network segment, in the range of 0 to 32. |

【Example】

Example 1：Config the RIP function on the specified network segment interface.

|  |
| --- |
| OLT(config-router)# network 192.168.20.12/24  OLT(config-router)# |

### Config the RIP function on the VLANIF interface

|  |  |
| --- | --- |
| Command | OLT(config-router)# (no) network vlanif vlan-id |
| **View** | router view |
| **Description** | This command is used to configure or delete the RIP function of the specified VLANIF interface. |
| vlan-id | The VLAN ID of the VLANIF interface to be configured, in the range of 1-4094. |

【Example】

Example 1：Configure the RIP function of vlanif interface 200.

|  |
| --- |
| OLT(config-router)# network vlanif 200  OLT(config-router)# |

### Config RIP metrics

|  |  |
| --- | --- |
| Command | OLT(config-router)# (no) offset-list access-list-name in|out metric-value interface-name |
| **View** | router view |
| **Description** | This command is used to configure or delete the metrics of RIP. |
| access-list-name | Access list name to be modified |
| metric-value | The metric value to be modified, ranging from 0 to 16. |
| interface-name | Specify the interface name |

【Example】

Example 1：The metric for the entry update of the configuration test list is 3.

|  |
| --- |
| OLT(config-router)# offset-list test in 3  OLT(config-router)# |

### Config the passive interface of RIP

|  |  |
| --- | --- |
| Command | OLT(config-router)# (no) passive-interface vlanif (vlan-list |all) |
| **View** | router view |
| **Description** | This command is used to enable or disable the passive interface of RIP. |
| (vlan-list |all) | Vlan-list: vlan id of the vlanif interface to be configured, in the range of 1-4094  All: Configure all vlanif interfaces. |

【Example】

Example 1：Enable the passive interface of RIP.

|  |
| --- |
| OLT(config-router)# passive-interface vlanif all  OLT(config-router)# |

### Config import routes in RIP

| Command | OLT(config-router)# (no) redistribute (babel|bgp|connected|isis|kernal|ospf|pim|static) metric metric-value route-map pointer-to-route-map-entries |
| --- | --- |
| **View** | router view |
| **Description** | This command is used to enable or disable the import of routes in RIP. |
| babel|bgp|connected|isis|kernal|ospf|pim|static | Babel: babel routing protocol  Bgp: Border Gateway Mind  Connected: Direct routing  Isis: intermediate system to intermediate system routing  Kernal: Kernel routing (not installed via zebra RIB)  Ospf: Develop shortest path first  Pim: Protocol Independent Multicast  Static: Static route |
| metric-value | The metric value to be configured, in the range of 0 to 16. |
| pointer-to-route-map-entries | Pointer to a route map entry |

【Example】

Example 1：Enable the import of routes into RIP.

|  |
| --- |
| OLT(config-router)# redistribute ospf metric 2  OLT(config-router)# |

### Config RIP static routes

|  |  |
| --- | --- |
| Command | OLT(config-router)# (no) route ip-address/mask |
| **View** | router view |
| **Description** | This command is used to enable or disable RIP static routes. |
| ip-address/mask | IP address and mask in the format x.x.x.x/m |

【Example】

Example 1：Configure a static route in RIP.

|  |
| --- |
| OLT(config-router)# route 192.168.12.10/24  OLT(config-router)# |

### Config the timer time of RIP

|  |  |
| --- | --- |
| Command | OLT(config-router)# (no) time basic update-time timeout garbage-collect |
| **View** | router view |
| **Description** | This command is used to set the RIP timer time. |
| update-time | The update time to be configured. The default is 30s, and the value ranges from 5 to 16777215. |
| timeout | The aging timeout period to be configured is 180s by default. The value ranges from 5 to 16777215. |
| garbage-collect | Recycle time to be configured. The default is 120s, and the value ranges from 5 to 16777215. |

【Example】

Example 1：Set the update time of the RIP timer to 50s, the timeout time to 200s, and the garbage-collect time to 150s.

|  |
| --- |
| OLT(config-router)# timers basic 50 200 150  OLT(config-router)# |

### Config the version of RIP

|  |  |
| --- | --- |
| Command | OLT(config-router)# (no) version id |
| **View** | router view |
| **Description** | This command is used to configure the version of RIP and delete it with no. |
| Id | The RIP version to be configured, in the range of 1-2. |

【Example】

Example 1：Set the RIP version to 1.

|  |
| --- |
| OLT(config-router)# version 1  OLT(config-router)# |

### Create/delete the key of the RIPv2 keychain

|  |  |
| --- | --- |
| Command | OLT(config-keychain)# key key-id |
| **View** | keychain view |
| **Description** | This command is used to create the key of the RIPv2 keychain or delete the key of the RIP authentication keychain. |
| key-id | Key-id to be configured, in the range 0-2147483647 |

【Example】

Example 1：Configure the key of the RIPv2 keychain and enter the key management interface.

|  |
| --- |
| OLT(config-keychain)# key 123  OLT(config-keychain-key)# |

Example 2：Delete the key of the RIPv2 keychain.

|  |
| --- |
| OLT(config-keychain)# no key 123  OLT(config-keychain)# |

### Create/delete an authentication key for the RIPv2 keychain

|  |  |
| --- | --- |
| Command | OLT(config-keychain-key)#(no) key-string auth-string |
| **View** | Keychain-key view |
| **Description** | This command is used to create an authentication key for the RIPv2 keychain or to delete the authentication key of the RIP authentication keychain. |
| auth-string | Configure a simple key string |

【Example】

Example 1：Configure the authentication key for the RIPv2 keychain.

|  |
| --- |
| OLT(config-keychain-key)# no accept-lifetime  OLT(config-keychain-key)# |

Example 2：Delete the authentication key of the RIPv2 keychain.

|  |
| --- |
| OLT(config-keychain-key)# no key-string  OLT(config-keychain-key)# |

### Create/delete the receive lifetime of the RIPv2 keychain

|  |  |
| --- | --- |
| Command | OLT(config-keychain-key)# (no) accept-lifetime start-time end-time |
| **View** | key view |
| **Description** | This command is used to set or delete the receive lifetime of the RIPv2 keychain. |
| start-time | Configuration method:  1.HH:MM:SS date<1-31> month<Jan-Dec> year<1993-2035>  2.HH:MM:SS month<Jan-Dec> date<1-31> year<1993-2035> |
| end-time | Configuration method:  1.HH:MM:SS date<1-31> month<Jan-Dec> year<1993-2035> 2.HH:MM:SS month<Jan-Dec> date<1-31> year<1993-2035>  3.duration：duration, in the range of 1 to 217483646, in seconds  4.infinite: never expires |

【Example】

Example 1：Configure the receive lifetime of the RIPv2 keychain.

|  |
| --- |
| OLT(config-keychain-key)# accept-lifetime 11:22:00 1 Aug 2019 12:00:00 3 Aug 2019  OLT(config-keychain-key)# |

Example 2：Delete the receive lifetime of the RIPv2 keychain.

|  |
| --- |
| OLT(config-keychain-key)# no accept-lifetime  OLT(config-keychain-key)# |

### Create/delete the transmit lifetime of the RIPv2 keychain

|  |  |
| --- | --- |
| Command | OLT(config-keychain-key)# (no) accept-lifetime start-time end-time |
| **View** | key view |
| **Description** | This command is used to set or delete the transmission lifetime of the RIPv2 keychain. |
| start-time | Configuration method:  1.HH:MM:SS date<1-31> month<Jan-Dec> year<1993-2035>  2.HH:MM:SS month<Jan-Dec> date<1-31> year<1993-2035> |
| end-time | Configuration method:  1.HH:MM:SS date<1-31> month<Jan-Dec> year<1993-2035> 2.HH:MM:SS month<Jan-Dec> date<1-31> year<1993-2035>  3.duration：duration, in the range of 1 to 217483646, in seconds  4.infinite: never expires |

【Example】

Example 1：Configure the transmit lifetime of the RIPv2 keychain.

|  |
| --- |
| OLT(config-keychain-key)# send-lifetime 14:05:00 10 Aug 2019 duration 21600  OLT(config-keychain-key)# |

Example 2：Delete the transmission lifetime of the RIPv2 keychain.

|  |
| --- |
| OLT(config-keychain-key)# no send-lifetime  OLT(config-keychain-key)# |

## Config the RIP function of the vlanif interface

### Config the authentication mode and parameters of RIP

|  |  |
| --- | --- |
| Command | OLT(config-interface-vlanif-100)# ip rip authentication ((key-chain name-of-key-chain)|(mode md5|text)|(string authentication-string)) |
| **View** | vlanif view |
| **Description** | This command is used to configure the RIP authentication mode and parameters of the vlanif interface. |
| name-of-key-chain | Configure the name of the RIP authentication keychain on the vlanif interface. |
| md5|text | Enable the RIP authentication mode of the vlanif interface: md5 is cipher text encryption, and text is plain text encryption. |
| authentication-string | Configure the RIP simple authentication key string for the vlanif interface. |

【Example】

Example 1：Configure the RIP authentication mode of the vlanif interface to 100 as cipher text encryption.

|  |
| --- |
| OLT(config-interface-vlanif-100)# ip rip authentication mode md5  OLT(config-interface-vlanif-100)# |

### Enable RIP to Send/Receive Messages

|  |  |
| --- | --- |
| Command | OLT(config-interface-vlanif-100)# ip rip (send|receive) version version-id |
| **View** | vlanif view |
| **Description** | This command is used to enable the function of sending/receiving packets on the vlanif interface. |
| version-id | Configure the version number of the RIP of the vlanif interface. |

【Example】

Example 1：Enable the RIP packet with the vlanif interface set to 100.

|  |
| --- |
| OLT(config-interface-vlanif-100)# ip rip send version 1  OLT(config-interface-vlanif-100)# |

### Config the split horizon function of RIP

|  |  |
| --- | --- |
| Command | OLT(config-interface-vlanif-100)# ip rip split-horizon poisoned-reverse |
| **View** | vlanif view |
| **Description** | This command is used to enable the split horizon function of RIP route update packets on the vlanif interface. |

【Example】

Example 1：Enable the horizontal split function of RIP route update packets with the vlanif interface being 100.

|  |
| --- |
| OLT(config-interface-vlanif-100)# ip rip split-horizon poisoned-reverse  OLT(config-interface-vlanif-100)# |

### Delete RIP configuration

| Command | OLT(config-interface-vlanif-100)# no ip rip ( (authentication ((key-chain name-of-key-chain)|(mode md5|text)|(string authentication-string)))|((send|receive) version version-id)|(split-horizon poisoned-reverse) |
| --- | --- |
| **View** | vlanif view |
| **Description** | This command is used to delete the RIP authentication mode of the vlanif interface, the function of receiving/sending packets, and the horizontal split function of routing updates. |
| name-of-key-chain | Configure the name of the RIP authentication keychain on the vlanif interface. |
| md5|text | Enable the RIP authentication mode of the vlanif interface: md5 is cipher text encryption, and text is plain text encryption. |
| authentication-string | Configure a RIP simple authentication key string for the vlanif interface. |
| version-id | Configure the version number of the RIP of the vlanif interface. |

【Example】

Example 1：Remove the RIP authentication mode, send packet function, and split horizon function of the vlanif interface to 100.

|  |
| --- |
| OLT(config-interface-vlanif-100)# no ip rip authentication mode md5  OLT(config-interface-vlanif-100)# no ip rip send version 1  OLT(config-interface-vlanif-100)# no ip rip split-horizon poisoned-reverse  OLT(config-interface-vlanif-100)# |

# OLT Profile Configuration

## OLT DBA Profile Configurations

### Create DBA Profile

|  |  |
| --- | --- |
| Command | OLT(config)#dba-profile {profile-id <profile-id>|profile-name <profile-name>} |
| **View** | Config view |
| **Description** | This command is used for add a dba-profile and enter dba-profile editing view.The deployment and control of uplink Bandwidth of ONU is realized through the Dynamic Bandwidth Allocation technology.dba-profile defines the uplink bandwidth of onu.Device adjusts the allocation of uplink bandwidth automatically according to the burst need of uplink services,which increases the uplink bandwidth service efficiency of pon system.When the default dba-profile can not satisfy the service needing and needs to create a new dba profile according to the real time service needing,using this command.“no”command is used for delete dba profile. |
| <profile-id> | dba profile id.System allocates a mini idle profile number if it is not specified by system.Proile 0 is the default profile.Onu with autoauth will match profile 0 automatically. |
| <profile-name> | DBA profile name.If it is not specified,system will adopt the default name“dba-profile\_id”. |

【Example】

Example 1：Create a new dba profile 10.

|  |
| --- |
| OLT(config)#dba-profile profile-id 10  OLT(config-dba-profile-10)# |

Example 2：Delete dba-profile id 10.

|  |
| --- |
| OLT(config)# no dba-profile profile-id 10    OLT(config)# |

### Config DBA Profile Bandwith

| Command | OLT(config-dba-profile-10)#type1 fix<fixed bandwidth>  OLT(config-dba-profile-10)#type2 assure<assure bandwidth>  OLT(config-dba-profile-10)#type3 assure<assure bandwidth> max <max bandwidth>  OLT(config-dba-profile-10)#type4 max <max bandwidth>  OLT(config-dba-profile-10)#type5 fix <fixed bandwidth>  assure <assure bandwidth> max <max bandwidth> |
| --- | --- |
| **View** | DBA profile view |
| **Description** | This command is used for configure the type of DBA control bandwidth and the size of the bandwidth. |
| <type1> | Fix bandwidth.It is reserved to specified onu or the specific service of onu,this bandwidth can not be used by other onu even if the onu has not uplink service stream.It is mainly used in the service with hypersensitive qos,such as TDM,VoIP and etc. |
| <type2> | Assure bandwidth.It assures that onu can obtain a specified bandwidth when it is in need.Device’s dba mechanism could allocate the surplus bandwidth to other onu’s service when the real time service stream of onu can not reach the assure bandwidth.its realtime performance is worse than fixed bandwidth for the reason that it needs to control the allocation of bandwidth according to dba mechanism. |
| <type3> | Type3 includes assure bandwidth and max bandwidth.Type3 is a combination bandwidth type which assures the user has a certain bandwidth and it commits that the user has a certain bandwidth to preempt.But the sum of assure bandwidth can not exceed the max bandwidth.This kind of bandwidth is mainly used in voip and iptv service. |
| <type4> | Max bandwidth.The upper limit of bandwidth that the onu can obtain.It is mainly used in internet service. |
| <type5> | Type5 includes fixed bandwidth and assure bandwidth and max bandwidth..Type5 is a combination bandwidth type.The sum of fix bandwidth and assure bandwidth can not exceed the max bandwidth. |
| <fix> | Fix bandwidth.This part of bandwidth is allocated to the user firmly,other user can not preempt it even if it is in idle state. |
| <assure> | Assure bandwidth.If it is in idle other user can preempt it. |
| <max> | Max bandwidth.the max available bandwidth for the user.  The sum of assure bandwidth in type3 can not exceed the max bandwidth.  The sum of fix bandwidth and assure bandwidth in type5 can not exceed the max bandwidth. |

【Example】

Example 1：Set the type of profile 10 as type5,fix bandwidth is 5Mbps,assure bandwidth is 10Mbps,max bandwidth is 30Mbps.

|  |
| --- |
| OLT(config-dba-profile-10)#type5 fix 5120 assure 10240 max 30720  OLT(config-dba-profile-10)# |

### Commit DBA Profile Config

|  |  |
| --- | --- |
| Command | OLT(config-dba-profile-10)#commit |
| **View** | DBA pprofile view |
| **Description** | This command is used for commit the current dba profile setting.All the parameter will take effect only after the command is committed. |

【Example】

Example 1：Commit the current dba profile setting.

|  |
| --- |
| OLT(config-dba-profile-10)#commit  OLT(config-dba-profile-10)# |

### Show OLT DBA Profile Information

|  |  |
| --- | --- |
| Command | OLT(config)#show dba-profile {all|profile-id <profile-id>|profile-name <profile-name>} |
| **View** | Config view |
| **Description** | This command is used for show dba profile info.dba profile describes the flow parameter of the link,onu allocates the bandwidth automatically by binding dba profile which can increase the bandwidth utilization. |
| <profile-id> | Profile id to be show. |
| <profile-name> | Profile name to be show. |

【Example】

Example 1：Show all the dba profile.

|  |
| --- |
| OLT(config)#show dba-profile all  -----------------------------------------------------------------------------  Profile Profile Type Fix Assure Max Bind  ID Name(kbps)(kbps)(kbps)times  ----------------------------------------------------------------------------  0 dba-profile\_0 4 0 0 1000000 1  1 dba-profile\_1 4 0 0 1000000 0  2 dba-profile\_2 4 0 0 1000000 0  10 dba-profile\_10 5 5120 10240 30720 0  -----------------------------------------------------------------------------  Total:4  OLT(config)# |

## ont-lineprofile Configuraton

### Create ont-lineprofile

|  |  |
| --- | --- |
| Command | OLT(config)#ont-lineprofile epon {profile-id <profile-id> profile-name <profile-name>} |
| **View** | Config view |
| **Description** | This command is used for create a new ont-lineprofile and enter the correspo hip between llid and dba profile. |
| <profile-id> | Profile id of ont-lineprofile.When it is unspecified,the system will match a minimum idle number.ont-lineprofile 0 is default profile.Autoauth’s onu will match ont-lineprofile 0 automatically. |
| <profile-name> | Ont-lineprofile name.the default name is“ont-lineprofile\_name” |

【Example】

Example 1：Create and enter ont-lineprofile 10.

|  |
| --- |
| OLT(config)#ont-lineprofile epon profile-id 10  OLT(config-epon-lineprofile-10)# |

### Bind DBA Profile in ont-lineprofile

|  |  |
| --- | --- |
| Command | OLT(config-epon-lineprofile-10)#llid <llid-id> dba-profile-id <profile-id> |
| **View** | ont-lineprofile view |
| **Description** | This command is used for bind dba profile. |
| <profile-id> | dba profile id.When it is unspecified,the system will match a minimum idle number.dba profile 0 is default profile.Autoauth’s onu will match dba profile 0 automatically. |

【Example】

Example 1：Bind dba profile 10 to ont-lineprofile 10.

|  |
| --- |
| OLT(config-epon-lineprofile-10)#llid 1 dba-profile-id 10  OLT(config-epon-lineprofile-10)# |

### Config FEC Function in ont-lineprofile

|  |  |
| --- | --- |
| Command | OLT(config-epon-lineprofile-10)#fec {enable|disable} |
| **View** | ont-lineprofile view |
| **Description** | This command is used for enable or disable FEC. |

【Example】

Example 1：Enable FEC in ont-lineprofile 10.

|  |
| --- |
| OLT(config-epon-lineprofile-10)#fec enable  OLT(config-epon-lineprofile-10)# |

### Config Data Encryption in ont-lineprofile

|  |  |
| --- | --- |
| Command | OLT(config-epon-lineprofile-10)#llid <llid-id> encrypt {enable|disable} |
| **View** | ont-lineprofile view |
| **Description** | This command is used for enable or disable data encryption. |

【Example】

Example 1：Enable data encryption in ont-lineprofile 10.

|  |
| --- |
| OLT(config-epon-lineprofile-10)#llid 1 encrypt enable  OLT(config-epon-lineprofile-10)# |

### Config ONU-Car in ont-lineprofile

|  |  |
| --- | --- |
| Command | OLT(config-epon-lineprofile-10)#llid <llid-id> ont-car <profile-id> |
| **View** | ont-lineprofile view |
| **Description** | This command is used for bind ont-car and the it is used in conjunction with traffic-profile command in config view. |
| <profile-id> | ont-car id,ont-car is created by traffic-profile command in config view. |

【Example】

Example 1：Bind ont-car 10 in ont-lineprfile 10.

|  |
| --- |
| OLT(config-epon-lineprofile-10)#llid 1 ont-car 10  OLT(config-epon-lineprofile-10)# |

### Config queue thresholds for DBA queue sets

|  |  |
| --- | --- |
| Command | OLT(config-epon-lineprofile-10)# (no) dba-threshold queue-set-index ( q1 value | q2 value | q3 value | q4 value | q5 value | q6 value | q7 value | q8 value ) |
| **View** | Lineprofile view |
| **Description** | This command is used to configure the queue threshold of the DBA queue set in the ONT line profile. Use this command when you need to configure the queue threshold of the DBA queue set in the ONT line profile. |
| queue-set-index | DBA queue set index value, ranging from 1-4 |
| value | Queue threshold, in the range 0-65535 |

【Example】

Example 1：In line template 10, the queue threshold for setting DBA queue set 1 is 512.

|  |
| --- |
| OLT(config-epon-lineprofile-10)# dba-threshold 1 q1 512  OLT(config-epon-lineprofile-10)# |

### Commit ont-lineprofile Configuration

|  |  |
| --- | --- |
| Command | OLT(config-epon-lineprofile-10)#commit |
| **View** | ont-lineprofile view |
| **Description** | This command is used for commit the current ont-lineprofile setting.All the parameter will take effect only after the command is committed. |

【Example】

Example 1：Commit current ont-lineprofile setting.

|  |
| --- |
| OLT(config-epon-lineprofile-10)#commit  OLT(config-epon-lineprofile-10)# |

### Show OLT ont-lineprofile Information

|  |  |
| --- | --- |
| Command | OLT(config)#show ont-lineprofile {all|profile-id <profile-id> |profile-name <profile-name>} |
| **View** | Config view |
| **Description** | This command is used for show ont-lineprofile info. |
| <profile-id> | Ont-lineprofile id to be show. |
| <profile-name> | Ont-lineprofile name to be show. |

【Example】

Example 1：Show ont-lineprofile 10 info.

|  |
| --- |
| OLT(config)#show ont-lineprofile epon profile-id 10  -----------------------------------------------------------------------------  Profile-ID:10  Profile-name:lineprofile\_10  Binding times:0  ----------------------------------------------------------------------------  FEC switch:Disable  Encrypt type:Off  DBA Profile-ID:0  Traffic profile ID:-  DBA-threshold:  ----------------------------------------------------------------------------  Queue-set-index Q1 Q2 Q3 Q4 Q5 Q6 Q7 Q8  ---------------------------------------------------------------------------  1--------  2--------  3--------  4--------  -----------------------------------------------------------------------------  OLT(config)# |

## ont-srvprofile Configuration

### Create ont-srvprofile

|  |  |
| --- | --- |
| Command | OLT(config)#ont-srvprofile epon {profile-id <profile-id> profile-name <profile-name>} |
| **View** | Config view |
| **Description** | This command is used for create ont-srvprofile or enter the created ont-srvprofile editing view.The association attribute of ont service can be set in ont-srvprofile.It needs to bind epon ont-srvprofile for ont when it is added to olt,if the ont-srvprofile is not specified,the system will bind the default ont-srvprofile to ont automatically. |
| <profile-id> | ont-srvprofile id.When it is not specified,system will allocate a minimum idle profile number automatically.the autoauth onu will be matched the ont-srvprofile 0. |
| <profile-name> | Ont-srvprofile name.The default name is ont-srvprofile\_id. |

【Example】

Example 1：Create ont-srvprofile 10 and enter its editing view.

|  |
| --- |
| OLT(config)#ont-srvprofile epon profile-id 10  OLT(config-epon-srvprofile-10)# |

### Config ONU Capability in ont-srvprofile

|  |  |
| --- | --- |
| Command | OLT(config-epon-srvprofile-10)#ont-port eth <number> catv <number> pots <number> |
| **View** | Ont-srvprofile view |
| **Description** | This command is used for set the ont-srvprofile capability set.it can set the number of each kind of port.The config-capability of ont port must be the same with ont real capability. |
| <number> | The number of ont’s port.  Eth:ethernet port  Pots:voice port  Catv:coaxial cable port |

【Example】

Example 1：Set ont capability of ont-profile 10,ethernet port is adaptive and 1 pots port.

|  |
| --- |
| OLT(config-epon-srvprofile-10)#ont-port eth adaptive pots 1  OLT(config-epon-srvprofile-10)# |

### Config ONU Port Native-vlan in ont-lineprofile

|  |  |
| --- | --- |
| Command | OLT(config-epon-srvprofile-10)#port native-vlan eth <port-list> <vlan id> priority <value> |
| **View** | Ont-srvprofile view |
| **Description** | This command is used for set ONU eth port native-vlan |
| <port-list> | Port list to be set |
| <vlan id> | Native-vlan id |
| <value> | vlan priority,range for 0-7,the default is 0. |

【Example】

Example 1：Set the native-vlan of eth1 in ont-srvprofile 10 as 100 and its priority is 0.

|  |
| --- |
| OLT(config-epon-srvprofile-10)#port native-vlan eth 1 100 priority 0  OLT(config-epon-srvprofile-10)# |

### Config ONU Port VLAN in ont-srvprofile

| Command | OLT(config-epon-srvprofile-10)#port vlan eth <port-list> <vlan id> <priority value> |
| --- | --- |
| **View** | Ont-srvprofile view |
| **Description** | This command is used for add ont port to the specified vlan in ont-srvprofile. |
| <port-list> | Port list to be set. |
| <vlan id> | Vlan id |
| <value> | vlan priority,range for 0-7,the default is 0. |

【Example】

Example 1：Add eth1 to vlan 100 in ont-srvprofile 10.

|  |
| --- |
| OLT(config-epon-srvprofile-10)#port vlan eth 1 100 1  OLT(config-epon-srvprofile-10)# |

### Config ONU VLAN Mode in ont-lineprofile

|  |  |
| --- | --- |
| Command | OLT(config-epon-srvprofile-10)#port vlan eth <port-list> <vlan mode> |
| **View** | Ont-srvprofile view |
| **Description** | This command is used for set vlan mode of the ONU port. |
| <vlan mode> | The mode of vlan are as follows:  Transparent,translation,vlan-pool |

【Example】

Example 1：Set vlan mode of eth 1 as vlan-pool 1 in ont-srvprofile 10,the vlan of eth 1 will be allocated by vlan-pool 1.

|  |
| --- |
| OLT(config-epon-srvprofile-10)#port vlan eth 1 vlan-pool 1  OLT(config-epon-srvprofile-10)# |

### Config ONU Port Multicast VLAN in ont-lineprofile

| Command | OLT(config-epon-srvprofile-10)#port multicast-vlan eth <port-list> <vlan id> |
| --- | --- |
| **View** | Ont-srvprofile view |
| **Description** | This command is used for set multicast vlan of ont’s port |
| <vlan id> | Multicast valn id |

【Example】

Example 1：Set multicast-vlan of eth1 as 100.

|  |
| --- |
| OLT(config-epon-srvprofile-10)#port multicast-vlan eth 1 100  OLT(config-epon-srvprofile-10)# |

### Config ONU Port Downstream Rate limit in ont-lineprofile

|  |  |
| --- | --- |
| Command | OLT(config-epon-srvprofile-10)#port eth 1 ds-policing {unconcern|<profile id>} |
| **View** | Ont-srvprofile view |
| **Description** | This command is used for set downstream rate limitation of ont port |
| unconcern | There is no rate limitation with downstream |
| <Profile ID> | traffic-profile id,it must be created in config view before it is called. |

【Example】

Example 1：Set eth1 downstream rate limitation,match eth1 to traffic-profile 20.

|  |
| --- |
| OLT(config-epon-srvprofile-10)#port eth 1 ds-policing 20  OLT(config-epon-srvprofile-10)# |

### Config ONU Port Upstream Rate limit in ont-lineprofile

|  |  |
| --- | --- |
| Command | OLT(config-epon-srvprofile-10)#port eth 1 up-policing {unconcern|<profile id>} |
| **View** | Ont-srvprofile view |
| **Description** | This command is used for set upstream rate limitation of ont port |
| unconcern | There is no rate limitation with downstream |
| <Profile ID> | traffic-profile id,it must be created in config view before it is called. |

【Example】

Example 1：Set eth1 upstream rate limitation,match eth1 to traffic-profile 20.

|  |
| --- |
| OLT(config-epon-srvprofile-10)#port eth 1 up-policing 20  OLT(config-epon-srvprofile-10)# |

### Config ONU Port MAC Count Limit in ont-lineprofile

|  |  |
| --- | --- |
| Command | OLT(config-epon-srvprofile-10)#port eth <port-list> max-mac-count {unlimited|<max mac count>} |
| **View** | Ont-srvprofile view |
| **Description** | This command is used for set max-mac-count of ont port. |
| unlimited | There is no rate limitation with mac address. |
| <max mac count> | The max mac address number,range for 1-64. |

【Example】

Example 1：Set max-mac-count of eth1 as 10 entries.

|  |
| --- |
| OLT(config-epon-srvprofile-10)#port eth 1 max-mac-count 10  OLT(config-epon-srvprofile-10)# |

### Config ONU Port IGMP Number in ont-lineprofile

|  |  |
| --- | --- |
| Command | OLT(config-epon-srvprofile-10)#port eth <port-list> group-num-max <max group num> |
| **View** | Ont-srvprofile view |
| **Description** | This command is used for set multicast group-num-max of ont port |
| <Max group num> | The max multicast group number,range for 0-255 |

【Example】

Example 1：Set the max multicast group number of eth1 as 20.

|  |
| --- |
| OLT(config-epon-srvprofile-10)#port eth 1 group-num-max 20  OLT(config-epon-srvprofile-10)# |

### Config ONU Port IGMP VLAN Process Mode in ont-lineprofile

|  |  |
| --- | --- |
| Command | OLT(config-epon-srvprofile-10)#port eth <port-list> multicast-tagstrip {tag|untag|translation} |
| **View** | Ont-srvprofile view |
| **Description** | This command is used for set vlan processing mode of ont port’s multicast stream. |
| tag|untag|translation | Tag:Add VLAN tag  Untag:Peel off VLAN tag  translation：translate vlan |

【Example】

Example 1：Set multicast vlan processing mode of eth1 as tag mode in ont-srvprofile.

|  |
| --- |
| OLT(config-epon-srvprofile-10)#port eth 1 multicast-tagstrip tag  OLT(config-epon-srvprofile-10)# |

### Config ONU IGMP Fast-leave Function in ont-lineprofile

|  |  |
| --- | --- |
| Command | OLT(config-epon-srvprofile-10)#multicast fast-leave {enable|disable} |
| **View** | Ont-srvprofile view |
| **Description** | This command is used for set ONU multicast fast-leave |
| {enable|disable} | Enable:enable multicast fast-leave  Disable:disable multicast fast-leave |

【Example】

Example 1：Enable multicast fast-leave

|  |
| --- |
| OLT(config-epon-srvprofile-10)#multicast fast-leave enable  OLT(config-epon-srvprofile-10)# |

### Enable or Disable ONU Loop Detect Function in ont-lineprofile

|  |  |
| --- | --- |
| Command | OLT(config-epon-srvprofile-10)#ring check { auto-shutdown no-recovery} |enable|disable |
| **View** | Ont-srvprofile view |
| **Description** | This command is used for set ring check function |
| {enable|disable} | Enable:enable ring check function  Disable:disable ring check function |

【Example】

Example 1：Enable ring check function in ont-srvprofile 10.

|  |
| --- |
| OLT(config-epon-srvprofile-10)#ring check enable  OLT(config-epon-srvprofile-10)# |

### Show ont-srvprofile Current Configuration

|  |  |
| --- | --- |
| Command | OLT(config-epon-srvprofile-10)#show ont-srvprofile current |
| **View** | Ont-srvprofile view |
| **Description** | This command is used for show current configuration of ont-srvprofile |

【Example】

Example 1：Show current configuration of ont-srvprofile

|  |
| --- |
| OLT(config-epon-srvprofile-10)#show ont-srvprofile current  -----------------------------------------------------------------------------  Profile-ID:10  ----------------------------------------------------------------------------  Port-type Port-number  ---------------------------------------------------------------------------  ETH adaptive  POTS 0  CATV 0  ----------------------------------------------------------------------------  Multicast fast leave switch:Enable  Ring check switch:Enable  ----------------------------------------------------------------------------  Port Port Up-traffic Down-traffic MAC-learn Classification  type ID CAR-ID CAR-ID count  ---------------------------------------------------------------------------  ETH 1 20 20 10 None  ETH 2 Unconcern Unconcern Unlimited None  ETH 3 Unconcern Unconcern Unlimited None  ETH 4 Unconcern Unconcern Unlimited None  ETH 5 Unconcern Unconcern Unlimited None  ETH 6 Unconcern Unconcern Unlimited None  ETH 7 Unconcern Unconcern Unlimited None  ETH 8 Unconcern Unconcern Unlimited None  ----------------------------------------------------------------------------  Port Port Multicast Multicast Multicast Multicast  type ID S-VLAN C-VLAN tag-strip group-num  ---------------------------------------------------------------------------  ETH 1--Tag 20  ETH 2--Tag 64  ETH 3--Tag 64  ETH 4--Tag 64  ETH 5--Tag 64  ETH 6--Tag 64  ETH 7--Tag 64  ETH 8--Tag 64  ----------------------------------------------------------------------------  Port Port Service-type Index N-VLAN N-PRI S-VLAN S-PRI C-VLAN C-PRI  type ID  ---------------------------------------------------------------------------  ETH 1 Transparent-------  ETH 2 Transparent-------  ETH 3 Transparent-------  ETH 4 Transparent-------  ETH 5 Transparent-------  ETH 6 Transparent------- |

### Commit ont-srvprofile Configuration

|  |  |
| --- | --- |
| Command | OLT(config-epon-srvprofile-10)#commit |
| **View** | Ont-srvprofile view |
| **Description** | This command is used for commit the current ont-srvprofile setting.All the parameter will take effect only after the command is committed. |

【Example】

Example 1：Commit current ont-srvprofile setting

|  |
| --- |
| OLT(config-epon-srvprofile-10)#commit  OLT(config-epon-srvprofile-10)# |

## ont-slaprofile Configuration

### Creat ont-slaprofile

| Command | OLT(config)# ont-slaprofile profile-id <profile-id > profile-name <profile-name> |
| --- | --- |
| **View** | SLA profile view |
| **Description** | This command is used to add the SLA (Service Level Agreement) template and enter the SLA template configuration mode. |
| <profile-id > | SLA template number. If not specified, the system automatically assigns the smallest idle template number. Template 0 is the default template for the system. |
| <profile-name> | SLA template name. If not specified, the system automatically adopts the default name "sla\_x", where "x" is the number of the SLA template. |

【Example】

Example 1：Create a new sla template with id 1. The template name is named by default and enters the sla template configuration mode.

|  |
| --- |
| OLT(config)# ont-slaprofile profile-id 1  OLT(sla-1)# |

### Config the Cycle Length of the SLA Template.

|  |  |
| --- | --- |
| Command | OLT(sla-1)# cycle-length <cycle-length> |
| **View** | SLA profile view |
| **Description** | This command is used to configure the period length of an SLA template. |
| <cycle-length> | Period length, in the range of 200-16777215, default is 25000 |

【Example】

Example 1：Configure the SLA template id1 to be 2048.

|  |
| --- |
| OLT(sla-1)# cycle-length 2048  OLT(sla-1)# |

### Config the Number of Services for the SLA Profile

| Command | OLT(sla-1)# services-num <number-of-service> |
| --- | --- |
| **View** | SLA profile view |
| **Description** | This command is used to configure the number of services in the SLA profile. The template supports eight service SLAs, and the priority increases as the SLA number increases. |
| <number-of-service> | Number of services, ranging from 1-8 |

【Example】

Example 1：Set the number of services of the SLA template id1 to 2.

|  |
| --- |
| OLT(sla-1)# services-num 2  OLT(sla-1)# |

### Config the Service Parameters of the SLA Profile.

| Command | OLT(sla-1)# service <service-id> fix 0|<fixed-packets-size> <fixed-bandwidth> guarante <guaranteed-bandwidth> best-effort <best-effort-bandwidth> wrr-weight <wrr-weight> |
| --- | --- |
| **View** | SLA profile view |
| **Description** | This command is used to configure the number of services in the SLA profile. The template supports eight service SLAs, and the priority increases as the SLA number increases. |
| <service-id> | Service index value, ranging from 1 to 8. |
| 0|<fixed-packets-size> | Fixed packet size of the specified service, in the range of 64-2000, unit is bytes. |
| <fixed-bandwidth> | Specifies the fixed bandwidth of the service, in the range of 0-999936, unit is kbps. |
| <guaranteed-bandwidth> | Specifies the guaranteed bandwidth of the service, in the range of 0-999936, unit is kbps. |
| <best-effort-bandwidth> | Specifies the best-effort bandwidth of the service, ranging from 0 to 999936,unit is kbps |
| <wrr-weight> | The weight of the specified service, ranging from 0 to 100. |

【Example】

Example 1：Configure the service parameters of the SLA template id1.

|  |
| --- |
| OLT(sla-1)# service 1 fix 1024 102400 guarante 102400 best-effort 102400 wrr-weight 0  OLT(sla-1)# |

### Commit ont-slaprofile Configuration

|  |  |
| --- | --- |
| Command | OLT(sla-1)# commit |
| **View** | SLA profile view |
| **Description** | This command is used to submit the configuration of the current SLA template. After the configuration is successful, all parameter configurations of the service template take effect. |

【Example】

Example 1：Commit the current SLA template configuration

|  |
| --- |
| OLT(sla-1)# commit  OLT(sla-1)# |

### Show ont-slaprofile Current Configuration

|  |  |
| --- | --- |
| Command | OLT(config)# show traffic-profile {all|profile-id < Profile ID>|profile-name <Profile name>} |
| **View** | SLA profile view |
| **Description** | This command is used to view traffic template parameters. |
| <Profile ID> | ID of the traffic profile, ranging from 1 to 256. |
| <Profile name> | Name of the traffic profile, in the range of 1 to 16. |

【Example】

Example 1 : Show the configuration of all current traffic templates

|  |
| --- |
| OLT(sla-1)# show ont-slaprofile current  -----------------------------------------------------------------------------  Profile-ID : 1  ----------------------------------------------------------------------------  Cycle length (TQ) : 25000  Number of services : 2  Fixed packet size of service 1 (Bytes) : 1024  Fixed bandwidth of service 1 (kbps) : 102400  Guaranteed bandwidth of service 1 (kbps) : 102400  Best effort bandwidth of service 1 (kbps) : 102400  WRR weight of service 1 : 0  Fixed packet size of service 2 (Bytes) : 0  Fixed bandwidth of service 2 (kbps) : 0  Guaranteed bandwidth of service 2 (kbps) : 0  Best effort bandwidth of service 2 (kbps) : 0  WRR weight of service 2 : 0  -----------------------------------------------------------------------------  OLT(sla-1)# |

## OLT traffic-profile Configuration

### Create traffic-profile

| Command | OLT(config)#traffic-profile profile-id <profile id> profile-name <profile name> cir <parameter> pir <parameter> cbs <parameter> pbs <parameter> |
| --- | --- |
| **View** | Config view |
| **Description** | This command is used for create traffic-profile and set traffic-profile parameters to coordinate with rate limitation. |
| <Profile ID> | traffic-profile id,range for 1-256 |
| <profile name> | traffic-profile name,range for 1-16 |
| cir | Committed Information Rate,range for 64-10240000,unit is kbps |
| pir | Peek Information Rate,range for 64-10240000,unit is kbps |
| cbs | Committed Burst Size,range for 2000-10240000,unit is byte |
| pbs | Peek Burst Size,range for 2000-10240000,uni is byte |

【Example】

Example 1：Create traffic profile 10,name it as test1,set cir as 128,pir as 256,cbs as 2000,pbs as 3000.

|  |
| --- |
| OLT(config)#traffic-profile profile-id 10 profile-name test1 cir 128 pir 256 cbs 2000 pbs 3000  OLT(config)# Example 1：Create traffic profile 10,name it as test1,set cir as 128,pir as 256,cbs as 2000,pbs as 3000.  Example 1：Create traffic profile 10,name it as test1,set cir as 128,pir as 256,cbs as 2000,pbs as 3000. |

### Modify traffic-profile

|  |  |
| --- | --- |
| Command | OLT(config)#traffic-profile modify {profile Id|profile name} {|cir|pir|cbs|pbs} |
| **View** | Config view |
| **Description** | This command is used for modify the traffic-profile. |
| <Profile ID> | Profile id,range for 1-256 |
| <profile name> | Profile name,range for 1-16 |
| cir | Committed Information Rate,range for 64-10240000,unit is kbps |
| pir | Peek Information Rate,range for 64-10240000,unit is kbps |
| cbs | Committed Burst Size,range for 2000-10240000,unit is byte |
| pbs | Peek Burst Size,range for 2000-10240000,uni is byte |

【Example】

Example 1：Modify cir as 150 in traffic-profile 10.

|  |
| --- |
| OLT(config)#traffic-profile modify profile-id 10 cir 150  OLT(config)# |

### Show OLT traffic-profile Information

|  |  |
| --- | --- |
| Command | OLT(config)#show traffic-profile all|profile id|profile name |
| **View** | Config view |
| **Description** | This command is used for show traffic-profile info |
| <Profile ID> | Profile id,range for 1-256 |
| <Profile name> | Profile name,range for 1-16 |

【Example】

Example 1：Show all of traffic-profile info.

|  |
| --- |
| OLT(config)#show traffic-profile all  -----------------------------------------------------------------------------  ID Profile-name CIR(kbps)PIR(kbps)CBS(bytes)PBS(bytes)Bind  ----------------------------------------------------------------------------  10 test1 150 256 2000 3000 0  20 test 222 222 2000 2000 2  -----------------------------------------------------------------------------  Total:2  OLT(config)# |

## Config Alarm Profile

### Creat Low Alarm Profile

| Command | OLT(config)# alarm-profile epon profile-id profile-id pofile-name profile-name (rx-crcerrors-alarm|rx-discards-alarm|rx-dropevents-alarm|rx-errors-alarm|rx-fragments-alarm|rx-jabbers-alarm|rx-oversizes-alarm|rx-undersizes-alarm|tx-crcerrors-alarm|tx-discards-alarm|tx-dropevents-alarm|tx-errors-alarm|tx-fragments-alarm|tx-jabbers-alarm|tx-oversizes-alarm|tx-undersizes-alarm) Threshold Restore-threshold |
| --- | --- |
| **View** | Config view |
| **Description** | This command is used for ONU bind to alarm profile. In the alarm profile, config a series of alarm parameter used for minitor onu performance. After set successfully, ONU will cite recoresponding parameters in alarm profile to minitor the ports performance. |
| profile-id | Alarm profile id. Range for 1-50. The default alarm id is 0, in it the alarm parameter values are all disable. |
| profile-name | Alarm profile name, length for 1-16 |
| rx-crcerrors-alarm | Upstream CRC error messages are reported when the number of messages exceeds the set alarm threshold |
| rx-discards-alarm | Upstream discard messages are reported when the number of messages exceeds the set alarm threshold |
| rx-dropevents-alarm | Upstream drop messages are reported when the number of messages exceeds the set alarm threshold |
| rx-errors-alarm | Upstream error messages are reported when the number of messages exceeds the set alarm threshold |
| rx-fragments-alarm | Upstream fragments messages are reported when the number of messages exceeds the set alarm threshold |
| rx-jabbers-alarm | Upstream jabbers messages are reported when the number of messages exceeds the set alarm threshold |
| rx-oversizes-alarm | Upstream oversize messages are reported when the number of messages exceeds the set alarm threshold |
| rx-undersizes-alarm | Upstream undersize messages are reported when the number of messages exceeds the set alarm threshold |
| tx-crcerrors-alarm | Downstream CRC error messages are reported when the number of messages exceeds the set alarm threshold |
| tx-discards-alarm | Downstream discard messages are reported when the number of messages exceeds the set alarm threshold |
| tx-dropevents-alarm | Downstream drop messages are reported when the number of messages exceeds the set alarm threshold |
| tx-errors-alarm | Downstream error messages are reported when the number of messages exceeds the set alarm threshold |
| tx-fragments-alarm | Downstream fragments messages are reported when the number of messages exceeds the set alarm threshold |
| tx-jabbers-alarm | Downstream jabbers messages are reported when the number of messages exceeds the set alarm threshold |
| tx-oversizes-alarm | Downstream oversize messages are reported when the number of messages exceeds the set alarm threshold |
| tx-undersizes-alarm | Downstream undersize messages are reported when the number of messages exceeds the set alarm threshold |
| Threshold | The threshold value,range for 0-4294967294 |
| Restore-threshold | The restore threshold,range for 0-4294967294 |

【Example】

Example1：Creat a new alarm profile 1,named test.And set upstream crc errors threshold is 100 and the restore threshold is 50.

|  |
| --- |
| OLT(config)# alarm-profile epon profile-id 1 profile-name test rx-crcerrors-alarm 100 50  OLT(config)# |

### Creat High Alarm Profile

| Command | OLT(config)# alarm-profile epon profile-id profile-id pofile-name profile-name (rx-crcerrors-warning|rx-discards-warning|rx-dropevents-warning|rx-errors-warning|rx-fragments-warning|rx-jabbers-warning|rx-oversizes-warning|rx-undersizes-warning|tx-crcerrors-warning|tx-discards-warning|tx-dropevents-warning|tx-errors-warning|tx-fragments-warning|tx-jabbers-warning|tx-oversizes-warning|tx-undersizes-warning) Threshold Restore-threshold |
| --- | --- |
| **View** | config view |
| **Description** | This command is used for ONU bind to alarm profile. In the alarm profile, config a series of alarm parameter used for minitor onu performance. After set successfully, ONU will cite recoresponding parameters in alarm profile to minitor the ports performance. |
| *profile-id* | Alarm profile id. Range for 1-50. The default alarm id is 0, in it the alarm parameter values are all disable. |
| profile-name | Alarm profile name, length for 1-16 |
| rx-crcerrors-warning | Upstream CRC error messages are reported when the number of messages exceeds the set alarm threshold |
| rx-discards-warning | Upstream discard messages are reported when the number of messages exceeds the set alarm threshold |
| rx-dropevents-warning | Upstream drop messages are reported when the number of messages exceeds the set alarm threshold |
| rx-errors-warning | Upstream error messages are reported when the number of messages exceeds the set alarm threshold |
| rx-fragments-warning | Upstream fragments messages are reported when the number of messages exceeds the set alarm threshold |
| rx-jabbers-warning | Upstream jabbers messages are reported when the number of messages exceeds the set alarm threshold |
| rx-oversizes-warning | Upstream oversize messages are reported when the number of messages exceeds the set alarm threshold |
| rx-undersizes-warning | Upstream undersize messages are reported when the number of messages exceeds the set alarm threshold |
| tx-crcerrors-warning | Downstream CRC error messages are reported when the number of messages exceeds the set alarm threshold |
| tx-discards-warning | Downstream discard messages are reported when the number of messages exceeds the set alarm threshold |
| tx-dropevents-warning | Downstream drop messages are reported when the number of messages exceeds the set alarm threshold |
| tx-errors-warning | Downstream error messages are reported when the number of messages exceeds the set alarm threshold |
| tx-fragments-warning | Downstream fragments messages are reported when the number of messages exceeds the set alarm threshold |
| tx-jabbers-warning | Downstream jabbers messages are reported when the number of messages exceeds the set alarm threshold |
| tx-oversizes-warning | Downstream oversize messages are reported when the number of messages exceeds the set alarm threshold |
| tx-undersizes-warning | Downstream undersize messages are reported when the number of messages exceeds the set alarm threshold |
| Threshold | The threshold value,range for 0-4294967294 |
| Restore-threshold | The restore threshold,range for 0-4294967294 |

【Example】

Example1：Creat a new alarm profile 2,named test2. And set upstream discard messages threshold is 20 and the restore threshold is 10.

|  |
| --- |
| OLT(config)# alarm-profile epon profile-id 2 profile-name test2 rx-discards-warning 20 10.  OLT(config)# |

### Show Alarm Profile

| Command | OLT(config)# show alarm-profile epon (all|profile-id profile-id |pofile-name profile-name) bound-info |
| --- | --- |
| **View** | Config view |
| **Description** | This command is used for show alarm profile which has been created. |
| profile-id | Alarm profile id,range for 0-50 |
| profile-name | Alarm profile name, length range for 1-16 |

【Example】

Example1：Show alarm profile id 1

|  |
| --- |
| OLT(config)# show alarm-profile epon profile-id 1  -----------------------------------------------------------------------------  Profile-ID : 1  Profile-name : test  Binding times : 0  ----------------------------------------------------------------------------  <Drop events alarm/warning>:  Transmitted drop events alarm: disable  Transmitted drop events warning: disable  Received drop events alarm: disable  Received drop events warning: disable  <CRC error alarm/warning>:  Transmitted CRC error frames alarm: disable  Transmitted CRC error frames warning: disable  Received CRC error frames alarm threshold: 100  Received CRC error frames alarm restore threshold: 50  Received CRC error frames warning: disable  <Undersize frames alarm/warning>:  Transmitted undersize frames alarm: disable  Transmitted undersize frames warning: disable  Received undersize frames alarm: disable  Received undersize frames warning: disable  <Oversize frames alarm/warning>:  Transmitted oversize frames alarm: disable  Transmitted oversize frames warning: disable  Received oversize frames alarm: disable  Received oversize frames warning: disable  <Fragments alarm/warning>:  Transmitted fragments alarm: disable  Transmitted fragments warning: disable  Received fragments alarm: disable  Received fragments warning: disable  <Jabbers alarm/warning>:  Transmitted jabbers alarm: disable  Transmitted jabbers warning: disable  Received jabbers alarm: disable  Received jabbers warning: disable  <Discards alarm/warning>:  Transmitted discards alarm: disable  Transmitted discards warning: disable  Received discards alarm: disable  Received discards warning: disable  <Errors alarm/warning>  Transmitted errors alarm: disable  Transmitted errors warning: disable  Received errors alarm: disable  Received errors warning: disable  -----------------------------------------------------------------------------  OLT(config)# |

### Delete Alarm Profile

| Command | OLT(config)# no alarm-profile epon (profile-id profile-id |pofile-name profile-name) |
| --- | --- |
| **View** | config view |
| **Description** | This command is used for delete alarm profile. |
| profile-id | Alarm profile id. Range for 1-50. The default alarm id is 0, in it the alarm parameter values are all disable. |
| profile-name | Alarm profile name, length for 1-16 |

【Example】

Example1：Delete alarm profile id 1

|  |
| --- |
| OLT(config)# no alarm-profile epon profile-id 1  OLT(config)# |

## Optical-alarm-profile Configuration

### Creat Optical Low Alarm Template

| Command | OLT(config)# optical-alarm-profile profile-id profile-id pofile-name profile-name (bias-high-alarm|bias-low-alarm|rx-power-high-alarm|rx-power-low-alarm|temperature-high-alarm|temperature-low-alarm|tx-power-high-alarm|tx-power-low-alarm|voltage-high-alarm|voltage-low-alarm) Threshold Restore-threshold |
| --- | --- |
| **View** | Config view |
| **Description** | This command is used to create a low alarm template for an optical module. Use this command when you need to adjust certain parameters of the optical module alarm template. |
| <Profile ID> | ID of the optical module template, ranging from 0 to 50. |
| <profile name> | Name of the optical module template, ranging from 1 to 24. |
| bias-high-alarm | Bias current threshold alarm upper limit value, ranging from 0 to 100, in mA |
| bias-low-alarm | Bias current threshold alarm lower limit value, ranging from 0 to 100, in mA |
| rx-power-high-alarm | Received optical power threshold alarm upper limit, in the range of -99-100, in dBm |
| rx-power-low-alarm | Received optical power threshold alarm upper limit, in the range of -99-100, in dBm |
| temperature-high-alarm | Upper limit of temperature threshold alarm, ranging from -99 to 300, unit：℃ |
| temperature-low-alarm | Lower threshold of the temperature threshold alarm, ranging from -99 to 300.unit：℃ |
| tx-power-high-alarm | Upper limit of the transmitted optical power threshold alarm, in the range of -99-100, in dBm |
| tx-power-low-alarm | The lower limit of the transmitted optical power threshold alarm, in the range of -99-100, in dBm |
| voltage-high-alarm | The upper limit of the power supply voltage threshold warning, the value range is 0-100, the unit is V |
| voltage-low-alarm | Supply voltage threshold warning lower limit, the value range is 0-100, the unit is V |
| Threshold | Threshold |
| Restore-threshold | Restore threshold |

【Example】

Example 1：Create an optical module with a low alarm profile id of 1, name test, set the bias current threshold to 150 mA, and restore the threshold to 100 mA.

|  |
| --- |
| OLT(config)# optical-alarm-profile profile-id 1 profile-name test bias-high-alarm 150 100  OLT(config)# |

### Creat Optical High Alarm Template

| Command | OLT(config)# optical-warning-profile profile-id profile-id pofile-name profile-name (bias-high-warning|bias-low-warning|rx-power-high-warning|rx-power-low-warning|temperature-high-warning|temperature-low-warning|tx-power-high-warning|tx-power-low-warning|voltage-high-warning|voltage-low-warning) Threshold Restore-threshold |
| --- | --- |
| **View** | Config view |
| **Description** | This command is used to create a high alarm template for an optical module. Use this command when you need to adjust certain parameters of the optical module alarm template. |
| <Profile ID> | ID of the optical module template, ranging from 0 to 50. |
| <profile name> | Name of the optical module template, ranging from 1 to 24. |
| bias-high-warning | Bias current threshold warning upper limit value, ranging from 0 to 100, in mA |
| bias-low-warning | Bias current threshold warning lower limit value, ranging from 0 to 100, in mA |
| rx-power-high-warning | Received optical power threshold warning upper limit, in the range of -99-100, in dBm |
| rx-power-low-warning | Received optical power threshold warning upper limit, in the range of -99-100, in dBm |
| temperature-high-warning | Upper limit of temperature threshold warning, ranging from -99 to 300, unit：℃ |
| temperature-low-warning | Lower threshold of the temperature threshold warning, ranging from -99 to 300.unit：℃ |
| tx-power-high-warning | Upper limit of the transmitted optical power threshold warning, in the range of -99-100, in dBm |
| tx-power-low-warning | The lower limit of the transmitted optical power threshold warning, in the range of -99-100, in dBm |
| voltage-high-warning | The upper limit of the power supply voltage threshold warning, the value range is 0-100, the unit is V |
| voltage-low-warning | Supply voltage threshold warning lower limit, the value range is 0-100, the unit is V |
| Threshold | Threshold |
| Restore-threshold | Restore threshold |

【Example】

Example 1：The low alarm profile id of the optical module is 2, and the name is test2. The alarm threshold is set to 200 V and the recovery threshold is 100 V.

|  |
| --- |
| OLT(config)# optical-alarm-profile profile-id 2 profile-name test2 temperature-high-warning 200 100  OLT(config)# |

### Show Optical-alarm-profile

|  |  |
| --- | --- |
| Command | OLT(config)# show optical-alarm-profile {all|profile-id < Profile ID>|profile-name <Profile name> bound-info} |
| **View** | Config view |
| **Description** | This command is used to view the parameters of the optical module alarm template and the binding status. |
| <Profile ID> | ID of the alarm template of the optical module, ranging from 0 to 50. |
| <Profile name> | Name of the alarm template of the optical module. The value ranges from 1 to 24. |

【Example】

Example 1 :View the configuration of all current optical module templates.

|  |
| --- |
| OLT(config)# show optical-alarm-profile all  -----------------------------------------------------------------------------  Profile-ID Profile-name Binding times  ----------------------------------------------------------------------------  0 optical-alarm-profile\_0 0  1 test 0  2 test2 0  -----------------------------------------------------------------------------  Total: 3  OLT(config)# |

## OLT VLAN Pool Configuration

### Create VLAN Pool

|  |  |
| --- | --- |
| Command | OLT(config)#vlan-pool add <vlan pool id> start-vid <vlan id> end-vid <vlan-id> <no-reused|reused> |
| **View** | Config view |
| **Description** | This command is used for create vlan-pool. |
| <VLAN pool ID> | Vlan-pool id,range for 1-128 |

【Example】

Example 1：Create vlan-pool 1,its range is start-vid 100 to end-vid 200.

|  |
| --- |
| OLT(config)#vlan-pool add 1 start-vid 100 end-vid 200  OLT(config)# |

### Modify VLAN Pool

| Command | OLT(config)#vlan-pool modify <vlan pool id> start-vid <vlan id> end-vid <vlan-id> |
| --- | --- |
| **View** | Config view |
| **Description** | This command is used for modify the parameter of vlan-pool |
| <vlan pool id> | Vlan-pool id,range for 1-128 |

【Example】

Example 1：Modify vlan-pool 1,its range is start-vid 100 to end-vid 300.

|  |
| --- |
| OLT(config)#vlan-pool modify 1 start-vid 200 end-vid 300  OLT(config)# |

### Delete VLAN Pool

|  |  |
| --- | --- |
| Command | OLT(config)#no vlan-pool <vlan pool id> |
| **View** | Config view |
| **Description** | This command is used for delete vlan-pool. |
| <vlan pool id> | Vlan-pool id,range for 1-128 |

【Example】

Example 1：Delete vlan-pool 1.

|  |
| --- |
| OLT(config)#no vlan-pool 1  OLT(config)# |

### Show OLT VLAN Pool Information

| Command | OLT(config)#show vlan-pool {all|<vlan pool id>} |
| --- | --- |
| **View** | Config view |
| **Description** | This command is used for show configuration info of vlan-pool. |
| <vlan pool id> | Vlan-pool id,range for 1-128 |

【Example】

Example 1：Show configuration info of all the vlan-pool.

|  |
| --- |
| OLT(config)#show vlan-pool all  -----------------------------------------------------------------------------  VLAN-Pool Start-VID End-VID  ----------------------------------------------------------------------------  1 200 300  -----------------------------------------------------------------------------  OLT(config)# |

# ONU Management

## ONU Authentication Management

### Enable or Disable ONU Autofind Function

|  |  |
| --- | --- |
| Command | OLT(config-interface-epon-0/0)#ont autofind <port-id> {enable|disable} |
| **View** | EPON interface view |
| **Description** | This command is used for enable or disable ont autofind function in pon port |
| <port-id> | Pon port id,range for 1-16 |
| {enable|disable} | Enable  Disable |

【Example】

Example 1：Disable ont autofind function in pon 1.

|  |
| --- |
| OLT(config-interface-epon-0/0)#ont autofind 1 disable  OLT(config-interface-epon-0/0)# |

### Show Autofind ONU

|  |  |
| --- | --- |
| Command | OLT(config-interface-epon-0/0)#show ont autofind <port-id> {all|mac|llid} |
| **View** | EPON interface view |
| **Description** | This command is used for show basic info of autofind ont.when adding ont,it can show mac address,autofind time and etc info of unauthentication ont. |
| <port-id> | Pon port id,range for 1-16 |
| {all|mac|llid} | All:Show all the autofind ont in the pon port.  Mac:Show the autofind ont according to the mac address in the pon port.  Llid:Show the autofind ont according to the llid in the pon port. |

【Example】

Example 1：Show all the autofind ont in pon 1.

|  |
| --- |
| OLT(config-interface-epon-0/0)#show ont autofind 1 all  -----------------------------------------------------------------------------  Index MAC Autofind-Time  ----------------------------------------------------------------------------  1 E0:67:B3:AA:BB:0C 2000-01-01 00:01:37  2 00:01:62:45:66:05 2000-01-01 08:02:24  3 00:01:62:45:99:07 2000-01-01 08:02:25  -----------------------------------------------------------------------------  Total:3 Total:3  -----------------------------------------------------------------------------  -----------------------------------------  OLT(config-interface-epon-0/0)# |

### Aging time configuration of offline ONT

|  |  |
| --- | --- |
| Command | OLT(config)# ont auto-aging (time|scan-interval interval|default) |( switch on|off) |
| **View** | Config view |
| **Descrition** | This command is used to set the automatic aging time for ONT registration. |
| interval | Set the automatic aging interval of the ONT, in the range of 1-180, in days. |
| default | Time default time is 30 days  Scan-interval scan interval default time is 7 days |
| on|off | Enables/disables the automatic aging time of ONT registration. Automatically clear long-time offline ONUs and automatically overwrite long-time offline ONUs after 64 |

【Example】

Example 1：Enable the automatic aging time of the ONT registration and set the automatic aging time of the ONT to 20 days.

|  |
| --- |
| OLT(config)# ont auto-aging switch on  OLT(config)# ont auto-aging time 20  OLT(config)# |

### Config the ONT registration migration detection switch

|  |  |
| --- | --- |
| Command | OLT(config)# ont moving-check enable|disable |
| **View** | config view |
| **Description** | This command is used to configure the ONT registration migration detection switch. |

【Example】

Example 1：Enable ONT registration migration detection.

|  |
| --- |
| OLT(config)# ont moving-check enable  OLT(config)# |

### MAC Address Method Authenticated ONU And Bind Profile

| Command | OLT(config-interface-epon-0/0)#ont add <port-id> <onu-id> mac-auth <mac-address> {ont-lineprofile-id<profile-id>|ont-lineprofile-name<profile-name>} {ont-srvprofile-id <profile-id>|ont-srvprofile-name<profile-name>} |
| --- | --- |
| **View** | EPON interface view |
| **Description** | This command is used for authenticate onu by mac-auth and bind the ont-lineprofile and ont-srvprofile.olt will check whether the mac reported by ont is the same with the setting mac,if yes,ont will online normally. |
| <port-id> | Pon port id,range for 1-16 |
| <onu-id> | Ont id,range for 1-64 |
| <mac-address> | Mac address of ont,format for xx:xx:xx:xx:xx:xx |
| <profile-id> | Profile id,0-512 |
| <profile-name> | Profile name,it supports 1-16 strings. |

【Example】

Example 1：Add an ont in pon1 and bind it to ont-lineprofile 5 and ont-srvprofile 5.

|  |
| --- |
| OLT(config-interface-epon-0/0)#ont add 1 9 mac-auth 11:11:11:11:11:11 ont-lineprofile-id 5 ont-srvprofile-id 5  OLT(config-interface-epon-0/0)# |

### Loid Method Authenticated ONU and Bind Profile

|  |  |
| --- | --- |
| Command | OLT(config-interface-epon-0/0)#ont add <port-id> <onu-id> loid-auth <loid> { ont-lineprofile-id <profile-id>| ont-lineprofile-name } {<profile-name> ont-srvprofile-id <profile-id>|ont-srvprofile-name <profile-name> } { always | once-aging | once-no-aging} |
| **View** | epon view |
| **Description** | This command is used for authenticate onu by loid-auth and bind the ont-lineprofile and ont-srvprofile.olt will check whether the loid reported by ont is the same with the setting loid,if yes,ont will online normally. |
| <port-id> | Pon port id,range for 1-16 |
| <onu-id> | Ont id,range for 1-64 |
| <loid> | Loid of ont,it supports 1-24 strings |
| <profile-id> | Profile id,0-512 |
| <profile-name> | Profile name,it supports 1-16 strings. |
| {always|once-aging|once-no-aging} | Always:ont can be authenticated at any time  once-aging:ont only can be authenticated for once time within the allotted time,ont will be cleared once it is offline.  once-no-aging:no limitation in authentication time for ont,but it will be cleared once it is offline. |

【Example】

Example 1：Add an ont in pon1 and bind it to ont-lineprofile 5 and ont-srvprofile 5.

|  |
| --- |
| OLT(config-interface-epon-0/0)#ont add 1 10 loid-auth loid ont-lineprofile-id 5 ont-srvprofile-id 5 always  OLT(config-interface-epon-0/0)# |

### Loid+Password Method Authenticated ONU and Bind Profile

|  |  |
| --- | --- |
| Command | OLT(config-interface-epon-0/0)#ont add <port-id> <onu-id> loid-auth <loid> password <password> { ont-lineprofile-id <profile-id>| ont-lineprofile-name <profile-name> } {ont-srvprofile-id <profile-id>|ont-srvprofile-name <profile-name> } { always | once-aging | once-no-aging} |
| **View** | EPON interface view |
| **Description** | This command is used for authenticate onu by loid-auth and password-auth and bind the ont-lineprofile and ont-srvprofile.olt will check whether the loid and password reported by ont is the same with the setting loid and password,if yes,ont will online normally. |
| <port-id> | Pon port id,range for 1-16 |
| <onu-id> | Ont id,range for 1-64 |
| <loid> | Loid of ont,it supports 1-24 strings |
| <password> | password of ont,it supports 1-12 strings |
| <profile-id> | Profile id,0-1024 |
| <profile-name> | Profile name,it supports 1-16 strings. |
| always|once-aging|once-no-aging | Always:ont can be authenticated at any time  once-aging:ont only can be authenticated for once time within the allotted time,ont will be cleared once it is offline.  once-no-aging:no limitation in authentication time for ont,but it will be cleared once it is offline. |

【Example】

Example 1：Add an ont in pon1 and bind it to ont-lineprofile 5 and ont-srvprofile 5.

|  |
| --- |
| OLT(config-interface-epon-0/0)#ont add 1 10 loid-auth test password-auth test ont-lineprofile-id 5 ont-srvprofile-id 5 always  OLT(config-interface-epon-0/0)# |

### Config ONU Authmode

|  |  |
| --- | --- |
| Command | OLT(config-interface-epon-0/0)#ont authmode <port-id><auth-mode> |
| **View** | epon view |
| **Description** | This command is used for set ont authmode in pon port. |
| <port-id> | Pon port id,range for 1-16 |
| <auth-mode> | Adaptive:Adaptive policy authenticated  Auto:All ont will be authenticated by mac address unconditional  Loid:authenticate ont by loid  Loid-password:authenticate ont by loid+password  Mac:authenticate ont by mac address  Mac-or-loid:authenticate ont by mac address or loid  Mac-or-loid-password:authenticate ont by mac addressor loid+password |

【Example】

Example 1：Set the authmode of pon 1 as mac.

|  |
| --- |
| OLT(config-interface-epon-0/0)#ont authmode 1 mac  OLT(config-interface-epon-0/0)# |

### Change ONU Bind Profile

| Command | OLT(config-interface-epon-0/0)#ont modify <port-id> {<onu-id>|<onu-list>} {ont-lineprofile-id <profile-id> |ont-lineprofile-name <profile-name> |ont-srvprofile-id <profile-id>| ont-srvprofile-name <profile-name>} |
| --- | --- |
| **View** | EPON interface view |
| **Description** | This command is used for modify the bound ont-lineprofile and ont-srvprofile of ont. |
| <port-id> | Pon port id,range for 1-16 |
| <onu-id>|<onu-llist> | Onu-id:ont id to be modified,range for 1-64  Onu-list:ont list to be modified,format for 1,3-5,8 |
| <profile-id> | profile id,range for 0-512 |
| <profile-name> | Profile name,it supports 1-16 strings. |

【Example】

Example 1：Modify the ont-lineprofile of ont 1 in pon 1 as ont-lineprofile 5

|  |
| --- |
| OLT(config-interface-epon-0/0)#ont modify 1 1 ont-lineprofile-id 5  OLT(config-interface-epon-0/0)# |

Example 2:Modify the ont-lineprofile and ont-srvprofile of ont 1 in pon 1 as ont-lineprofile 5 and ont-srvprofile 5.

|  |
| --- |
| OLT(config-interface-epon-0/0)#ont modify 1 1 ont-lineprofile-id 5 ont-srvprofile-id 5  OLT(config-interface-epon-0/0)# |

### Config Pre-binding ONU Profile

| Command | OLT(config-interface-epon-0/0)ont predetermine <port-id> {< onu-id >|<onu-list>} { ont-lineprofile-id <profile-id> |ont-lineprofile-name <profile-id>} {ont-srvprofile-id <profile-name>| ont-srvprofile-name <profile-name>} |
| --- | --- |
| **View** | EPON interface view |
| **Description** | This command is used for predetermine the ont-lineprofile and ont-srvprofile for unregister ont in pon port,these profile will be applied to ont once it is online. |
| <port-id> | Pon port id,range for 1-16 |
| <onu-id>|<onu-llist> | Onu-id:ont id,range for 1-64  Onu-list:ont list,format for 1,3-5,8 |
| <profile-id> | profile id,range for 0-512 |
| <profile-name> | Profile name,it supports 1-16 strings. |

【Example】

Example 1：Predetermine the ont-lineprofile 5 and ont-srvprofile 5 for ont 1 in pon 1.

|  |
| --- |
| OLT(config-interface-epon-0/0)#ont predetermine 1 1 ont-lineprofile-id 5 ont-srvprofile-id 5  OLT(config-interface-epon-0/0)# |

### Confirm Autofind ONU

| Command | OLT(config-interface-epon-0/0)#ont confirm <port-id> {all |mac-auth <mac-address> | loid-auth <loid>} {password-auth <password>} {ont-lineprofile-id <profile-id> | ont-lineprofile-name <profile-name> ont-srvprofile-id <profile-id> | ont-srvprofile-name <profile-name>} |
| --- | --- |
| **View** | epon view |
| **Description** | This command is used for confirm the discovered ont.If ont autofind is enable,olt will obtain the register info of ont after accessing the ont to olt,at this time,ont is in‘autofind’state.ont will turn into working state and can be configured after confirming.Batch of ont registration is supported. |
| <port-id> | Pon port id,range for 1-16 |
| <mac-address> | Mac address of ont,format is xx:xx:xx:xx:xx:xx |
| <loid> | Loid of ont,it supports 1-24 strings |
| <password> | password of ont,it supports 1-12 strings |
| <profile-id> | Profile id,0-512 |
| <profile-name> | Profile name,it supports 1-16 strings. |

【Example】

Example 1：Authenticate all the autofind ont in pon1 according to mac address.

|  |
| --- |
| OLT(config-interface-epon-0/0)#ont confirm 1 all mac-auth  Number of ONUs that can be added:0,success:0  OLT(config-interface-epon-0/0)# |

Example 2:Authenticate all the autofind ont in pon1 according to loid“test”.

|  |
| --- |
| OLT(config-interface-epon-0/0)#ont confirm 1 loid-auth test  Add port 1 ONU 1 successfully.  OLT(config-interface-epon-0/0)# |

### Cancel Autofind ONU

|  |  |
| --- | --- |
| Command | OLT(config-interface-epon-0/0)#ont cance l<port-id> {<mac-address>|all} |
| **View** | epon view |
| **Description** | This command is used for cancel the autofind ont |
| <port-id> | Pon port id,range for 1-16 |
| <mac-address> | Mac saddress of ont,format is xx:xx:xx:xx:xx:xx |
| all | All the autofind ont in corresponding pon port |

【Example】

Example 1：Cancel the autofind ont in pon1,its mac address is E0:67:B3:12:11:8A.

|  |
| --- |
| OLT(config-interface-epon-0/0)#ont cancel 1 E0:67:B3:12:11:8A  OLT(config-interface-epon-0/0)# |

### Re-register ONU

|  |  |
| --- | --- |
| Command | OLT(config-interface-epon-0/0)#ont re-register <port-id> {<onu-id>|all} |
| **View** | epon view |
| **Description** | This command is used for re-register the specified ont or all the ont in corresponding pon port. |
| <port-id> | Pon port id,range for 1-16 |
| {<onu-id>|all} | onu-id:ont id to be re-register,range for 1-64  All:re-register all the ont in pon port |

【Example】

Example 1：Re-register onu1 in pon 1.

|  |
| --- |
| OLT(config-interface-epon-0/0)#ont re-register 1 1  2000-01-08 02:02:49 PON 0/0/1 ONU 1 onu is offline  2000-01-08 02:02:49 PON 0/0/1 pon port link down  2000-01-08 02:02:56 PON 0/0/1 ONU 1 onu is online  2000-01-08 02:02:56 PON 0/0/1 pon port link up  OLT(config-interface-epon-0/0)# |

### Modify ONU Authmode

| Command | OLT(config-interface-epon-0/0)#ont modify <port-id> <onu-id> auth-type {mac-auth <mac-address> | loid-auth <loid>} {password-auth <password>} |
| --- | --- |
| **View** | Config view |
| **Description** | This command is used for modify ont authmode |
| <port-id> | Pon port id,range for 1-16 |
| <onu-id> | Ont id,range for 1-64 |
| <mac-address> | Mac address of ont,format is xx:xx:xx:xx:xx:xx |
| <loid> | Loid of ont,it supports 1-24 strings |
| <password> | password of ont,it supports 1-12 strings |

【Example】

Example 1：Modify the auth-type of onu 1 as mac-auth in pon1,its mac is 11:11:11:11:11:11.

|  |
| --- |
| OLT(config-interface-epon-0/0)#ont modify 1 1 auth-type mac-auth 11:11:11:11:11:11  OLT(config-interface-epon-0/0)# |

Example 2:Modify the auth-type of onu 1 as loid-auth in pon1,its loid is test.

|  |
| --- |
| OLT(config-interface-epon-0/0)#ont modify 1 1 auth-type loid-auth test  OLT(config-interface-epon-0/0)# |

Example 3:Modify the auth-type of onu 1 as loid-password in pon1,its loid is test,password is test1.

|  |
| --- |
| OLT(config-interface-epon-0/0)#ont modify 1 1 auth-type loid-auth test password-auth test1  OLT(config-interface-epon-0/0)# |

### Config ONU Black-list

| Command | OLT(config-interface-epon-0/0)# ont black-list add port-id (mac-address | all) |
| --- | --- |
| **View** | EPON interface view |
| **Description** | This command is used for add the ONT of the specified PON port to the blacklist, and then the blacklist ONT authentication is unsuccessful. |
| port-id | Pon port id,range for 1-16 |
| mac-address | Mac address of blacklist ont,format for xx:xx:xx:xx:xx:xx |
| all | All of the blacklist ont in the pon port |

【Example】

Example 1：Config ONU black-list in pon port 5.

|  |
| --- |
| OLT(config-interface-epon-0/0)# ont black-list add 5 E0:67:B3:12:04:67  2000-01-08 04:13:49 PON 0/0/5 ONU 11 onu is offline  OLT(config-interface-epon-0/0)# 2000-01-08 04:13:49 PON 0/0/5 ONU 11 onu optical down  2000-01-08 04:13:49 PON 0/0/5 pon port link down  OLT(config-interface-epon-0/0)# 2000-01-08 04:13:55 PON 0/0/5 ONU 255 onu mac auth fails |

### Delete Black-list Auth ONU

|  |  |
| --- | --- |
| Command | OLT(config-interface-epon-0/0)#ont blacklist del <port-id> {<mac-address>|all} |
| **View** | EPON interface view |
| **Description** | This command is used for delete the blacklist ont in specified pon port. |
| <port-id> | Pon port id,range for 1-16 |
| <mac-address> | Mac address of blacklist ont,format for xx:xx:xx:xx:xx:xx |
| all | All of the blacklist ont in the pon port |

【Example】

Example 1：Delete all the blacklist ont in pon 1.

|  |
| --- |
| OLT(config-interface-epon-0/0)#ont black-list del 1 all  Number of ONUs that can be delete:1,success:1  OLT(config-interface-epon-0/0)# |

### Delete Authentication ONU

|  |  |
| --- | --- |
| Command | OLT(config-interface-epon-0/0)# ont delete <port-id> {<onu-id>|all} |
| **View** | EPON interface view |
| **Description** | This command is used for delete the ont in pon port |
| <port-id> | Pon port id,range for 1-16 |
| <onu-id> | Ont id,range for 1-64 |
| all | Delete all ont in pon port |

【Example】

Example 1：Delete all ont in pon1.

|  |
| --- |
| OLT(config-interface-epon-0/0)# ont delete 1 all  This command will delete all the ONUs in port.Are you sure to execute this command?(y/n):y 2000-01-04 11:32:30 ONU 0/0 1 1 is offline  Number of ONUs that can be delete:1,success:1  OLT(config-interface-epon-0/0)#2000-01-04 11:32:30 PON 0/0/1 ONU 1 onu is offline |

### Show ONU BlackList Authenticated Config

| Command | OLT(config-interface-epon-0/0)#show ont black-list {<port-id> all} |
| --- | --- |
| **View** | EPON interface view |
| **Description** | This command is used for show black-list ont in specified pon port |
| <port-id> | Pon port id,range for 1-16 |

【Example】

Example 1：Show all the black-list ont in pon 1.

|  |
| --- |
| OLT(config-interface-epon-0/0)#show ONU black-list 1 all  -----------------------------------------------------------------------------  Index MAC Try-Count Last-Auth-Time  ----------------------------------------------------------------------------  1 12:12:12:12:12:12 0 1900-01-00 00:00:00  -----------------------------------------------------------------------------  Total:1  OLT(config-interface-epon)# |

### Show ONU Black List

|  |  |
| --- | --- |
| Command | OLT(config-interface-epon-0/0)# show ont black-list port-id all |
| **View** | Epon view |
| **Description** | This command is used for show ONU which have added black list. |
| port-id | Pon port id,range for 1-16 |

【Example】

Example 1：Show PON9，a list of ONU blacklists that have been added.

|  |
| --- |
| OLT(config-interface-epon-0/0)# show ont black-list 9 all  -----------------------------------------------------------------------------  Index F/S P MAC  ----------------------------------------------------------------------------  1 0/0 9 E0:67:B3:12:04:99  -----------------------------------------------------------------------------  Total: 1  OLT(config-interface-epon-0/0)# |

### Show ONU Predetermine Information

|  |  |
| --- | --- |
| Command | OLT(config-interface-epon-0/0)# show ont predetermine port-id |
| **View** | Epon view |
| **Description** | This command is used for show ONU predetermine information. |
| port-id | Pon port id,range for 1-16 |

【Example】

Example 1：Show PON9 predetermine information.

|  |
| --- |
| OLT(config-interface-epon-0/0)# show ont predetermine 9  -----------------------------------------------------------------------------  F/S P ONT Line profile Server profile  ID ID  ----------------------------------------------------------------------------  0/0 9 4 10 10  -----------------------------------------------------------------------------  OLT(config-interface-epon-0/0)# |

### Show ONU registration statistics

|  |  |
| --- | --- |
| Command | OLT(config-interface-epon-0/0)# show ont register-statistics port-id|all |
| **View** | Epon view |
| **Description** | This command is used for show ONU registration statistics |
| port-id | Pon port id,range for 1-16 |

【Example】

Example 1：Show the onu registration statistics of all pon ports.

|  |
| --- |
| OLT(config-interface-epon-0/0)# show ont register-statistics all  -----------------------------------------------------------------------------  F/S P Autofind Authenticated Online  ----------------------------------------------------------------------------  0/0 1 0 4 1  0/0 2 0 0 0  0/0 3 0 4 0  0/0 4 0 0 0  0/0 5 0 0 0  0/0 6 0 0 0  0/0 7 0 0 0  0/0 8 0 0 0  0/0 9 0 5 0  0/0 10 0 0 0  0/0 11 0 0 0  0/0 12 0 0 0  0/0 13 0 0 0  0/0 14 0 0 0  0/0 15 0 2 0  0/0 16 0 0 0  -----------------------------------------------------------------------------  Total: 0 15 1  OLT(config-interface-epon-0/0)# |

### Delete the user template of the predetermine ONU

|  |  |
| --- | --- |
| Command | OLT(config-interface-epon-0/0)# no ont predetermine <port-id> < onu-id > |
| **View** | epon view |
| **Description** | This command is used for delete the user template of the predetermine ONU. |
| <port-id> | Pon port id,range for 1-16 |
| < onu-id > | onu-id:ont id to be show,range for 1-64。 |

【Example】

Example 1：Delete PON7 ONU1 predetermine template.

|  |
| --- |
| OLT(config-interface-epon-0/0)# no ont predetermine 7 1  OLT(config-interface-epon-0/0)# |

### Show ONU Registered Status and Information

|  |  |
| --- | --- |
| Command | OLT(config-interface-epon-0/0)#show ont info <port-id>< {onu-id>|all} |
| **View** | EPON interface view |
| **Description** | This command is used for show ont state info(including current state,relative configuration of ont)  Port:The pon port id that the ont had registered in  ONU ID:the setting ont id  MAC:Mac address of ont  Control flag：  Active:Ont is in active state.Only if the ont is in active state the ont can register in olt.  Deactive:Ont is in deactive state.When ont is in deactive state,we can active the ont by“ont active”command.  Run state:The running sigh of ont,it includes“online”,“offline”,“online”state indicates that ont has registered in olt normally.  Config state:This state can describe whether the config state is in normal.it includes 3 kinds of state:  Initial:Ont is in configuration issuing or recovering state  Failed:Failed to issue or recover the configuration  Success:Success to issue or recover the configuration |
| <port-id> | Pon port id,range for 1-16 |
| {<onu-id>  |all} | onu-id:ont id to be show,range for 1-64。  All:Show all of the ont state in current pon port |

【Example】

Example1:Show all of the ont state in pon 1.

|  |
| --- |
| OLT(config-interface-epon-0/0)#show ont info 1 all  -----------------------------------------------------------------------------  F/S P ONU MAC Control Run Config Match Desc  ID flag state state state  ----------------------------------------------------------------------------  0/0 1 1 E0:67:B3:00:00:09 active online success match  0/0 1 2 00:13:25:00:00:01 active offline initial initial  0/0 1 3 E0:67:B3:1B:8F:35 active offline initial initial  0/0 1 4 00:13:25:01:02:01 active offline initial initial  -----------------------------------------------------------------------------  Total:4,online 1  OLT(config-interface-epon-0/0)# |

### Check the aging time configuration of the ONU

|  |  |
| --- | --- |
| Command | OLT(config)# show ont auto-aging info |
| **View** | epon view |
| **Description** | This command is used to view the aging time configuration of the ONU. |

【Example】

Example 1：Check the aging time configuration of the ONU.

|  |
| --- |
| OLT(config)# show ont auto-aging info  Auto-aging switch: ON  Auto-aging time: 20 day(s)  Auto-aging scan-interval: 7 day(s)  OLT(config)# |

### Check the ONU registration migration detection status

|  |  |
| --- | --- |
| Command | OLT(config)# show ont moving-check |
| **View** | epon view |
| **Description** | This command is used to view the ONU registration migration detection status. |

【Example】

Example 1：Check the ONU registration migration detection status configuration.

|  |
| --- |
| OLT(config)# show ont moving-check  ONT moving check : enable  OLT(config)# |

## Policy-auth ONU and Batch Delivery Configuration Manage

### Enable or Disable Global Policy-auth ONU

|  |  |
| --- | --- |
| Command | OLT(config)# ont policy-auth {enable|disable} |
| **View** | config view |
| **Description** | This command is used for enable or disable the global ONU policy authentication function. The default policy adopted by the OLT is that the ONU defaults to match the line profile 0 and the service profile. The OLT supports the following methods to match different ONUs, and then match different configurations for different ONUs. |
| {enable|disable} | Enable:Enable policy-auth of ont  Disable:Disable policy-auth of ont |

【Example】

Example 1： Enable global ONU policy authentication.

|  |
| --- |
| OLT(config)# ont policy-auth enable  OLT(config)# |

### Enable or Disable Policy-auth ONU Under PON Port

|  |  |
| --- | --- |
| Command | OLT(config-interface-epon-0/0)#ont policy-auth <port-id> {enable|disable} |
| **View** | EPON interface view |
| **Description** | This command is used for enable or disable policy-auth of ont under OLT PON port. |
| <port-id> | Pon port id,range for 1-16 |
| {enable|disable} | Enable:Enable policy-auth of ont  Disable:Disable policy-auth of ont |

【Example】

Example 1：Enable policy-auth of ont in pon1

|  |
| --- |
| OLT(config-interface-epon-0/0)#ont policy-auth 1 enable  OLT(config-interface-epon-0/0)# |

### Config Policy-auth ONU Mode

| Command | OLT(config)# ont policy-auth mode {all |model-auth |model-swver-auth |model-vendor-hwver-auth|vendor-auth}  to {loid-auth |loid-password-auth |mac-auth} {always|once-no-aging} |
| --- | --- |
| **View** | Config view |
| **Description** | This command is used for configure the ONU policy authentication mode. Mainly configures what the ONU is based on to match the policy. The ONU is based on what is registered, and the number of times the policy action is executed. |
| <all |model-auth |model-swver-auth |model-vendor-hwver-auth|vendor-auth > | **All:** The object that executes the policy is all online ONUs.  **Model-auth :** Match different strategies model-swver-auth according to different model ids: match different strategies according to different model id and software version  **Model-vendor-hwver-auth:** Match different strategies according to different model id, software version and hardware version  **Vendor-auth :** match different strategies based on different vendor ids |
| <loid-auth |loid-password-auth |mac-auth>  <always|once-no-aging> | Mac-auth: onu is registered based on mac address  Loid-auth: onu is registered based on loid id  Loid-password-auth:onu is registered based on loid id and password  Always: the action of executing the policy is always executed  Once-no-aging: the action of executing the policy is executed only once |

【Example】

Example 1： Configure the ONU to match the policy by model id, register based on mac address, and always execute the policy.

|  |
| --- |
| OLT(config)# ont policy-auth mode model-auth to mac-auth always  OLT(config)# |

### Config Policy-auth ONU Mode and Batch Delivery Configuration Match Mode

| Command | OLT(config)# ont policy-auth {all |model-auth |model-swver-auth |model-vendor-hwver-auth|vendor-auth }  <parameter> { ont-lineprofile-id <profile-id> |ont-lineprofile-name <profile-id>} {ont-srvprofile-id <profile-name>| ont-srvprofile-name <profile-name>} |
| --- | --- |
| **View** | Config view |
| **Description** | This command is used for configure the matching policy of the ONU, configure specific parameters to match the policy, and configure line profiles and service templates that match the ONUs of the policy. |
| <all |model-auth |model-swver-auth |model-vendor-hwver-auth|vendor-auth > | **All:** The object that executes the policy is all online ONUs.  **Model-auth :** Match different strategies model-swver-auth according to different model ids: match different strategies according to different model id and software version  **Model-vendor-hwver-auth:** Match different strategies according to different model id, software version and hardware version  **Vendor-auth :** match different strategies based on different vendor ids |
| <ont-lineprofile-id|ont-lineprofile-name> | Configure the line profile id or name matching the online ONU that matches the policy. |
| <ont-srvprofile-id|ont-srvprofile-name> | Configure the service template id or name matching the online ONU that matches the policy. |

【Example】

Example 1： Configure the ONU on the line that has the model id of 0x31303053 to automatically match the line profile 10 and the service profile 10.

|  |
| --- |
| OLT(config)# ont policy-auth policy model-auth 0x31303053 ont-lineprofile-id 10 ont-srvprofile-id 10  OLT(config)# |

Example 2: The ONU of the PON1 with the model id of 0x31303053 is configured based on the mac address authentication. The line-up always matches the line profile 10 and the service profile 10 automatically. All the configurations required are as follows:

|  |
| --- |
| OLT(config)# ont policy-auth enable  OLT(config)# ont policy-auth mode model-auth to mac-auth always  OLT(config)# ont policy-auth policy model-auth 0x31303053 ont-lineprofile-id 10 ont-srvprofile-id 10  OLT(config)# interface epon 0/0  OLT(config-interface-epon-0/0)# ont policy-auth 1 enable  OLT(config-interface-epon-0/0)# ont authmode 1 adaptive  OLT(config-interface-epon-0/0)# ont autofind 1 enable |

### Show Policy-auth ONT Configuration Information

|  |  |
| --- | --- |
| Command | OLT(config)# show ont policy-auth |
| **View** | Config view |
| **Description** | This command is used for view the configuration of the current ONU policy authentication of the OLT. |

【Example】

Example 1： Check the configuration of the current ONU policy authentication of the OLT.

|  |
| --- |
| OLT(config)# show ont policy-auth  -----------------------------------------------------------------------------  Policy-auth Switch : enable  Policy-auth Mode : model-auth  Target auth Mode : mac-auth  Time Mode : always  -----------------------------------------------------------------------------  OLT(config)# |

## ONU Basic Function Management

### Active ONU

|  |  |
| --- | --- |
| Command | OLT(config-interface-epon-0/0)#ont activate <port-id> {<onu-id>|all} |
| **View** | EPON interface view |
| **Description** | This command is used for active the ont with disactive state.Ont will work in normal only when it is in active state.ont is in active state by default. |
| <port-id> | Pon port id,range for 1-16 |
| <onu-id>|all | Ont id,range for 1-64  All:all of the ont |

【Example】

Example 1：Active the ont 1 in pon 1.

|  |
| --- |
| OLT(config-interface-epon-0/0)#ont activate 1 1  OLT(config-interface-epon-0/0)# |

### Deactive ONU

|  |  |
| --- | --- |
| Command | OLT(config-interface-epon-0/0)#ont deactivate <port-id> {<onu-id>|all} |
| **View** | EPON interface view |
| **Description** | This command is used for disactive the ont with active state.Ont will work in normal only when it is in active state.ont is in active state by default. |
| <port-id> | Pon port id,range for 1-16 |
| {<onu-id>|all} | Ont id,range for 1-64  All:all of the ont |

【Example】

Example 1：Disactive the ont 1 in pon 1.

|  |
| --- |
| OLT(config-interface-epon-0/0)#ont deactivate 1 1  OLT(config-interface-epon-0/0)# |

### Reboot ONU

|  |  |
| --- | --- |
| Command | OLT(config-interface-epon-0/0)#ont reboot <port-id> {<onu-id>|all} |
| **View** | EPON interface view |
| **Description** | This command is used for reboot the specified ont or all of the ont. |
| <port-id> | Pon port id,range for 1-16 |
| {<onu-id>|all} | Ont id,range for 1-64  All:all of the ont |

【Example】

Example 1：Reboot the ont 1 in pon 1.

|  |
| --- |
| OLT(config-interface-epon-0/0)#ont reboot 1 1  OLT(config-interface-epon-0/0)# |

### Restore the ONU to factory settings

|  |  |
| --- | --- |
| Command | OLT(config-interface-epon-0/0)# ont default-setting <port-id> <onu-id> | all |
| **View** | EPON interface view |
| **Description** | This command is used for restore the factory settings of the specified or all ONUs under the pon port. |
| <port-id> | Pon port id,range for 1-16 |
| {<onu-id>|all} | Ont id,range for 1-64  All:all of the ont |

【Example】

Example 1：Restore all ONUs under PON1 to factory settings

|  |
| --- |
| OLT(config-interface-epon-0/0)# ont default-setting 1 all  Number of ONUs that can be restore default: 0, success: 0  OLT(config-interface-epon-0/0)# |

### ONU Remote Manage IP Function Config

| Command | OLT(config-interface-epon-0/0)#ont ipconfig <port-id> < onu-id > ip-address <ip-address> mask <mask> gateway <gateway-ip> manage-vlan <vlan-id> priority <priority> |
| --- | --- |
| **View** | EPON interface view |
| **Description** | This command is used for set the management ip,netmask,gateway,manage vlan and priority and etc. |
| <port-id> | Pon port id,range for 1-16 |
| <onu-id> | Ont id,range for 1-64 |
| <ip-address> | Manage ip,format for xx:xx:xx:xx:xx:xx |
| <mask> | Netmask,format for xx:xx:xx:xx:xx:xx |
| <gateway-ip> | Gateway ip,format for xx:xx:xx:xx:xx:xx |
| <vlan-id> | vlan id.range for 1-4094 |
| <priority> | Priority,range for 0-7 |

【Example】

Example 1：Set the parameters of ont 1 in pon 1,set its management ip as 192.168.101.1,netmask as 255.255.255.0,gateway ip is 192.168.101.254,management vlan as 101,priority as 0.

|  |
| --- |
| OLT(config-interface-epon-0/0)#ont ipconfig 1 1 ip-address 192.168.101.1 mask 255.255.255.0 gateway 192.168.101.254 manage-vlan 101 priority 0  OLT(config-interface-epon-0/0)# |

### ONU Upstream Rate Limit Function Config

| Command | OLT(config-interface-epon-0/0)#ont sla <port-id> < onu-id > upstream {assure <assured-bandwidth> | fix <fixed-bandwidth> | max <max-bandwidth>} |
| --- | --- |
| **View** | EPON interface view |
| **Description** | This command is used for set upstream rate limitation of ont |
| <port-id> | Pon port id,range for 1-16 |
| <onu-id> | Ont id,range for 1-64 |
| <assured-bandwidth> | Assure-bandwidth,range for 1-1000000,unit is kpbs |
| <fixed-bandwidth> | Fixed-bandwidth,range for 1-1000000,unit is kpbs |
| <max-bandwidth> | Max-bandwidth,range for 512-1000000,unit is kpbs |

【Example】

Example 1：Set the fixed-bandwidth of ont 1 in pon1 as 100000kbps

|  |
| --- |
| OLT(config-interface-epon-0/0)#ont sla 1 1 upstream fix 100000  OLT(config-interface-epon-0/0)# |

### ONU Downstream Rate Limit Function Config

|  |  |
| --- | --- |
| Command | OLT(config-interface-epon-0/0)#ont sla <port-id> < onu-id > downstream max <max-bandwidth> |
| **View** | EPON interface view |
| **Description** | This command is used for set downstream rate limitation of ont |
| <port-id> | Pon port id,range for 1-16 |
| <onu-id> | Ont id,range for 1-64 |
| <max-bandwidth> | Max-bandwidth,range for 64-1000000,unit is kpbs |

【Example】

Example 1：Set the max-bandwidth of ont 1 in pon1 as 100000kbps

|  |
| --- |
| OLT(config-interface-epon-0/0)#ont sla 1 1 downstream max 100000  OLT(config-interface-epon-0/0)# |

### ONU MAC Aging Time Config

|  |  |
| --- | --- |
| Command | OLT(config-interface-epon-0/0)# ont mac-aging <port-id> <onu-id> aging-time <aging-time> |
| **View** | EPON interface view |
| **Description** | This command is used for set mac-aging time of specified ont |
| <port-id> | Pon port id,range for 1-16 |
| <ont-id> | Ont id,range fro 1-64 |
| <aging-time> | Mac-aging time,range for 0-36000.”0”means without aging. |

【Example】

Example 1：Set the mac-aging time of onu 4 in pon 1 as 12s.

|  |
| --- |
| OLT(config-interface-epon-0/0)#ont mac-aging 1 4 aging-time 12  OLT(config-interface-epon-0/0)# |

### Add ONU Description Information

|  |  |
| --- | --- |
| Command | OLT(config-interface-epon-0/0)#ont description <port-id> <onu-id> <description> |
| **View** | EPON interface view |
| **Description** | This command is used for add description for ontt |
| <port-id> | Pon port id,range for 1-16 |
| <onu-id> | Ont id,range for 1-64 |
| <description> | Description info of ont,it supports 1-64 strings. |

【Example】

Example 1：Add description“test”for ont 1 in pon1.

|  |
| --- |
| OLT(config-interface-epon-0/0)#ont description 1 1 test  OLT(config-interface-epon-0/0)# |

### ONU Encryption Function Config

|  |  |
| --- | --- |
| Command | OLT(config-interface-epon-0/0)#ont encrypt <port-id> <onu-id> {enable|disable} |
| **View** | EPON interface view |
| **Description** | This command is used for set encryption function of ont.the message between specified pon port and specified ont will be encrypted after executing this command. |
| <port-id> | Pon port id,range for 1-16 |
| <onu-id> | Ont id,range for 1-64 |
| {enable|disable} | Enable:enable the encryption function  Disable:disable the encryption function |

【Example】

Example 1：Enable the encryption function of onu 1 in pon 1.

|  |
| --- |
| OLT(config-interface-epon-0/0)#ont encrypt 1 1 enable  OLT(config-interface-epon-0/0)# |

### Enable or Disable ONU FEC Function

|  |  |
| --- | --- |
| Command | OLT(config-interface-epon-0/0)#ont fec <port-id> <onu-id> {enable|disable} |
| **View** | EPON interface view |
| **Description** | This command is used for enable or disable FEC function of specified ont in pon port. |
| <port-id> | Pon port id,range for 1-16 |
| <onu-id> | Ont id,range for 1-64 |
| {enable|disable} | Enable:enable FEC function  Disable:disable FEC function |

【Example】

Example 1：enable FEC function of ont 1 in pon 1.

|  |
| --- |
| OLT(config-interface-epon-0/0)#ont fec 1 1 enable  OLT(config-interface-epon-0/0)# |

### ONU Service-sla Function Config

|  |  |
| --- | --- |
| Command | OLT(config-interface-epon-0/0)#ont service-sla <port-id> {all | <onu-id>} {profile-id <profile-id>|profile-name <profile-name>} |
| **View** | EPON interface view |
| **Description** | This command is used for bind ont-slaprofile to ont.Firstly,it needs to create a n ont-slaprofile in config view. |
| <port-id> | Pon port id,range for 1-16 |
| {all|<onu-id>} | Ont id,range for 1-64  All:all of the ont |
| <profile-id> | Profile id,range for 0-256 |
| <profile-name> | profile name,it supports 1-16 strings |

【Example】

Example 1：Bind ont-slaprofile 5 to ont 1 in pon 1.

|  |
| --- |
| OLT(config-interface-epon-0/0)#ont service-sla 1 1 profile-id 5  OLT(config-interface-epon-0/0)# |

### ONU SNMP Function Config

| Command | OLT(config-interface-epon-0/0)#ont snmp-config <port-id> < onu-id > v2c <readgroup> <writegroup> <trap-ip> <snmp-port> { <trap-port> <security-name> } |
| --- | --- |
| **View** | EPON interface view |
| **Description** | This command is used for set snmp parameters of ONU |
| <port-id> | Pon port id,range for 1-16 |
| <onu-id> | Ont id,range for 1-64 |
| <readgroup> | read group,it supports 1-32 strings |
| <writegroup> | write group,it supports 1-32 strings |
| <trap-ip> | Trap ip,format for xx:xx:xx:xx:xx:xx |
| <snmp-port> | Snmp port,range for 1-65535 |
| <trap-port> | Trap port,range for 1-65535 |
| <security-name> | Security-name,it supports 1-32 strings |

【Example】

Example 1：Set snmp parameters of ONU,Set read group as public,write group as private,trap ip as 192.168.5.200,snmp port is 23,trap port is 161,security name is test.

|  |
| --- |
| OLT(config-interface-epon-0/0)#ont snmp-config 1 1 v2c public private 192.168.5.200 23 161 test  OLT(config-interface-epon-0/0)# |

### Enable or Disable ONU Tx Optical Power Supply

| Command | OLT(config-interface-epon-0/0)#ont tx-power-supply <port-id> <onu-id|all> {enable/disable} {<disable-time>|forever} |
| --- | --- |
| **View** | EPON interface view |
| **Description** | This command is used for set the tx-power-supply limitation of specified ont and its shining time. |
| <port-id> | Pon port id,range for 1-16 |
| <ont-id> | Ont id,range fro 1-64 |
| {enable|disable} | Enable:ont shine in normal  Disable:ont unshining |
| <disable-time>|forever | <disable-time>:unshining time of ont,range for 1-65534s  Forever:make onu unshining forever |

【Example】

Example 1：Set ont 3 in pon 1 un-shining for 3s.

|  |
| --- |
| OLT(config-interface-epon-0/0)#ont tx-power-supply 1 3 disable 3  OLT(config-interface-epon-0/0)#  2000-01-01 00:07:06 PON 0/0/1 ONU 3 onu is offline  2000-01-01 00:07:10 PON 0/0/1 ONU 3 onu is online |

### Show ONU ipconfig(Remote Manage IP Address)

|  |  |
| --- | --- |
| Command | OLT(config-interface-epon-0/0)#show ont ipconfig <port-id> <onu-id> |
| **View** | EPON interface view |
| **Description** | This command is used for show ont ipconfig,it includes manage ip,gateway,manage vlan and etc. |
| <port-id> | Pon port id,range for 1-16 |
| <onu-id> | Ont id,range for 1-64 |

【Example】

Example 1：Show ipconfig of ont 1 in pon 1.

|  |
| --- |
| OLT(config-interface-epon-0/0)#show ont ipconfig 1 1  -----------------------------------------------------------------------------  Frame/Slot:0/0  Port:1  ONU-ID:1  IP:192.168.1.1  Subnet mask:255.255.255.0  Gateway:192.168.1.100  Manage VLAN:100  Manage priority:5  -----------------------------------------------------------------------------  OLT(config-interface-epon-0/0)# |

### Show ONU SNMP Configuration

|  |  |
| --- | --- |
| Command | OLT(config-interface-epon-0/0)#show ont snmp-config <port-id> <onu-id> |
| **View** | EPON interface view |
| **Description** | This command is used for show snmp configuration of ont |
| <port-id> | Pon port id,range for 1-16 |
| <onu-id> | Ont id,range for 1-64 |

【Example】

Example 1：Show snmp configuration of ont 1 in pon 1.

|  |
| --- |
| OLT(config-interface-epon-0/0)#show ont snmp-config 1 1  -----------------------------------------------------------------------------  Frame/Slot:0/0  Port:1  ONU-ID:1  Version:v2c  Read group name:public  Write group name:private  Destination IP:192.168.5.200  Snmp port:162  Trap port:162  SNMP body name:  -----------------------------------------------------------------------------  OLT(config-interface-epon-0/0)# |

### Show ONU Capability Information

|  |  |
| --- | --- |
| Command | OLT(config-interface-epon-0/0)#show ont capability <port-id> <onu-id> |
| **View** | EPON interface view |
| **Description** | This command is used for show ont capability info,including ont port type,number and etc. |
| <port-id> | Pon port id,range for 1-16 |
| <onu-id> | Ont id,range for 1-64 |

【Example】

Example 1：Show ont 3 capability info in pon 1.

|  |
| --- |
| OLT(config-interface-epon-0/0)#show ont capability 1 3  -----------------------------------------------------------------------------  Frame/Slot:0/0  Port:1  ONU-ID:3  Type:SFU  Number of uplink PON ports:1  Number of ETH ports:4(4FE+0GE)  Number of POTS ports:0  Number of CATV ports:1  Number of uplink queues:8  MAX number of uplink queues:8  Number of downlink queues:8  MAX number of downlink queues:8  Number of LLID:1  Fast leave ability:non-fast-leave in snooping mode  fast-leave in snooping mode  non-fast-leave in CTC mode  fast-leave in CTC mode  non-fast-leave in MLD snooping mode  fast-leave in MLD snooping mode  -----------------------------------------------------------------------------  OLT(config-interface-epon-0/0)# |

### Show ONU Configured Capability

|  |  |
| --- | --- |
| Command | OLT(config-interface-epon-0/0)#show ont config-capability <port-id> <onu-id> |
| **View** | EPON interface view |
| **Description** | This command is used for show ont config-capability.It can check whether the ability is matched according to compare config-capability with capability. |
| <port-id> | Pon port id,range for 1-16 |
| <onu-id> | Ont id,range for 1-64 |

【Example】

Example 1：Show config-capability of ont 3 in pon 1.

|  |
| --- |
| OLT(config-interface-epon-0/0)#show ont config-capability 1 3  -----------------------------------------------------------------------------  Frame/Slot:0/0  Port:1  ONU-ID:3  Number of ETH ports:adaptive  Number of POTS ports:adaptive  Number of CATV ports:adaptive  -----------------------------------------------------------------------------  OLT(config-interface-epon-0/0)# |

### Show ONU Opitcal Power Information

|  |  |
| --- | --- |
| Command | OLT(config-interface-epon-0/0)#show ont optical-info <port-id> <onu-id> |
| **View** | EPON interface view |
| **Description** | This command is used for show optical info of ont in pon port.Generally,it is used for routine maintenance and troubleshooting of ont,it can show optical info of ont to check whether the optical module is in normal. |
| <port-id> | Pon port id,range for 1-16 |
| <onu-id> | Ont id,range for 1-64 |

【Example】

Example 1：Show optical info of ont 3 in pon 3.

|  |
| --- |
| OLT(config-interface-epon-0/0)#show ont optical-info 1 3  -----------------------------------------------------------------------------  Frame/Slot:0/0  Port:1  ONU-ID:3  ONU-MAC:E0:67:B3:31:85:8A  Voltage(V):3.34  Tx optical power(dBm):1.72  Rx optical power(dBm):-3.73  Laser bias current(mA):18.20  Temperature(C):45.07  -----------------------------------------------------------------------------  OLT(config-interface-epon-0/0)# |

### Show ONU Firmware Version

|  |  |
| --- | --- |
| Command | OLT(config-interface-epon-0/0)#show ont version <port-id> <onu-id> |
| **View** | EPON interface view |
| **Description** | This command is used for show ont version info,it can show software,hardware,vendor and etc info of ont. |
| <port-id> | Pon port id,range for 1-16 |
| <onu-id> | Ont id,range for 1-64 |

【Example】

Example 1：Show version info of ont 3 in pon 1.

|  |
| --- |
| OLT(config-interface-epon-0/0)#show ont version 1 3  -----------------------------------------------------------------------------  Frame/Slot:0/0  Port:1  ONU-ID:3  Vendor-ID:PON  OUI Version:CTC3.0  ONU model:572R(0x35373252)  Extended model:GT832T\_R  ONU mac address:E0:67:B3:31:85:8A  ONU hardware version:V1.2  ONU software version:V2.1.5.b3  ONU chipset vendor ID:RL  ONU chipset model:9603  ONU chipset revision:01  ONU chipset version/date:00.00.07  ONU firmware version:0x56322e312e352e623320202d  ----------------------------------------------------------------------------- |

### Show ONU SNMP Config parameters

|  |  |
| --- | --- |
| Command | OLT(config-interface-epon-0/0)# show ont snmp-config port-id onu-id |
| **View** | epon view |
| **Description** | This command is used for show ONU SNMP config parameters. |
| port-id | Pon port id,range for 1-16 |
| onu-id | Ont id,range for 1-64 |

【Example】

Example1：Show PON9 ONU4 SNMPconfig parameters.

|  |
| --- |
| OLT(config-interface-epon-0/0)# show ont snmp-config 9 4  -----------------------------------------------------------------------------  Frame/Slot : 0/0  Port : 9  ONT-ID : 4  Version : v2c  Read group name : public  Write group name : private  Destination IP : 192.168.1.123  Snmp port : 161  Trap port : 162  SNMP body name :  -----------------------------------------------------------------------------  OLT(config-interface-epon-0/0)# |

### Show Basic Information about all ONUs on the pon port

|  |  |
| --- | --- |
| Command | OLT(config-interface-epon-0/0)# show ont basic-info port-id all |
| **View** | Epon view |
| **Description** | This command is used for show basic informations about all ONUs on the pon port, It can query the ONU number, MAC address, type, ranging distance, startup time, and model number. |
| port-id | Pon port id,range for 1-16 |

【Example】

Example1：Show all ONUs basic information under pon 9

|  |
| --- |
| OLT(config-interface-epon-0/0)# show ont basic-info 9 all  -----------------------------------------------------------------------------  F/S P ONT MAC Type Distance Up Extended  ID (m) Time Model  ----------------------------------------------------------------------------  0/0 9 1 E0:67:B3:3B:07:32 --  0/0 9 2 E0:67:B3:00:00:01 --  0/0 9 3 00:12:D6:6F:7D:0A --  0/0 9 4 E0:FA:07:F5:03:FD HGU 24 0:01:17:23 FD600\_111GW\_HR630  -----------------------------------------------------------------------------  Total: 4, online 1  OLT(config-interface-epon-0/0)# |

### Show the ONU binding Rate Limit Template Information

|  |  |
| --- | --- |
| Command | OLT(config-interface-epon-0/0)# show ont service-sla port-id ont-id |
| **View** | Epon view |
| **Description** | This command is used for show the ONU binding the rate limit template information. |
| port-id | Pon port id,range for 1-16 |
| ont-id | Ont id,range for 1-64 |

【Example】

Example 1：Show the PON9 ONU4 binding the rate limit template information.

|  |
| --- |
| OLT(config-interface-epon-0/0)# show ont service-sla 9 4  -----------------------------------------------------------------------------  Frame/Slot : 0/0  Port : 9  ONT-ID : 4  Profile-ID : 5  Profile-name : sla\_5  ----------------------------------------------------------------------------  Cycle length (TQ) : 25000  Number of services : 1  Fixed packet size of service 1 (Bytes) : 1500  Fixed bandwidth of service 1 (kbps) : 124416  Guaranteed bandwidth of service 1 (kbps) : 299776  Best effort bandwidth of service 1 (kbps) : 399872  WRR weight of service 1 : 0  -----------------------------------------------------------------------------  OLT(config-interface-epon-0/0)# |

### Show the ONU speed limit template information

|  |  |
| --- | --- |
| Command | OLT(config-interface-epon-0/0)# show ont sla port-id onu-id upstream|downstream |
| **View** | Epon view |
| **Description** | This command is used for show the ONU speed limit template information. |
| port-id | Pon port id,range for 1-16 |
| onu-id | Ont id,range for 1-64 |

【Example】

Example 1：Show the PON9 ONU4 upstream speed limit template information.

|  |
| --- |
| OLT(config-interface-epon-0/0)# show ont sla 9 4 upstream  -----------------------------------------------------------------------------  Frame/Slot : 0/0  Port : 9  ONT-ID : 4  ----------------------------------------------------------------------------  Line profile ID : 0  Line profile Name : lineprofile\_0  ----------------------------------------------------------------------------  DBA profile ID : 0  DBA profile Name : lineprofile\_0  ----------------------------------------------------------------------------  Fix(kbps) Assure(kbps) Max(kbps)  ----------------------------------------------------------------------------  0 0 1000000  -----------------------------------------------------------------------------  OLT(config-interface-epon-0/0)# |

### Show the Reason for the Offline of all ONUs under the PON Port

|  |  |
| --- | --- |
| Command | OLT(config-interface-epon-0/0)# show ont offline-list port-id all |
| **View** | Epon view |
| **Description** | This command is used for show the reason for the offline of all ONUs under the PON port. |
| port-id | Pon port id,range for 1-16 |

【Example】

Example 1：Show the reason for the offline of the PON1.

|  |
| --- |
| OLT(config-interface-epon-0/0)# show ont offline-list 1 all  The current time : 2000-01-04 07:03:55  -----------------------------------------------------------------------------  Ont id : 1 Mac : E0:67:B3:33:A7:88  Seq Up Time Down Time Down Reason  -----------------------------------------------------------------------------  Ont id : 2 Mac : E0:67:B3:1E:F3:D1  Seq Up Time Down Time Down Reason  1 2000-01-04 06:35:01 2000-01-04 06:49:02 losi  2 2000-01-04 04:18:44 2000-01-04 05:48:35 dying-gasp  -----------------------------------------------------------------------------  OLT(config-interface-epon-0/0)# |

### Show the Reason of ONU Offline under the PON Port

|  |  |
| --- | --- |
| Command | OLT(config-interface-epon-0/0)# show ont up-down-log port-id ont-id |
| **View** | Epon View |
| **Description** | This command is used for show the reason of ONU offline under the pon port. |
| port-id | Pon port id,range for 1-16 |
| ont-id | Ont id,range for 1-64 |

【Example】

Example 1：Show PON 7 ONU1 the reason of offline.

|  |
| --- |
| OLT(config-interface-epon-0/0)# show ont up-down-log 7 1  The current time : 2000-01-03 06:36:18  -----------------------------------------------------------------------------  Seq Up Time Down Time Down Reason  1 2000-01-03 06:34:10  2 2000-01-03 05:30:06 2000-01-03 06:33:18 dying-gasp  OLT(config-interface-epon-0/0)# |

### Delete ONU Encrypt Feature

|  |  |
| --- | --- |
| Command | OLT(config-interface-epon-0/0)# no ont encrypt port-id ont-id |
| **View** | epon view |
| **Description** | This command is used for delete ONU encrypt feature. |
| port-id | Pon port id,range for 1-16 |
| ont-id | Ont id,range for 1-64 |

【Example】

Example1：Delete PON 7 ONU1 encrypt feature.

|  |
| --- |
| OLT(config-interface-epon-0/0)# no ont encrypt 7 1  Restore to the profile configuration successfully  OLT(config-interface-epon-0/0)# |

### Delete ONU FEC Feature

|  |  |
| --- | --- |
| Command | OLT(config-interface-epon-0/0)# no ont fec port-id ont-id |
| **View** | epon view |
| **Description** | This command is used for delete the FEC (Forward Error Correction) function of the specified ONU under the pon port. |
| port-id | Pon port id,range for 1-16 |
| ont-id | Ont id,range for 1-64 |

【Example】

Example1：Delete PON7 ONU1 FEC feature

|  |
| --- |
| OLT(config-interface-epon-0/0)# no ont fec 7 1  Restore to the profile configuration successfully  OLT(config-interface-epon-0/0)# |

### Delete ONU Remote Management IP config

|  |  |
| --- | --- |
| Command | OLT(config-interface-epon-0/0)# no ont ipconfig port-id ont-id |
| **View** | epon view |
| **Description** | This command is used for delete the remote management IP of the specified ONU under the pon port. |
| port-id | Pon port id,range for 1-16 |
| ont-id | Ont id,range for 1-64 |

【Example】

Example 1：Delete PON7 ONU1 remote manegement ip config

|  |
| --- |
| OLT(config-interface-epon-0/0)# no ont ipconfig 7 1  OLT(config-interface-epon-0/0)# |

### Delete SLA Template Bount to ONU

|  |  |
| --- | --- |
| Command | OLT(config-interface-epon-0/0)# no ont service-sla port-id ont-id |
| **View** | epon view |
| **Description** | This command is used for delete the sla template bound to the ONU. |
| port-id | Pon port id,range for 1-16 |
| ont-id | Ont id,range for 1-64 |

【Example】

Example1：Delete PON7 ONU1 sla template bound to ONU.

|  |
| --- |
| OLT(config-interface-epon-0/0)# no ont service-sla 7 1  OLT(config-interface-epon-0/0)# |

### Delete ONU Rate Limit Function Config

|  |  |
| --- | --- |
| Command | OLT(config-interface-epon-0/0)# no ont sla port-id ont-id upstream|downstream |
| **View** | epon view |
| **Description** | This command is used for delete the ONU rate limit function config. |
| port-id | Pon port id,range for 1-16 |
| ont-id | Ont id,range for 1-64 |

【Example】

Example1：Delete PON7 ONU1 downstream rate limit config.

|  |
| --- |
| OLT(config-interface-epon-0/0)# no ont sla 7 1 downstream  OLT(config-interface-epon-0/0)# |

### Delete ONU SNMP Function Config

|  |  |
| --- | --- |
| Command | OLT(config-interface-epon-0/0)# no ont snmp-config port-id onu-id |
| **View** | epon view |
| **Description** | This command is used for delete the ONU snmp function config. |
| port-id | Pon port id,range for 1-16 |
| ont-id | Ont id,range for 1-64 |

【Example】

Example1：Delete PON7 ONU1 snmp config.

|  |
| --- |
| OLT(config-interface-epon-0/0)# no ont snmp-config 7 1  OLT(config-interface-epon-0/0)# |

## ONU Port VLAN Configuration(Non-template Mode)

### ONU Port Native-vlan(access) Configs

|  |  |
| --- | --- |
| Command | OLT(config-interface-epon-0/0)#ont port native-vlan <port-id> <onu-id> eth <eth-port-id> vlan <vlan-id> priority <priority> |
| **View** | EPON interface view |
| **Description** | This command is used for set native vlan of ont port.Caution:a corresponding vlan must be set in ont port firstly by the command of“ont port vlan”. |
| <port-id> | Pon port id,range for 1-16 |
| <onu-id> | Ont id,range for 1-64 |
| <eth-port-id> | eth port id,range for 1-24 |
| <vlan-id> | Vlan id,range for 1-4094 |
| <priority> | Priority,range for 0-7 |

【Example】

Example1:Set the native vlan of ont 1 eth 1 in pon 1 as 100,and set its priority as 3.

|  |
| --- |
| OLT(config-interface-epon-0/0)#ont port native-vlan 1 1 eth 1 vlan 100 priority 3  OLT(config-interface-epon-0/0)# |

### ONU Port Vlan Config

| Command | OLT(config-interface-epon-0/0)#ont port vlan <port-id> <onu-id> eth <eth-port-id> <vlan-id> priority <priority> |
| --- | --- |
| **View** | EPON interface view |
| **Description** | This command is used for set ont port vlan. |
| <port-id> | Pon port id,range for 1-16 |
| <onu-id> | Ont id,range for 1-64 |
| <eth-port-id> | eth port id,range for 1-24 |
| <vlan-id> | Vlan id,range for 1-4094 |
| <priority> | Priority,range for 0-7 |

【Example】

Example 1：Set the port vlan of ont 1 eth 1 in pon 1 as 100,and set its priority as 5.

|  |
| --- |
| OLT(config-interface-epon-0/0)#ont port vlan 1 1 eth 1 100 5  OLT(config-interface-epon-0/0)# |

### ONU Port Translation Mode VLAN Config

|  |  |
| --- | --- |
| Command | OLT(config-interface-epon-0/0)#ont port vlan <port-id> <onu-id> eth <eth-port-id> translation <service-vlan-id> <priority> <customer-vlan-id> <priority> |
| **View** | EPON interface view |
| **Description** | This command is used for set vlan translation of ont port,it translates the service vlan to customer vlan in downstream direction. |
| <port-id> | Pon port id,range for 1-16 |
| <onu-id> | Ont id,range for 1-64 |
| <eth-port-id> | eth port id,range for 1-24 |
| <service-vlan-id> | service vlan id,range for 1-4094 |
| <customer-vlan-id> | Customer vlan id,range for 1-4094 |
| <priority> | Priority,range for 0-7 |

【Example】

Example 1：Set vlan mode of ont 1 eth 1 in pon 1 as translation and translate its service vlan 12 to customer vlan 13.

|  |
| --- |
| OLT(config-interface-epon-0/0)#ont port vlan 1 1 eth 1 translation 12 user-vlan 13  OLT(config-interface-epon-0/0)# |

### ONU Port VLAN Pool Function Config

| Command | OLT(config-interface-epon-0/0)#ont port vlan <port-id> <onu-id> eth <eth-port-id> vlan-pool <vlan-pool-id> |
| --- | --- |
| **View** | EPON interface view |
| **Description** | This command is used for set vlan-pool of ont port.it needs to create a vlan-pool in config view firstly. |
| <port-id> | Pon port id,range for 1-16 |
| <onu-id> | Ont id,range for 1-64 |
| <eth-port-id> | eth port id,range for 1-24 |
| <vlan-pool-id> | Vlan-pool id,range for 1-128 |

【Example】

Example 1：Bind vlan-pool 2 to ont 1 eth 1 in pon 1.

|  |
| --- |
| OLT(config-interface-epon-0/0)#ont port vlan 1 1 eth 1 vlan-pool 2  OLT(config-interface-epon-0/0)# |

### ONU Port Transparent Mode VLAN Config

| Command | OLT(config-interface-epon-0/0)#ont port vlan <port-id> <onu-id> eth <eth-port-id> transparent |
| --- | --- |
| **View** | EPON interface view |
| **Description** | This command is used for set vlan transparent mode of ont port |
| <port-id> | Pon port id,range for 1-16 |
| <onu-id> | Ont id,range for 1-64 |
| <eth-port-id> | eth port id,range for 1-24 |

【Example】

Example 1：Set vlan mode of ont 1 eth 1 in pon 1 as transparent.

|  |
| --- |
| OLT(config-interface-epon-0/0)#ont port vlan 1 1 eth 1 transparent  OLT(config-interface-epon-0/0)# |

### Show ONU Port VLAN Configuration

|  |  |
| --- | --- |
| Command | OLT(config-interface-epon-0/0)#show ont port vlan <port-id> <onu-id> eth <onu-port id> |
| **View** | EPON interface view |
| **Description** | This command is used for show specified eth port vlan of ont |
| <port-id> | Pon port id,range for 1-16 |
| <onu-id> | Ont id,range for 1-64 |
| <onu-port id> | Eth port id,range for 1-24 |

【Example】

Example 1：Show eth 1 port vlan of ont 2 in pon 1.

|  |
| --- |
| OLT(config-interface-epon-0/0)#show ont port vlan 1 2 eth 1  -----------------------------------------------------------------------------  Frame/Slot:0/0  Port:1  ONU ID:2  Port ID:1  ----------------------------------------------------------------------------  Service Profile ID:0  Service Profile name:srvprofile\_0  ----------------------------------------------------------------------------  Service-type Index N-VLAN N-PRI S-VLAN S-PRI C-VLAN C-PRI  ---------------------------------------------------------------------------  Transparent-------  -----------------------------------------------------------------------------  OLT(config-interface-epon-0/0)# |

### Show Real-time Information about the ONU Ethernet Port

|  |  |
| --- | --- |
| Command | OLT(config-interface-epon-0/0)#show ont port vlan remote <port-id> <ONU-id> eth <ONU-port id> |
| **View** | Epon view |
| **Description** | This command is used for show real-time information about the onu ethernet port. |
| <port-id> | Pon port id,range for 1-16 |
| <onu-id> | Ont id,range for 1-64 |
| <ONU-port id> | Eth port id,range for 1-24 |

【Example】

Example 1：Show real-time information about the PON1 ONU3 ETH1.

|  |
| --- |
| OLT(config-interface-epon-0/0)# show ont port vlan remote 1 3 eth 1  -----------------------------------------------------------------------------  Frame/Slot : 0/0  Port : 1  ONT ID : 3  Port ID : 1  ----------------------------------------------------------------------------  VLAN type : Transparent  -----------------------------------------------------------------------------  OLT(config-interface-epon-0/0)# |

### Delete VLAN that has been Added to an ONU Port

|  |  |
| --- | --- |
| Command | OLT(config-interface-epon-0/0)# no ont port vlan <port-id> < onu-id > eth <eth-port-id> <vlan-id> |vlan-pool |
| **View** | Epon view |
| **Description** | This command is used for delete vlan that has been added to an ONU port. |
| <port-id> | Pon port id,range for 1-16 |
| < onu-id > | Ont id,range for 1-64 |
| <eth-port-id> | Eth port id,range for 1-24 |
| <vlan-id> | Vlan id，range for 1-4094 |

【Example】

Example 1：Delete the vlan that has been added to the PON7 ONU1 ETH1.

|  |
| --- |
| OLT(config-interface-epon-0/0)# no ont port vlan 7 1 eth 1 10  OLT(config-interface-epon-0/0)# |

## ONU Port Management

### Enable or Disable ONU Port

|  |  |
| --- | --- |
| Command | OLT(config-interface-epon-0/0)#ont port attribute <port-id> <onu-id> eth <eth-port-id> operational-state {on/off} |
| **View** | EPON interface view |
| **Description** | This command is used for enable or disable ont port.ont port can communicate normally when it is in enabling state,else it can’t. |
| <port-id> | Pon port id,range for 1-16 |
| <onu-id> | Ont id,range for 1-64 |
| <eth-port-id> | eth port id,range for 1-24 |
| {on/off} | On:enable eth port  Off:disable eth port |

【Example】

Example 1：Disable ont 1 eth 1 in pon 1.

|  |
| --- |
| OLT(config-interface-epon-0/0)#ont port attribute 1 1 eth 1 operational-state off  OLT(config-interface-epon-0/0)# |

### ONU Port Isolate Function Config

| Command | OLT(config-interface-epon-0/0)#ont port-isolate <port-id> <onu-id> {enable|disable} |
| --- | --- |
| **View** | EPON interface view |
| **Description** | This command is used for enable or disable ont port isolation function.If it is enabled,port to port of ont can not communicate,else they can communicate with each other. |
| <port-id> | Pon port id,range for 1-16 |
| <onu-id> | Ont id,range for 1-64 |
| {enable|disable} | Enable:enable ont port isolation function  Disable:disable ont port isolation function |

【Example】

Example 1：enable ont 1 port isolation function in pon 1.

|  |
| --- |
| OLT(config-interface-epon-0/0)#ont port-isolate 1 1 enable  OLT(config-interface-epon-0/0)# |

### ONU PON Port Performance Statistics Config

| Command | OLT(config-interface-epon-0/0)# ont statistics port-id (( onu-id eth eth-port-id ) |(all eth all)) enable/disable period period |
| --- | --- |
| **View** | EPON interface view |
| **Description** | This command is used for set performance statistics of ont’s pon port and set its statistic period. |
| port-id | Pon port id,range for 1-16 |
| onu-id | Ont id,range for 1-64 |
| eth-port-id | Eth id of ONU , range for 1-24 |
| enable/disable | Enable:enable ont’s pon port performance statistic function  Disable:disable ont’s pon port performance statistic function |
| period | The period of performance statistic,range for 1-864000,unit is second. |

【Example】

Example 1：Enable the performance statistic of ont1’s pon port in pon 1 and set its period as 100s.

|  |
| --- |
| OLT(config-interface-epon-0/0)#ont statistics 1 1 pon enable period 100  OLT(config-interface-epon-0/0)# |

### ONU ETH Port Performance Statistics Config

|  |  |
| --- | --- |
| Command | OLT(config-interface-epon-0/0)# ont statistics port-id (( onu-id eth eth-port-id ) |(all eth all)) enable/disable period period |
| **View** | EPON interface view |
| **Description** | This command is used for set performance statistics of ont’s eth port and set its statistic period. |
| port-id | Pon port id,range for 1-16 |
| onu-id | Ont id,range for 1-64 |
| eth-port-id | eth port id,range for 1-24 |
| enable|disable | Enable:enable ont’s eth port performance statistic function  Disable:disable ont’s eth port performance statistic function |
| period | The period of performance statistic,range for 1-864000,unit is second. |

【Example】

Example 1：Enable the performance statistic of ont1’s eth 1 in pon 1 and set its period as 100s.

|  |
| --- |
| OLT(config-interface-epon-0/0)#ont statistics 1 1 eth 1 enable period 100  OLT(config-interface-epon-0/0)# |

### ONU CATV Port Enable or Disable

| Command | OLT(config-interface-epon-0/0)#ont port attribute <port-id> <onu-id> catv <catv-port-id> operational-status {on/off} |
| --- | --- |
| **View** | EPON interface view |
| **Description** | This command is used for enable or disable CATV port of ont |
| <port-id> | Pon port id,range for 1-16 |
| <onu-id> | Ont id,range for 1-64 |
| <catv-port-id> | CATV port id,value is 1 |
| {on/off} | On:enable CATV port  Off:disable CATV port |

【Example】

Example1:Enable CATV port of ont 1 in pon 1.

|  |
| --- |
| OLT(config-interface-epon-0/0)#ont port attribute 1 1 catv 1 operational-state on  OLT(config-interface-epon-0/0)# |

### ONU Port Auto-negotiation Function Config

|  |  |
| --- | --- |
| Command | OLT(config-interface-epon-0/0)#ont port attribute <port-id> <onu-id> eth <eth-port-id> auto-neg {restart} |
| **View** | EPON interface view |
| **Description** | This command is used to |
| <port-id> | Pon port id,range for 1-16 |
| <onu-id> | Ont id,range for 1-64 |
| <eth-port-id> | eth port id,range for 1-24 |
| restart | Optional parameter,it is used for reset the autonegotiation function |

【Example】

Example 1：Reset the autonegotiation function of ont 1 eth 1 in pon 1.

|  |
| --- |
| OLT(config-interface-epon-0/0)#ont port attribute 1 1 eth 1 auto-neg restart  OLT(config-interface-epon-0/0)# |

### ONU Port Downstream Rate Limit Config

| Command | OLT(config-interface-epon-0/0)#ont port attribute <port-id> <onu-id> eth <eth-port-id> ds-policing {unconcern|cir <cir-bandwidth> pir <pir-bandwidth>} |
| --- | --- |
| **View** | EPON interface view |
| **Description** | This command is used for set downstream rate limitation of ont port |
| <port-id> | Pon port id,range for 1-16 |
| <onu-id> | Ont id,range for 1-64 |
| <eth-port-id> | eth port id,range for 1-24 |
| Unconcern | It means that there is no limitation in this eth port. |
| <cir-bandwidth> | Committed Information Rate,range for 64-1024000,unit is kbps |
| <pir-bandwidth> | Peak Information Rate,range for 64-1024000,unit is kbps |

【Example】

Example 1：Set downstream rate limitation of ont 1 eth 1 in pon 1,cir is 10000kpbs,pir is 100000kpbs.

|  |
| --- |
| OLT(config-interface-epon-0/0)#ont port attribute 1 1 eth 1 ds-policing cir 10000 pir 100000  OLT(config-interface-epon-0/0)# |

### ONU Port Upstream Rate Limit Config

| Command | OLT(config-interface-epon-0/0)#ont port attribute <port-id> <onu-id> eth <eth-port-id> up-policing {unconcern|cir <cir-bandwidth> cbs <cbs> ebs <ebs>} |
| --- | --- |
| **View** | EPON interface view |
| **Description** | This command is used for set upstream rate limitation of ont port |
| <port-id> | Pon port id,range for 1-16 |
| <onu-id> | Ont id,range for 1-64 |
| <eth-port-id> | eth port id,range for 1-24 |
| Unconcern | It means that there is no limitation in this eth port. |
| <cir-bandwidth> | Committed Information Rate,range for 64-1024000,unit is kbps |
| <cbs> | Committed Burst Size,range for 64-1024000,unit is kbps |
| <ebs> | Excess Burst Size,range for 2000-1024000,unit is kbps |

【Example】

Example 1：Set upstream rate limitation of ont 1 eth 1 in pon 1,cir is 10000kpbs,cbs is 1234kpbs,ebs is 2345kpbs.

|  |
| --- |
| OLT(config-interface-epon-0/0)#ont port attribute 1 1 eth 1 up-policing cir 10000 cbs 1234 ebs 2345  OLT(config-interface-epon-0/0)# |

### Enable or Disable ONU Port Flow Control Function

| Command | OLT(config-interface-epon-0/0)#ont port attribute <port-id> <onu-id> eth <eth-port-id> flow-control {on/off} |
| --- | --- |
| **View** | EPON interface view |
| **Description** | This command is used for enable or disable flow control of ont port |
| <port-id> | Pon port id,range for 1-16 |
| <onu-id> | Ont id,range for 1-64 |
| <eth-port-id> | eth port id,range for 1-24 |
| {on/off} | On:enable flow control of ont port  Off:disable flow control of ont port |

【Example】

Example 1：enable flow control of ont 1 eth 1 in pon 1.

|  |
| --- |
| OLT(config-interface-epon-0/0)#ont port attribute 1 1 eth 1 flow-control on  OLT(config-interface-epon-0/0)# |

### Clear ONU Port Learned MAC

|  |  |
| --- | --- |
| Command | OLT(config-interface-epon-0/0)#ont port learned-mac-clear <port-id> <onu-id> eth <eth-port-id> |
| **View** | EPON interface view |
| **Description** | This command is used for clear the learned mac of ont port |
| <port-id> | Pon port id,range for 1-16 |
| <onu-id> | Ont id,range for 1-64 |
| <eth-port-id> | eth port id,range for 1-24 |

【Example】

Example 1：Clear the learned mac of ont 1 eth 1 in pon 1.

|  |
| --- |
| OLT(config-interface-epon-0/0)#ont port learned-mac-clear 1 1 eth 1  OLT(config-interface-epon-0/0)# |

### Clear Performance Statistics of the ONU Port

|  |  |
| --- | --- |
| Command | OLT(config-interface-epon-0/0)# reset statistics ont-pon port-id ont-id | ont-eth port-id ont-id eth ont-port-id |
| **View** | epon view |
| **Description** | This command is used for clear performance statistics of onu port. |
| port-id | Pon port id,range for 1-16 |
| ont-id | Ont id,range for 1-64 |
| ont-port-id | eth port id,range for 1-24 |

【Example】

Example 1：Clear performance statistics of PON 9 ONU 4.

|  |
| --- |
| OLT(config-interface-epon-0/0)# reset statistics ont-pon 9 4  OLT(config-interface-epon-0/0)# |

### ONU Port MAC Count Limit Function Config

|  |  |
| --- | --- |
| Command | OLT(config-interface-epon-0/0)#ont port attribute <port-id> <onu-id> eth <eth-port-id> max-mac-count {<max-mac-count> |no-learning|unlimited} |
| **View** | EPON interface view |
| **Description** | This command is used for limit the learned mac count of ont port. |
| <port-id> | Pon port id,range for 1-16 |
| <onu-id> | Ont id,range for 1-64 |
| <eth-port-id> | eth port id,range for 1-24 |
| {<max-mac-count>|no-learning|unlimited} | Max-mac-count:range for 1-254  No-learning:no learning mac address  Unlimited:unlimit the count of learned mac address |

【Example】

Example 1：Limit the learned mac address count of ont 1 eth 1 in pon 1 as 100 entries.

|  |
| --- |
| OLT(config-interface-epon-0/0)#ont port attribute 1 1 eth 1 max-mac-count 100  OLT(config-interface-epon-0/0)# |

### ONU Port Multicast Group Number Limit Config

|  |  |
| --- | --- |
| Command | OLT(config-interface-epon-0/0)#ont port attribute <port-id> <onu-id> eth <eth-port-id> multicast-max-group-num <number> |
| **View** | EPON interface view |
| **Description** | This command is used for limit the multicast group number of ont port |
| <port-id> | Pon port id,range for 1-16 |
| <onu-id> | Ont id,range for 1-64 |
| <eth-port-id> | eth port id,range for 1-24 |
| <number> | Max multicast group number,range for 0-255 |

【Example】

Example 1：Limit the multicast group number of ont 1 eth 1 in pon 1 as 5 entries.

|  |
| --- |
| OLT(config-interface-epon-0/0)#ont port attribute 1 1 eth 1 multicast-max-group-num 5  OLT(config-interface-epon-0/0)# |

### ONU Port Multicast VLAN Process Mode Config

| Command | OLT(config-interface-epon-0/0)#ont port attribute <port-id> <onu-id> eth <eth-port-id> multicast-tagstrip {tag|untag|translation} {<service-vlan><customer-vlan>} |
| --- | --- |
| **View** | EPON interface view |
| **Description** | This command is used for set the multicast vlan mode of ont eth port. |
| <port-id> | Pon port id,range for 1-16 |
| <onu-id> | Ont id,range for 1-64 |
| <eth-port-id> | eth port id,range for 1-24 |
| {tag|untag|translation} | Tag:no peeling off multicast VLAN tag  Untag:peel off multicast VLAN tag  Translation:translates the multicast vlan |
| <service-vlan> | Server-side VLAN,range for 1-4094 |
| <customer-vlan> | Customer VLAN,range for 1-4094 |

【Example】

Example 1：Set the multicast vlan mode of ont 1 eth 1 in pon 1 as tag.

|  |
| --- |
| OLT(config-interface-epon-0/0)#ont port attribute 1 1 eth 1 multicast-tagstrip untag  OLT(config-interface-epon-0/0)# |

Example 2:Set the multicast vlan mode of ont 1 eth 1 in pon 1 as translation,translate the server-side vlan 10 to customer vlan 11.

|  |
| --- |
| OLT(config-interface-epon-0/0)#ont port attribute 1 1 eth 1 multicast-tagstrip translation 10 11  OLT(config-interface-epon-0/0)# |

### ONU Port Speed and Duplex Mode Config

| Command | OLT(config-interface-epon-0/0)#ont port attribute <port-id> <onu-id> eth <eth-port-id> speed <speed> dulepx {full/half} |
| --- | --- |
| **View** | EPON interface view |
| **Description** | This command is used for set the speed and duplex mode of ont port. |
| <port-id> | Pon port id,range for 1-16 |
| <onu-id> | Ont id,range for 1-64 |
| <eth-port-id> | eth port id,range for 1-24 |
| <speed> | 10：10Mb/s  100：100Mb/s  1000：1000Mb/s |
| full/half | Full:full duplex  Half:half duplex |

【Example】

Example 1：Set the speed of ont 1 eth 1 in pon 1 as 1000Mbps,and set its duplex mode as full.

|  |
| --- |
| OLT(config-interface-epon-0/0)#ont port attribute 1 1 eth 1 speed 1000 dulepx full  OLT(config-interface-epon-0/0)# |

### ONU Port Storm-ctrl Function Config

| Command | OLT(config-interface-epon-0/0)#ont port attribute <port-id> <onu-id> eth <eth-port-id> xstorm-ctrl admin {disable/enable} type {all|bcmc|bcuc|broadcast|mcuc|multicast|unicast} rate<rate> |
| --- | --- |
| **View** | EPON interface view |
| **Description** | This command is used for set strom-ctrl funcction of ont port and set its rate limitation |
| <port-id> | Pon port id,range for 1-16 |
| <onu-id> | Ont id,range for 1-64 |
| <eth-port-id> | eth port id,range for 1-24 |
| {disable|enable} | Disable:disable storm-ctrl function  Enable:enable storm-ctrl function |
| all|bcmc|bcuc|broadcast|mcuc|multicast|unicast | All:all of the broadcast message,multicast message,and unicast message  Bcmc:broadcast message and multicast message  Bcuc:broadcast message and unicast message  Broadcast:broadcast message  Mcuc:multicast message and unicast message  Multicast:multicast message  Unicast:unknown unicast message |
| <rate> | Rate,range for 8-16777215,unit is kbps |

【Example】

Example 1：Enable the storm-ctrl function of ont 1 eth 1 in pon 1,and set its unknown unicast rate limitation as 5000kbps.

|  |
| --- |
| OLT(config-interface-epon-0/0)#ont port attribute 1 1 eth 1 storm-ctrl admin enable type unicast rate 5000  OLT(config-interface-epon-0/0)# |

### Enable or Disable ONU Port Loop Detect Function

| Command | OLT(config-interface-epon-0/0)#ont ring check <port-id> <onu-id> {enable|disable} |
| --- | --- |
| **View** | EPON interface view |
| **Description** | This command is used for enable or disable the ring check of specified ont in pon port.After enabling this function,the olt will alarm if there is a ring in ont. |
| <port-id> | Pon port id,range for 1-16 |
| <onu-id> | Ont id,range for 1-64 |
| {enable|disable} | Enable  Disable |

【Example】

Example 1：Enable ring check of ont 1 in pon 1.

|  |
| --- |
| OLT(config-interface-epon-0/0)#ont ring check 1 1 enable  OLT(config-interface-epon-0/0)# |

### Enable or Disable ONU Port Loop Detected

**Auto-shutdown Function**

| Command | OLT(config-interface-epon-0/0)#ont ring check <port-id> <onu-id> auto-shutdown {enable|disable} |
| --- | --- |
| **View** | EPON interface view |
| **Description** | This command is used for enable or disable auto-shutdown eth port when ring occurs in ont.After executing this command,if ont has a ring,ont will shutdown the port to prevent the ring from affecting the upper network.the default is“enable” |
| <port-id> | Pon port id,range for 1-16 |
| <onu-id> | Ont id,range for 1-64 |
| {enable|disable} | Enable  Disable |

【Example】

Example 1：Enable auto-shutdown eth port of ont 1 in pon 1.

|  |
| --- |
| OLT(config-interface-epon-0/0)#ont ring check 1 1 auto-shutdown enable  OLT(config-interface-epon-0/0)# |

### ONU Port Upstream classification/mapping/priority-mark Rule Config

| Command | OLT(config-interface-epon-0/0)#ont port classification <port-id> < onu-id > eth <eth-port-id> acl <acl-id> rule <rule-id> { precedence <precedence> queue-mapped <queue-id> priority-mark <priority>|no-priority-mark } |
| --- | --- |
| **View** | EPON interface view |
| **Description** | This command is used for set upstream classification/mapping/priority-mark rule of ont port |
| <port-id> | Pon port id,range for 1-16 |
| <onu-id> | Ont id,range for 1-64 |
| <eth-port-id> | eth port id,range for 1-24 |
| <acl-id> | Acl id,range for 9000-9499 |
| <rule-id> | Rule id,range for 1-8 |
| <precedence> | Priority,range for 0-255 |
| <queue-id> | Queue id,range for 0-7 |
| <priority>|no-priority-mark | <priority>:priority mark,range for 0-7  no-priority-mark |

【Example】

Example 1：Map the ont 1 eth 1 in pon 1 to acl 9000 and rule 1.

|  |
| --- |
| OLT(config-interface-epon-0/0)#ont port classification 1 1 eth 1 acl 9000 rule 1  OLT(config-interface-epon-0/0)# |

### Show ONU Port Performance State

| Command | OLT(config-interface-epon-0/0)#show ont statistics <port-id> <onu-id> eth <eth-port-id> status |
| --- | --- |
| **View** | EPON interface view |
| **Description** | This command is used for show performance statistics of ont port |
| <port-id> | Pon port id,range for 1-16 |
| <onu-id> | Ont id,range for 1-64 |
| <eth-port-id> | eth port id,range for 1-24 |

【Example】

Example 1：Show performance statistics of ont 1 eth 1 in pon 1.

|  |
| --- |
| OLT(config-interface-epon-0/0)#show ont statistics 1 1 eth 1 status  -----------------------------------------------------------------------------  S/P:0/1  ONU ID:1  Port ID:UNI1  Statistics status:Disable  Statistics period:0  -----------------------------------------------------------------------------  OLT(config-interface-epon-0/0)# |

### Show ONU Port Performance Statistics

| Command | OLT(config-interface-epon-0/0)# show statistics <ont-pon port-id onu-id|ont-eth port-id onu-id eth eth-id > current|history |
| --- | --- |
| **View** | epon view |
| **Description** | This command is used for show ONU port performance statistics. |
| port-id | Pon port id,range for 1-16 |
| onu-id | Ont id,range for 1-64 |
| eth-id | eth port id,range for 1-24 |

【Example】

Example 1：Show PON11 ONU6 pon port performance statistics currently.

|  |
| --- |
| OLT(config-interface-epon-0/0)# show statistics ont-pon 11 6 current  Downstream DropEvents : 0  Downstream Octets : 0  Downstream Frames : 0  Downstream Broadcast Frames : 0  Downstream Multicast Frames : 0  Downstream CRC errored frames : 0  Downstream Undersize Frames : 0  Downstream Oversize Frames : 0  Downstream Fragments : 0  Downstream Jabbers : 0  Downstream Frames 64 octets : 0  Downstream Frames 65 to 127 octets : 0  Downstream Frames 128 to 255 octets : 0  Downstream Frames 256 to 511 octets : 0  Downstream Frames 512 to 1023 octets : 0  Downstream Frames 1024 to 1518 octets : 0  Downstream Discard Frames : 0  Downstream error Frames : 0    Upstream DropEvents : 0  Upstream Octets : 0  Upstream Frames : 0  Upstream Broadcast Frames : 0  Upstream Multicast Frames : 0  Upstream CRC errored frames : 0  Upstream Undersize Frames : 0  Upstream Oversize Frames : 0  Upstream Fragments : 0  Upstream Jabbers : 0  Upstream Frames 64 octets : 0  Upstream Frames 65 to 127 octets : 0  Upstream Frames 128 to 255 octets : 0  Upstream Frames 256 to 511 octets : 0  Upstream Frames 512 to 1023 octets: 0  Upstream Frames 1024 to 1518 octets : 0  Upstream Discard Frames : 0  Upstream error Frames : 0    Status Change times : 0  OLT(config-interface-epon-0/0)# |

### Show the service flow classification/mapping/priority marking information of the ONU port.

| Command | OLT(config-interface-epon-0/0)# show ont port classification port-id ont-id eth eth-port-id|all |
| --- | --- |
| **View** | epon view |
| **Description** | This command is used for show the service flow classification/ mapping/priority marking information of the ONU port. |
| port-id | Pon port id,range for 1-16 |
| ont-id | Ont id,range for 1-64 |
| eth-port-id | eth port id,range for 1-24 |

【Example】

Example 1：Show PON1 ONU3 eth1 classification rule.

|  |
| --- |
| OLT(config-interface-epon-0/0)# show ont port classification 1 3 eth 1  ERROR: There is no ACL bound to current ONT port.  OLT(config-interface-epon-0/0)# |

### Show the MAC address learned on the ONU port

| Command | OLT(config-interface-epon-0/0)# show ont port learned-mac port-id ont-id eth eth-port-id |
| --- | --- |
| **View** | epon view |
| **Description** | This command is used for show the mac address learned on the ONU port. |
| port-id | Pon port id,range for 1-16 |
| ont-id | Ont id,range for 1-64 |
| eth-port-id | eth port id,range for 1-24 |

【Example】

Example 1：Show PON1 ONU3 eth1 learned mac address.

|  |
| --- |
| OLT(config-interface-epon-0/0)# show ont port learned-mac 1 3 eth 1  There is not any MAC address record!  OLT(config-interface-epon-0/0)# |

### Show the Policy Information of the ONU Ethernet Port

|  |  |
| --- | --- |
| Command | OLT(config-interface-epon-0/0)# show ont port attribute <port-id> <onu-id> eth <eth-id> policing |
| **View** | epon view |
| **Description** | This command is used for show the policy information of the ONU Ethernet port. |
| <port-id> | Pon port id,range for 1-16 |
| <onu-id> | Ont id,range for 1-64 |
| <eth-id> | eth port id,range for 1-24 |

【Example】

Example 1：Show PON9 ONU5 eth1 policy information.

|  |
| --- |
| OLT(config-interface-epon-0/0)# show ont port attribute 9 5 eth 1 policing  -----------------------------------------------------------------------------  Frame/Slot : 0/0  Port : 9  ONT ID : 5  Port ID : 1  ----------------------------------------------------------------------------  UP policing : unconcern  ----------------------------------------------------------------------------  DN policing : unconcern  -----------------------------------------------------------------------------  OLT(config-interface-epon-0/0)# |

### Show the Storm Control Config of the ONU Ethernet Port

|  |  |
| --- | --- |
| Command | OLT(config-interface-epon-0/0)# show ont storm-ctrl <port-id> < onu-id > eth <eth-id> |
| **View** | epon view |
| **Description** | This command is used for show the storm control config of the ONU ethernet port. |
| <port-id> | Pon port id,range for 1-16 |
| < onu-id > | Ont id,range for 1-64 |
| <eth-id> | eth port id,range for 1-24 |

【Example】

Example 1：Show PON1 ONU13 eth1 storm control config.

|  |
| --- |
| OLT(config-interface-epon-0/0)# show ont port storm-ctrl 1 3 eth 1  -----------------------------------------------------------------------------  Frame/Slot : 0/0  Port : 1  ONT-ID : 3  Port ID : 1  Flow control switch : disable  -----------------------------------------------------------------------------  OLT(config-interface-epon-0/0)# |

### Show ONU Port Attribute(Configuration)

|  |  |
| --- | --- |
| Command | OLT(config-interface-epon-0/0)#show ont port attribute <port-id> <onu-id> eth all |
| **View** | EPON interface view |
| **Description** | This command is used for show ont port attribute |
| <port-id> | Pon port id,range for 1-16 |
| <onu-id> | Ont id,range for 1-64 |
| all | All the eth port |

【Example】

Example 1：Show all the eth port attribute of ont 3 in pon 3.

|  |
| --- |
| OLT(config-interface-epon-0/0)#show ont port attribute 3 3 eth all  -----------------------------------------------------------------------------  ONU ONU Auto-neg Speed Duplex Port Flow Mac  port(Mbps)switch control Limit  ----------------------------------------------------------------------------  3 1 Enable Auto Auto on off unlimited  3 2 Enable Auto Auto on off unlimited  3 3 Enable Auto Auto on off unlimited  3 4 Enable Auto Auto on off unlimited  3 5 Enable Auto Auto on off unlimited  3 6 Enable Auto Auto on off unlimited  3 7 Enable Auto Auto on off unlimited  3 8 Enable Auto Auto on off unlimited  -----------------------------------------------------------------------------  OLT(config-interface-epon-0/0)# |

### Show ONU CATV Port Status

|  |  |
| --- | --- |
| Command | OLT(config-interface-epon-0/0)#show ont port state <port-id> <onu-id> {eth|catv<onu-portid>} |
| **View** | EPON interface view |
| **Description** | Ths command is used for show state of ont’s eth port and catv port |
| <port-id> | Pon port id,range for 1-16 |
| <onu-id> | Ont id,range for 1-64 |
| <ONU-portid> | Port id of eth or catv |

【Example】

Example 1：Show all eth port state of ont 2 in pon 1.

|  |
| --- |
| OLT(config-interface-epon-0/0)#show ont port state 1 2 eth all  -----------------------------------------------------------------------------  Port Type Port-switch Link Flow-cONUrol Auto-neg Max-MAC  ----------------------------------------------------------------------------  1 eth on on off enable unlimit  2 eth on off off enable unlimit  3 eth on off off enable unlimit  4 eth on off off enable unlimit  -----------------------------------------------------------------------------  OLT(config-interface-epon-0/0)# |

### Show ONU Port Learned MAC Address Information

|  |  |
| --- | --- |
| Command | OLT(config-interface-epon-0/0)#show ont port learned-mac <port-id> <onu-id> eth <eth-id> |
| **View** | EPON interface view |
| **Description** | This command is used for show learned-mac address of ont port |
| <port-id> | Pon port id,range for 1-16 |
| <onu-id> | Ont id,range for 1-64 |
| all | All the eth port |

【Example】

Example 1：Show learned-mac address of ont3’s all eth port in pon 3.

|  |
| --- |
| OLT(config-interface-epon-0/0)#show ont port learned-mac 1 5 eth 1  -----------------------------------------------------------------------------  Index MAC  ----------------------------------------------------------------------------  1 F0:DE:F1:62:C5:97  2 74:D0:2B:A1:F1:84  3 E0:67:B3:00:57:3E  4 5C:FF:35:0D:D8:C5  5 EC:6C:9F:05:49:79  6 20:6A:8A:54:6C:7D  -----------------------------------------------------------------------------  OLT(config-interface-epon)# |

### Show ONU PON Port Performance Statistics

|  |  |
| --- | --- |
| Command | OLT(config-interface-epon-0/0)#show ont statistics <port-id> <onu-id> pon status |
| **View** | EPON interface view |
| **Description** | This command is used for show performance statistics of ont’s pon port |
| <port-id> | Pon port id,range for 1-16 |
| <onu-id> | Ont id,range for 1-64 |

【Example】

Example 1：Show performance statistics of ont 1’s pon port in pon 1.

|  |
| --- |
| OLT(config-interface-epon-0/0)#show ont statistics 1 1 pon status  -----------------------------------------------------------------------------  S/P:0/1  ONU ID:1  Port ID:PON1  Statistics status:Disable  Statistics period:0  -----------------------------------------------------------------------------  OLT(config-interface-epon-0/0)# |

### Delete the Configured Bandwidth Rate Limit of ONU Port

|  |  |
| --- | --- |
| Command | OLT(config-interface-epon-0/0)# no ont port attribute <port-id> < onu-id > eth <eth-port-id> up-policing|ds-policing |
| **View** | epon view |
| **Description** | This command is used for delete the configured bandwidth rate limit of the ONU port. |
| <port-id> | Pon port id,range for 1-16 |
| < onu-id > | Ont id,range for 1-64 |
| <eth-port-id> | eth port id,range for 1-24 |

【Example】

Example 1：Delete the upstream bandwidth rate limit of PON7 ONU1.

|  |
| --- |
| OLT(config-interface-epon-0/0)# no ont port attribute 7 1 eth 1 up-policing  Restore to the profile configuration successfully  OLT(config-interface-epon-0/0)# |

### Delete the Number of Learned MAC Addresses Restricted by the ONU Port

| Command | OLT(config-interface-epon-0/0)# no ont port attribute <port-id> < onu-id > eth <eth-port-id> max-mac-ount |
| --- | --- |
| **View** | Epon view |
| **Description** | This command is used for delete the number of learned MAC addresses restricted by the ONU port. |
| <port-id> | Pon port id,range for 1-16 |
| < onu-id > | Ont id,range for 1-64 |
| <eth-port-id> | eth port id,range for 1-24 |

【Example】

Example 1：delete the number of learned MAC addresses restricted by PON7 ONU1.

|  |
| --- |
| OLT(config-interface-epon-0/0)# no ont port attribute 7 1 eth 1 max-mac-count  Restore to the profile configuration successfully  OLT(config-interface-epon-0/0)# |

### Delete the Maximum Number of Multicast Groups Restricted by the ONU Port

|  |  |
| --- | --- |
| Command | OLT(config-interface-epon-0/0)# no ont port attribute <port-id> < onu-id > eth <eth-port-id> multicast-max-group-num |
| **View** | epon view |
| **Description** | This command is used for delete the maximum number of multicast groups restricted by the ONU port. |
| <port-id> | Pon port id,range for 1-16 |
| < onu-id > | Ont id,range for 1-64 |
| <eth-port-id> | eth port id,range for 1-24 |

【Example】

Example 1：Delete PON7 ONU1 ETH1 the maximum number of multicast groups restricted

|  |
| --- |
| OLT(config-interface-epon-0/0)# no ont port attribute 7 1 eth 1 multicast-max-group-num  Restore to the profile configuration successfully  OLT(config-interface-epon-0/0)# |

### Delete the Processing Mode of the Multicast Stream VLAN on the ONU Port

| Command | OLT(config-interface-epon-0/0)# no ont port attribute <port-id> < onu-id > eth <eth-port-id> multicast-tagstrip translation <service-vlan> |
| --- | --- |
| **View** | epon view |
| **Description** | This command is used for delete the processing mode of the multicast stream VLAN on the ONU port. |
| <port-id> | Pon port id,range for 1-16 |
| < onu-id > | Ont id,range for 1-64 |
| <eth-port-id> | eth port id,range for 1-24 |
| <service-vlan> | Service VLAN，range for 1-4094 |

【Example】

Example 1：Delete PON7 ONU1 ETH1 the conversion mode of multicast stream VLAN100.

|  |
| --- |
| OLT(config-interface-epon-0/0)# no ont port attribute 7 1 eth 1 multicast-tagstrip translation 100  OLT(config-interface-epon-0/0)# |

### Delete the Rules of ONU Port for the Upstream Service Flow

| Command | OLT(config-interface-epon-0/0)# no ont port classification <port-id> < onu-id > eth <eth-port-id> acl <acl-id> rule <rule-id> |
| --- | --- |
| **View** | epon view |
| **Description** | This command is used for delete the rules of the ONU port for the upstream service flow. |
| <port-id> | Pon port id,range for 1-16 |
| < onu-id > | Ont id,range for 1-64 |
| <eth-port-id> | eth port id,range for 1-24 |
| <acl-id> | Acl id，range for 9000-9499 |
| <rule-id> | Rule id，range for 1-8 |

【Example】

Example 1：Delete PON7 ONU1 ETH1 ACL9000 rule1.

|  |
| --- |
| OLT(config-interface-epon-0/0)# no ont port classification 7 1 eth 1 acl 9000 rule 1  ERROR: The acl has not been installed before  OLT(config-interface-epon-0/0)# |

## ONU WIFI Config

### Enable or Disable WIFI

|  |  |
| --- | --- |
| Command | OLT(config-interface-epon-0/0)# ont wifi port-id ont-id admin enable|disable |
| **View** | epon view |
| **Description** | This command is used for enable/disable onu wifi. |
| port-id | Pon port id,range for 1-16 |
| ont-id | Ont id,range for 1-64 |

【Example】

Example 1：Enable PON 7 ONU 2 wifi

|  |
| --- |
| OLT(config-interface-epon-0/0)# ont wifi 7 2 admin enable  OLT(config-interface-epon-0/0)# |

### Config Maximum Number of Wireless SSID User accesses

| Command | OLT(config-interface-epon-0/0)# ont wifi port-id ont-id ssid ontwifi-ssid-id max-user-count max-access-number |
| --- | --- |
| **View** | epon view |
| **Description** | This command is used for config ONU WIFI the maximum number ofwireless ssid user accesses. |
| port-id | Pon port id,range for 1-16 |
| ont-id | Ont id,range for 1-64 |
| ontwifi-ssid-id | Ssid index，range for 1-4 |
| max-access-number | Maximum number of user accesses, range for 0-128,default as 10. |

【Example】

Example 1：Config PON 7 ONU 2 maximum user accesses of wireless ssid is 100

|  |
| --- |
| OLT(config-interface-epon-0/0)# ont wifi 7 2 ssid 1 max-user-count 100  OLT(config-interface-epon-0/0)# |

### Config Wireless SSID

| Command | OLT(config-interface-epon-0/0)# ont wifi port-id ont-id ssid ontwifi-ssid-id admin (enable broadcast-admin enable|disable SSID-Name (none|wep |wpa|wpa2|wpa\_wpa2 ENCRYPTKEY) |disable) |
| --- | --- |
| **View** | epon view |
| **Description** | This command is used for config the ONU WIFI wireless ssid parameter. |
| port-id | Pon port id,range for 1-16 |
| ont-id | Ont id,range for 1-64 |
| ontwifi-ssid-id | Ssid index，range for 1-4 |
| SSID-Name | Ssid name，range for 1-32 |
| none|wep |wpa|wpa2|wpa\_wpa2 | Wireless encryption method |
| ENCRYPTKEY | Encryption key, supporting 1-64 characters length. |

【Example】

Example 1：Set the maximum number of wifi ssid users with PON7 port ONU id 2 to 100.

|  |
| --- |
| OLT(config-interface-epon-0/0)# ont wifi 7 2 ssid 1 admin enable broadcast-admin enable HGW-1211C8 wpa 123  OLT(config-interface-epon-0/0)# |

### Config WIFI Properties

| Command | OLT(config-interface-epon-0/0)# ont wifi attribute port-id ont-id channel-id wifi-channel-id wlan-standard (802.11b|802.11g|802.11n |802.11b/g|802.11b/g/n) channel-bandwidth (forty-minus| forty-plus|twenty) txpower-mode (energy|noclip|standard) |
| --- | --- |
| **View** | epon view |
| **Description** | This command is used for config wifi properties, such as wifi channel,bandwidth,etc. |
| port-id | Pon port id,range for 1-16 |
| ont-id | Ont id,range for 1-64 |
| wifi-channel-id | Config wireless network working channel, range for 0-13. |
| forty-minus| forty-plus| twenty | The channel width occupied when setting up wireless data transmission:  Twenty: 20MHz, channel selection 0-13  Forty-minus: 40MHz-, channel selection 1-9  Forty-plus: 40MHz+, channel selection 5-12 |
| energy|noclip| standard | Set the transmit power: energy is energy saving; noclip is through the wall (maximum power); standard is standard (default). |

【Example】

Example 1：Set the wifi attribute of the PON9 port ONU id to 4.

|  |
| --- |
| OLT(config-interface-epon-0/0)# ont wifi attribute 9 4 channel-id 6 wlan-standard 802.11n channel-bandwidth twenty txpower-mode standard  OLT(config-interface-epon-0/0)# |

### WIFI Factory Reset

|  |  |
| --- | --- |
| Command | OLT(config-interface-epon-0/0)# ont wifi default-setting port-id ont-id |
| **View** | epon view |
| **Description** | This command is used for WIFI factory reset. |
| port-id | Pon port id,range for 1-16 |
| ont-id | Ont id,range for 1-64 |

【Example】

Example 1：Config pon 9 onu 4 wifi to factory reset.

|  |
| --- |
| OLT(config-interface-epon-0/0)# ont wifi default-setting 9 4  OLT(config-interface-epon-0/0)# |

### Show Wireless SSID Information

|  |  |
| --- | --- |
| Command | OLT(config-interface-epon-0/0)# show ont wifi port-id ont-id ssid all|ssid-index |
| **View** | epon view |
| **Description** | This command is used for show wireless ssid information. |
| port-id | Pon port id,range for 1-16 |
| ont-id | Ont id,range for 1-64 |
| all|ssid-index | All：all SSID；  Ssid-index：ssid index，range for 1-4 |

【Example】

Example 1：Show PON9 ONU 4 WIFI ssid information

|  |
| --- |
| OLT(config-interface-epon-0/0)# show ont wifi 11 1 ssid all  ---------------------------------------------------------------------------------------  Ssid Name Admin BcastAdmin EncryptMode EncryptKey MaxUsers  --------------------------------------------------------------------------------------  1 testwifi enable enable wpa2 12345678 10  2 AP-1111 disable enable none 10  3 AP-2222 disable enable none 10  4 AP-3333 disable enable none 10  ---------------------------------------------------------------------------------------  OLT(config-interface-epon-0/0)# |

### Show WIFI Information

|  |  |
| --- | --- |
| Command | OLT(config-interface-epon-0/0)# show ont wifi info port-id ont-id |
| **View** | epon view |
| **Description** | This command is used for show ONU wifi information. |
| port-id | Pon port id,range for 1-16 |
| ont-id | Ont id,range for 1-64 |

【Example】

Example 1：Show PON9 ONU 4 wifi information.

|  |
| --- |
| OLT(config-interface-epon-0/0)# show ont wifi info 9 4  -----------------------------------------------------------------------------  Frame/Slot : 0/0  Port : 9  ONT-ID : 4  Wifi state : enable  Channel ID : 0  Wlan Standard : 802.11b/g/n  Channel Bandwidth : 40MHz+  TxPower Mode : noclip  -----------------------------------------------------------------------------  OLT(config-interface-epon-0/0)# |

### Show WIFI Version

|  |  |
| --- | --- |
| Command | OLT(config-interface-epon-0/0)# show ont wifi version port-id ont-id |
| **View** | epon view |
| **Description** | This command is used for show wifi version information. |
| port-id | Pon port id,range for 1-16 |
| ont-id | Ont id,range for 1-64 |

【Example】

Example 1：Show PON9 ONU 4 wifi version

|  |
| --- |
| OLT(config-interface-epon-0/0)# show ont wifi version 9 4  -----------------------------------------------------------------------------  Frame/Slot : 0/0  Port : 9  ONT-ID : 4  Wifi hardware Ver : V1.0.0  Wifi software Ver : V2.1.11  -----------------------------------------------------------------------------  OLT(config-interface-epon-0/0)# |

## ONU IGMP Function Configuration(Non-template Mode)

### ONU IGMP Mode Config

| Command | OLT(config-interface-epon-0/0)#ont multicast-mode <port-id> <onu-id> <mode> |
| --- | --- |
| **View** | EPON interface view |
| **Description** | This command is used for set multicast mode of ont |
| <port-id> | Pon port id,range for 1-16 |
| <onu-id> | Ont id,range for 1-64 |
| <mode> | Ctc:controllable multicast mode  transparent  igmp-snooping |

【Example】

Example 1：Set the multicast mode of ont 4 in pon 1 as snooping mode.

|  |
| --- |
| OLT(config-interface-epon-0/0)#ont multicast-mode 1 4 igmp-snooping  OLT(config-interface-epon-0/0)# |

### ONU Fsast-leave Function Config

|  |  |
| --- | --- |
| Command | OLT(config-interface-epon-0/0)#ont multicast fast-leave <port-id> <onu-id> {enable|disable} |
| **View** | EPON interface view |
| **Description** | This command is used for set ont multicast fast-leave. |
| <port-id> | Pon port id,range for 1-16 |
| <onu-id> | Ont id,range for 1-64 |
| {enable|disable} | Enable:enable multicast fast-leave  Disable:disable multicast fast-leave |

【Example】

Example 1：Enable multicast fast-leave in pon 1 onu 4.

|  |
| --- |
| OLT(config-interface-epon-0/0)#ont multicast fast-leave 1 4 enable  OLT(config-interface-epon-0/0)# |

### Config the multicast VLAN of the ONU port

| Command | OLT(config-interface-epon-0/0)# ont port multicast-vlan port-id ont-id eth ont-port-list vlan-id |
| --- | --- |
| **View** | epon view |
| **Description** | This command is used for configure the multicast VLAN of an ONT port. Use this command when you need to divide an ONT port into a specified multicast VLAN. You need to configure the ONT port multicast mode in epon mode before executing this command. |
| port-id | Pon port id,range for 1-16 |
| ont-id | Ont id,range for 1-64 |
| ont-port-list | Pon port id,range for 1-16 |
| vlan-id | Ont id,range for 1-64 |

【Example】

Example 1：Add the multicast vlan 100 to the pon1 ONU1 Eth port 1

|  |
| --- |
| OLT(config-interface-epon-0/0)# ont port multicast-vlan 1 1 eth 1 100  OLT(config-interface-epon-0/0)# |

### Show ONU Multicast-group Record

|  |  |
| --- | --- |
| Command | OLT(config-interface-epon-0/0)#show ont multicast-group <port-id> <onu-id> |
| **View** | EPON interface view |
| **Description** | This command is used for show multicast-group of ont. |
| <port-id> | Pon port id,range for 1-16 |
| <onu-id> | Ont id,range for 1-64 |

【Example】

Example 1：Show multicast-group of ont 1 in pon 1.

|  |
| --- |
| OLT(config-interface-epon-0/0)#show ont multicast-group 1 1  ERROR:There is not any onu group record  OLT(config-interface-epon-0/0)# |

### Show ONU IGMP Mode

|  |  |
| --- | --- |
| Command | OLT(config-interface-epon-0/0)#show ont multicast-mode <port-id> <onu-id> |
| **View** | EPON interface view |
| **Description** | This command is used for show multicast-mode of ont. |
| <port-id> | Pon port id,range for 1-16 |
| <onu-id> | Ont id,range for 1-64 |

【Example】

Example 1：Show multicast-mode of ont 3 in pon 3.

|  |
| --- |
| OLT(config-interface-epon-0/0)#show ont multicast-mode 3 3  -----------------------------------------------------------------------------  Frame/Slot:0/0  Port:3  ONU-ID:3  Multicast mode:Transparent  -----------------------------------------------------------------------------  OLT(config-interface-epon-0/0)# |

### Show ONU Port IGMP VLAN Tagstrip Mode

| Command | OLT(config-interface-epon-0/0)#show ont port attribute <port-id> <onu-id> eth <eth-id> multicast-tagstrip |
| --- | --- |
| **View** | EPON interface view |
| **Description** | This command is used for show multicast-tagstrip mode of ont eth port |
| <port-id> | Pon port id,range for 1-16 |
| <onu-id> | Ont id,range for 1-64 |
| <eth-id> | Eth port id,range for 1-24 |

【Example】

Example 1：Show multicast-tagstrip mode of ont 3 eth 1 in pon 3.

|  |
| --- |
| OLT(config-interface-epon-0/0)#show ont port attribute 3 3 eth 1 multicast-tagstrip  -----------------------------------------------------------------------------  Frame/Slot:0/0  Port:3  ONU ID:3  Port ID:1  ----------------------------------------------------------------------------  Service Profile ID:0  Service Profile name:srvprofile\_0  ----------------------------------------------------------------------------  Tag strip mode:tag  -----------------------------------------------------------------------------  OLT(config-interface-epon-0/0)# |

### Show ONU Port Multicast VLAN

|  |  |
| --- | --- |
| Command | OLT(config-interface-epon-0/0)# show ont port multicast-vlan port-id onu-id eth eth-id |
| **View** | epon view |
| **Description** | This command is used for show ONU port multicast vlan. |
| port-id | Pon port id,range for 1-16 |
| onu-id | Ont id,range for 1-64 |
| eth-id | Eth port id,range for 1-24 |

【Example】

Example 1：Show PON 1 ONU3 ETH1 multicast-vlan mde.

|  |
| --- |
| OLT(config-interface-epon-0/0)# show ont port multicast-vlan 1 3 eth 1  -----------------------------------------------------------------------------  Frame/Slot : 0/0  Port : 1  ONT-ID : 3  Port ID : 1  Multicast vlan : 100,  -----------------------------------------------------------------------------  OLT(config-interface-epon-0/0)# |

### Disable the Multicast Fast Leave Function of the ONU

|  |  |
| --- | --- |
| Command | OLT(config-interface-epon-0/0)# no ont multicast fast-leave port-id ont-id |
| **View** | epon view |
| **Description** | This command is used for disable the multicast fast leave function of the ONU. |
| port-id | Pon port id,range for 1-16 |
| ont-id | Ont id,range for 1-64 |

【Example】

Example 1：Disable PON7 ONU1 multicast fast-leave function.

|  |
| --- |
| OLT(config-interface-epon-0/0)# no ont multicast fast-leave 7 1  Restore to the profile configuration successfully  OLT(config-interface-epon-0/0)# |

### Delete the Multicast VLAN of the ONU Port

| Command | OLT(config-interface-epon-0/0)# no ont multicast-vlan port-id ont-id eth eth-portid vlan-id |
| --- | --- |
| **View** | epon view |
| **Description** | This command is used for delete the multicast vlan of the ONU port. |
| port-id | Pon port id,range for 1-16 |
| ont-id | Ont id,range for 1-64 |
| eth-portid | Eth port id,range for 1-24 |
| vlan-id | Multicast vlan id,range for 1-4094 |

【Example】

Example 1：Delete the multicast vlan of PON7 ONU1 eth1.

|  |
| --- |
| OLT(config-interface-epon-0/0)# no ont port multicast-vlan 7 1 eth 1 100  OLT(config-interface-epon-0/0)# |

## ONU Upgrade Management

### Transfer ONU Firmware to OLT

| Command | OLT(config)# load file {ftp <ip-address> <ftp-user-name> < ftp-user-password> < FILE-NAME>} | {tftp <ip-address> < FILE-NAME>} |
| --- | --- |
| **View** | Config view |
| **Description** | This command is used for transfer the upgrade file of the ONU to the OLT. |
| ftp | Use the ftp protocol to transfer ONU upgrade files to the OLT. |
| <ip-address> | IP address of ftp or tftp server, format X.X.X.X |
| <ftp-user-name> | User name of the ftp server, ranging from 1 to 32 characters. |
| <ftp-user-password> | Access password of the ftp server, ranging from 1 to 32 characters. |
| < FILE-NAME> | The name of the upgrade file of the ONU, ranging from 1 to 64 characters. The extension of the ONT upgrade file is required. |
| tftp | Transfer the ONT upgrade file to the OLT using the tftp protocol. |

【Example】

Example 1： Use the ftp method to transfer the ONT upgrade file 111.tar to the OLT.

|  |
| --- |
| OLT(config)# load file ftp 192.168.5.111 test test 111.tar  OLT(config)# |

### Batch Upgrade ONU

|  |  |
| --- | --- |
| Command | OLT(config)# ont load select {all | model < MODEL-ID >} |
| **View** | Config view |
| **Description** | This command is used for configure the OLT to upgrade the ONUs in batches. |
| all | Configure to upgrade all ONUs |
| < MODEL-ID > | Configure batch upgrade of ONUs based on the model id of the ONU. |

【Example】

Example 1： Configure the ONUs in batches according to the model id 0x31303053 of

the ONU.

|  |
| --- |
| OLT(config)# ont load select model 0x31303053  Number of ONTs that can be selected: 0, success: 0    OLT(config)# |

### Start or Stop Batch Upgrade ONU

|  |  |
| --- | --- |
| Command | OLT(config)# ont load start <FILENAME >commit-mode {auto | manual}  OLT(config)# ont load stop |
| **View** | Config view |
| **Description** | This command is used for start or stop the ONU batch upgrade. |
| load start | Configure to upgrade all ONUs |
| <FILENAME > | Configure the ONU upgrade file name for starting batch upgrade. |
| commit-mode | Select the new upgrade file to take effect mode. When not input, the default is ONU auto take effect in next time reboot. |
| auto | The effective mode of the ONU loading policy is that the graceful reset takes effect. That is, after loading the file to the ONU according to the loading policy, the ONU decides whether to restart immediately according to its own related settings to make the loading take effect (for example, whether there is an emergency call). The ONU waits for up to four hours, and when it is exceeded, it is forced to restart. |
| manaul | After the loading is completed, the ONU is manually restarted to make the loading take effect. |
| load stop | Delete the ONU load data. This parameter is enabled when you want to delete all load tasks and data on the ONU immediately. |

【Example】

Example 1：Start the ONU to use the 111.tar upgrade file for batch upgrade. After the upgrade, it will automatically restart to make the upgrade take effect.

|  |
| --- |
| OLT(config)# ont load start 111.tar commit-mode auto    OLT(config) |

### Show ONU Upgrade Configuration Information

| Command | OLT(config)# show ont load info |
| --- | --- |
| **View** | Config view |
| **Description** | This command is used for view the configuration information of the ONU upgrade that needs to be upgraded. |

【Example】

Example 1：Check the ONU upgrade information configured on the OLT.

|  |
| --- |
| OLT(config)# show ont load info  -----------------------------------------------------------------------------  File name :  Load state : stop  Commit mode : auto  -----------------------------------------------------------------------------    OLT(config)# |

### Show ONU Upgrade Progress

|  |  |
| --- | --- |
| Command | OLT(config)# show ont load select |
| **View** | Config view |
| **Description** | This command is used for check the progress of the ONU upgrade. |

【Example】

Example 1：Check the progress of the ONU upgrade under the OLT.

|  |
| --- |
| OLT(config)# show ont load select  -----------------------------------------------------------------------------  F/S PON ONT ID State Progress  ----------------------------------------------------------------------------  0/0 3 1 waiting 0%  -----------------------------------------------------------------------------  Total: 1, waiting: 1, fail: 0, success: 0, loading: 0, cancel: 0    OLT(config)# |

### Separately Upgrade ONU Under PON Port

|  |  |
| --- | --- |
| Command | OLT(config)# show ont load select |
| **View** | EPON interface view |
| **Description** | This command is used for select an ONU that needs to be upgraded separately under the PON port. |
| <port-id> | Specifies the PON port number where the ONU is located. The value is 1-16. |
| <onu-id> | The ONU id to be upgraded, in the range of 1-64. |
| all | Configure all ONU upgrades to the specified PON port. |
| < MODEL-ID > | Configure the ONU for the specified PON port to upgrade the ONU according to the model id. |

【Example】

Example 1：Select the first ONU under the PON1 port to be upgraded.

|  |
| --- |
| OLT(config-interface-epon-0/0)# ont load select 1 1  Number of ONUs that can be added: 1, success: 1  OLT(config-interface-epon-0/0)# |

### Active and Commit ONU New Firmware

| Command | OLT(config-interface-epon-0/0)#ont load commit <port-id> {<onu-id> | all} |
| --- | --- |
| **View** | EPON interface view |
| **Description** | This command is used for activate the image of the ONU. After the ONU is upgraded, the command will be executed. After the ONU restarts, the new mirror software will be run. Otherwise, the ONU will only run the software image before the upgrade. |
| <port-id> | Specifies the PON port number where the ONU is located. The value is 1-16 |
| <onu-id> | The ONU id of the new software to be activated, in the range of 1-64. |
| all | Activate new software for all ONUs under the specified PON port. |

【Example】

Example 1：Activate the software image of the first ONU under the PON1 port.

|  |
| --- |
| OLT(config-interface-epon-0/0)# ont load commit 1 1  Number of ONUs that can be commit: 1, success: 1  OLT(config-interface-epon-0/0)# |

### Delete the ONU that Needs to be Upgraded

|  |  |
| --- | --- |
| Command | OLT(config-interface-epon-0/0)# no ont load select port-id ont-id |
| **View** | epon view |
| **Description** | This command is used for delete the ONU that needs to be upgraded. |
| port-id | Pon port id,range for 1-16 |
| ont-id | Ont id,range for 1-64 |

【Example】

Example 1：Delete the PON7 ONU1 that needs to be upgraded.

|  |
| --- |
| OLT(config-interface-epon-0/0)# no ont load select 7 1  Number of ONTs that can be deleted: 1, success: 1  OLT(config-interface-epon-0/0)# |

## Home Gateway Upgrade

|  |  |
| --- | --- |
| Command | OLT(config-interface-epon-0/0)# ont wifi upgrade port-id ont-id file-name file-type (config|image) server-ip server-ip-address server-port server-port user-name password clear-flag (yes|no) |
| **View** | Epon View |
| **Discription** | This command is used for upgrade the home gateway. |
| port-id | Specifies the PON port number where the ONU is located. The value is 1-16 |
| ont-id | The ONU id of the new software to be activated, in the range of 1-64. |
| file-name | File name，range for 1-32. |
| config|image | File type：image is firmware，configis configuration file. |
| server-ip-address | Upgrade’s server ip address format is x.x.x.x |
| server-port | Upgrade’s server application port, range for 1-65535. |
| user-name | User name, range for 1-32. |
| password | Password, range for 1-16. |
| yes|no | Whether to clear the original configuration. |

【Example】

Example 1：Upgrade PON port 1 ONU id 1 home gateway；

|  |
| --- |
| OLT(config-interface-epon-0/0)# ont wifi upgrade 1 1 upgrade.img file-type image server-ip 192.168.1.11 server-port 21 admin admin clear-flag no  OLT(config-interface-epon-0/0)# |

## ONU Alarm Management

### ONU Opitcal Bias Current Alarm Function Config

| Command | OLT(config-interface-epon-0/0)#ont alarm optical <port-id> <onu-id> {bias-high-alarm|bias-high-warning|bias-low-alarm|bias-low-warning} {enable|disable} <threshold><restore-threshold> |
| --- | --- |
| **View** | EPON interface view |
| **Description** | This command is used for enable or disable bias current alarm of specified ont and set its alarm threshold |
| <port-id> | Pon port id,range for 1-16 |
| <onu-id> | Onu-id:ont id,range for 1-64 |
| bias-high-alarm bias-high-warning  bias-low-alarm bias-low-warning | bias-high-alarm:bias current overtops the highest alarm threshold.  bias-high-warning:warning the high bias current  bias-low-alarm:alarming the bias current lower than threshold  bias-low-warning:warning the low bias current |
| {enable|disable} | Enable  Disable |
| <threshold> | The alarm threshold,range for 0-10000,unit is mA |
| <restore-threshold> | The alarm restored threshold,range for 0-10000,unit is mA |

【Example】

Example 1：Enable the bias current alarm of ont 1 in pon 1,set its alarm threshold as 50,restore-threshold as 45.

|  |
| --- |
| OLT(config-interface-epon-0/0)#ont alarm optical 1 1 bias-high-alarm enable 50 45  OLT(config-interface-epon-0/0)# |

### ONU Optical Voltage Alarm Function Config

| Command | OLT(config-interface-epon-0/0)#ont alarm optical <port-id> <onu-id> {voltage-high-alarm|voltage-high-warning|voltage-low-alarm|voltage-low-warning{enable|disable} <threshold><restore-threshold>} |
| --- | --- |
| **View** | EPON interface view |
| **Description** | This command is used for enable or disable voltage alarm of specified ont and set its alarm threshold |
| <port-id> | Pon port id,range for 1-16 |
| <onu-id> | Onu-id:ont id,range for 1-64 |
| voltage-high-alarm  voltage-high-warning voltage-low-alarm voltage-low-warning | voltage-high-alarm:voltage overtops the alarm threshold  voltage-high-warning:warning the higher voltage  voltage-low-alarm:alarming the voltage is lower than threshold  voltage-low-warning:warning the lower voltage |
| {enable|disable} | Enable  Disable |
| <threshold> | The alarm threshold,range for 0.00-100.00,unit is V |
| <restore-threshold> | The alarm restored threshold,range for 0.00-100.00,unit is V |

【Example】

Example 1：Enable the voltage alarm of ont 1 in pon 1,set its range of threshold as 1-5V.

|  |
| --- |
| OLT(config-interface-epon-0/0)#ont alarm optical 1 1 voltage-high-alarm enable 1 5  OLT(config-interface-epon-0/0)# |

### ONU Opitcal Power Alarm Function Config

| Command | OLT(config-interface-epon-0/0)#ont alarm optical <port-id> <onu-id> {rx-power-high-alarm|rx-power-high-warning|rx-power-low-alarm|rx-power-low-warning|tx-power-high-alarm|tx-power-high-warning|tx-power-low-alarm|tx-power-low-warning} {enable|disable} <threshold> <restore-threshold> |
| --- | --- |
| **View** | EPON interface view |
| **Description** | This command is used for enable or disable optical power alarm of specified ont and set its alarm threshold |
| <port-id> | Pon port id,range for 1-16 |
| <onu-id> | Onu-id:ont id,range for 1-64 |
| rx-power-high-alarm rx-power-high-warning rx-power-low-alarm rx-power-low-warning tx-power-high-alarm tx-power-high-warning tx-power-low-alarm tx-power-low-warning | rx-power-high-alarm:rx-power overtops the alarm threshold  rx-power-high-warning:warning the high rx-power  rx-power-low-alarm:rx-power is lower than alarm threshold  rx-power-low-warning:warning the low rx-power  tx-power-high-alarm:tx-power overtops the alarm threshold  tx-power-high-warning:warning the high tx-power  tx-power-low-alarm:tx-power is lower than alarm threshold  tx-power-low-warning:warning the low tx-power |
| {enable|disable} | Enable  Disable |
| <threshold> | The alarm threshold,range for(-99)-100.00,unit is dbm |
| <restore-threshold> | The alarm restored threshold,range for(-99)-100.00,unit is dbm |

【Example】

Example 1：Enable the rx-power alarm of ont 1 in pon 1,set itsalarm threshold as-3,restore-threshold as-4.

|  |
| --- |
| OLT(config-interface-epon-0/0)#ont alarm optical 1 1 rx-power-high-alarm enable-3-4  OLT(config-interface-epon-0/0)# |

### ONU Opitcal Temperature Alarm Function Config

| Command | OLT(config-interface-epon-0/0)#ont alarm optical <port-id> <onu-id> {temperature-high-alarm|temperature-high-warning|temperature-low-alarm|temperature-low-warning{enable|disable} <threshold> <restore-threshold> |
| --- | --- |
| **View** | EPON interface view |
| **Description** | This command is used for enable or disable temperature alarm of specified ont and set its alarm threshold |
| <port-id> | Pon port id,range for 1-16 |
| <onu-id> | Onu-id:ont id,range for 1-64 |
| temperature-high-alarm temperature-high-warning temperature-low-alarm temperature-low-warning | temperature-high-alarm:temperature overtops the alarm threshold  temperature-high-warning:warning high temperature but not reaching the alarm threshold  temperature-low-alarm:temperature is lower than alarm threshold  temperature-low-warning:warning low temperature but not reaching the alarm threshold |
| {enable|disable} | Enable  Disable |
| <threshold> | The alarm threshold,range for(-99)-300,unit is℃ |
| <restore-threshold> | The alarm restored threshold,range for(-99)-300,unit is℃ |

【Example】

Example 1：Enable the temperature alarm of ont 1 in pon 1,set its alarm threshold as 55℃,restore-threshold as 45℃.

|  |
| --- |
| OLT(config-interface-epon-0/0)#ont alarm optical 1 1 temperature-high-alarm enable 55 45  OLT(config-interface-epon-0/0)# |

### ONU Port CRC Checkout Alarm Function Config

| Command | OLT(config-interface-epon-0/0)#ont alarm port <port-id> <onu-id> {pon|eth} <eth-port-id> {rx-crcerrors-alarm|rx-crcerrors-warning|tx-crcerrors-alarm|tx-crcerrors-warning} {enable|disable} <threshold> <restore-threshold> |
| --- | --- |
| **View** | EPON interface view |
| **Description** | This command is used for enable or disable error message CRC checkout alarm of specified ont port and set its alarm threshold |
| <port-id> | Pon port id,range for 1-16 |
| <onu-id> | Onu-id:ont id,range for 1-64 |
| {pon|eth} | Pon:ont’s pon port  Eth:ont’s ethernet port |
| <eth-port-id> | Ont’s ethernet port id,range for 1-24 |
| rx-crcerrors-alarm|rx-crcerrors-warning|tx-crcerrors-alarm|tx-crcerrors-warning | rx-crcerrors-alarm:receive the crc checkout message error alarm  rx-crcerrors-warning:receive the crc checkout message error warning  tx-crcerrors-alarm:transmit the crc checkout message error alarm  tx-crcerrors-warning:transmit the crc checkout message error warning |
| {enable|disable} | enable  disable |
| <threshold> | The alarm threshold,range for 0-4294967294 |
| <restore-threshold> | The alarm restore threshold,range for 0-4294967294 |

【Example】

Example 1：Enable the crc checkout alarm of eth1 in pon 1 ont 1,set its alarm threshold as 234,restore-threshold as 150.

|  |
| --- |
| OLT(config-interface-epon-0/0)#ont alarm port 1 1 pon rx-crcerrors-alarm enable 234 150  OLT(config-interface-epon-0/0)# |

### ONU Port Dropping Message Alarm Function Config

| Command | OLT(config-interface-epon-0/0)#ont alarm port <port-id> <onu-id> {pon|eth} <eth-port-id> {rx-discards-alarm|rx-discards-warning|tx-discards-alarm|tx-discards-warning} {enable|disable} <threshold> <restore-threshold> |
| --- | --- |
| **View** | EPON interface view |
| **Description** | This command is used for enable or disable dropping message alarm of specified ont port and set its alarm threshold |
| <port-id> | Pon port id,range for 1-16 |
| <onu-id> | Onu-id:ont id,range for 1-64 |
| {pon|eth} | Pon:ont’s pon port  Eth:ont’s ethernet port |
| <eth-port-id> | Ont’s ethernet port id,range for 1-24 |
| rx-discards-alarm|rx-discards-warning|tx-discards-alarm|tx-discards-warning | rx-discards-alarm:receive the alarm of discarded message  rx-discards-warning:receive the warning of discarded message  tx-discards-alarm:transmit the alarm of discarded message  tx-discards-warning:transmit the warning of discarded message |
| {enable|disable} | enable  disable |
| <threshold> | The alarm threshold,range for 0-4294967294 |
| <restore-threshold> | The alarm restored threshold,range for 0-4294967294 |

【Example】

Example 1：Enable and receive the alarm of discarded message of eth1 in pon 1 ont 1,set its alarm threshold as 200,restore-threshold as 150.

|  |
| --- |
| OLT(config-interface-epon-0/0)#ont alarm port 1 1 eth 1 rx-discards-alarm enable 200 150  OLT(config-interface-epon-0/0)# |

### ONU Port Dropevents Alarm Function Config

| Command | OLT(config-interface-epon-0/0)#ont alarm port <port-id> <onu-id> {pon|eth} <eth-port-id> {rx-dropevents-alarm |rx-dropevents-warning|tx-dropevents-alarm|tx-dropevents-warning} {enable|disable} <threshold> <restore-threshold> |
| --- | --- |
| **View** | EPON interface view |
| **Description** | This command is used for enable or disable droppevents alarm of specified ont port and set its alarm threshold |
| <port-id> | Pon port id,range for 1-16 |
| <onu-id> | Onu-id:ont id,range for 1-64 |
| {pon|eth} | Pon:ont’s pon port  Eth:ont’s ethernet port |
| <eth-port-id> | Ont’s ethernet port id,range for 1-24 |
| rx-dropevents-alarm|rx-dropevents-warning|tx-dropevents-alarm|tx-dropevents-warning | rx-dropevents-alarm:receive the alarm of drop event  rx-dropevents-warning:receive the warning of drop event  tx-dropevents-alarm:transmit the alarm of drop event  tx-dropevents-alarm:transmit the warning of drop event |
| {enable|disable} | enable  disable |
| <threshold> | The alarm threshold,range for 0-4294967294 |
| <restore-threshold> | The alarm stored threshold,range for 0-4294967294 |

【Example】

Example 1：Enable and receive the alarm of dropevents of eth1 in pon 1 ont 1,set its alarm threshold as 123,restore-threshold as 100.

|  |
| --- |
| OLT(config-interface-epon-0/0)#ont alarm port 1 1 eth 1 rx-dropevents-alarm enable 123 100  OLT(config-interface-epon-0/0)# |

### ONU Port Error Message Alarm Function Config

| Command | OLT(config-interface-epon-0/0)#ont alarm port <port-id> <onu-id> {pon|eth} <eth-port-id> {rx-errors-alarm|rx-errors-warning|tx-errors-alarm|tx-errors-warning} {enable|disable} <threshold> <restore-threshold> |
| --- | --- |
| **View** | EPON interface view |
| **Description** | This command is used for enable or disable error message alarm of specified ont port and set its alarm threshold |
| <port-id> | Pon port id,range for 1-16 |
| <onu-id> | Onu-id:ont id,range for 1-64 |
| {pon|eth} | Pon:ont’s pon port  Eth:ont’s ethernet port |
| <eth-port-id> | Ont’s ethernet port id,range for 1-24 |
| rx-errors-alarm|rx-errors-warning|tx-errors-alarm|tx-errors-warning | rx-errors-alarm:receive the alarm of error message  rx-errors-warning:receive the warning of error message  tx-errors-alarm:transmit the alarm of error message  tx-errors-alarm:transmit the warning of error message |
| {enable|disable} | enable  disable |
| <threshold> | The alarm threshold,range for 0-4294967294 |
| <restore-threshold> | The alarm restored threshold,range for 0-4294967294 |

【Example】

Example 1：Enable and receive the alarm of error message of eth1 in pon 1 ont 1,set its alarm threshold as 123,restore-threshold as 100.

|  |
| --- |
| OLT(config-interface-epon-0/0)#ont alarm port 1 1 eth 1 rx-errors-alarm enable 123 100  OLT(config-interface-epon-0/0)# |

### ONU Port Message Fragment Alarm Function Config

| Command | OLT(config-interface-epon-0/0)#ont alarm port <port-id> <onu-id> {pon|eth} <eth-port-id> {rx-fragments-alarm |rx-fragments-warning |tx-fragments-alarm|tx-fragments-warning} {enable|disable} <threshold> <restore-threshold> |
| --- | --- |
| **View** | EPON interface view |
| **Description** | This command is used for enable or disable message fragment alarm of specified ont port and set its alarm threshold |
| <port-id> | Pon port id,range for 1-16 |
| <onu-id> | Onu-id:ont id,range for 1-64 |
| {pon|eth} | Pon:ont’s pon port  Eth:ont’s ethernet port |
| <eth-port-id> | Ont’s ethernet port id,range for 1-24 |
| rx-fragments-alarm|rx-fragments-warning|tx-fragments-alarm|tx-fragments-warning | rx-fragments-alarm:receive the alarm of message fragment  rx-fragments-warning:receive the warning of message fragment  tx-fragments-alarm:transmit the alarm of message fragment  tx-fragments-alarm:transmit the warning of error message |
| {enable|disable} | enable  disable |
| <threshold> | The alarm threshold,range for 0-4294967294 |
| <restore-threshold> | The alarm restored threshold,range for 0-4294967294 |

【Example】

Example 1：Enable and receive the alarm of message fragment of eth1 in pon 1 ont 1,set its alarm threshold as 123,restore-threshold as 100.

|  |
| --- |
| OLT(config-interface-epon-0/0)#ont alarm port 1 1 eth 1 rx-fragments-alarm enable 123 100  OLT(config-interface-epon-0/0)# |

### ONU Port Message Jabber(time out) Alarm Function Config

| Command | OLT(config-interface-epon-0/0)#ont alarm port <port-id> <onu-id> {pon|eth} <eth-port-id> {rx-jabbers-alarm |rx-jabbers-warning |tx-jabbers-alarm|tx-jabbers-warning} {enable|disable} <threshold> <restore-threshold> |
| --- | --- |
| **View** | EPON interface view |
| **Description** | This command is used for enable or disable message jabber alarm of specified ont port and set its alarm threshold,it means when the message has crc error and it is out of the range,it will alarm. |
| <port-id> | Pon port id,range for 1-16 |
| <onu-id> | Onu-id:ont id,range for 1-64 |
| {pon|eth} | Pon:ont’s pon port  Eth:ont’s ethernet port |
| <eth-port-id> | Ont’s ethernet port id,range for 1-24 |
| rx-jabbers-alarm|rx-jabbers-warning|tx-jabbers-alarm|tx-jabbers-warning | rx-jabbers-alarm:receive the alarm of message jabber  rx-jabbers-warning:receive the warning of message jabber  tx-jabbers-alarm:transmit the alarm of message jabber  tx-jabbers-alarm:transmit the warning of message jabber |
| {enable|disable} | enable  disable |
| <threshold> | The alarm threshold,range for 0-4294967294 |
| <restore-threshold> | The alarm restored threshold,range for 0-4294967294 |

【Example】

Example 1：Enable and receive the alarm of message jabber of eth1 in pon 1 ont 1,set its alarm threshold as 1518,restore-threshold as 1500.

|  |
| --- |
| OLT(config-interface-epon-0/0)#ont alarm port 1 1 eth 1 rx-jabbers-alarm enable 1518 1500  OLT(config-interface-epon-0/0)# |

### ONU Port Oversize Message Alarm Function Config

| Command | OLT(config-interface-epon-0/0)#ont alarm port <port-id> <onu-id> {pon|eth} <eth-port-id> {rx-oversizes-alarm |rx-oversizes-warning |tx-oversizes-alarm|tx-oversizes-warning} {enable|disable} <threshold> <restore-threshold> |
| --- | --- |
| **View** | EPON interface view |
| **Description** | This command is used for enable or disable oversize message alarm of specified ont port and set its alarm threshold,it means crc of message is correct but the size of it is over range,it will alarm. |
| <port-id> | Pon port id,range for 1-16 |
| <onu-id> | Onu-id:ont id,range for 1-64 |
| {pon|eth} | Pon:ont’s pon port  Eth:ont’s ethernet port |
| <eth-port-id> | Ont’s ethernet port id,range for 1-24 |
| rx-oversizes-alarm|rx-oversizes-warning|tx-oversizes-alarm|tx-oversizes-warning | rx-oversizes-alarm:receive the alarm of oversize message  rx-oversizes-warning:receive the warning of oversize message  tx-oversizes-alarm:transmit the alarm of oversize message  tx-oversizes-alarm:transmit the warning of oversize message |
| {enable|disable} | enable  disable |
| <threshold> | The lowest alarm threshold,range for 0-4294967294 |
| <restore-threshold> | The highest alarm threshold,range for 0-4294967294 |

【Example】

Example 1：Enable and receive the alarm of oversize message of eth1 in pon 1 ont 1,set its alarm threshold as 1518,restore-threshold as 1500.

|  |
| --- |
| OLT(config-interface-epon-0/0)#ont alarm port 1 1 eth 1 rx-oversizes-alarm enable 1518 1500  OLT(config-interface-epon-0/0)# |

### ONU Port Ultra Short Message Alarm Function Config

| Command | OLT(config-interface-epon-0/0)#ont alarm port <port-id> <onu-id> {pon|eth} <eth-port-id> {rx-undersizes-alarm | rx-undersizes-warning|tx-undersizes-alarm|tx-undersizes-warning} {enable|disable} <threshold> <restore-threshold>} |
| --- | --- |
| **View** | EPON interface view |
| **Description** | This command is used for enable or disable ultra short message alarm of specified ont port and set its alarm threshold |
| <port-id> | Pon port id,range for 1-16 |
| <onu-id> | Onu-id:ont id,range for 1-64 |
| {pon|eth} | Pon:ont’s pon port  Eth:ont’s ethernet port |
| <eth-port-id> | Ont’s ethernet port id,range for 1-24 |
| rx-undersizes-alarm|rx-undersizes-warning|tx-undersizes-alarm|tx-undersizes-warning | rx-undersizes-alarm:receive the alarm of ultra short message  rx-undersizes-warning:receive the warning of ultra short message  tx-undersizes-alarm:transmit the alarm of ultra short message  tx-undersizes-alarm:transmit the warning of ultra short message |
| {enable|disable} | enable  disable |
| <threshold> | The alarm threshold,range for 0-4294967294 |
| <restore-threshold> | The alarm restored threshold,range for 0-4294967294 |

【Example】

Example 1：Enable and receive the alarm of ultra short message of eth1 in pon 1 ont 1,set its alarm threshold as 60,restore-threshold as 61.

|  |
| --- |
| OLT(config-interface-epon-0/0)#ont alarm port 1 1 eth 1 rx-undersizes-alarm enable 60 61  OLT(config-interface-epon-0/0)# |

### ONU CATV Alarm Threshold Config

| Command | OLT(config-interface-epon-0/0)# ont catv alarm port-id onu-id  (rx-power-alarm HIGH-THRESHOLD LOW-THRESHOLD) |(tx-voltage-alarm HIGH-THRESHOLD LOW-THRESHOLD ) |(voltage-alarm HIGH-THRESHOLD LOW-THRESHOLD ) |(temperature-alarm HIGH-THRESHOLD LOW-THRESHOLD) |
| --- | --- |
| **View** | epon view |
| **Discription** | This command is used for config the ONU catv alarm threshold. |
| port-id | Pon port id,range for 1-16 |
| onu-id | Onu-id:ont id,range for 1-64 |
| rx-power-alarm HIGH-THRESHOLD LOW-THRESHOLD | Receive optical power alarm:  High alarm threshold, range for -99.0-100.0, unit is dBm  Low alarm threshold, range for -99.0-100.0, unit is dBm |
| tx-voltage-alarm HIGH-THRESHOLD LOW-THRESHOLD | Output level alarm：  High alarm threshold, range for 0.0-100.0, unit is dBuV  Low alarm threshold, range for 0.0-100.0, unit is dBuV |
| voltage-alarm HIGH-THRESHOLD LOW-THRESHOLD | Voltage alarm：  High alarm threshold, range for 0.0-100.0, unit is V  Low alarm threshold, range for 0.0-100.0, unit is V |
| temperature-alarm HIGH-THRESHOLD LOW-THRESHOLD | Working temperature alarm：  High alarm threshold, range for -99.0-300.0, unit is ℃  Low alarm threshold, range for -99.0-300.0, unit is ℃ |

【Example】

Example 1：Configure a high alarm threshold of 70 dBm for the ONU11CATV receiving power of the PON5 port and a low alarm threshold of 0 dBm.

|  |
| --- |
| OLT(config-interface-epon-0/0)# ont catv alarm 5 11 rx-power-alarm 70 0  OLT(config-interface-epon-0/0)# |

### ONU CATV Output Gain Control Config

| Command | OLT(config-interface-epon-0/0)# ont catv gain-control port-id onu-id  type (agc AGC-Up-Value AGC-Range )|(mgc MGC-Tx-Attenuation ) |
| --- | --- |
| **View** | Epon view |
| **Discription** | This command is used for config output gain control of the ONU catv. |
| port-id | Pon port id,range for 1-16 |
| onu-id | Onu-id:ont id,range for 1-64 |
| agc AGC-Up-Value AGC-Range | Automatic gain control:  Upper limit of input optical power in AGC mode, range -6.0-2.0 dBm  Input optical power range value in AGC mode, range 0.0-8.0 dBm |
| mgc MGC-Tx-Attenuation | Manual gain control:  Output level attenuation value, range 0.0-15.0 dBm |

【Example】

Example 1：Config the onu catv output gain control numbered 11 in the agc mode under the PON5 port.

|  |
| --- |
| OLT(config-interface-epon-0/0)# ont catv gain-control 5 11 type agc 1 2  OLT(config-interface-epon-0/0)# |

### Enable or Disable ONU Dying-gasp Alarm Function

|  |  |
| --- | --- |
| Command | OLT(config-interface-epon-0/0)#ont alarm dying-gasp <port-id> {enable|disable} |
| **View** | EPON interface view |
| **Description** | This command is used for enable or disable dying-gasp alarm of specified ont |
| <port-id> | Pon port id,range for 1-16 |
| {enable|disable} | Enable:enable dying-gasp alarm of onu  Disable:disable dying-gasp alarm of onu |

【Example】

Example 1：Enable dying-gasp alarm of onu 1 in pon 1.

|  |
| --- |
| OLT(config-interface-epon-0/0)#ont alarm dying-gasp 1 enable  OLT(config-interface-epon-0/0)# |

### Bind Alarm-config to ONU

|  |  |
| --- | --- |
| Command | OLT(config-interface-epon-0/0)#ont alarm-config <port-id> {all|<onu-id>} {profile-id <profile-id>|profile-name<profile-name>} |
| **View** | EPON interface view |
| **Description** | This command is used for bind the alarm-config to ont.but first of all,the alarm-profile should be created in config view. |
| <port-id> | Pon port id,range for 1-16 |
| all|<onu-id> | All:all of the ont  onu-id:Onu-id:ont id,range for 1-64 |
| <profile-id> | Profile id,range for 1-50 |
| <profile-name> | Profile name,it supports 1-16 strings |

【Example】

Example 1：Bind alarm-profile 5 to ont 1 in pon 1.

|  |
| --- |
| OLT(config-interface-epon-0/0)#ont alarm-config 1 1 profile-id 5  OLT(config-interface-epon-0/0)# |

### Bind Optical-alarm-config to ONU

|  |  |
| --- | --- |
| Command | OLT(config-interface-epon-0/0)#ont optical-alarm-config <port-id> {all|<onu-id>} {profile-id <profile-id>|profile-name<profile-name>} |
| **View** | EPON interface view |
| **Description** | This command is used for bind the optical-alarm-config to ont.but first of all,the alarm-profile should be created in config view. |
| <port-id> | Pon port id,range for 1-16 |
| all|<onu-id> | All:all of the ont  onu-id:Onu-id:ont id,range for 1-64 |
| <profile-id> | Profile id,range for 1-50 |
| <profile-name> | Profile name,it supports 1-24 strings |

【Example】

Example 1：Bind optical-alarm-profile 5 to ont 1 in pon 1.

|  |
| --- |
| OLT(config-interface-epon-0/0)#ont optical-alarm-profile 1 1 profile-id 5  OLT(config-interface-epon-0/0)# |

### Show ONU Dying-gasp Alarm Config Status

| Command | OLT(config-interface-epon-0/0)#show ont alarm dying-gasp {<port-id> |all} |
| --- | --- |
| **View** | EPON interface view |
| **Description** | This command is used for show configured state of ont dying-gasp alarm |
| {<port-id>|all} | port-id:Pon port id,range for 1-16  All:all the pon ports |

【Example】

Example 1：Show ont alarm dying-gasp of all the pon port

|  |
| --- |
| OLT(config-interface-epon-0/0)#show ont alarm dying-gasp all  -----------------------------------------------------------------------------  F/S P State  ----------------------------------------------------------------------------  0/0 1 enable  0/0 2 enable  0/0 3 enable  0/0 4 enable  0/0 5 enable  0/0 6 enable  0/0 7 enable  0/0 8 enable  0/0 9 enable  0/0 10 enable  0/0 11 enable  0/0 12 enable  0/0 13 enable  0/0 14 enable  0/0 15 enable  0/0 16 enable  -----------------------------------------------------------------------------  OLT(config-interface-epon-0/0)# |

### Show ONU Optical power Alarm Config Status

|  |  |
| --- | --- |
| Command | OLT(config-interface-epon-0/0)#show ont alarm optical <port-id> <onu-id> |
| **View** | EPON interface view |
| **Description** | This command is used for show the configured state of optical alarm and temperature alarm and voltage alarm and etc. |
| <port-id> | Pon port id,range for 1-16 |
| <onu-id> | Ont id,range for 1-64 |

【Example】

Example 1：Show the configured state of optical alarm in pon 1 ont 1.

|  |
| --- |
| OLT(config-interface-epon-0/0)#show ont alarm optical 1 1  -----------------------------------------------------------------------------  Rx optical power high alarm:disable  Rx optical power low alarm:disable  Rx optical power high warning:disable  Rx optical power low warning:disable  Tx optical power high alarm:disable  Tx optical power low alarm:disable  Tx optical power high warning:disable  Tx optical power low warning:disable  Bias current high alarm:disable  Bias current low alarm:disable  Bias current high warning:disable  Bias current low warning:disable  Supply voltage high alarm:disable  Supply voltage low alarm:disable  Supply voltage high warning:disable  Supply voltage low warning:disable  Temperature high alarm:disable  Temperature low alarm:disable  Temperature high warning:disable  Temperature low warning:disable  -----------------------------------------------------------------------------  OLT(config-interface-epon-0/0)# |

### Show ONU ETH Port Alarm Config Status

|  |  |
| --- | --- |
| Command | OLT(config-interface-epon-0/0)#show ont alarm port <port-id> <onu-id> eth <eth-port-id> |
| **View** | EPON interface view |
| **Description** | This command is used for show configured state of ont eth port alarm |
| <port-id> | Pon port id,range for 1-16 |
| <onu-id> | Ont id,range for 1-64 |
| <eth-port-id> | Eth port id,range for 1-24 |

【Example】

Example 1：Show eth port alarm’s configured state of ont 1 eth 1 in pon 1.

|  |
| --- |
| OLT(config-interface-epon-0/0)#show ont alarm port 1 1 eth 1  -----------------------------------------------------------------------------  F/S P ONU-ID ONU-Port Alarm/Warning State Threshold Restore-Threshold  ----------------------------------------------------------------------------  0/0 1 1 1 tx-dropevents-alarm disable--  0/0 1 1 1 rx-dropevents-alarm disable--  0/0 1 1 1 tx-crcerrors-alarm disable--  0/0 1 1 1 rx-crcerrors-alarm disable--  0/0 1 1 1 tx-undersizes-alarm disable--  0/0 1 1 1 rx-undersizes-alarm disable--  0/0 1 1 1 tx-oversizes-alarm disable--  0/0 1 1 1 rx-oversizes-alarm disable--  0/0 1 1 1 tx-fragments-alarm disable--  0/0 1 1 1 rx-fragments-alarm disable--  0/0 1 1 1 tx-jabbers-alarm disable--  0/0 1 1 1 rx-jabbers-alarm disable--  0/0 1 1 1 tx-discards-alarm disable--  0/0 1 1 1 rx-discards-alarm disable--  0/0 1 1 1 tx-errors-alarm disable--  0/0 1 1 1 rx-errors-alarm disable--  0/0 1 1 1 tx-dropevents-warning disable--  0/0 1 1 1 rx-dropevents-warning disable--  0/0 1 1 1 tx-crcerrors-warning disable--  0/0 1 1 1 rx-crcerrors-warning disable--  0/0 1 1 1 tx-undersizes-warning disable--  0/0 1 1 1 rx-undersizes-warning disable--  0/0 1 1 1 tx-oversizes-warning disable--  0/0 1 1 1 rx-oversizes-warning disable--  0/0 1 1 1 tx-fragments-warning disable--  0/0 1 1 1 rx-fragments-warning disable--  0/0 1 1 1 tx-jabbers-warning disable--  0/0 1 1 1 rx-jabbers-warning disable--  0/0 1 1 1 tx-discards-warning disable--  0/0 1 1 1 rx-discards-warning disable--  0/0 1 1 1 tx-errors-warning disable--  0/0 1 1 1 rx-errors-warning disable--  -----------------------------------------------------------------------------  OLT(config-interface-epon-0/0)# |

### Show ONU PON Port Alarm Config Status

|  |  |
| --- | --- |
| Command | OLT(config-interface-epon-0/0)#show ont alarm port <port-id> <onu-id> pon |
| **View** | EPON interface view |
| **Description** | This command is used for show configured state of ont pon port alarm |
| <port-id> | Pon port id,range for 1-16 |
| <onu-id> | Ont id,range for 1-64 |

【Example】

Example 1：Show configured state of ont 1’s pon port alarm in pon 1.

|  |
| --- |
| OLT(config-interface-epon-0/0)#show ont alarm port 1 1 pon  -----------------------------------------------------------------------------  F/S P ONU-ID Alarm/Warning State Threshold Restore-Threshold  ----------------------------------------------------------------------------  0/0 1 1 rx-dropevents-alarm disable--  0/0 1 1 tx-dropevents-alarm disable--  0/0 1 1 rx-crcerrors-alarm disable--  0/0 1 1 tx-crcerrors-alarm disable--  0/0 1 1 rx-undersizes-alarm disable--  0/0 1 1 tx-undersizes-alarm disable--  0/0 1 1 rx-oversizes-alarm disable--  0/0 1 1 tx-oversizes-alarm disable--  0/0 1 1 rx-fragments-alarm disable--  0/0 1 1 tx-fragments-alarm disable--  0/0 1 1 rx-jabbers-alarm disable--  0/0 1 1 tx-jabbers-alarm disable--  0/0 1 1 rx-discards-alarm disable--  0/0 1 1 tx-discards-alarm disable--  0/0 1 1 rx-errors-alarm disable--  0/0 1 1 tx-errors-alarm disable--  0/0 1 1 rx-dropevents-warning disable--  0/0 1 1 tx-dropevents-warning disable--  0/0 1 1 rx-crcerrors-warning disable--  0/0 1 1 tx-crcerrors-warning disable--  0/0 1 1 rx-undersizes-warning disable--  0/0 1 1 tx-undersizes-warning disable--  0/0 1 1 rx-ossversizes-warning disable--  0/0 1 1 tx-oversizes-warning disable--  0/0 1 1 rx-fragments-warning disable--  0/0 1 1 tx-fragments-warning disable--  0/0 1 1 rx-jabbers-warning disable--  0/0 1 1 tx-jabbers-warning disable--  0/0 1 1 rx-discards-warning disable--  0/0 1 1 tx-discards-warning disable--  0/0 1 1 rx-errors-warning disable--  0/0 1 1 tx-errors-warning disable--  -----------------------------------------------------------------------------  OLT(config-interface-epon-0/0)# |

### Show ONU CATV Output Gain Control Information

|  |  |
| --- | --- |
| Command | OLT(config-interface-epon-0/0)# show ont catv gain-control-info port-id ont-id |
| **View** | epon view |
| **Description** | This command is used for show ONU CATV output gain control information. |
| port-id | Pon port id,range for 1-16 |
| ont-id | Ont id,range for 1-64 |

【Example】

Example 1：Show PON9 ONU5 catv output gain control information.

|  |
| --- |
| OLT(config-interface-epon-0/0)# show ont catv gain-control-info 9 5  ----------------------------------------------------------------------------  Frame/Slot : 0/0  Port : 9  ONT-ID : 5  Gain Control Type : AGC  AGC Up Value : -4.00(dBm)  AGC Range : 7.00(dBm)  -----------------------------------------------------------------------------  OLT(config-interface-epon-0/0)# |

### Show the ONU CATV Alarm Threshold Information.

| Command | OLT(config-interface-epon-0/0)# show ont catv alarm-threshold-info port-id ont-id |
| --- | --- |
| **View** | epon view |
| **Description** | This command is used for show the ONU CATV alarm threshold information. |
| port-id | Pon port id,range for 1-16 |
| ont-id | Ont id,range for 1-64 |

【Example】

Example 1：show PON9 ONU5 CATV alarm threshold information.

|  |
| --- |
| OLT(config-interface-epon-0/0)# show ont catv alarm-threshold-info 9 5  ----------------------------------------------------------------------------  Frame/Slot : 0/0  Port : 9  ONT-ID : 5  Alarm Threshold Low High  Rx Power(dBm) -18.00 0.00  Tx Voltage(dBuV) 60.00 95.00  Voltage(V) 10.80 13.20  Temperature(C) -10.00 90.00  -----------------------------------------------------------------------------  OLT(config-interface-epon-0/0)# |

### Show the Optical Alarm Template Information of the ONU

|  |  |
| --- | --- |
| Command | OLT(config-interface-epon-0/0)# show ont optical-alarm-profile port-id ont-id |
| **View** | epon view |
| **Description** | This command is used for show the optical alarm template information of the ONU. |
| port-id | Pon port id,range for 1-16 |
| ont-id | Ont id,range for 1-64 |

【Example】

Example 1：Show PON9 ONU5 optical alarm template information.

|  |
| --- |
| OLT(config-interface-epon-0/0)# show ont optical-alarm-profile 9 5  -----------------------------------------------------------------------------  Frame/Slot : 0/0  Port : 9  ONT-ID : 5  Profile-ID : 1  Profile-name : RX  ----------------------------------------------------------------------------  Rx optical power high alarm threshold (dBm) : 0.00  Rx optical power high alarm restore threshold (dBm) : -3.00  Rx optical power low alarm : disable  Rx optical power high warning : disable  Rx optical power low warning : disable  Tx optical power high alarm : disable  Tx optical power low alarm : disable  Tx optical power high warning : disable  Tx optical power low warning : disable  Bias current high alarm : disable  Bias current low alarm : disable  Bias current high warning : disable  Bias current low warning : disable  Supply voltage high alarm : disable  Supply voltage low alarm : disable  Supply voltage high warning : disable  Supply voltage low warning : disable  Temperature high alarm : disable  Temperature low alarm : disable  Temperature high warning : disable  Temperature low warning : disable  -----------------------------------------------------------------------------  -----------------------------------------------------------------------------  OLT(config-interface-epon-0/0)# |

### Show ONU Alarm Template Information

|  |  |
| --- | --- |
| Command | OLT(config-interface-epon-0/0)# show ont alarm-config port-id ont-id |
| **View** | epon view |
| **Description** | This command is used for show ONU alarm config information. |
| port-id | Pon port id,range for 1-16 |
| onu-id | Ont id,range for 1-64 |

【Example】

Example 1：Show PON9 ONU4 alarm template information.

|  |
| --- |
| OLT(config-interface-epon-0/0)# show ont alarm-config 9 4  -----------------------------------------------------------------------------  Frame/Slot : 0/0  Port : 9  ONT-ID : 4  Profile-ID : 1  Profile-name : test1  ----------------------------------------------------------------------------  <Drop events alarm/warning>:  Transmitted drop events alarm: disable  Transmitted drop events warning: disable  Received drop events alarm: disable  Received drop events warning: disable  <CRC error alarm/warning>:  Transmitted CRC error frames alarm: disable  Transmitted CRC error frames warning: disable  Received CRC error frames alarm threshold: 500  Received CRC error frames alarm restore threshold: 20000  Received CRC error frames warning: disable  <Undersize frames alarm/warning>:  Transmitted undersize frames alarm: disable  Transmitted undersize frames warning: disable  Received undersize frames alarm: disable  Received undersize frames warning: disable  <Oversize frames alarm/warning>:  Transmitted oversize frames alarm: disable  Transmitted oversize frames warning: disable  Received oversize frames alarm: disable  Received oversize frames warning: disable  <Fragments alarm/warning>:  Transmitted fragments alarm: disable  Transmitted fragments warning: disable  Received fragments alarm: disable  Received fragments warning: disable  <Jabbers alarm/warning>:  Transmitted jabbers alarm: disable  Transmitted jabbers warning: disable  Received jabbers alarm: disable  Received jabbers warning: disable  <Discards alarm/warning>:  Transmitted discards alarm: disable  Transmitted discards warning: disable  Received discards alarm: disable  Received discards warning: disable  <Errors alarm/warning>  Transmitted errors alarm: disable  Transmitted errors warning: disable  Received errors alarm: disable  Received errors warning: disable  -----------------------------------------------------------------------------  OLT(config-interface-epon-0/0)# |

### Delete an Alarm Template bound to ONU

|  |  |
| --- | --- |
| Command | OLT(config-interface-epon-0/0)# no ont alarm-config port-id onu-id |
| **View** | epon view |
| **Description** | This command is used for delete alarm template bound to ONU. |
| port-id | Pon port id,range for 1-16 |
| onu-id | Ont id,range for 1-64 |

【Example】

Example 1：Delete PON7 ONU1 has been bound alarm template.

|  |
| --- |
| OLT(config-interface-epon-0/0)# no ont alarm-config 7 1  OLT(config-interface-epon-0/0)# |

### Delete the optical alarm template bound to the ONU

|  |  |
| --- | --- |
| Command | OLT(config-interface-epon-0/0)# no ont optical-alarm-profile port-id onu-id |
| **View** | epon view |
| **Description** | This command is used for delete optical alarm template bound to ONU. |
| port-id | Pon port id,range for 1-16 |
| onu-id | Ont id,range for 1-64 |

【Example】

Example 1：Delete the optical alarm template bound to PON7 ONU1.

|  |
| --- |
| OLT(config-interface-epon-0/0)# no ont optical-alarm-profile 7 1  OLT(config-interface-epon-0/0)# |

## ONU WAN Management

### Config parameters for the ONU WAN service

| Command | OLT(config-interface-epon-0/0)# ont wan config port-id ont-id WANNAME vlan (enable vlan-id priority|disable) connection-mode (bridge|route) service-type (internet ip-mode (dhcp|static|pppoe)|mgmt|tr069|vod|voip) mtu mtu-value bind-if ( bind-portlist|not-bind ) |
| --- | --- |
| **View** | Epon view |
| **Description** | This command is used for add or modify the ONU wan configuration. |
| port-id | Pon port id,range for 1-16 |
| ont-id | Ont id,range for 1-64 |
| WANNAME | ONU WAN name，Support length is 1-32 characters |
| vlan-id | Add the Vlan id ，range for 1-4094 |
| priority | priority，range for 0-7 |
| internet|mgmt|tr069|vod|voip | Internet: Internet service  Mgmt:  Tr-069:  Vod:Video on demand service, also known as interactive TV on demand system;  Voip:IP-based voice service; |
| mtu-value | MTU value，range for 64-1500 |
| bind-portlist | Ssid range for 1-4，ONU LAN port is 5-8，format is 1,3-5,8 |

【Example】

Example 1：Add a bridge wan to the ONU with PON7 ONUid 1. Enable vlan100, route mode, DHCP access, MTU set to 1500, and bind ONU LAN1 port.

|  |
| --- |
| OLT(config-interface-epon-0/0)# ont wan config 7 1 1 vlan enable 100 0 connection-mode route service-type internet dhcp mtu 1500 bind-if 5  OLT(config-interface-epon-0/0)# |

### Clear ONU WAN Config

|  |  |
| --- | --- |
| Command | OLT(config-interface-epon-0/0)# ont wan clear port-id ont-id (WANNAME |all) |
| **View** | Epon view |
| **Description** | This command is used for clear the ONU wan config. |
| port-id | Pon port id,range for 1-16 |
| ont-id | Ont id,range for 1-64 |
| WANNAME|all | WANNAME: ONU WAN name，Support length is 1-32 characters  All: All wan that has been created |

【Example】

Example 1：Clear PON port 7 ONU id 2 wan config

|  |
| --- |
| OLT(config-interface-epon-0/0)# ont wan clear 7 2 all  OLT(config-interface-epon-0/0)#  OLT(config-interface-epon-0/0)# show ont wan status 7 2 all  ONT wan is not exist!  OLT(config-interface-epon-0/0)# |

### Show ONU WAN Name information

| Command | OLT(config-interface-epon-0/0)# show ont wan name port-id ont-id WANNAME |
| --- | --- |
| **View** | Epon View |
| **Discription** | This command is used for show ONU WAN name information. |
| port-id | Pon port id,range for 1-16 |
| ont-id | Ont id,range for 1-64 |
| WANNAME | ONU WAN name，Support length is 1-32 characters |

【Example】

Example 1：Show PON port 7 ONU id 2 Wan name information.

|  |
| --- |
| OLT(config-interface-epon-0/0)# show ont wan name 7 2 1\_INTERNET\_R\_VID\_507  ----------------------------------------------------------------------------  Frame/Slot : 0/0  Port : 7  ONT-ID : 2  WAN-Name : 1\_INTERNET\_R\_VID\_507  Connection Mode : route  IP Mode : Static  IP Addr : 192.168.5.145  IP Mask : 255.255.255.0  Default IPGW : 192.168.5.1  Primary DNS : 192.168.5.1  Secondary DNS : 114.114.114.114  Mtu : 1500  VLAN ID : 507  802.1P : 0  Service Type : Internet  Bind Interface : SSID-1 LAN1  ----------------------------------------------------------------------------  OLT(config-interface-epon-0/0)# |

### Show ONU WAN State Information

| Command | OLT(config-interface-epon-0/0)# show ont wan state port-id ont-id (WANNAME |all) |
| --- | --- |
| **View** | Epon View |
| **Discription** | This command is used for show ONU WAN state information. |
| port-id | Pon port id,range for 1-16 |
| ont-id | Ont id,range for 1-64 |
| WANNAME|all | WANNAME: ONU WAN name，Support length is 1-32 characters  All: All wan that has been created |

【Example】

Example 1：Show PON port 7 ONU id 2 Wan state information.

|  |
| --- |
| OLT(config-interface-epon-0/0)# show ont wan status 7 2 all  -----------------------------------------------------------------------------  Index wanName IpMode IPAddr Mask  ----------------------------------------------------------------------------  1 1\_INTERNET\_R\_VID\_507 static 192.168. 5.145 255.255.255. 0  -----------------------------------------------------------------------------  Index DefGw PrimaryDNS SecondaryDNS Status  ----------------------------------------------------------------------------  1 192.168. 5. 1 192.168. 5. 1 114.114.114.114 Connect  -----------------------------------------------------------------------------  OLT(config-interface-epon-0/0)# |

## ONU voice service management

### Config Parameters for the Fax/Modem Service

| Command | OLT(config-interface-epon-0/0)# ont voip fax-modem port-id ont-id (t30|t38) (auto-vbd|negotiation) |
| --- | --- |
| **View** | EPON interface view |
| **Description** | This command is used for configure the parameter configuration of the fax/modem service of the ONU voice module. |
| port-id | Pon port id,range for 1-16 |
| ont-id | Ont id,range for 1-64 |
| (t30|t38) | T30: voice service transparent transmission mode  T38: t38 mode |
| (auto-vbd| negotiation) | Auto-vbd: Automatic voice bandwidth data  Negotiation: Negotiation |

【Example】

Example 1：Configure the voice fax/modem parameter of the PON11 port ONU1 as t30 negotiation mode.

|  |
| --- |
| OLT(config-interface-epon-0/0)# ont voip fax-modem 11 1 t30 negotiation  OLT(config-interface-epon-0/0)# |

### Config Global Parameters of the ONU Voice Module

| Command | OLT(config-interface-epon-0/0)# ont voip global-config ((dhcp-mode port-id ont-id ) |(pppoe-mode port-id ont-id (chap|auto|pap) username password )|(static-mode port-id ont-id ip-address netmask default-gateway)) (stacking|tag|transparent) voice-cvlan voice-svlan voice-priority) |
| --- | --- |
| **View** | EPON interface view |
| **Description** | This command is used for configure the global parameter configuration of the ONU voice module. |
| port-id | Pon port id,range for 1-16. |
| ont-id | Ont id,range for 1-64. |
| voice-cvlan | Voice service cvlan,range for 0-4094. |
| voice-svlan | Voice service svlan,currently svlan support single layer vlan.The default is 0. |
| voice-priority | Voice service priority,range for 0-7. |

【Example】

Example 1：Configure the voice global parameter of the PON11 port ONU1 as DHCP and vlan100 transparently.

|  |
| --- |
| OLT(config-interface-epon-0/0)# ont voip global-config dhcp-mode 11 1 transparent 100 100 0  OLT(config-interface-epon-0/0)# |

### Config Parameters of the H.248 Protocol of the ONU Voice Module

| Command | OLT(config-interface-epon-0/0)# ont voip h248-config port-id ont-id MGPortNo MGCIP MGCComPortNo (device-name|domain-name |ip-addr) MID Backup-MGCIP Backup-MGCComPortNo (china-ctc |closed) Heartbeat-cycle Heartbeat-count |
| --- | --- |
| **View** | EPON interface view |
| **Description** | This command is used for configure the parameters of the H248 protocol of the ONU voice module. |
| port-id | Pon port id,range for 1-16. |
| ont-id | Ont id,range for 1-64. |
| MGPortNo | Port number of the media gateway, range for 1024-65535 |
| MGCIP | IP address of the main softswitch platform, formatted as X.X.X.X |
| MGCComPortNo | Port number of the active softswitch platform, range for 1024-65535 |
| (device-name|domain-name |ip-addr) | The registration method is selected: device-name is registered according to the device name; domain-name is registered according to the domain name; ip-addr is registered according to the IP address. |
| MID | The MG identifier, the global unique identifier used by the MG to register with the softswitch platform, supports 1-64 characters. |
| Backup-MGCIP | IP address of the alternate softswitch platform in the format x.x.x.x |
| Backup-MGCComPortNo | Port number of the standby software for the platform, in the range of 1024-65535 |
| (china-ctc |closed) | Link detection mode; China-ctc: H.248 - China Telecom standard Notify command, default is china-ctc; closed: closed. |
| Heartbeat-cycle | Heartbeat cycle, default is 60s |
| Heartbeat-count | Heartbeat detection times, the default is 3 times |

【Example】

Example 1：Configure the H.248 protocol configuration parameters of the voice module of the PON11 port ONU1.

|  |
| --- |
| OLT(config-interface-epon-0/0)# ont voip h248-config 11 1 1024 192.168.10.12 1024 device-name aaa 192.168.2.2 1024 china-ctc 100 5  OLT(config-interface-epon-0/0)# |

### Config Parameters for H.248 RTP TID of the ONU Voice Module

| Command | OLT(config-interface-epon-0/0)# ont voip h248-rtp-tid port-id ont-id number-of-RTP-TID PREFIX RTP-TID-Digit-Begin (alignment |no-alignment) RTP-TID-Digit-Length |
| --- | --- |
| **View** | EPON interface view |
| **Description** | This command is used for configure the H.248 RTP TID parameters of the ONU voice module. |
| port-id | PON port id,range for 1-16 |
| ont-id | ONT id,range for 1-64 |
| number-of-RTP-TID | Number of RTP-TID,range for 1-10 |
| PREFIX | Prefix of RTP-TID,support length for 1-16 |
| RTP-TID-Digit-Begin | The starting value of the digital part of RTP-TID,range for 0-99999999 |
| (alignment |no-alignment) | Digital partial alignment: alignment: alignment; no-alignment: not aligned |
| RTP-TID-Digit-Length | The number of digits in the RTP-TID digital part, ranging from 1 to 8. Note that the number of alignment digits is greater than or equal to the starting digit. For example, if the RTP-TID starting value is 555, the alignment digit is greater than or equal to 3. |

【Example】

Example1：Configure the H.248-RTP-TID parameter of the voice module of the PON11 port ONU1.

|  |
| --- |
| OLT(config-interface-epon-0/0)# ont voip h248-rtp-tid 11 1 1 aaa 1024 alignment 1  OLT(config-interface-epon-0/0)# |

### Config Parameters for H.248 User TID of the ONU Voice Module

| Command | OLT(config-interface-epon-0/0)# ont voip h248-user-tid port-id ont-id pots ONT-Pots-Number User-Tid |
| --- | --- |
| **View** | EPON interface view |
| **Description** | This command is used for configure the H.248 User TID parameter of the ONU voice module. |
| port-id | PON port id,range for 1-16 |
| ont-id | ONT id,range for 1-64 |
| ONT-Pots-Number | Number of ONT pots ,range for 1-2 |
| User-Tid | Name User-TID,support length 1-32 |

【Example】

Example1：Configure the H.248-User-TID parameter of the voice module of the PON11 port ONU1.

|  |
| --- |
| OLT(config-interface-epon-0/0)# ont voip h248-user-tid 11 1 pots 1 1  OLT(config-interface-epon-0/0)# |

### Config Thread Operation of the ONU Voice Module

| Command | OLT(config-interface-epon-0/0)# ont voip iad-operation port-id ont-id (log-off|re-registration|reset) |
| --- | --- |
| **View** | EPON interface view |
| **Description** | This command is used for configure the thread operation of the ONU voice module. |
| port-id | PON port id,range for 1-16 |
| ont-id | ONT id,range for 1-64 |
| (log-off|re-registration|reset) | Log-off: logout from the softswitch platform;  Re-registration: re-registration of the softswitch platform;  Reset: reset, only reset the voice module; |

【Example】

Example1：The thread operation of the voice module of the ONU1 of the PON11 port is configured to reset only the voice module.

|  |
| --- |
| OLT(config-interface-epon-0/0)# ont voip iad-operation 11 1 reset  OLT(config-interface-epon-0/0)# |

### Config Switch for VOIP Ports of ONU Voice Module

| Command | OLT(config-interface-epon-0/0)# ont voip pots-admin port-id ont-id pots ONT-Pots-Port-ID (enable|disable) |
| --- | --- |
| **View** | EPON interface view |
| **Description** | This command is used for configure the management of the VOIP module of the ONU voice module. |
| port-id | PON port id,range for 1-16 |
| ont-id | ONT id,range for 1-64 |
| ONT-Pots-Port-ID | Port id of ONTvoice port, range for 1-2 |

【Example】

Example1：Enable VOIP port 1 of the voice module of PON11 port ONU1.

|  |
| --- |
| OLT(config-interface-epon-0/0)# ont voip pots-admin 11 1 pots 1 enable  OLT(config-interface-epon-0/0)# |

### Config Parameters for SIP Protocol of ONU Voice Module

| Command | OLT(config-interface-epon-0/0)# ont voip sip-config port-id ont-id <MGPortNo> <SIP-Proxy-serverIP> <SIP-Proxy-Server-ComPortNo> <Backup-SIP-Proxy-ServerIP> <Backup-SIP-Proxy-Server-ComPortNo> <Sip-Register-ServerIP> <SIP-Register-Server-ComPortNo> <Backup-SIP-Register-ServerIP><Backup-SIP-Register-Server-ComPortNo> <OutBand-ServerIP> <OutBand-Server-ComPortNo> <SIP-Register-Interval> (enable|disable) <Heartbeat-cycle seconds> <Heartbeat-count> |
| --- | --- |
| **View** | EPON interface view |
| **Description** | This command is used for configure the voice parameters of the ONU voice module under the SIP protocol. |
| port-id | PON port id,range for 1-16 |
| ont-id | ONT id,range for 1-64 |
| <MGPortNo> | The port number of the media gateway,range for 1024-65535 |
| <SIP-Proxy-serverIP> | The IP address of the primary SIP proxy server, in the format X.X.X.X |
| <SIP-Proxy-Server-ComPortNo> | Port number of the primary SIP proxy server,range for 1024-65535 |
| <Backup-SIP-Proxy-ServerIP> | IP address of the alternate SIP proxy server,format as x.x.x.x |
| <Backup-SIP-Proxy-Server-ComPortNo> | The port number of the alternate SIP proxy server,range for 1024-65535 |
| <Sip-Register-ServerIP> | The IP address of the primary SIP registration server,format as X.X.X.X |
| <SIP-Register-Server-ComPortNo> | The port number of the primary SIP registration server,range for 1024-65535 |
| <Backup-SIP-Register-ServerIP> | IP address of the standby SIP registration server,format as X.X.X.X |
| <Backup-SIP-Register-Server-ComPortNo> | The port number of the standby SIP registration server,range for 1024-65535 |
| <OutBand-ServerIP> | The IP address of the outgoing server,format as x.x.x.x |
| <OutBand-Server-ComPortNo> | The port number of the outgoing server,range for 1024-65535 |
| <SIP-Register-Interval> | Register refresh cycle , the unit is s.The default is 3600s |
| <Heartbeat-cycle seconds> | Heartbeat cycle, the unit is s,range for为10-600，The default is 60s |
| <Heartbeat-count> | Number of heartbeats,range for 1-10，The default is 3. |

【Example】

Example1：Enable the parameters of the SIP protocol of the voice module of the PON11 port ONU1.

|  |
| --- |
| OLT(config-interface-epon-0/0)# ont voip sip-config 11 1 1024 192.168.2.12 1024 192.168.3.12 1024 1.1.1.1 1024 192.168.3.22 1024 192.168.2.22 1024 10 enable 10 2  OLT(config-interface-epon-0/0)# |

### Config Parameters for User SIP Protocol of the ONU Voice Module

| Command | OLT(config-interface-epon-0/0)# ont voip sip-user-config port-id ont-id pots ont-pots-port-id user-account user-name user-password |
| --- | --- |
| **View** | EPON interface view |
| **Description** | This command is used for configure the user parameters of the SIP protocol of the ONU voice module. |
| port-id | PON port id,range for 1-16 |
| ont-id | ONT id,range for 1-64 |
| ont-pots-port-id | ONU POTS port，range for1-2 |
| user-account | User phone number,support 1-16 characters |
| user-name | SIP port user. Support for 1-32 characters |
| user-password | SIPport password. Support for 1-16 characters |

【Example】

Example1：Configure the user parameters of the SIP protocol of the voice module of the PON5 port ONU1.

|  |
| --- |
| OLT(config-interface-epon-0/0)# ont voip sip-user-config 5 1 pots 1 555 test test  OLT(config-interface-epon-0/0)# |

### Show Basic Information about the ONU Voice Module.

|  |  |
| --- | --- |
| Command | OLT(config-interface-epon-0/0)# show ont voip iad-info port-id ont-id |
| **View** | Epon view |
| **Description** | This command is used for show information about the voice protocol, software version, and number of ports currently supported by the ONU voice module. |
| port-id | PON port id,range for 1-16 |
| ont-id | ONT id,range for 1-64 |

【Example】

Example 1：Show PON7 ONU7 voice module.

|  |
| --- |
| OLT(config-interface-epon-0/0)# show ont voip iad-info 7 7  -----------------------------------------------------------------------------  Frame/Slot : 0/0  Port : 7  ONT-ID : 7  iad mac-address : E0:67:B3:00:00:BB  protocolSupported : SIP  software-version : V1.0.1  software-time : 20180417111656  voip-pots-num : 2  -----------------------------------------------------------------------------  OLT(config-interface-epon-0/0)# |

### Show the POTS Port Status of the ONU Voice Module User.

| Command | OLT(config-interface-epon-0/0)# show ont voip pots-status port-id ont-id pots ont-pots-port-id |
| --- | --- |
| **View** | Epon view |
| **Description** | This command is used for show the POTS port status of the ONU voice module user. |
| port-id | PON port id,range for 1-16 |
| ont-id | ONT id,range for 1-64 |
| ONT-Pots-Port-ID | ONU POTS port，range for1-2 |

【Example】

Example 1：Show the POTS port status of the voice module user of the PON7 port ONU7.

|  |
| --- |
| OLT(config-interface-epon-0/0)# show ont voip pots-status 7 7 pots 1  -----------------------------------------------------------------------------  Frame/Slot : 0/0  Port : 7  ONT-ID : 1  POTS-ID : 1  Admin-state : Disable  IADPots-State : Notactivated  IADPots-ServiceState : Endlocal  IADPots-CodeMode : Unknown  -----------------------------------------------------------------------------  OLT(config-interface-epon-0/0)# |

### Show the Parameters of the Fax/Modem Service.

|  |  |
| --- | --- |
| Command | OLT(config-interface-epon-0/0)# show ont voip fax-modem port-id ont-id |
| **View** | Epon view |
| **Description** | This command is used for show the parameter configuration of the fax/modem service of the ONU voice module. |
| port-id | PON port id,range for 1-16 |
| ont-id | ONT id,range for 1-64 |

【Example】

Example 1：Show fax/modem service parameters of PON7 port ONU7.

|  |
| --- |
| OLT(config-interface-epon-0/0)# show ont voip fax-modem 7 7  -----------------------------------------------------------------------------  Frame/Slot : 0/0  Port : 7  ONT-ID : 7  FaxModem-Mode : T30  FaxModem-Control : Nego  -----------------------------------------------------------------------------  OLT(config-interface-epon-0/0)# |

### Show Global Parameters of the ONU Voice Module

|  |  |
| --- | --- |
| Command | OLT(config-interface-epon-0/0)# show ont voip global-config port-id ont-id |
| **View** | Epon view |
| **Description** | This command is used for show global parameters of the ONU voice module. |
| port-id | PON port id,range for 1-16 |
| ont-id | ONT id,range for 1-64 |

【Example】

Example 1：show global parameters of the PON7 ONU7 voice module.

|  |
| --- |
| OLT(config-interface-epon-0/0)# show ont voip global-config 7 7  -----------------------------------------------------------------------------  Frame/Slot : 0/0  Port : 7  ONT-ID : 7  Voice ip mode : static  Ip address : 0.0.0.0  Netmask : 0.0.0.0  Default gateway : 0.0.0.0  Voice tag-mode : transparent  Cvlan : 0  Svlan : 0  Priority : 0  -----------------------------------------------------------------------------  OLT(config-interface-epon-0/0)# |

### Show the Parameters of the H.248 Protocol of the ONU Voice Module

|  |  |
| --- | --- |
| Command | OLT(config-interface-epon-0/0)# show ont voip h248-config port-id ont-id |
| **View** | Epon view |
| **Description** | This command is used for show the parameters of the H.248 protocol of the ONU voice module. |
| port-id | PON port id,range for 1-16 |
| ont-id | ONT id,range for 1-64 |

【Example】

Example 1：Show the parameters of the H.248 protocol of the PON7 ONU7 voice module.

|  |
| --- |
| OLT(config-interface-epon-0/0)# show ont voip h248-config 7 7  -----------------------------------------------------------------------------  Frame/Slot : 0/0  Port : 7  ONT-ID : 7  H248Param-MGPortNum : 2944  H248Param-MGCIP : 0.0.0.0  H248Param-MgcComPortNo : 2944  H248Param-ActiveMGC : active  H248Param-regMode : ip Address  H248Param-mid :  H248Param-MGCBackupIP : 0.0.0.0  H248Param-MGCBackupComPortNo : 2944  H248Param-Heartbeatmode :  H248Param-Heartbeatcycle : 90  H248Param-Heartbeatcount : 0  -----------------------------------------------------------------------------  OLT(config-interface-epon-0/0)# |

### Show the Parameters of the H.248 RTP TID of the ONU Voice Module

|  |  |
| --- | --- |
| Command | OLT(config-interface-epon-0/0)# show ont voip h248-rtp-tid port-id ont-id |
| **View** | Epon view |
| **Description** | This command is used for show the parameter configuration under the H.248 RTP TID of the ONU voice module. But not to the onu query, for the query olt local configuration. Query RTP TID number, prefix, alignment and number of bits and other information. |
| port-id | PON port id,range for 1-16 |
| ont-id | ONT id,range for 1-64 |

【Example】

Example 1：Show the parameter configuration under H.248 RTP TID of the PON7 ONU7 voice module.

|  |
| --- |
| OLT(config-interface-epon-0/0)# show ont voip h248-rtp-tid 7 7  -----------------------------------------------------------------------------  Frame/Slot : 0/0  Port : 7  ONT-ID : 7  H248RtpTid-num : 1  H248RtpTid-prefix : test  H248RtpTid-digit : 1  H248RtpTid-mode : no-alignment  H248RtpTid-length : 8  -----------------------------------------------------------------------------  OLT(config-interface-epon-0/0)# |

### Show the Parameters of the H.248-rtp-tid-info of the ONU Voice Module

|  |  |
| --- | --- |
| Command | OLT(config-interface-epon-0/0)# show ont voip h248-rtp-tid-info port-id ont-id |
| **View** | Epon view |
| **Description** | This command is used for show the parameter configuration under H.248-rtp-tid-info of the ONU voice module, and query the RTP TID name. |
| port-id | PON port id,range for 1-16 |
| ont-id | ONT id,range for 1-64 |

【Example】

Example 1：Show the parameter configuration of H.248-rtp-tid-info on the PON7 ONU7 voice module.

|  |
| --- |
| OLT(config-interface-epon-0/0)# show ont voip h248-rtp-tid-info 7 7  -----------------------------------------------------------------------------  Frame/Slot : 0/0  Port : 7  ONT-ID : 7  H248RtpTid-num : 0  H248RtpTid-firstname : RTP/00000  -----------------------------------------------------------------------------  OLT(config-interface-epon-0/0)# |

### Show the H.248 User TID Parameters of the ONU Voice Module

| Command | OLT(config-interface-epon-0/0)# show ont voip h248-user-tid port-id ont-id pots ONT-Pots-Number |
| --- | --- |
| **View** | Epon view |
| **Description** | This command is used for shw the H.248 User TID parameters of the ONU voice module. |
| port-id | PON port id,range for 1-16 |
| ont-id | ONT id,range for 1-64 |
| ONT-Pots-Number | ONU POTS port，range for1-2 |

【Example】

Example 1：Show the H.248-User-TID parameter of the voice module of the PON7 ONU7.

|  |
| --- |
| OLT(config-interface-epon-0/0)# show ont voip h248-user-tid 7 7 pots 1  -----------------------------------------------------------------------------  Frame/Slot : 0/0  Port : 7  ONT-ID : 7  POTS-ID : 1  H248-UserTid : AG58900  -----------------------------------------------------------------------------  OLT(config-interface-epon-0/0)# |

### Show the Running Status of the IAD under the H.248 Protocol of the ONU Voice Module

| Command | OLT(config-interface-epon-0/0)# show ont voip iad-status port-id ont-id |
| --- | --- |
| **View** | Epon view |
| **Description** | This command is used for show the running status of the IAD under the H.248 protocol of the ONU voice module. |
| port-id | PON port id,range for 1-16 |
| ont-id | ONT id,range for 1-64 |
| ONT-Pots-Number | ONU POTS port，range for1-2 |

【Example】

Example 1:Show the running status of the IAD under the H.248 protocol of the voice module of the PON7 ONU7.

|  |
| --- |
| OLT(config-interface-epon-0/0)# show ont voip iad-status 7 7  -----------------------------------------------------------------------------  Frame/Slot : 0/0  Port : 7  ONT-ID : 7  iad state : re-registration  -----------------------------------------------------------------------------  OLT(config-interface-epon-0/0)# |

### Show the Parameters of the SIP Protocol of the ONU Voice Module

|  |  |
| --- | --- |
| Command | OLT(config-interface-epon-0/0)# show ont voip sip-config port-id ont-id |
| **View** | Epon view |
| **Description** | This command is used for show the parameters of the SIP protocol of the ONU voice module. |
| port-id | PON port id,range for 1-16 |
| ont-id | ONT id,range for 1-64 |

【Example】

Example 1：Show the parameters of the SIP protocol of the voice module of the PON7 ONU7.

|  |
| --- |
| OLT(config-interface-epon-0/0)# show ont voip sip-config 7 7  -----------------------------------------------------------------------------  Frame/Slot : 0/0  Port : 7  ONT-ID : 7  SipConfig-MGPort : 5060  SipConfig-proxyIp : 192.168.2.201  SipConfig-proxyPortNo : 5060  SipConfig-activeSipProxyServer : 192.168.2.201  SipConfig-outBoundIp : 192.168.2.201  SipConfig-outBoundPort : 5060  SipConfig-regIp : 192.168.2.201  SipConfig-regPortNo : 5060  SipConfig-regInterval : 3600s  SipConfig-backupProxyIp : 0.0.0.0  SipConfig-backupProxyPort : 5060  SipConfig-backupRegIp : 0.0.0.0  SipConfig-backupRegPort : 5060  SipConfig-Heartbeatmode : enable  SipConfig-Heartbeatcycle : 60  SipConfig-Heartbeatcount : 3  -----------------------------------------------------------------------------  OLT(config-interface-epon-0/0)# |

### Show the User Parameters of the SIP Protocol of the ONU Voice Module

| Command | OLT(config-interface-epon-0/0)# show ont voip sip-user-config port-id ont-id pots ONT-Pots-Number |
| --- | --- |
| **View** | Epon view |
| **Description** | This command is used for show the user parameters of the SIP protocol of the ONU voice module. |
| port-id | PON port id,range for 1-16 |
| ont-id | ONT id,range for 1-64 |
| ONT-Pots-Number | ONU POTS port，range for1-2 |

【Example】

Example 1：Show the user parameters of the SIP protocol of the voice module of the PON7 ONU7.

|  |
| --- |
| OLT(config-interface-epon-0/0)# show ont voip sip-user-config 7 7 pots 1  -----------------------------------------------------------------------------  Frame/Slot : 0/0  Port : 7  ONT-ID : 7  POTS-ID : 1  SipUser-account : 897  SipUser-user : 897  SipUser-password : 123456  -----------------------------------------------------------------------------  OLT(config-interface-epon-0/0)# |

## Config the DBA Queue Set of the ONU

### Config Queue Thresholds for DBA Queue Sets

| Command | OLT(config-interface-epon-0/0)# ont dba-threshold port-id ont-id Queue-set-index (q1 Threshold |q2 Threshold |q3 Threshold |q4 Threshold |q5 Threshold |q6 Threshold |q7 Threshold |q8 Threshold ) |
| --- | --- |
| **View** | Epon view |
| **Description** | This command is used for configure the queue threshold of the DBA queue set in the ONT line profile. Use this command when you need to configure the queue threshold of the DBA queue set in the ONT line profile. |
| port-id | PON port id,range for 1-16 |
| ont-id | ONT id,range for 1-64 |
| Queue-set-index | DBA queue set index,range for 1-4 |
| q1|q2|q3|q4|q5|q6|q7|q8 | DBA queue |
| Threshold | Threshold,range for 0-65535 |

【Example】

Example 1：Config the threshold bit 100 of DBA queue 1 of ONT1 on the PON5 interface.

|  |
| --- |
| OLT(config-interface-epon-0/0)# ont dba-threshold 5 1 1 q1 100  OLT(config-interface-epon-0/0)# |

### Delete queue thresholds for DBA queue sets

|  |  |
| --- | --- |
| Command | OLT(config-interface-epon-0/0)# no ont dba-threshold port-id ont-id |
| **View** | Epon view |
| **Description** | This command is used for delete queue threshold for DBA queue sets. |
| port-id | PON port id,range for 1-16 |
| ont-id | ONT id,range for 1-64 |

【Example】

Example 1：Delete the DBA queue sets of PON7 ONU1.

|  |
| --- |
| OLT(config-interface-epon-0/0)# no ont dba-threshold 7 1  Restore to the profile configuration successfully  OLT(config-interface-epon-0/0)# |

# OLT Log Management and Query

## Add Syslog Record Server

|  |  |
| --- | --- |
| Command | OLT(config)#loghost add <ip-address> <hostname> |
| **View** | Config view |
| **Description** | This command is used for add log server.Device will generate lots of log info when it is in running,but the storage space of device is limited,when it needs to set log server to collect the log info,using this command.After successful adding the log server,some of important log info of device will be recorded in this host by Syslog mechanism |
| <ip-address> | IP address of syslog server |
| <Hostname> | Name of syslog server.It used to distinct with other syslog server and uniquely identify the syslog server. |

【Example】

Example 1：Add syslog server,its ip is 192.168.1.223,server name is log.

|  |
| --- |
| OLT(config)#loghost add 192.168.1.223 log  OLT(config)# |

## Delete Syslog Record Server

|  |  |
| --- | --- |
| Command | OLT(config)#loghost delete ip <ip-address> name <hostname> |
| **View** | Config view |
| **Description** | This command is used for delete syslog server.when the syslog server is unnecessary or its ip address has been changed,this command can delete the log server.after that,we can add new log server or reset the old log server’s ip. |
| <ip-address> | IP address of syslog server |
| <Hostname> | Name of syslog server.It used to distinct with other syslog server and uniquely identify the syslog server. |

【Example】

Example 1：Delete the syslog server,its ip is 192.168.2.245,server name is test.

|  |
| --- |
| OLT(config)#loghost delete ip 192.168.2.245 name test  Delete syslog host successed!  OLT(config)# |

## Enable or Disable Syslog Record to Server

|  |  |
| --- | --- |
| Command | OLT(config)#loghost operlog {enable|disable} |
| **View** | Config view |
| **Description** | This command is used for set the switch of whether the olt log will transmit to log server. |
| {enable|disable} | Enable:olt log will transmit to log server  Disable:olt log will not transmit to log server |

【Example】

Example 1：olt log won’t transmit to log server

|  |
| --- |
| OLT(config)#loghost operlog disable  OLT(config)# |

## Enable or Disable Alarmlog Record to Server

|  |  |
| --- | --- |
| Command | OLT(config)#loghost alarmlog {enable|disable} |
| **View** | Config view |
| **Description** | This command is used for set the switch of whether the alarmlog of olt will transmit to log server. |
| {enable|disable} | Enable:alarmlog of olt will transmit to log server.  Disable:alarmlog of olt won’t transmit to log server. |

【Example】

Example 1：Set alarmlog of olt won’t transmit to log server.

|  |
| --- |
| OLT(config)#loghost alarmlog disable  OLT(config)# |

## Active Syslog Record server

|  |  |
| --- | --- |
| Command | OLT(config)#loghost activate ip<ip-address> name <hostname> |
| **View** | Config view |
| **Description** | This command is used for active the host of log server.When setting the control level of log host info output or it needs to active the switch of log output,using this command.System will report the log to the corresponding host only after the log host is active successfully. |
| <ip-address> | IP address of syslog server |
| <Hostname> | Name of syslog server.It used to distinct with other syslog server and uniquely identify the syslog server. |

【Example】

Example 1：Active the syslog server,its ip is 192.168.2.223,server name is loghost.

|  |
| --- |
| OLT(config)#loghost activate ip 192.168.2.223 name loghost  Activate syslog host successed!  OLT(config)# |

## Deactive Syslog Record Server

| Command | OLT(config)#loghost deactivate ip <ip-address> name <hostname> |
| --- | --- |
| **View** | Config view |
| **Description** | This command is used for deactive the host of log server.When an active log host is standing off and it needs to change the state of this log host,using this command.After setting,system won’t report the log info to the log host. |
| <ip-address> | IP address of syslog server |
| <Hostname> | Name of syslog server.It used to distinct with other syslog server and uniquely identify the syslog server. |

【Example】

Example 1：Deactive the syslog server,its ip is 192.168.2.223,server name is loghost.

|  |
| --- |
| OLT(config)#loghost deactivate ip 192.168.2.223 name loghost  Deactivate syslog host successed!  OLT(config)# |

## Show Syslog Record Server Config Status

|  |  |
| --- | --- |
| Command | OLT(config)#show loghost list |
| **View** | Config view |
| **Description** | This command is used for show the configuration info of loghost.including host ip address,host name,host state and etc. |

【Example】

Example 1：Show the configuration info of loghost

|  |
| --- |
| OLT(config)#show loghost list  ----------------------------------------------------------------------------  IP address Host name Terminal state  192.168.2.223 loghost active  ----------------------------------------------------------------------------  OLT(config)# |

## Backup OLT Log

| Command | OLT(config)#backup log ftp <server-ip-address> <user-name> <user-password> <filename> |
| --- | --- |
| **View** | Enable view,config view |
| **Description** | This command is used for save the log to ftp server by manually. |
| <server-ip-address> | IP address of ftp server |
| <user-name> | User name of ftp server |
| <user-password> | Password of ftp server |
| <filename> | The name of the backup log |

【Example】

Example 1：Save the log to ftp server 192.168.1.223,user name is admin,password is admin,file name is log.

|  |
| --- |
| OLT(config)#backup log ftp 192.168.1.223 admin admin logback  Start backup log files  The backup is successful |

## Erase OLT Log

|  |  |
| --- | --- |
| Command | OLT(config)#erase log |
| **View** | Config view |
| **Description** | This command is used for delete the log of olt |

【Example】

Example 1：Erase the log of olt.

|  |
| --- |
| OLT(config)#erase log  OLT(config)# |

## Show OLT Log

| Command | OLT(config)#show log |
| --- | --- |
| **View** | enable view,config view |
| **Description** | Show all the log of olt |

【Example】

Example 1：Show all the log of olt

|  |
| --- |
| OLT(config)#show log  2000/01/03 11:39:16[root@Console:13]logoff  2000/01/03 11:44:05[root@192.168.5.70:43]logoff  2000/01/03 12:33:20[root@192.168.5.70:43]logon via Telnet successfully  2000/01/03 12:33:21[192.168.5.70@root]cmd:enable  2000/01/03 12:33:22[192.168.5.70@root]cmd:config  2000/01/03 12:33:31[192.168.5.70@root]cmd:interface link-aggregation  2000/01/03 12:38:54[root@192.168.5.70:43]logoff  OLT(config)# |

# OLT Alarm Management and Query

## Clear Specified Active Alarm Entry

|  |  |
| --- | --- |
| Command | OLT(config)#alarm active clear <alarm-raising-number> |
| **View** | Config view |
| **Description** | This command is used for clear the specified active alarm entry |
| <alarm-raising-number> | Clear the active alarm according to alarm-raising-number.range for 1-4294967295.alarm-raising-number needs to use the follow command to show its detail info:  alarm output detail on  show alarm active all |

【Example】

Example 1：Clear active alarm 2.

|  |
| --- |
| OLT(config)#alarm active clear 2  OLT(config)# |

## Clear Active Alarm by Specified Alarmlevel

|  |  |
| --- | --- |
| Command | OLT(config)#alarm active clear alarmlevel<1-4> |
| **View** | Config view |
| **Description** | This command is used for clear active alarm by specified alarmlevel |
| <1-4> | 1. Critical 2. major 3. minor 4. warning |

【Example】

Example 1：Clear the warning active alarm

|  |
| --- |
| OLT(config)#alarm active clear alarmlevel 4  OLT(config)# |

## Clear Active Alarm by Specified Board

|  |  |
| --- | --- |
| Command | OLT(config)#alarm active clear alarmparameter board <F/S> |
| **View** | Config view |
| **Description** | This command is used for clear active alarm by specified board. |
| <F/S> | Frame/slot:the default is 0/0 |

【Example】

Example 1：Clear active alarm in 0/0.

|  |
| --- |
| OLT(config)#alarm active clear alarmparameter board 0/0  OLT(config)# |

## Clear Active Alarm by Specified GE Port

|  |  |
| --- | --- |
| Command | OLT(config)#alarm active clear alarmparameter ge <F/S/P> |
| **View** | Config view |
| **Description** | This command is used for clear active alarm by specified GE port |
| <F/S/P> | Frame/slot/ge port id,range for 0/0/1–0/0/8 |

【Example】

Example 1：Clear the active alarm of ge1.

|  |
| --- |
| OLT(config)#alarm active clear alarmparameter ge 0/0/1  OLT(config)# |

## Clear Active Alarm by Specified PON Port

| Command | OLT(config)#alarm active clear alarmparameter pon <F/S/P> |
| --- | --- |
| **View** | Config view |
| **Description** | This command is used for clear active alarm by specified pon port |
| <F/S/P> | Frame/slot/pon port id,range for 0/0/1–0/0/16 |

【Example】

Example 1：Clear the active alarm of pon 1.

|  |
| --- |
| OLT(config)#alarm active clear alarmparameter pon 0/0/1  OLT(config)# |

## Clear Active Alarm by Specified XGE Port

|  |  |
| --- | --- |
| Command | OLT(config)#alarm active clear alarmparameter xge <F/S/P> |
| **View** | Config view |
| **Description** | This command is used for clear active alarm by specified XGE port |
| <F/S/P> | Frame/slot/xge port id,range for 0/0/1–0/0/2 |

【Example】

Example 1：Clear the active alarm of xge 1.

|  |
| --- |
| OLT(config)#alarm active clear alarmparameter xge 0/0/1  OLT(config)# |

## Config Alarmlevel for Specified Alarm

| Command | OLT(config)#alarm alarmlevel<alarm-id> <1-4> |
| --- | --- |
| **View** | Config view |
| **Description** | This command is used for set alarmlevel for specified alarm |
| <alarm-id> | alarm-raising-number.range for 1-4294967295 |
| <0-4> | 1. Default 2. critical 3. major 4. minor 5. warning |

【Example】

Example 1：Set the alarmlevel of 102th alarm as 1(critical).

|  |
| --- |
| OLT(config)#alarm alarmlevel 102 1  OLT(config)# |

## Enable and Config Alarm Jitter-interval Time

|  |  |
| --- | --- |
| Command | OLT(config)#alarm jitter-interval<interval> |
| **View** | Config view |
| **Description** | This command is used for enable and set alarm jitter-interval.When this command is executed,alarm of the system will wait for a jitter-interval and then report it to network management,if the alarm state has recover during a jitter-interval,this alarm won’t be reported to network management. |
| <interval> | alarm interval,range for 1-60,unit is second. |

【Example】

Example 1：Set alarm jitter-interval as 3s.

|  |
| --- |
| OLT(config)#alarm jitter-interval 3  OLT(config)# |

## Enable or Disable Alarm Jitter-proof Function

| Command | OLT(config)#alarm jitter-proof (disable | enable） |
| --- | --- |
| **View** | Config view |
| **Description** | This command is used for turn on/off alarm jitter-proof function. |
| <switch> | Enable:turn on function  Disable：turn off function |

【Example】

Example 1：Turn off alarm jitter-proof function

|  |
| --- |
| OLT(config)#alarm jitter-proof disable  OLT(config)# |

## Enable or Disable Specified Alarm Record Output

|  |  |
| --- | --- |
| Command | OLT(config)#alarm output alarmid <alarm-id> {enable|disable} |
| **View** | Config view |
| **Description** | This command is enable and disable the specified alarm record output.When state is“enable”,permitting the specified alarm record reporting to EMS.When state is“disable”,denying the specified alarm record reporting to EMS. |
| <alarm-id> | alarm ID,the value range is 1-4294967294. |
| {enable|disable} | Enable:turn on function  Disable：turn off function |

【Example】

Example 1：Disable the 102 alarm record output.

|  |
| --- |
| OLT(config)#alarm output alarmid 102 disable  OLT(config)# |

## Enable or Disable Specified Level Alarm Output

| Command | OLT(config)#alarm output alarmlevel <alarmlevel> {enable|disable} |
| --- | --- |
| **View** | Config view |
| **Description** | This command is enable or disable the specified level alarm record output.When state is“enable”,permitting the specified level alarm record reporting to EMS.When state is“disable”,denying the specified level alarm record reporting to EMS. |
| <alarm-level> | 1. Critical 2. Major 3. Minor 4. Warning |
| {enable|disable} | Enable：turn on function  Disable：turn off function |

【Example】

Example 1：Disable level 4 alarm output.

|  |
| --- |
| OLT(config)#alarm output alarmlevel 4 disable  OLT(config)# |

## Enable or Disable All Alarms Output

|  |  |
| --- | --- |
| Command | OLT(config)#alarm output all {enable|disable} |
| **View** | Config view |
| **Description** | This command is enable or disable all alarm output.When state is“enable”,permitting all alarms reporting to EMS.When state is“disable”,denying all alarms reporting to EMS. |
| {enable|disable} | Enable：turn on function  Disable：turn off function |

【Example】

Example 1：Disable all alarms output.

|  |
| --- |
| OLT(config)#alarm output all disable  OLT(config)# |

## Enable or Disable Detail Alarm Output

|  |  |
| --- | --- |
| Command | OLT(config)#alarm output detail {enable|disable} |
| **View** | Config view |
| **Description** | This command is used for turn on or off alarm detail input function.When state is“on”,outputting detail alarm information.When state is“off”,outputting simple alarm information. |
| {enable|disable} | on：enable  off：disable |

【Example】

Example 1：Turn off alarm output detail information function.

|  |
| --- |
| OLT(config)#alarm output detail disable  OLT(config)# |

## Show Specified Active Alarm Record

|  |  |
| --- | --- |
| Command | OLT(config)#show alarm active alarmid <alarm-id> |
| **View** | Config view |
| **Description** | This command is use to view the specified active alarm record. |
| <alarm-id> | Alarm-ID,the value range is 1-4294967294. |

【Example】

Example 1：View active alarm record of alarm-id 204.

|  |
| --- |
| OLT(config)#show alarm active alarmid 204  ALARM 15 Major 204 2000-01-02 02:22:51  ALARM NAME:pon port link down  INSTANCE:PON FrameID:0,SlotID:0,PortID:3  REPEAT TIME:1  FIRST OCCUR:2000-01-02 02:22:51  LAST OCCUR:2000-01-02 02:22:51  DESCRIPTION:  total number:1  OLT(config)# |

## Show Active Alarm Logs by Specified Level

|  |  |
| --- | --- |
| Command | OLT(config)#show alarm active alarmlevel <1-4> |
| **View** | Config view |
| **Description** | This command is used for view active alarm logs of the specified level. |
| <1-4> | 1. Critical 2. major 3. minor 4. warning |

【Example】

Example 1：View active alarm logs of level 2.

|  |
| --- |
| OLT(config)#show alarm active alarmlevel 2  ALARM 15 Major 204 2000-01-02 02:22:51  ALARM NAME:pon port link down  INSTANCE:PON FrameID:0,SlotID:0,PortID:3  REPEAT TIME:1  FIRST OCCUR:2000-01-02 02:22:51  LAST OCCUR:2000-01-02 02:22:51  DESCRIPTION:  total number:1  OLT(config)# |

## Show Active Alarm Logs by Specified Board

|  |  |
| --- | --- |
| Command | OLT(config)#show alarm active alarmparameter board <F/S> |
| **View** | Config view |
| **Description** | This command is used for view active alarm logs of the specified board. |
| <F/S> | Card slot number,the value is 0/0. |

【Example】

Example 1：View active alarm logs of board 0/0.

|  |
| --- |
| OLT(config)#show alarm active alarmparameter board 0/0  ALARM 15 Major 204 2000-01-02 02:22:51  ALARM NAME:pon port link down  INSTANCE:PON FrameID:0,SlotID:0,PortID:3  REPEAT TIME:1  FIRST OCCUR:2000-01-02 02:22:51  LAST OCCUR:2000-01-02 02:22:51  DESCRIPTION:  total number:1  OLT(config)# |

## Show Active Alarm Logs by Specified GE Port

|  |  |
| --- | --- |
| Command | OLT(config)#show alarm active alarmparameter ge <F/S/P> |
| **View** | Config view |
| **Description** | This command is use to view active alarm logs of the specified GE port. |
| <F/S/P> | GE port number,the value range is 0/0/1–0/0/8. |

【Example】

Example 1：View active alarm logs of ge8 port.

|  |
| --- |
| OLT(config)#show alarm active alarmparameter ge 0/0/8  ALARM 18 Critical 203 2000-01-02 02:48:48  ALARM NAME:sni port link down  INSTANCE:GE FrameID:0,SlotID:0,PortID:8  REPEAT TIME:1  FIRST OCCUR:2000-01-02 02:48:48  LAST OCCUR:2000-01-02 02:48:48  DESCRIPTION:  total number:1  OLT(config)# |

## Show Active Alarm Logs by Specified PON Port

|  |  |
| --- | --- |
| Command | OLT(config)#show alarm active alarmparameter pon <F/S/P> |
| **View** | Config view |
| **Description** | This command is used for view active alarm logs of the specified PON port. |
| <F/S/P> | Pon port number,the value range is 0/0/1–0/0/16. |

【Example】

Example 1：View active alarm logs of pon 3 port

|  |
| --- |
| OLT(config)#show alarm active alarmparameter pon 0/0/3  ALARM 15 Major 204 2000-01-02 02:22:51  ALARM NAME:pon port link down  INSTANCE:PON FrameID:0,SlotID:0,PortID:3  REPEAT TIME:1  FIRST OCCUR:2000-01-02 02:22:51  LAST OCCUR:2000-01-02 02:22:51  DESCRIPTION:  total number:1  OLT(config)# |

## Show Active Alarm Logs by Specified XGE Port

|  |  |
| --- | --- |
| Command | OLT(config)#show alarm active alarmparameter xge <F/S/P> |
| **View** | Config view |
| **Description** | This command is used for view active alarm logs of the specified XGE port. |
| <F/S/P> | Card slot number,the value range is 0/0/1–0/0/2. |

【Example】

Example 1：View active alarm logs of xge1 port.

|  |
| --- |
| OLT(config)#show alarm active alarmparameter xge 0/0/1  ALARM 26 Critical 131082 2000-01-02 04:18:33  ALARM NAME:The sni port is unpluged  INSTANCE:XGE FrameID:0,SlotID:0,PortID:1  REPEAT TIME:1  FIRST OCCUR:2000-01-02 04:18:33  LAST OCCUR:2000-01-02 04:18:33  DESCRIPTION:  total number:1  OLT(config)# |

## Show All Active Alarm Log

|  |  |
| --- | --- |
| Command | OLT(config)#show alarm active all |
| **View** | Config view |
| **Description** | This command is used for view all alarm active logs. |

【Example】

Example 1：View all alarm active logs.

|  |
| --- |
| OLT(config)#show alarm active all  ALARM 28 Critical 131082 2000-01-02 04:18:53  ALARM NAME:The sni port is unpluged  INSTANCE:XGE FrameID:0,SlotID:0,PortID:2  DESCRIPTION:  ALARM 26 Critical 131082 2000-01-02 04:18:33  ALARM NAME:The sni port is unpluged  INSTANCE:XGE FrameID:0,SlotID:0,PortID:1  DESCRIPTION:  ALARM 23 Critical 203 2000-01-02 04:17:40  ALARM NAME:sni port link down  INSTANCE:GE FrameID:0,SlotID:0,PortID:5  DESCRIPTION:  ALARM 18 Critical 203 2000-01-02 02:48:48  ALARM NAME:sni port link down  INSTANCE:GE FrameID:0,SlotID:0,PortID:8  DESCRIPTION:  ALARM 15 Major 204 2000-01-02 02:22:51  ALARM NAME:pon port link down  INSTANCE:PON FrameID:0,SlotID:0,PortID:3  DESCRIPTION:  total number:5  OLT(config)# |

## Show Specified Alarm History Record

|  |  |
| --- | --- |
| Command | OLT(config)#show alarm history alarmid<alarm-id> |
| **View** | Config view |
| **Description** | This command is used for view the specified alarm history records |
| <alarm-id> | Alarm ID,the value range is 1-4294967294. |

【Example】

Example 1：View alarm history records of alarm-ID 204.

|  |
| --- |
| OLT(config)#show alarm history alarmid 204  ALARM 35 Cleared 204 2000-01-02 07:05:07  ALARM NAME:pon port link up  INSTANCE:PON FrameID:0,SlotID:0,PortID:1  DESCRIPTION:  ALARM 34 Major 204 2000-01-02 07:02:33  ALARM NAME:pon port link down  INSTANCE:PON FrameID:0,SlotID:0,PortID:1  DESCRIPTION:  ALARM 32 Cleared 204 2000-01-02 07:01:39  ALARM NAME:pon port link up  INSTANCE:PON FrameID:0,SlotID:0,PortID:1  DESCRIPTION: |

## Show Alarm History Record by Specified Level

|  |  |
| --- | --- |
| Command | OLT(config)#show alarm history alarmlevel<1-4> |
| **View** | Config view |
| **Description** | This command is used for view alarm history records of the specified level. |
| <1-4> | 1. Critical 2. major 3. minor 4. warning |

【Example】

Example 1：View alarm history records of level 4.

|  |
| --- |
| OLT(config)#show alarm history alarmlevel 4  ALARM 38 Cleared 401 2000-01-02 07:07:06  ALARM NAME:uni link up  INSTANCE:FrameID:0,SlotID:0,PortID:1,OnuID:4,SlotID:0,Uni:1  DESCRIPTION:  ALARM 37 Warning 401 2000-01-02 07:06:57  ALARM NAME:uni link down  INSTANCE:FrameID:0,SlotID:0,PortID:1,OnuID:4,SlotID:0,Uni:1  DESCRIPTION:  ALARM 30 Cleared 401 2000-01-02 05:57:49  ALARM NAME:uni link up  INSTANCE:FrameID:0,SlotID:0,PortID:1,OnuID:3,SlotID:0,Uni:1  DESCRIPTION: |

## Show Alarm History Record by Specified Board

|  |  |
| --- | --- |
| Command | OLT(config)#show alarm history alarmparameter board <F/S> |
| **View** | Config view |
| **Description** | This command is used for view alarm history records of the specified board. |
| <F/S> | Card slot number,the value is 0/0. |

【Example】

Example 1：View alarm history records of board 0/0.

|  |
| --- |
| OLT(config)#show alarm history alarmparameter board 0/0  ALARM 38 Cleared 401 2000-01-02 07:07:06  ALARM NAME:uni link up  INSTANCE:FrameID:0,SlotID:0,PortID:1,OnuID:4,SlotID:0,Uni:1  DESCRIPTION:  ALARM 37 Warning 401 2000-01-02 07:06:57  ALARM NAME:uni link down  INSTANCE:FrameID:0,SlotID:0,PortID:1,OnuID:4,SlotID:0,Uni:1  DESCRIPTION:  ALARM 36 Critical 403 2000-01-02 07:05:47  ALARM NAME:Onu ethernet port autoNegotiation failure  INSTANCE:FrameID:0,SlotID:0,PortID:1,OnuID:5,SlotID:0,Uni:1  DESCRIPTION: |

## Show Alarm History Record by Specified GE Port

|  |  |
| --- | --- |
| Command | OLT(config)#show alarm history alarmparameter ge <F/S/P> |
| **View** | Config view |
| **Description** | This command is used for view alarm history records of the specified GE port |
| <F/S/P> | GE port number,the value range is 0/0/1–0/0/8. |

【Example】

Example 1：View alarm history records of ge8 port.

|  |
| --- |
| OLT(config)#show alarm history alarmparameter ge 0/0/8  ALARM 18 Critical 203 2000-01-02 02:48:48  ALARM NAME:sni port link down  INSTANCE:GE FrameID:0,SlotID:0,PortID:8  DESCRIPTION:  ALARM 17 Cleared 203 2000-01-02 02:48:05  ALARM NAME:sni port link up  INSTANCE:GE FrameID:0,SlotID:0,PortID:8  DESCRIPTION: |

## Show Alarm History Record by Specified PON Port

|  |  |
| --- | --- |
| Command | OLT(config)#show alarm history alarmparameter pon <F/S/P> |
| **View** | Config view |
| **Description** | This command is used for view alarm history records of the specified PON port. |
| <F/S/P> | Pon port number,the value range is 0/0/1–0/0/16. |

【Example】

Example 1：View alarm history records of pon1 port.

|  |
| --- |
| OLT(config)#show alarm history alarmparameter pon 0/0/1  ALARM 40 Cleared 401 2000-01-02 23:42:34  ALARM NAME:uni link up  INSTANCE:FrameID:0,SlotID:0,PortID:1,OnuID:4,SlotID:0,Uni:1  DESCRIPTION:  ALARM 39 Warning 401 2000-01-02 23:42:31  ALARM NAME:uni link down  INSTANCE:FrameID:0,SlotID:0,PortID:1,OnuID:4,SlotID:0,Uni:1  DESCRIPTION: |

## Show Alarm History Record by Specified XGE Port

|  |  |
| --- | --- |
| Command | OLT(config)#show alarm history alarmparameter xge <F/S/P> |
| **View** | Config view |
| **Description** | This command is used for view alarm history records of the specified XGE port. |
| <F/S/P> | Card slot number,the value range is 0/0/1–0/0/2. |

【Example】

Example 1：View alarm history records of xge1 port.

|  |
| --- |
| OLT(config)#show alarm history alarmparameter xge 0/0/1  ALARM 26 Critical 131082 2000-01-02 04:18:33  ALARM NAME:The sni port is unpluged  INSTANCE:XGE FrameID:0,SlotID:0,PortID:1  DESCRIPTION:  ALARM 25 Cleared 131082 2000-01-02 04:18:15  ALARM NAME:The sni port is pluged  INSTANCE:XGE FrameID:0,SlotID:0,PortID:1  DESCRIPTION: |

## Show All Alarm History Record

|  |  |
| --- | --- |
| Command | OLT(config)#show alarm history all |
| **View** | Config view |
| **Description** | This command is use to view all alarm history records. |

【Example】

Example 1：View all alarm history records.

|  |
| --- |
| OLT(config)#show alarm history all  ALARM 40 Cleared 401 2000-01-02 23:42:34  ALARM NAME:uni link up  INSTANCE:FrameID:0,SlotID:0,PortID:1,OnuID:4,SlotID:0,Uni:1  DESCRIPTION:  ALARM 39 Warning 401 2000-01-02 23:42:31  ALARM NAME:uni link down  INSTANCE:FrameID:0,SlotID:0,PortID:1,OnuID:4,SlotID:0,Uni:1  DESCRIPTION: |

## Show Alarm Jitter-proof Interval Time

|  |  |
| --- | --- |
| Command | OLT(config)#show alarm jitter |
| **View** | Config view |
| **Description** | This command is used for view alarm jitter-proof interval. |

【Example】

Example 1：View OLT’s alarm jitter-proof interval

|  |
| --- |
| OLT(config)#show alarm jitter  Jitter-Interval:5s  OLT(config)# |

## Show Alarm Basic Information

|  |  |
| --- | --- |
| Command | OLT(config)#show alarm list |
| **View** | Config view |
| **Description** | This command is used for view alarm basic information. |

【Example】

Example 1：View OLT’s alarm basic information.

|  |
| --- |
| OLT(config)#show alarm list  ----------------------------------------------------------------------------  AlarmId Output Level Def Level Name  102 Yes Major Major The board reset  104 Yes Warning Warning The temperature is abnormal  105 Yes Major Major The fan is abnormal  107 Yes Major Major The device power fault  201 Yes Critical Critical Pon port loopback link  202 Yes Major Major Pon los alarm raise  203 Yes Critical Critical sni port link down  204 Yes Major Major pon port link down  205 Yes Warning Warning The number of register llid is exceeded  206 Yes Major Major long luminescence  301 Yes Major Major onu critical event  302 Yes Warning Warning onu exchange key fails  303 Yes Critical Critical onu oam timeout  304 Yes Major Major onu mac auth fails  305 Yes Minor Minor the RX received power of the epon optical port is lower than the lower threshold  306 Yes Minor Minor the RX received power of the epon optical port is higher than the higher threshold  307 Yes Minor Minor the TX output power of the epon optical port is lower than the lower threshold  308 Yes Minor Minor the TX output power of the epon optical port is higher than the higher threshold  310 Yes Warning Warning onu power down  311 Yes Minor Minor the downstream BER is higher than threshold  312 Yes Minor Minor the downstream FER is higher than threshold  313 Yes Minor Minor the upstream BER is higher than threshold  314 Yes Minor Minor the upstream FER is higher than threshold  315 Yes Major Major The performance statistics upper crossed  316 Yes Major Major The performance statistics lower crossed  317 Yes Minor Minor the temperature of the optical module is higher than the higher threshold  318 Yes Minor Minor the temperature of the optical module is lower than the lower threshold  319 Yes Minor Minor the voltage of the optical module is higher than the higher threshold  320 Yes Minor Minor the voltage of the optical module is lower than the lower threshold  321 Yes Warning Warning onu optical down  401 Yes Warning Warning uni link down  402 Yes Minor Minor loopback of onu port is detected  403 Yes Critical Critical Onu ethernet port autoNegotiation failure  131082 Yes Critical Critical The sni port is unpluged  131083 Yes Critical Critical Sni port loopback link  ----------------------------------------------------------------------------  OLT(config)# |

# OLT Event Management and Query

## Config Event Level

|  |  |
| --- | --- |
| Command | OLT(config)#event eventlevel <event-id> <0-4> |
| **View** | Config view |
| **Description** | This command is used for configure the specified event level. |
| <event-id> | Event ID,only on behalf of one event alarm |
| <0-4> | 1. Default 2. critical 3. major 4. Minor 5. Warning |

【Example】

Example 1：Configure event level 3 for event ID 10001

|  |
| --- |
| OLT(config)#event eventlevel 10001 3  OLT(config)# |

## Enable or Disable All Events Output

|  |  |
| --- | --- |
| Command | OLT(config)#event output all {enable|disable} |
| **View** | Config view |
| **Description** | This command is used for configure all event output in the CLI.When state is“enable”,all events can output in the CLI,or it can’t be |
| {enable|disable} | Enable:turn on function  Disable:turn off function |

【Example】

Example 1：Turn off all events output function.

|  |
| --- |
| OLT(config)#event output all disable  OLT(config)# |

## Enable or Disable Detail Event Output

|  |  |
| --- | --- |
| Command | OLT(config)#event output detail {on|off} |
| **View** | Config view |
| **Description** | This command is used for set the switch of event output detail function.When state is“on”,events can all output detail in the CLI.When state is“off”,thus outputting simple event information. |
| {on|off} | on：enable  off：disable |

【Example】

Example 1：Turn on event output detail function.

|  |
| --- |
| OLT(config)#event output detail on  OLT(config)# |

## Enable or Disable Specified Event Output

|  |  |
| --- | --- |
| Command | OLT(config)#event output eventid <eventid> {enable|disable} |
| **View** | Config view |
| **Description** | This command is used for permit or deny the output of the specified event.When state is“enable”,permitting the output of the specified event in the terminal;when state is“disable”,denying the output of the specified event in the terminal. |
| <eventid> | Event ID,the value range is 1-4294967294. |
| {enable|disable} | Enable:turn on function  Disable:turn off function |

【Example】

Example 1：Permit event 10001 output in the terminal.

|  |
| --- |
| OLT(config)#event output eventid 10001 enable  OLT(config)# |

## Enable or Disable Specified Level Event Output

|  |  |
| --- | --- |
| Command | OLT(config)#event output eventlevel <eventlevel> {enable|disable} |
| **View** | Config view |
| **Description** | This command is used for permit or deny the output of the specified level event.When state is“enable”,permitting the specified level event output in the terminal;when state is“disable”,denying the specified level event output in the terminal. |
| <eventlevel> | 1. Critical 2. Major 3. Minor 4. Warning |
| {enable|disable} | Enable：turn on function  Disable：turn off function |

【Example】

Example 1：Permit the event output of the level 3.

|  |
| --- |
| OLT(config)#event output eventlevel 3 enable  OLT(config)# |

## Show All Event History Record

|  |  |
| --- | --- |
| Command | OLT(config)#show event history all |
| **View** | Config view |
| **Description** | This command is used for view all event history records. |

【Example】

Example 1：View all event history event records.

|  |
| --- |
| OLT(config)#show event history all  EVENT 13 Warning 13002 2000-01-02 07:05:56  EVENT NAME:onu is offline  INSTANCE:FrameID:0,SlotID:0,PortID:1,OnuID:5  EVENT 12 Warning 13001 2000-01-02 07:05:43  EVENT NAME:onu is online  INSTANCE:FrameID:0,SlotID:0,PortID:1,OnuID:5 |

## Show Specified Event History Record

|  |  |
| --- | --- |
| Command | OLT(config)#show event history eventid <eventid> |
| **View** | Config view |
| **Description** | This command is used for view history record of the specified event. |
| <eventid> | Event ID,the value range is 1-4294967294. |

【Example】

Example 1：View history record of event 13002.

|  |
| --- |
| OLT(config)#show event history eventid 13002  EVENT 14 Warning 13002 2000-01-03 05:27:27  EVENT NAME:onu is offline  INSTANCE:FrameID:0,SlotID:0,PortID:1,OnuID:4  DESCRIPTION:E067B312118A00012770  EVENT 13 Warning 13002 2000-01-02 07:05:56  EVENT NAME:onu is offline  INSTANCE:FrameID:0,SlotID:0,PortID:1,OnuID:5  DESCRIPTION:E067B300000100012770 |

## Show Specified Level Event History Record

| Command | OLT(config)#show event history eventlevel <eventlevel> |
| --- | --- |
| **View** | Config view |
| **Description** | This command is used for view history record of the specified level event. |
| <eventlevel> | 1. Critical 2. Major 3. Minor 4. Warning |

【Example】

Example 1：View history records of event level 4.

|  |
| --- |
| OLT(config)#show event history event level 4  EVENT 14 Warning 13002 2000-01-03 05:27:27  EVENT NAME:onu is offline  INSTANCE:FrameID:0,SlotID:0,PortID:1,OnuID:4  DESCRIPTION:E067B312118A00012770  EVENT 13 Warning 13002 2000-01-02 07:05:56  EVENT NAME:onu is offline  INSTANCE:FrameID:0,SlotID:0,PortID:1,OnuID:5  DESCRIPTION:E067B300000100012770 |

## Show Event History Record by Specified Board

|  |  |
| --- | --- |
| Command | OLT(config)#show event history eventparameter board <F/S> |
| **View** | Config view |
| **Description** | This command is used for view the history records of the specified board |
| <F/S> | Board number,the value is 0/0. |

【Example】

Example 1：View the event history records of the specified board 0/0.

|  |
| --- |
| OLT(config)#show event history eventparameter board 0/0  EVENT 14 Warning 13002 2000-01-03 05:27:27  EVENT NAME:onu is offline  INSTANCE:FrameID:0,SlotID:0,PortID:1,OnuID:4  DESCRIPTION:E067B312118A00012770  EVENT 13 Warning 13002 2000-01-02 07:05:56  EVENT NAME:onu is offline  INSTANCE:FrameID:0,SlotID:0,PortID:1,OnuID:5  DESCRIPTION:E067B300000100012770 |

## Show Event History Record by Specified GE Port

|  |  |
| --- | --- |
| Command | OLT(config)#show event history eventparameter ge <F/S/P> |
| **View** | Config view |
| **Description** | This command is used for view the event history record of the specified GE port. |
| <F/S/P> | GE port number,the value range is 0/0/1–0/0/8. |

【Example】

Example 1：View the event history record of the specified ge8 port.

|  |
| --- |
| OLT(config)#show event history eventparameter ge 0/0/8  total number:0  OLT(config)# |

## Show Event History Record by Specified PON Port

|  |  |
| --- | --- |
| Command | OLT(config)#show event history eventparameter pon <F/S/P> |
| **View** | Config view |
| **Description** | This command is used for view the event history records of the specified PON port |
| <F/S/P> | Pon port number,the value range is 0/0/1–0/0/16. |

【Example】

Example 1：View the event history records of the pon1 port.

|  |
| --- |
| OLT(config)#show event history eventparameter pon 0/0/3  EVENT 7 Warning 13002 2000-01-02 02:22:51  EVENT NAME:onu is offline  INSTANCE:FrameID:0,SlotID:0,PortID:3,OnuID:2  DESCRIPTION:E067B301010100012770  EVENT 6 Warning 13001 2000-01-02 02:22:40  EVENT NAME:onu is online  INSTANCE:FrameID:0,SlotID:0,PortID:3,OnuID:2  DESCRIPTION:E067B301010100012708 |

## Show Event History Record by Specified XGE Port

|  |  |
| --- | --- |
| Command | OLT(config)#show event history eventparameter xge<F/S/P> |
| **View** | Config view |
| **Description** | This command is used for view the event history records of the specified XGE port |
| <F/S/P> | Slot number,the value range is 0/0/1-0/0/2. |

【Example】

Example 1：View the event history records of xge1 port.

|  |
| --- |
| OLT(config)#show event history eventparameter xge 0/0/2  total number:0  OLT(config)# |

## Show Event Basic Information

|  |  |
| --- | --- |
| Command | OLT(config)#show event list |
| **View** | Config view |
| **Description** | This command is used for view the basic information of the event. |

【Example】

Example 1：view the basic information of the event

|  |
| --- |
| OLT(config)#show event list  ----------------------------------------------------------------------------  EventId Output Level Def Level Name  10001 Yes Minor Warning The device reset  13001 Yes Warning Warning onu is online  13002 Yes Warning Warning onu is offline  ----------------------------------------------------------------------------  OLT(config)# |

# Device Diagnostic Management

## Ping Diagnostic Test

|  |  |
| --- | --- |
| Command | OLT(config)#ping {<destination-ip>|<hostname>} |
| **View** | Any view |
| **Description** | This command is used for testing network accessibility between device and target host. |
| <destination-ip> | Destination IP address.There are five kinds of IP address,user can choose suitable IP address according to factual circumstance.Host IP address is not all 0 or 1,format for x.x.x.x. |
| <hostname> | Destination hostname |

【Example】

Example 1：Ping destination IP address 192.168.5.50

|  |
| --- |
| OLT(config)#ping 192.168.5.50  PING 192.168.5.50(192.168.5.50):56 data bytes  64 bytes from 192.168.5.50:seq=0 ttl=64 time=0.449 ms  64 bytes from 192.168.5.50:seq=1 ttl=64 time=0.379 ms  64 bytes from 192.168.5.50:seq=2 ttl=64 time=0.365 ms  64 bytes from 192.168.5.50:seq=3 ttl=64 time=0.612 ms  ---192.168.5.50 ping statistics---  4 packets transmitted,4 packets received,0%packet loss  round-trip min/avg/max=0.365/0.451/0.612 ms  OLT(config)# |

## 28.2 Traceroute Diagnostic Test

| Command | OLT(config)#traceroute {<destination-ip>|<hostname>} hops <hops-id> timeout <time-id> ttl <ttl-id> |
| --- | --- |
| **View** | Any view |
| **Description** | Through traceroute,you can know about data packet transmission path from this host to the other end host |
| <Destination-IP> | Destination IP address.There are five kinds of IP address,user can choose suitable IP address according to factual circumstance.Host IP address is not all 0 or 1,format for x.x.x.x. |
| <Hostname> | Destination hostname |
| <hops-id> | Passed max router numbers that data messages arrive final host |
| <time-id> | Wait for the time(unit millisecond)specified by timeout for each response |
| <ttl-id> | Data packet Time-To-Live |

【Example】

Example 1：traceroute destination IP address 192.168.5.50

|  |
| --- |
| OLT(config)#traceroute 192.168.5.50  traceroute to 192.168.5.50(192.168.5.50),30 hops max,38 byte packets  1 192.168.5.50 0.954 ms 0.473 ms 0.189 ms  OLT(config)# |

# 

# Appendix 1

**The processing of messages in different VLAN modes is as follows:**

|  |  |  |  |
| --- | --- | --- | --- |
| VLAN mode | Actions(in the inbound direction) | | Actions(in the  outbound direction) |
| **Untagged frame** | **Tagged frame** |
| Access | Tag the frame with  the native VLAN  tag. | * Drop the frame if its VLAN id is the same as the native VLAN id.   Drop the frame if its VLAN id is different from the native VLAN id | Remove the native VLAN  tag and send the frame |
| Trunk | Tag the frame with  native VLAN tag. | * Receive the frame if its VLAN is carried on the port   Drop the frame if its VLAN is not carried on the port. | * Send the frame and removing the tag if the frame is the same as native VLAN id. * Send the frame without removing the tag if its VLAN is carried on the port but is different from the native VLAN. |
| Hybrid | Send the frame if its VLAN is carried on the port.The  frame is sent with the VLAN tag removed or intact depending on your configuration with the VLAN hybrid command. |

# Concluding Remarks

Thanks for choosing our company products!